PRODUCT NAME:  VAX LN03 Image Support Software,         SSA 31.52.00-A
               Version 1.0 

HARDWARE REQUIREMENTS 

Processors Supported

VAXstation:  	  VAXstation 3200, VAXstation 3520/3540, VAXstation 3500, 
                  VAXstation II, VAXstation 8000 

Processors Not Supported

VAXstation:  	  VAXstation 3100, VAXstation 2000

Other Hardware Required

LN03 Image Laser Printer 

LNV21-xx Q-bus controller

Block Space Requirements (Block Cluster Size = 1):

Disk space required for installation:			     3,000 blocks
							    (1536K bytes)

Disk space required for use (permanent):		     2,640 blocks
							    (1351K bytes)

These block counts refer to the disk space required on the system disk. 
The sizes are approximate; actual sizes may vary depending on the user's 
system environment, configuration, and software options selected.

OPTIONAL HARDWARE

MD300-xx VAXimage Scanning Subsystem

VAXCLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid and 
licensed VAXcluster* configuration without restrictions.  The HARDWARE 
REQUIRMENTS sections of this product's Software Product Description and 
System Support Addendum detail any special hardware required by this 
product

* V5.x VAXcluster configurations are fully described in the VAXcluster 
  Software Product Description (29.78.xx) and include CI, Ethernet, and 
  Mixed Interconnect configurations.

SOFTWARE REQUIREMENTS

VMS Operating System V5.1

VAX ScriptPrinter Software V2.1

OPTIONAL SOFTWARE

VAXimage Scanning Application V1.0 

VAXimage Application Services for VMS V1.0

VAX Distributed Queuing Service V1.1 

VMS Tailoring

For VMS 5.x systems, the following classes of VMS are required for full 
functionality of this layered product:

^ VMS Required Saveset

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of    
this product may be different from the minimum requirements for the     
current version.                                                        
                                                                           
DISTRIBUTION MEDIA
                            
Tape:	  9-track 1600 BPI Magtape, TK50 Streaming Tape 

ORDERING INFORMATION

Software Licenses:  QL-VZRA*-**
Software Media: QA-VZRA*-**
Software Documentation: QA-VZRAA-GZ
Software Product Services: QT-VZRA*-**

* Denotes variant fields.  For additional information on available 
  licenses, services and media, refer to the appropriate price book.

The above information is valid at time of release.  Please contact your 
local DIGITAL office for the most up-to-date information.

