LAN Traffic Monitor for VMS, Version 1.2			SSA 27.80.02-A

HARDWARE REQUIREMENTS

Processors Supported
    
VAX:	 VAX 6000 Model 200 Series, VAX 6000 Model 300 Series, VAX 6000 
         Model 400 Series

	 VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500, VAX 8530, VAX 
         8550, VAX 8600, VAX 8650, VAX 8700, VAX 8800, VAX 8810, VAX 8820, 
         VAX 8830, VAX 8840, VAX 8842, VAX 8974, VAX 8978

	 VAX-11/750, VAX-11/780, VAX-11/785

MicroVAX:	   MicroVAX II, MicroVAX 2000, MicroVAX 3100, MicroVAX 
                   3300, MicroVAX 3400, MicroVAX 3500, MicroVAX 3600, 
                   MicroVAX 3800, MicroVAX 3900

VAXstation:	   VAXstation II, VAXstation 2000, VAXstation 3100 Series, 
                   VAXstation 3200, VAXstation 3500, VAXstation 3520, 
                   VAXstation 3540, VAXstation 8000
                                                      
VAXserver:	   VAXserver 3100, VAXserver 3300, VAXserver 3400, 
                   VAXserver 3500, VAXserver 3600, VAXserver 3602, 
                   VAXserver 3800, VAXserver 3900, VAXserver 6000-210, 
                   VAXserver 6000-310, VAXserver 6000-410, VAXserver 
                   6000-420

Processors Not Supported

VAX:	 VAX-11/725, VAX-11/730, VAX-11/782 

MicroVAX:	   MicroVAX I

VAXstation:	   VAXstation I, VAXstation 8000

Other Hardware Requirements

oo   A VT24x, VT330, or VT340 Terminal is required to display color graphics 
    for systems with no DECwindows interface.

oo   To run the Listener, one of the following is required:

    A LAN Bridge 100 with ROM ECO Revision E or later

    A LAN Bridge 150

    A Chipcom (TM) Ethermodem (TM) III Bridge [Part Numbers 8318BS
    (18Mhz) or 8312BS (12 Mhz)

Block Space Requirements (Block Cluster Size = 1):

Disk space required for installation:
						      1,100 blocks
						      (0.55M bytes)

Disk space required for use (permanent):
						      600 blocks
						      (0.3M bytes)

These counts refer to the disk space required on the system disk.  The 
sizes are approximate; actual sizes may vary depending on the user's system 
environment, configuration, and software options. 

CLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid and 
licensed VAXcluster* configuration without restrictions.  The HARDWARE 
REQUIREMENTS sections of this product's Software Product Description and 
System Support Addendum detail any special hardware required by this 
product.

*   V5.x VAXcluster configurations are fully described in the VAXcluster 
    Software Product Description (29.78.xx) and include CI, Ethernet, and 
    Mixed Interconnect configurations.

SOFTWARE REQUIREMENTS

oo   VMS Operating System V5.2 - V5.3

oo   DECnet-VAX V5.2 - V5.3

VMS Tailoring 

For VMS V5.x systems, the following VMS classes are required for full 
functionality of this layered product: 

oo   VMS Required Saveset

oo   Network Support

oo   Programming Support

oo   Secure User's Environment

oo    Utilities

For more information on VMS classes and tailoring, refer to the VMS 
Operating System Software Product Description (25.01.xx). 

OPTIONAL SOFTWARE

oo   Remote Bridge Management Software (RBMS) V2.0 

oo   NMCC/VAX ETHERnim V2.2
 
For more information refer to the RBMS Software Product Description (SPD 
27.12.xx) and NMCC/VAX ETHERnim Software Product Description (SPD 
26.96.xx).

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of this 
product may be different from the minimum requirements for the current 
version. 

Additional LAN Bridge units can be purchased and configured with LTM 
Listener software after LAN Traffic Monitor VMS has been installed.  By 
creating a separate VMS process (or subprocess), a single user account on 
the VAX host may simultaneously be collecting data from multiple LTM 
Listener units. The LTM Listener can be started in either private mode 
(sending to a single destination Ethernet address) or shared mode 
(multicasting its traffic reports).

Also, while multiple hosts may simultaneously view a single LTM Listener 
unit (thereby requiring additional licenses of the software be purchased 
for each additional processor), multiple accounts on a single host may NOT 
simultaneously view a single LTM Listener unit. 

DISTRIBUTION MEDIA

Tape: 9-track 1600 BPI Magtape, TK50 Streaming Tape

This product is also available as part of the VMS Consolidated Software 
Distribution on CDROM.

ORDERING INFORMATION 

Software Licenses:  QL-VEHA*-**
Software Media:  QA-VEHA*-**
Software Documentation:  QA-VEHAA-GZ
Software Product Services:  QT-VEHA*-**

*   Denotes variant fields.  For additional information on available 
    licenses, services, and media, refer to the appropriate price book.

The above information is valid at the time of release.  Please contact your 
local Digital office for the most up-to-date information.

(TM) Chipcom and Ethermodem are trademarks of Chipcom Corporation.
(R)  The DIGITAL Logo is a registered trademark of Digital Equipment 
     Corporation.
(TM) DECnet, DECwindows, LAN Traffic Monitor, LAN Bridge, MicroVAX, VAX, 
     VAXstation, VAXserver, and VT are trademarks of Digital Equipment 
     Corporation.


