 






           System
           Support
           Addendum

           _________________________________________________________
           _________________________________________________________

           PRODUCT NAME: DECmcc Extended LAN Manager AM, SSA 31.33.01-A
                         Version 1.0

           HARDWARE REQUIREMENTS

           Processors Supported

           VAX:       VAX 4000 Model 200,
                      VAX 4000 Model 300

                      VAX 6000 Model 200 Series,
                      VAX 6000 Model 300 Series,
                      VAX 6000 Model 400 Series,
                      VAX 6000 Model 500 Series

                      VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX
                      8500, VAX 8530, VAX 8550, VAX 8600, VAX 8650,
                      VAX 8700, VAX 8800, VAX 8810, VAX 8820, VAX
                      8830, VAX 8840

                      VAX 9000 Model 210,
                      VAX 9000 Model 400 Series

                      VAXft 3000 Model 310

                      VAX-11/750, VAX-11/780, VAX-11/785

           MicroVAX:  MicroVAX II, MicroVAX 2000,
                      MicroVAX 3100, MicroVAX 3300,
                      MicroVAX 3400, MicroVAX 3500,
                      MicroVAX 3600, MicroVAX 3800,


                                    DIGITAL                June 1991

                                                         AE-PH33B-TE

 



           DECmcc Extended LAN Manager AM,           SSA 31.33.01-A
           Version 1.0


                      MicroVAX 3900

           VAXstation:VAXstation II, VAXstation 2000,
                      VAXstation 3100 Series, VAXstation 3200,
                      VAXstation 3500, VAXstation 3520,
                      VAXstation 3540

           VAXserver: VAXserver 3100, VAXserver 3300, VAXserver
                      3400, VAXserver 3500, VAXserver 3600,
                      VAXserver 3602, VAXserver 3800, VAXserver
                      3900

                      VAXserver 6000 Model 210,
                      VAXserver 6000 Model 220,
                      VAXserver 6000 Model 310,
                      VAXserver 6000 Model 320,
                      VAXserver 6000 Model 410,
                      VAXserver 6000 Model 420,
                      VAXserver 6000 Model 510,
                      VAXserver 6000 Model 520

           Processors Not Supported

           MicroVAX I, VAXstation I, VAXstatiion II, VAxstation 2000,
           VAX-11/725, VAX-11/730, VAXstation 8000

           Processor Restrictions

           A TK50 Tape Drive is required for standalone MicroVAX 2000
           and VAXstation 2000 systems.

           Other Hardware Required

           RA60 system disk is required at a minimum.






                                       2

 



           DECmcc Extended LAN Manager AM,           SSA 31.33.01-A
           Version 1.0

           Disk Space Requirements (Block Cluster Size = 1):

           Disk space required for     5,700 blocks
           installation:
                                       (2.9M bytes)

           Disk space required for     5,700 blocks
           use (permanent):
                                       (2.9M Kbytes)

           These counts refer to the disk space required on the sys-
           tem disk. The sizes are approximate; actual sizes may vary
           depending on the user's system environment, configuration,
           and software options.

           CLUSTER ENVIRONMENT

           This layered product is fully supported when installed on
           any valid and licensed VAXcluster* configuration without re-
           strictions. The HARDWARE REQUIREMENTS sections of this prod-
           uct's Software Product Description and System Support Ad-
           dendum detail any special hardware required by this prod-
           uct.

           *  V5.x VAXcluster configurations are fully described in the
              VAXcluster Software Product Description (29.78.xx) and
              include CI, Ethernet, and Mixed Interconnect configura-
              tions.

           SOFTWARE REQUIREMENTS

           VMS Operating System V5.3 - V5.4

           DECmcc (Plus one of the following required):

           DECmcc Director for VMS V1.1
           DECmcc Basic Management System for VMS V1.1
           DECmcc Site Management Station for VMS V2.1
           DECmcc Enterprise Management Station for VMS V2.1


                                       3

 



           DECmcc Extended LAN Manager AM,           SSA 31.33.01-A
           Version 1.0

           VMS Tailoring

           For VMS V5.x systems, the following VMS classes are required
           for full functionality of this layered product:

           o  VMS Required Saveset

           o  Network Support

           o  Utilities

           For more information on VMS classes and tailoring, refer to
           the VMS Operating System Software Product Description (SPD
           25.01.xx).

           OPTIONAL SOFTWARE

           When running DECmcc Extended LAN Manager AM V1.0 on the DECmcc
           Directory, the DECmcc Extended LAN Manager FM license is re-
           quired (QL-GX9A*-**).

           This license is not required when running DECmcc Extended
           LAN Manager AM on DEcmcc Basic Management System V1.1, DECmcc
           Site Management Station V2.1, or DECmcc Enterprise Manage-
           ment Station V2.1.

           Refer to the following DECmcc, for specific DECmcc infor-
           mation.

           DECmcc Director for VMS V1.1 (SPD 32.46.xx)
           DECmcc Basic Management System for VMS V1.1 (SPD 32.48.xx)
           DECmcc Site Management Station for VMS V2.1 (SPD 31.87.xx)
           DECmcc Enterprise Management Station for VMS V2.1 (SPD 31.88.xx)

           GROWTH CONSIDERATIONS

           The minimum hardware/software requirements for any future
           version of this product may be different from the require-
           ments for the current version.


                                       4

 



           DECmcc Extended LAN Manager AM,           SSA 31.33.01-A
           Version 1.0

           DISTRIBUTION MEDIA

           9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

           This product is also available as part of the VMS Consol-
           idated Software Distribution on CDROM.

           The software documentation for this product is also avail-
           able as part of the VMS Online Documentation Library on CDROM.

           ORDERING INFORMATION

           Software Licenses: QL-GX8A*-**
           Software Media and Documentation: QA-GX8AA-**
           Software Documentation: QA-GX8AA-GZ
           Software Product Services: QT-GX8A*-**

           (License Required with DECmcc Director 1.1)

           Software License: QL-GX9A*-**

           Software Product Services: QT-GX9A*-**

           *  Denotes variant fields. For additional information on avail-
              able licenses, services, and media refer to the appro-
              priate price book.

           The above information is valid at time of release. Please
           contact your local Digital office for the most up-to-date
           information.

           [R] Chipcom is a registered trademark of Chipcom Corpora-
               tion.

           [TM]Ethermodem is a trademark of Chipcom Corporation.






                                       5

 



           DECmcc Extended LAN Manager AM,           SSA 31.33.01-A
           Version 1.0


           [TM]The Digital Logo, CI, DECmcc, DECbridge, DECconcen-
               trator,DECelms, METROWAVE, VAXcluster, VAXft, VAX,
               VMS, MicroVAX, VAXstation and VAXserver are trade-
               marks of Digital Equipment Corporation.

       


















                                       6
