 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  DECmcc Enterprise Management Station (EMS),   SSA
     31.88.02-A
                    Version 2.1

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAXft 3000-310,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series

               VAX 9000-210, VAX 9000 Model 400 Series

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840

               VAX-11/780, VAX-11/785

     MicroVAX:   MicroVAX 3100, MicroVAX 3300,
                 MicroVAX 3400, MicroVAX 3500,
                 MicroVAX 3600, MicroVAX 3800,
                 MicroVAX 3900





                                  DIGITAL                    May 1991

                                                          AE-PAWAC-TE

 


     DECmcc Enterprise Management Station (EMS),       SSA 31.88.02-A
     Version 2.1



     VAXstation: VAXstation 3100 Series, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540

     VAXserver:  VAXserver 3100, VAXserver 3300,
                 VAXserver 3400, VAXserver 3500,
                 VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900,
                 VAXserver 4000-300

                 VAXserver 6000-210, VAXserver 6000-220,
                 VAXserver 6000-310, VAXserver 6000-320,
                 VAXserver 6000-410, VAXserver 6000-420,
                 VAXserver 6000-510, VAXserver 6000-520

     Processors Not Supported

     VAX-11/725, VAX-11/730, VAX-11/750, VAX-11/782, VAX 4000 Model
     200, VAX 4000 Model 300, MicroVAX I, MicroVAX II, MicroVAX 2000,
     VAXstation I, VAXstation II, VAXstation 2000, VAXstation 8000

     Other Hardware Required

     A DECwindows supported color monitor is required; otherwise, a
     VT24x, VT330, or a VT340 terminal is required for systems with
     no DECwindows interface.

     To run the LTM Listener, one of the following is required:

     o  LAN Bridge 100 with ROM ECO Revision E or later

     o  LAN Bridge 150

     o  Chipcom[R] Ethermodem III Bridge (Option Numbers 8318BS
        (18Mhz) or 8312BS (12Mhz))

     Disk Space Requirements (Block Cluster Size = 1):

                                     2

 


     DECmcc Enterprise Management Station (EMS),       SSA 31.88.02-A
     Version 2.1



     Disk space required for      108,800 blocks
     installation:
     (Includes NMCC/DECnet        55,705 Kbytes
     Monitor
     database installation):

     Disk space required for      105,600 blocks
     use (permanent):
                                  (54,067 Kbytes)

     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     Minimum Recommended Configuration

     A VAXstation 3100, Model 38 or 48, with 32 Mbytes of memory and
     one RZ56 (665 Mbytes) disk drive.

     OPTIONAL HARDWARE

     In large network configurations where performance of the network
     management system is critical, it is recommended that additional
     memory and additional disk space be utilized.

     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet and Mixed Interconnect configurations.

                                     3

 


     DECmcc Enterprise Management Station (EMS),       SSA 31.88.02-A
     Version 2.1


     SOFTWARE REQUIREMENTS

     For Systems Using Terminals (No DECwindows
     Interface):

     VMS Operating System V5.3 - V5.4
     DECnet-VAX V5.3 - V5.4
     VAX Rdb/VMS V4.0 (Run-time Option)
     DEC GKS for VMS V4.1 (Run-time Option)
     VAX Distributed Name Service V1.1

     For Workstations Running DECwindows:

     VMS Operating System V5.3 - V5.4
     DECnet-VAX V5.3 - V5.4
     VAX Rdb/VMS V4.0 (Run-time Option)
     DEC GKS for VMS V4.1 (Run-time Option)
     VAX Distributed Name Service V1.1

     This product may run in either of the following ways:

     o  Stand-alone execution - Running the X11 display server and
        the client application on the same machine.

     o  Remote execution - Running the X11 display server and the
        client application on different machines.

     VMS DECwindows is part of the VMS Operating System but must
     be installed separately. Installation of VMS DECwindows gives
     users the option to install any or all of the following three
     components:

     o  VMS DECwindows Compute Server (Base kit; includes runtime
        support)

     o  VMS DECwindows Device Support

     o  VMS DECwindows Programming Support

     For stand-alone execution, the following DECwindows components
     must be installed on the machine:

                                     4

 


     DECmcc Enterprise Management Station (EMS),       SSA 31.88.02-A
     Version 2.1


     o  VMS DECwindows Compute Server

     o  VMS DECwindows Device Support

     For remote execution, the following DECwindows components must
     be installed on the machine:

     Server Machine

     o  VMS DECwindows Compute Server

     o  VMS DECwindows Device Support

     Client Machine

     o  VMS DECwindows Compute Server

     o  VMS DECwindows Device Support

     VMS Tailoring

     For VMS V5.x systems, the following VMS classes are required for
     full functionality of this layered product:

     o  VMS Required Saveset

     o  Network Support

     o  Programming Support

     o  Secure User's Environment

     o  Utilities

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).


                                     5

 


     DECmcc Enterprise Management Station (EMS),       SSA 31.88.02-A
     Version 2.1


     OPTIONAL SOFTWARE

     The following Digital VMS layered software products may be op-
     tionally installed with DECmcc EMS and run in the DECwindows en-
     vironment. Note that individual product memory and CPU require-
     ments may vary. Refer to the appropriate SPDs for information
     about these products.

     VAX DATATRIEVE V5.1
     VAX DECgraph V1.6
     VAX CDD/Plus V4.3
     DECnet/SNA VMS 3270 Terminal Emulator V1.5

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the requirements for
     the current version.

     Additional LAN Bridge units can be purchased and configured with
     LTM Listener software after LAN Traffic Monitor VMS has been
     installed. By creating a separate VMS process (or subprocess),
     a single user account on the VAX host may simultaneously be
     collecting data from multiple LTM Listener units. The LTM Lis-
     tener can be started in either private mode (sending to a single
     destination Ethernet address) or shared mode (multicasting its
     traffic reports).

     Also, while multiple hosts may simultaneously view a single
     LTM Listener unit (thereby requiring additional licenses of the
     software be purchased for each additional processor), multiple
     accounts on a single host may NOT simultaneously view a single
     LTM Listener unit.






                                     6

 


     DECmcc Enterprise Management Station (EMS),       SSA 31.88.02-A
     Version 2.1


     DISTRIBUTION MEDIA

     9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     This product is also available as part of the VMS Consolidated
     Software Distribution on CDROM.

     ORDERING INFORMATION

     Software License: QL-YFVA9-AA
     Software Media: QA-YFVAA-H*
     Software Documentation: QA-YFVAA-GZ
     Software Product Services: QT-YFVA*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services, and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [R]   Chipcom is a registered trademark of Chipcom Corporation.

     [TM]  The DIGITAL Logo, CI, CDD/Plus, DATATRIEVE, DECgraph,
           DECmcc, DECnet, DECwindows, DELNI, DEMPR, VAX, VMS, LAT,
           MicroVAX, Rdb/VMS, VAXstation, VAXserver, VAXcluster,
           VT, VT220, VT330, and VT340 are trademarks of Digital
           Equipment Corporation.










                                     7
