 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  DECndu (Network Device Upgrade) Utility       SSA
     33.47.00-A
                    for VMS, Version 1.0

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840, VAX 8842,
               VAX 8974, VAX 8978

               VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX: MicroVAX II, MicroVAX 2000,
               MicroVAX 3100, MicroVAX 3300,
               MicroVAX 3400, MicroVAX 3500,
               MicroVAX 3600, MicroVAX 3800,
               MicroVAX 3900

     VAXstationVAXstation II, VAXstation 2000,
               VAXstation 3100, VAXstation 3200,
               VAXstation 3500, VAXstation 3520,
               VAXstation 3540


                                  DIGITAL                October 1990

                                                          AE-PE7QA-TE

 


     DECndu (Network Device Upgrade) Utility           SSA 33.47.00-A
     for VMS, Version 1.0



     VAXserver:VAXserver 3100, VAXserver 3300,
               VAXserver 3400, VAXserver 3500,
               VAXserver 3600, VAXserver 3602,
               VAXserver 3800, VAXserver 3900

               VAXserver 6000-210, VAXserver 6000-310,
               VAXserver 6000-410, VAXserver 6000-420

     Processors Not Supported

     MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXstation
     8000

     Processor Restrictions

     A TK50 Tape Drive is required for standalone MicroVAX 2000 and
     VAXstation 2000 systems. Other Hardware Required

     o  A network adapter installed in the system using DECndu

     o  A DECbridge 500 if the system using DECndu does not have a
        FDDI network adapter

     For additional information regarding systems and adapters, refer
     to the appropriate systems and options catalog.

     Block Space Requirements (Block Cluster Size = 1):

     Disk space required for      700 blocks
     installation:
                                  (358K bytes)

     Disk space required for      600 blocks
     use (permanent):
                                  (307K bytes)



                                     2

 


     DECndu (Network Device Upgrade) Utility           SSA 33.47.00-A
     for VMS, Version 1.0


     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     VMS Operating System V5.3 - V5.4

     VMS Tailoring

     For VMS V5.x, the following VMS classes are required for full
     functionality of this layered product:

     o  VMS Required Saveset

     o  Network Support

     o  Utilities

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     OPTIONAL SOFTWARE

     None

     GROWTH CONSIDERATIONS

                                     3

 


     DECndu (Network Device Upgrade) Utility           SSA 33.47.00-A
     for VMS, Version 1.0


     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the minimum require-
     ments for the current version.

     DISTRIBUTION MEDIA

     Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     This product is also available as part of the VMS Consolidated
     Software Distribution on CDROM. ORDERING INFORMATION

     QB-YX2A9-A* FDDI DECconcentrator 500 Software Upgrade Package
     for VMS

     QB-YX3A9-A* FDDI DECbridge 500 Software Upgrade Package for VMS

     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [TM]  The DIGITAL Logo, VAX, MicroVAX, VAXstation, VAXserver and
           VMS are trademarks of Digital Equipment Corporation.













                                     4
