DECpage, Version 3.1						SSA 26.29.09-A

HARDWARE REQUIREMENTS

Processors Supported

VAX:	 VAX 6000 Model 200 Series
	 VAX 6000 Model 300 Series
	 VAX 6000 Model 400 Series

	 VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500, VAX 8530, VAX 
         8550, VAX 8600, VAX 8650, VAX 8700, VAX 8800, VAX 8810, VAX 8820, 
         VAX 8830, VAX 8840, VAX 8842, VAX 8974, VAX 8978
     
VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

MicroVAX:	   MicroVAX II, MicroVAX 2000, MicroVAX 3100, MicroVAX 
                   3300, MicroVAX 3400, MicroVAX 3500, MicroVAX 3600, 
                   MicroVAX 3800, MicroVAX 3900

VAXstation:	   VAXstation II, VAXstation 2000, VAXstation 3100 Series, 
                   VAXstation 3200, VAXstation 3500, VAXstation 3520, 
                   VAXstation 3540, VAXstation 8000

VAXserver:	   VAXserver 3100, VAXserver 3300, VAXserver 3400, 
                   VAXserver 3500, VAXserver 3600, VAXserver 3602, 
                   VAXserver 3800, VAXserver 3900, VAXserver 6000-210, 
                   VAXserver 6000-220, VAXserver 6000-310, VAXserver 
                   6000-320, VAXserver 6000-410, VAXserver 6000-420

Processors Not Supported

VAX:	      VAX-11/725

MicroVAX:	   MicroVAX I

VAXstation:	   VAXstation I

Processor Restrictions

A TK50 Tape Drive is required for standalone MicroVAX 2000 and VAXstation 
2000 systems.

At least one of the following printers is required:

oo   PrintServer 20 (LPS20)

oo   PrintServer 40 (LPS40)

oo   PrintServer 40 Plus (LPS40 PLUS)

oo   ScriptPrinter (LN03R)

oo   LN03 (rev level 4.4) with 2 RAM (LN03X-CR) cartridges

oo   LN03 PLUS with 2 RAM (LN03X-CR) cartridges

The following table shows printers and formats supported by DECpage, V3.1.

         Printer                  DECpage Supported Format

PrintServer 20			  PostScript (R) text & graphics;
				  ReGIS, Sixel, and GKS graphics by means 
                                  of translation software

PrintServer 40			  PostScript text & graphics; ReGIS, Sixel, 
                                  and GKS graphics by means of translation 
                                  software

PrintServer 40 Plus		  PostScript text & graphics; ReGIS, Sixel, 
                                  AND GKS graphics by means of translation 
                                  software

ScriptPrinter			  PostScript text & graphics; ReGIS, Sixel, 
                                  and GKS graphics by means of translation 
                                  software

LN03				  ANSI Text & Sixel Graphics (for simple 
                                  business graphics)                     

LN03 PLUS			  ANSI Text & Sixel Graphics (for full page 
                                  bit mapped graphics)                


Block Space Requirements (Block Cluster Size = 1):

Disk space required for installation:
						 40,000 blocks
						 (20,480K bytes)

Disk space required for use (permanent):
						 35,000 blocks
						 (17,920K bytes)

These counts refer to the disk space required on the system disk.  The 
sizes are approximate; actual sizes may vary depending on the user's system 
environment, configuration, and software options.

OPTIONAL HARDWARE

VT125, VT240/241 or VT330/340 series video terminal to display ReGIS or 
Sixel graphics

CLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid and 
licensed VAXcluster* configuration without restrictions.  The HARDWARE       
REQUIREMENTS sections of this product's Software Product Description and 
System Support Addendum detail any special hardware required by this 
product.                                                  

*   V5.x VAXcluster configurations are fully described in the VAXcluster 
    Software Product Description (29.78.xx) and include CI, Ethernet and 
    Mixed Interconnect configurations.

SOFTWARE REQUIREMENTS

Operating System

VMS Operating System V5.1 - V5.3

Layered Products

WPS-PLUS/VMS V3.0 or V3.1
Any other Language Variant of V3.0 or V3.1
 
or

ALL-IN-1 V2.3 - V2.4
Any other Language Variant of V2.3 or V2.4

VAX ScriptPrinter Software V2.1 is required to print PostScript and         
non-PostScript files to a ScriptPrinter.

VAX PrintServer Supporting Host Software V3.1 and VAX PrintServer Client 
Software, V3.0 are required to print PostScript and non-PostScript files to 
PrintServers.

Fonts

DECpage LN03 Basic Office Font Package V1.3 if outputting to an LN03 or 
LN03 PLUS.

No font package is required when printing to a ScriptPrinter, PrintServer 
20, PrintServer 40, or PrintServer 40 Plus in native mode.

For prerequisite software, refer to the Software Product Description and
System Support Addendum for WPS-PLUS/VMS (SPD/SSA 26.27.xx-x) or ALL-IN-1
(SPD/SSA 27.30.xx-x)

VMS Tailoring

For VMS V5.x systems, the following VMS classes are required for full 
functionality of this layered product:

oo   VMS Required Saveset
oo   Network Support
oo   Programming Support
oo   Secure User's Environment
oo   Utilities

For more information on VMS classes and tailoring, refer to the VMS 
Operating System Software Product Description (SPD 25.01.xx).

OPTIONAL SOFTWARE

DEC GKS for VMS V4.0 - Required for GKS to PostScript output to either 
ScriptPrinter, PrintServer 20, PrintServer 40, or PrintServer 40 Plus

VAX DECslide V1.3, VAX DECgraph V1.5 or a base ReGIS software package

Adobe Illustrator V1.1 for PostScript graphics

DECpage LN03 Upgrade and Complete Office Font Packages V1.3 if outputting 
to an LN03 or LN03 PLUS

VAX ReGIS to Sixels Converter (RETOS) V1.0 - ReGIS to Sixel graphics 
converter

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of this 
product may be different from the minimum requirements for the  current 
version.

DISTRIBUTION MEDIA

Tape:	 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

This product is also available as part of the VMS Consolidated Software 
Distribution on CDROM.

ORDERING INFORMATION

Software Licenses: QL-AANA*-**
Software Media:  QA-AANA*-**
Software Documentation:  QA-AANAA-GZ
Software Product Services:  QT-AANA*-**

*   Denotes variant fields.  For additional information on available 
    licenses, services and media, refer to the appropriate price book.

The above information is valid at time of release.  Please contact your 
local Digital office for the most up-to-date information.

(R)  PostScript is a registered trademark of Adobe Systems Inc.
(TM) Adobe Illustration is a trademark of Adobe Systems Inc.
(R)  The DIGITAL Logo is a registered trademark of Digital Equipment 
     Corporation.
(TM) ALL-IN-1, DEC, Ethernet, GKS, ReGIS, WPS-PLUS/VMS, LN03, LN03 PLUS, LN03R, 
     PrintServer, PrintServer 40, PrintServer 40 PLUS, VAX, MicroVAX, 
     VAXserver, VAXstation, and VT are trademarks of Digital Equipment 
     Corporation.  

