 






     4

     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  PATHWORKS FOR VMS Version 4.0      SSA 30.50.07-A
                    (Formerly VMS Services for PCs)

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAXft 3000-310,
               VAX 4000 Model 300,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840
               VAX 9000-210, VAX 9000 Model 400 Series

               VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX:   MicroVAX II, MicroVAX 2000,
                 MicroVAX 3100, MicroVAX 3300,
                 MicroVAX 3400, MicroVAX 3500,
                 MicroVAX 3600, MicroVAX 3800,
                 MicroVAX 3900



                                  DIGITAL               February 1991

                                                          AE-LX88F-TK

 


     PATHWORKS FOR VMS Version 4.0                     SSA 30.50.07-A
     (Formerly VMS Services for PCs)



     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540

     VAXserver:  VAXserver 3100, VAXserver 3300,
                 VAXserver 3400, VAXserver 3500,
                 VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900

                 VAXserver 6000-210, VAXserver 6000-220,
                 VAXserver 6000-310, VAXserver 6000-320,
                 VAXserver 6000-410, VAXserver 6000-420,
                 VAXserver 6000-510, VAXserver 6000-520

     Processors Not Supported

     VAX-11/725, VAX-11/730, VAX-11/782, MicroVAX I, VAXstation I,
     VAXstation 8000

     The VAX system must be connected to the same DECnet network as
     the PC client systems.

     A minimum of 4MB of memory is required, however, 8MB of mem-
     ory is recommended. Memory requirements vary depending on the
     server CPU, the number of clients using the server and the other
     applications running on the server.

     Disk Space Requirements (Block Cluster Size = 1):

     Disk space required for      7,000 blocks
     installation:
                                  (3.50M bytes)

     Disk space required for      5,500 blocks
     use (permanent):


                                     2

 


     PATHWORKS FOR VMS Version 4.0                     SSA 30.50.07-A
     (Formerly VMS Services for PCs)



                                  (2.25M bytes)

     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     OPTIONAL HARDWARE

     o  LA75

     o  LN03R

     o  LJ250

     o  LA210

     o  PrintServer 40

     o  PrintServer 20

     o  HP Laser Jet

     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of the product's Soft-
     ware Product Description and System Support Addendum detail any
     special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet, and Mixed Interconnect configurations.




                                     3

 


     PATHWORKS FOR VMS Version 4.0                     SSA 30.50.07-A
     (Formerly VMS Services for PCs)


     SOFTWARE REQUIREMENTS

     For Systems Using Terminals (No DECwindows Interface):

     o  VMS Operating System V5.3 - V5.4

     o  DECnet-VAX V5.3 - V5.4

     For Workstations Running VWS:

     o  VMS Operating System V5.3 - V5.4

     Note: Support for VMS DECwindows applications in PATHWORKS for
     DOS requires VMS Operating System V5.3 - V5.4.

     VMS Tailoring

     For VMS V5.x systems, the following VMS classes are required for
     full functionality:

     o  VMS Required Saveset

     o  Network Support

     o  System Programming

     o  Secure User's Environment

     o  OPTL - Miscellaneous File

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     OPTIONAL SOFTWARE

     VMS/ULTRIX Connection V1.3 is required for TCP/IP support.

     Certain versions of these products depend upon a specific ver-
     sion of the operating system. Please see the System Support
     Addendum of the product in question to determine which version
     is necessary.

     GROWTH CONSIDERATIONS

                                     4

 


     PATHWORKS FOR VMS Version 4.0                     SSA 30.50.07-A
     (Formerly VMS Services for PCs)


     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the minimum require-
     ments for the current version.

     DISTRIBUTION MEDIA

     Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape, CDROM

     ORDERING INFORMATION

     Software Media: QA-A93A*-**
     Software Documentation: QA-A93*A-GZ
     Software Media and Documentation: QA-A93*A-H*
     Software Product Services: QT-A93**-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [R]   MS-DOS and Microsoft are registered trademarks of Mi-
           crosoft Corporation.

     [R]   Macintosh is a registered trademark of Apple Computer,
           Inc.

     [R]   PostScript is a registered trademark of Adobe System, Inc.

     [R]   IBM and OS/2 are registered trademarks of International
           Business Machines Corporation.






                                     5

 


     PATHWORKS FOR VMS Version 4.0                     SSA 30.50.07-A
     (Formerly VMS Services for PCs)



     [TM]  The DIGITAL Logo, VMS, VAX, VAXstation, VAXmate, MicroVAX,
           VAXserver, DECnet, PCSA, ULTRIX, VAXcluster, LA75, LA210,
           LN03, LN03 PLUS, LVP16, and LA50 are trademarks of Digital
           Equipment Corporation.


































                                     6
