 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  DECpresent for VMS, Version 1.0    SSA 32.07.00-A

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAXft 3000-310,
               VAX 4000 Model 300,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series,

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840,

               VAX 9000 Model-210, VAX 9000 Model-410

               VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX: MicroVAX II, MicroVAX 2000,
               MicroVAX 3100, MicroVAX 3300,
               MicroVAX 3400, MicroVAX 3500,
               MicroVAX 3600, MicroVAX 3800,
               MicroVAX 3900





                                  DIGITAL               December 1990

                                                          AE-PE5EA-TE

 


     DECpresent for VMS, Version 1.0                   SSA 32.07.00-A




     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100 Series, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540

     VAXserver:  VAXserver 3100, VAXserver 3300,
                 VAXserver 3400, VAXserver 3500,
                 VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900,
                 VAXserver 4000 Model 300

                 VAXserver 6000-210, VAXserver 6000-210,
                 VAXserver 6000-310, VAXserver 6000-320,
                 VAXserver 6000-410, VAXserver 6000-420,
                 VAXserver 6000-510, VAXserver 6000-520

     Processors Not Supported

     VAX-11/725, VAX-11/782, MicroVAX I, VAXstation I, VAXstation
     8000

     Processor Restrictions

     A TK50 Tape Drive is required for standalone MicroVAX 2000 and
     VAXstation 2000 systems.

     Disk Space Requirements (Block Cluster Size = 1):

     Disk space required for      35,000 blocks
     installation:
                                  (17,920K bytes)

     Disk space required for      34,500 blocks
     use (permanent):
                                  (17,664K bytes)



                                     2

 


     DECpresent for VMS, Version 1.0                   SSA 32.07.00-A



     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     Memory Requirements for DECwindows Support:

     A minimum of 8MB of memory is required on a workstation to
     operate DECpresent and VMS whether DECpresent is running on
     the workstation or on another processor.

     OPTIONAL HARDWARE

     DECpresent files can be printed using any Digital PostScript[R]
     printer, ScriptPrinter (LN03R), PrintServer 20, PrintServer 40,
     PrintServer 40 Plus laser printer, and for color PostScript, the
     Colormate PS.

     DECchart produces both monochrome and color PostScript.
     Monochrome PostScript can be printed using any Digital
     PostScript printers listed above. If the DEC GKS product, or
     runtime system is installed, and the CDA Converter Library is
     installed, the DDIF Graphics Hardcopy converter can be used to
     generate the color and monochrome sixel formats (printed on the
     Digital LJ250 Companion Color Printer) and the HPGL[TM] for-
     mat (printed on the Digital LVP16). If the DECprint Utility
     for PostScript to Sixel Printing for VMS is installed, DECchart
     PostScript output (either color or monochrome) can be printed on
     the Digital LJ250 Companion Color Printer.

     DECpresent will accept images scanned with the MD-300 Scanner.

     Optional Third Party Hardware

     For 35mm film recording, Digital refers the customer to the AGFA
     ChromaScript and AGFA film recorder or the Management Graphics
     Inc. Solitaire file recorder system. Digital does not offer a
     warranty or directly support these third party devices.

                                     3

 


     DECpresent for VMS, Version 1.0                   SSA 32.07.00-A



     Digital does not offer a warranty or directly support these
     third party devices.


     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     o  VMS Operating System V5.3 - V5.4 (and necessary components of
        VMS DECwindows

     This product may run in either of the following ways:

     o  Stand-alone execution - running the X11 display server and
        the client application on the same machine.

     o  Remote execution - running the X11 display server and the
        client application on different machines.

     VMS DECwindows is part of the VMS Operating System but must
     be installed separately. Installation of VMS DECwindows gives
     users the option to install any or all of the following three
     components:

     o  VMS DECwindows Compute Server (Base kit; includes runtime
        support)

     o  VMS DECwindows Device Support

     o  VMS DECwindows Programming Support

                                     4

 


     DECpresent for VMS, Version 1.0                   SSA 32.07.00-A



     For stand-alone execution, the following DECwindows components
     must be installed on the machine:

     o  VMS DECwindows Compute Server

     o  VMS DECwindows Device Support

     For remote execution, the following DECwindows components must
     be installed on the machine:

     Server Machine

     o  VMS DECwindows Compute Server

     o  VMS DECwindows Device Support

     Client Machine

     o  VMS DECwindows Compute Server

     o  VMS DECwindows Device Support

     VMS Tailoring:

     For VMS V5.x systems, the following VMS classes are required for
     full functionality of this layered product:

     o  VMS Required Saveset

     o  VMS Workstation Support

     o  Programming Support

     Optional:

     o  Network Support - Provides support for cluster and client/server
        systems.

     o  Utilities - Mail provides support for sending files created
        with DECpresent.

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

                                     5

 


     DECpresent for VMS, Version 1.0                   SSA 32.07.00-A



     PC DECwindows Display Facility

     The PC DECwindows Display Facility is an MS-DOS[R] application
     that implements an X server that uses the industry-standard X
     Window System, Version 11 (X11) protocol. DECpresent executing
     on a remote VMS system with DECnet may be displayed on and
     receive input from the personal computer. The PC DECwindows
     Display Facility is supported only on Intel 80286 and 80386
     machines. Refer to the DECnet PCSA Client for DOS, Version
     3.0 Software Product Description and System Support Addendum
     (SPD 55.07.08 and SSA 55.07.08-x) for full hardware/software
     requirements.

     OPTIONAL SOFTWARE

     o  DECprint Printing Services for VMS V4.0

     o  DECwrite for VMS V1.1

     o  DECdecision for VMS V1.1

     o  DECimage Scan Software for VMS V2.0

     o  DECnet PCSA Client for DOS, V3.0

     o  International Lexicons for VMS, V1.0

           International Lexicon/Français for VMS V1.0
           International Lexicon/Deutsch for VMS V1.0
           International Lexicon/British for VMS V1.0
           International Lexicon/Español for VMS V1.0
           International Lexicon/Nederlands for VMS V1.0
           International Lexicon/Svenska for VMS V1.0
           International Lexicon/American English for VMS V1.0
              (included with the U.S. version)
           International Lexicon/American Business for
              VMS V1.0
           International Lexicon/American Medical for
              VMS V1.0

                                     6

 


     DECpresent for VMS, Version 1.0                   SSA 32.07.00-A



     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the requirements for
     the current version.

     DISTRIBUTION MEDIA

     Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     This product is also available as part of the VMS Consolidated
     Software Distribution on CDROM.

     ORDERING INFORMATION

     Software Licenses: QL-YHEA9-PB
     Software Media: QA-YHEAA-H*
     Software Documentation: QA-YHEAA-GZ
     Software Product Services: QT-YHEA*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     International Hyphenators, and International CorrectSpell li-
     censed from Houghton Mifflin Company. Copyright (c) 1985, 1987,
     1988 by Houghton Mifflin. German (c) 1985, 1987 by Langenscheidt
     K.G. French in cooperation with Libraire Larousse. Italian
     (c) 1988 by Nicola Zanichelli. All rights reserved. U.S. Pat.
     Nos. 4,580,241, 4,724,523 and 4,771,401. Canadian. Pat. No.
     1,203,916. Thesaurus U.S. Pat. No. 4,724,523. English based upon
     The AMERICAN HERITAGE DICTIONARY. Reproduction or disassembly of
     embodied computer programs or algorithms prohibited.


                                     7

 


     DECpresent for VMS, Version 1.0                   SSA 32.07.00-A



     Arts and Letters[R] clipart licensed to Digital Equipment Corpo-
     ration, Maynard, Massachusetts. Copyright (c) Computer Support
     Corporation 1985-1990. All rights reserved.

     [R]  Arts and Letters is a registered trademark of Computer
          Support Corporation.

     [R]  Lotus 1-2-3 is a registered trademark of Lotus Development
          Corporation.

     [R]  MS-DOS is a registered trademark of Microsoft Corporation.

     [R]  PostScript is a registered trademark of Adobe Systems, Inc.

     [TM] HPGL is a trademark of Hewlett-Packard Corporation.

     [TM] The DIGITAL Logo, CDA, GOLD KEY, DECpresent, DECwrite,
          DECdecision, DECalc, DECalc-PLUS, DECgraph, DECwindows,
          LiveLink, LN03, LVP16, PrintServer, VAX, MicroVAX, VAXsta-
          tion, VAXserver and VMS are trademarks of Digital Equipment
          Corporation.


















                                     8
