 






           System
           Support
           Addendum

           _________________________________________________________
           _________________________________________________________

           PRODUCT NAME:  VAX RALLY, Version 2.3      SSA 27.03.06-A

           HARDWARE REQUIREMENTS

           Processors Supported

           VAX:     VAXft 3000-310

                    VAX 4000 Model 200
                    VAX 4000 Model 300

                    VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series,
                    VAX 6000 Model 500 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840

                    VAX 9000-210, VAX 9000 Model 400 Series

                    VAX-11/730, VAX-11/750, VAX-11/780,
                    VAX-11/785

           MicroVAX:MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,




                                    DIGITAL                 May 1991

                                                         AE-LX94G-TE

 



           VAX RALLY, Version 2.3                    SSA 27.03.06-A



                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900

           VAXstatioVAXstation II, VAXstation 2000,
                    VAXstation 3100 Series, VAXstation 3200,
                    VAXstation 3500, VAXstation 3520,
                    VAXstation 3540

           VAXserverVAXserver 3100, VAXserver 3300,
                    VAXserver 3400, VAXserver 3500,
                    VAXserver 3600, VAXserver 3602,
                    VAXserver 3800, VAXserver 3900

                    VAXserver 4000 Model 200,
                    VAXserver 4000 Model 300

                    VAXserver 6000-210, VAXserver 6000-220,
                    VAXserver 6000-310, VAXserver 6000-320,
                    VAXserver 6000-410, VAXserver 6000-420,
                    VAXserver 6000-510, VAXserver 6000-520

           Processors Not Supported

           VAX-11/725, VAX-11/782, MicroVAX I, VAXstation I, VAXsta-
           tion 8000

           Processor Restrictions

           A TK50 Tape Drive is required for standalone MicroVAX 2000
           and VAXstation 2000 systems.

           A minimum of 4 MB of memory is required, although typical
           configurations will require more than 4 MB of memory. There
           is a recommendation of 0.75 MB per concurrent user.

           Other Hardware Required

           Terminals


                                       2

 



           VAX RALLY, Version 2.3                    SSA 27.03.06-A


           VAX RALLY Development Option and VAX RALLY Run-Time Option
           can be run on any VT100 (with AVO), VT100 compatible ter-
           minal emulators on VAXstations, VT102, VT125 (with AVO), VT220,
           VT240/241, VT320, VT330, VT340, or VT420 terminal.

           Disk Space Requirements (Block Cluster Size =1):

           Disk space required for installation:

           VAX RALLY Development Option:

           With Examples:              26,000 blocks
                                       (13.3 Mbytes)

           Without Examples:           18,000 blocks
                                       (9.2 Mbytes)

           VAX RALLY Run-Time Option:

           With Examples:              10,000 blocks
                                       (5.1 Mbytes)

           Without Examples:           7,000 blocks
                                       (3.6 Mbytes)

           Disk space required for use (permanent):

           VAX RALLY Development Option:

           With Examples:              20,000 blocks
                                       (10.2 Mbytes)

           Without Examples:           15,000 blocks
                                       (7.7 Mbytes)

           VAX RALLY Run-Time Option:

           With Examples:              8,000 blocks
                                       (4.1 Mbytes)


                                       3

 



           VAX RALLY, Version 2.3                    SSA 27.03.06-A



           Without Examples:           2,000 blocks
                                       (1.0 Mbytes)

           In addition, VAX RALLY Development Option includes a text-
           based instruction course (TBI) entitled Getting Started with
           VAX RALLY. If this course is installed, it requires:

           Disk space required for     6,000 blocks
           installation:
                                       (3.1 Mbytes)

           Disk space required for     3,000 blocks
           use (permanent):
                                       (1.5 Mbytes)

           Note: These amounts are in addition to the amounts listed
           previously.

           These counts refer to the disk space required on the sys-
           tem disk. The sizes are approximate; actual sizes may vary
           depending on the users' system environment, configuration,
           and software options.

           OPTIONAL HARDWARE

           Any device supported by the prerequisite/optional software.

           CLUSTER ENVIRONMENT

           This layered product is fully supported when installed on
           any valid and licensed VAXcluster* configuration without re-
           strictions. The HARDWARE REQUIREMENTS sections of this prod-
           uct's Software Product Description and System Support Ad-
           dendum detail any special hardware required by this prod-
           uct.





                                       4

 



           VAX RALLY, Version 2.3                    SSA 27.03.06-A


           *  V5.x VAXcluster configurations are fully described in the
              VAXcluster Software Product Description (29.78.xx) and
              include CI, Ethernet, and Mixed Interconnect configura-
              tions.


           SOFTWARE REQUIREMENTS

           For Systems Using Terminals (No DECwindows Interface):

           VMS Operating System V5.2-V5.4

           For Workstations Running VWS:

           VMS Operating System V5.2-V5.4
           VMS Workstation Software V4.2-V4.3

           For Workstations Running DECwindows:

           VMS Operating System V5.2-V5.4 (and necessary components of
           VMS DECwindows)

           This product may run under DECterm in either of the follow-
           ing ways:

           o  Stand-alone execution-running the X11 display server and
              the client application on the same machine.

           o  Remote execution-running the X11 display server and the
              client application on different machines.

           VMS DECwindows is part of the VMS Operating System but must
           be installed separately on versions prior to V5.4. Instal-
           lation of VMS DECwindows gives users the option to install
           any or all of the following three components:

           o  VMS DECwindows Compute Server (Base kit; includes Run-
              Time support)

           o  VMS DECwindows Device Support

           o  VMS DECwindows Programming Support

                                       5

 



           VAX RALLY, Version 2.3                    SSA 27.03.06-A


           For stand-alone execution, the following DECwindows compo-
           nents must be installed on the machine:

           o  VMS DECwindows Compute Server

           o  VMS DECwindows Device Support

           o  VMS DECwindows Programming Support

           For remote execution, the following DECwindows components
           must be installed on the machine:

           Server Machine

           o  VMS DECwindows Compute Server

           o  VMS DECwindows Device Support

           o  VMS DECwindows Programming Support

           Client Machine

           o  VMS DECwindows Compute Server

           o  VMS DECwindows Device Support

           o  VMS DECwindows Programming Support

           Layered Products

           VAX Rdb/VMS (Interactive or Development System) V3.1B-V4.0
           is required for the VAX RALLY Development Option.

           VAX Rdb/VMS V4.0 is required for the Two-Phase Commit Op-
           tion.

           VAX Rdb/VMS (Run-Time, Interactive, or Development) is re-
           quired for the VAX RALLY Run-Time Option if the application
           uses VAX Rdb/VMS. If using the VAX RALLY Run-Time Option with
           RMS files only, VAX Rdb/VMS is NOT required.

           VAX CDD/Plus V4.0-V4.2A is required for the VAX RALLY De-
           velopment Option, but not required for the VAX RALLY Run-
           Time Option.

                                       6

 



           VAX RALLY, Version 2.3                    SSA 27.03.06-A


           VMS Tailoring

           For VMS V5.x systems, the following VMS classes are required
           for full functionality of this layered product:

           o  VMS Required Saveset

           o  Secure User's Environment

           o  Programming Support (Not required for VAX RALLY Run-Time
              Option)

           For more information on VMS classes and tailoring, refer to
           the VMS Operating System Software Product Description (SPD
           25.01.xx).

           OPTIONAL SOFTWARE

           ALL-IN-1 V2.3
           VAX TEAMDATA V1.4
           VAX DATATRIEVE V5.1
           VAX DBMS V4.2
           VAX Language-Sensitive Editor/
              Source Code Analyzer V3.1

           GROWTH CONSIDERATIONS

           The minimum hardware/software requirements for any future
           version of this product may be different from the require-
           ments for the current version.

           DISTRIBUTION MEDIA

           9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

           This product is also available as part of the VMS Consol-
           idated Software Distribution on CDROM.




                                       7

 



           VAX RALLY, Version 2.3                    SSA 27.03.06-A


           ORDERING INFORMATION

           VAX RALLY Development Option (includes VAX RALLY Run-Time
           Option):

           Software Licenses: QL-A86A*-**
           Software Media: QA-A86A*-**
           Software Documentation: QA-A86AA-GZ
           Software Product Services: QT-A86A*-**

           VAX RALLY Run-Time Option:

           Software Licenses: QL-VF4A*-**
           Software Media: QA-VF4A*-**
           Software Documentation: QA-VF4AA-GZ
           Software Product Services: QT-VF4A*-**

           *  Denotes variant fields. For additional information on avail-
              able licenses, services, and media, refer to the appro-
              priate price book.

           The above information is valid at time of release. Please
           contact your local Digital office for the most up-to-date
           information.

           [TM]The DIGITAL Logo, ALL-IN-1, CI, DATATRIEVE, DBMS,
               DECterm, DECwindows, Micro/VAX, RALLY, Rdb/VMS,
               TEAMDATA, TK50, VAX, VAX ACMS, VAX CDD/Plus, VAX
               DOCUMENT, VMS, VAXstation, VAXserver, VAXcluster,
               VT, and WPS-PLUS are trademarks of Digital Equipment
               Corporation.










                                       8
