 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  VAX Rdb/ELN, Version 2.3           SSA 28.03.09-A
                     (Relational Database Management System)

     HARDWARE REQUIREMENTS

     Host Processors Supported

     VAX:      VAX 4000 Model 200 Series,
               VAX 4000 Model 300 Series,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840
               VAX 9000-210, VAX 9000 Model 400 Series

               VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX:   MicroVAX II, MicroVAX 2000,
                 MicroVAX 3100, MicroVAX 3300,
                 MicroVAX 3400, MicroVAX 3500,
                 MicroVAX 3600, MicroVAX 3800,
                 MicroVAX 3900

     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,


                                  DIGITAL               February 1991

                                                          AE-LT39C-TE

 


     VAX Rdb/ELN, Version 2.3                          SSA 28.03.09-A
      (Relational Database Management System)



                 VAXstation 3540

     Processor Restriction

     The VAX-11/782 processor is not supported by the VMS Operating
     System V5.0 or later.

     Target System Processor Support

     VAX:        VAX 4000 Model 200,
                 VAX 4000 Model 300
                 VAX 6000 Model 200 Series,
                 VAX 6000 Model 300 Series,
                 VAX 6000 Model 400 Series

                 VAX 8200, VAX 8250, VAX 8500, VAX 8530, VAX 8550,
                 VAX 8700, VAX 8800, VAX 8810

                 VAX-11/730, VAX-11/750

     MicroVAX:   MicroVAX II, MicroVAX 2000, MicroVAX 3100, MicroVAX
                 3300, MicroVAX 3400, MicroVAX 3500, MicroVAX 3600,
                 MicroVAX 3800, MicroVAX 3900

     Board         KA620-BA
     Products:

     rtVAX         rtVAX 1000, rtVAX 3200, rtVAX 3300,
     Products:
                   rtVAX 3400, rtVAX 3500, rtVAX 3600, rtVAX 3800

                   rtVAX 4000 Model 200 and 300,
                   rtVAX 6000 Model 200 and 300,

                   rtVAX 8550, rtVAX 8700,



                                     2

 


     VAX Rdb/ELN, Version 2.3                          SSA 28.03.09-A
      (Relational Database Management System)



                   rtVAXstation 3100 Models 30 and 38, rtVAX 3305

     IVAX          IVAX 620, IVAX 630
     Products:

     VAXstation:   VAXstation 2000, VAXstation 3100, VAXstation
                   3150, VAXstation 3200, VAXstation 3500, VAXstation
                   II/GPX

     Note: VAXstation support is for color only.




























                                     3

 


     VAX Rdb/ELN, Version 2.3                          SSA 28.03.09-A
      (Relational Database Management System)


     Processors Not Supported as Targets

     VAX:          VAX 6312, VAX 6333, VAX 8300, VAX 8350, VAX 8600,
                   VAX 8650, VAX 8820, VAX 8830, VAX 8840

                   VAX-11/780, VAX-11/782, VAX-11/785

     rtVAX         rtVAX300
     Products:

     VAXstation:   VAXstation II, VAXstation 3520, VAXstation 3540

     Other Hardware Requirements

     For Development Systems:

     Any valid VAXELN V4.1 or V4.2 Development System configuration.

     Refer to the VAXELN Toolkit Software Product Description (SPD
     28.02.xx) for valid VAXELN Development Configurations.

     Disk Space Requirements (Block Cluster Size = 1):

     Disk space required for      16,062 blocks
     installation:
                                  (8,031K bytes)

     Disk space required for      8,600 blocks
     use (permanent):
                                  (4,300K bytes)

     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     For VAX-11/730 Systems:

     Dual RL02 disk drives installed on a VAX-11/730 system is not a
     supported configuration.

                                     4

 


     VAX Rdb/ELN, Version 2.3                          SSA 28.03.09-A
      (Relational Database Management System)


     For Target Systems:

     Any valid VAXELN Version 4.2 Target System configuration.

     Refer to the VAXELN Toolkit Software Product Description (SPD
     28.02.xx) for valid VAXELN Target System Configurations.

     OPTIONAL HARDWARE

     Refer to the VAXELN Toolkit System Support Addendum (SSA
     28.02.12-x) for supported Optional Hardware.

     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     For Development Systems:

     VMS Operating System V5.1 - V5.4

     Layered Products:

     VAXELN Toolkit V4.1 - V4.2

     VAX Rdb/VMS V4.0

     DECnet-VAX V5.0 - V5.1 is required for down-line loading, remote
     debugging, and communicating between VAXELN and VMS.

     VMS Tailoring

                                     5

 


     VAX Rdb/ELN, Version 2.3                          SSA 28.03.09-A
      (Relational Database Management System)


     For VMS V5.x systems, the following VMS classes are required for
     full functionality of this layered product:

     o  VMS Required Saveset

     o  Network Support (If using the VAXELN Remote Debugger feature)

     o  Programming Support

     o  Utilities

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     28.03.xx).

     OPTIONAL SOFTWARE

     Refer to the VAXELN Toolkit System Support Addendum (SSA
     28.02.12-x) for for optional software which may be used.

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the minimum require-
     ments for the current version.

     DISTRIBUTION MEDIA

     Disk: RA60 Disk Cartridge, RX33 Floppy Diskette

     Tape: 9-track 1600 BPI Magtape, TK50 Streaming Tape








                                     6

 


     VAX Rdb/ELN, Version 2.3                          SSA 28.03.09-A
      (Relational Database Management System)


     ORDERING INFORMATION

     Development System:

     Software Licenses: QL-D07A*-**
     Software Media: QA-D07A*- **
     Software Documentation: QA-D07AA-GZ
     Software Product Services: QT-D07A*-**

     Target System:

     Software Licenses: QL-D08A*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [TM]  The DIGITAL Logo, VMS, DATATRIEVE, VAX C, Rdb/VMS, VAX,
           VAXstation, VAXserver, MicroVAX, VAXELN and VAX Rdb/ELN
           are trademarks of Digital Equipment Corporation.















                                     7
