 






          System
          Support
          Addendum

          ________________________________________________________________

          PRODUCT NAME:  VAX Remote Environmental Monitoring Software,
          Version 1.2                                       SSA 29.73.02-A
                         (VAX REMS)

          HARDWARE REQUIREMENTS

          Processors Supported

          VAX:      VAX 4000 Model 300,
                    VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840, VAX 8842,
                    VAX 8974, VAX 8978

                    VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

          MicroVAX: MicroVAX II, MicroVAX 2000,
                    MicroVAX 3300, MicroVAX 3400,
                    MicroVAX 3500, MicroVAX 3600,
                    MicroVAX 3800, MicroVAX 3900

          VAXstationVAXstation II, VAXstation 2000,
                    VAXstation 3200, VAXstation 3500,
                    VAXstation 3520, VAXstation 3540,




                                       DIGITAL                   June 1990

                                                               AE-MC08C-TE

 


          VAX Remote Environmental Monitoring Software, VersSSA 29.73.02-A




          VAXserver:VAXserver 3300, VAXserver 3400,
                    VAXserver 3500, VAXserver 3600,
                    VAXserver 3602, VAXserver 3800,
                    VAXserver 3900

                    VAXserver 6000-210, VAXserver 6000-310,
                    VAXserver 6000-410, VAXserver 6000-420

          Processors Not Supported

          VAX-11/725, VAX-11/730, MicroVAX I, MicroVAX 3100, VAXstation I,
          VAXstation 3100 Series, VAXserver 3100, VAXstation 8000

          Other Hardware Required

          o  H7310 EMS or

          o  H7317 PDS+ or

          o  H7318 PCS+ or

          o  HA3000 UPS

          o  RS232 Data Cable

          o  DECserver 200 (optional)

          Block Space Requirements (Block Cluster Size = 1):

          Disk space required for      5,500 blocks
          installation:
                                       (2,745K bytes)

          Disk space required for      3,600 blocks
          use (permanent):
                                       (1,792K bytes)

          These counts refer to the disk space required on the system
          disk. The sizes are approximate; actual sizes may vary depending
          on the user's system environment, configuration, and software
          options.

                                          2

 


          VAX Remote Environmental Monitoring Software, VersSSA 29.73.02-A



          CLUSTER ENVIRONMENT

          This layered product is fully supported when installed on any
          valid and licensed VAXcluster* configuration without restric-
          tions. The HARDWARE REQUIREMENTS sections of this product's
          Software Product Description and System Support Addendum detail
          any special hardware required by this product.

          *  V5.x VAXcluster configurations are fully described in the
             VAXcluster Software Product Description (29.78.xx) and in-
             clude CI, Ethernet and Mixed Interconnect configurations.

          SOFTWARE REQUIREMENTS

          For Systems Using Terminals (No DECwindows Interface):

          VMS Operating System V4.7 - V5.3
          VAX FMS Forms Driver V2.3 - V2.4

          For Workstations Running VWS:

          VMS Operating System V4.7 - V5.3
          VMS Workstation Software V4.2
          VMS FMS Forms Driver V2.3 - V2.4















                                          3

 


          VAX Remote Environmental Monitoring Software, VersSSA 29.73.02-A



          VMS Tailoring

          For VMS V5.x, the following VMS classes are required for full
          functionality of this layered product:

          o  VMS Required Saveset

          o  Network Support

          o  Programming Support

          o  Utilities

          For more information on VMS classes and tailoring, refer to
          the VMS Operating System Software Product Description (SPD
          25.01.xx).

          OPTIONAL SOFTWARE

          None

          GROWTH CONSIDERATIONS

          The minimum hardware/software requirements for any future ver-
          sion of this product may be different from the minimum require-
          ments for the current version.

          DISTRIBUTION MEDIA

          Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

          This product is also available as part of the VMS Consolidated
          Software Distribution on CDROM.

          ORDERING INFORMATION

          Software Licenses: QL-VI5A*-**
          Software Media: QA-VI5A*-**
          Software Documentation: QA-VI5AA-GZ
          Software Product Services: QT-VI5A*-**

                                          4

 


          VAX Remote Environmental Monitoring Software, VersSSA 29.73.02-A



          *  Denotes variant fields. For additional information on avail-
             able licenses, services and media refer to the appropriate
             price book.

          The above information is valid at time of release. Please con-
          tact your local Digital office for the most up-to-date informa-
          tion.

          [R]   The DIGITAL Logo is a registered trademark of Digital
                Equipment Corporation.


          [TM]  VAX, MicroVAX, VAXstation, VAXserver and VMS are trade-
                marks of Digital Equipment Corporation.

























                                          5
