 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  DEC Realtime Test Integrator for VMS, Version 2.0
     SSA 28.30.07-A

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAXft 3000-310,
               VAX 4000 Model 200,
               VAX 4000 Model 300,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840

               VAX 9000-210,
               VAX 9000 Model 400 Series

               VAX-11/730, VAX-11/750, VAX-11/780,
               VAX-11/785

     MicroVAX: MicroVAX II, MicroVAX 2000,
               MicroVAX 3100, MicroVAX 3300,
               MicroVAX 3400, MicroVAX 3500,
               MicroVAX 3600, MicroVAX 3800,


                                  DIGITAL                  April 1991

                                                          AE-PEHNC-TE

 


     DEC Realtime Test Integrator for VMS, Version 2.0 SSA 28.30.07-A




               MicroVAX 3900

     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100 Series, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540


     VAXserver:  VAXserver 3100, VAXserver 3300,
                 VAXserver 3400, VAXserver 3500,
                 VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900,
                 VAXserver 4000 Model 300

                 VAXserver 6000-210, VAXserver 6000-220,
                 VAXserver 6000-310, VAXserver 6000-320,
                 VAXserver 6000-410, VAXserver 6000-420,
                 VAXserver 6000-510, VAXserver 6000-520

     Processors Not Supported

     MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXstation
     8000

     Processor Restrictions

     A minimum system configuration includes:

     o  One RD-series, RA-series or RZ-series disk

     o  One TK50 or TK70 cartridge tape drive

     o  8 MB memory

     o  Console terminal

     Disk Space Requirements (Block Cluster Size = 1):

                                     2

 


     DEC Realtime Test Integrator for VMS, Version 2.0 SSA 28.30.07-A



     Development Kit

     Disk space required for      17,000 blocks
     installation:                (9.0 Mbytes)

     Disk space required for      16,200 blocks
     use (permanent):
                                  (8.3 Mbytes)

     Runtime Kit

     Disk space required for      11,000 blocks
     installation:                (6.0 Mbytes)

     Disk space required for      10,000 blocks
     use (permanent):
                                  (5.1 Mbytes)

     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     Memory Requirements for DECwindows Support

     The minimum supported memory for this application running in
     a standalone DECwindows environment with both the client and
     server executing on that same system is 9 MB.

     OPTIONAL HARDWARE

     LIO and Icon Support

     o  IEZ11*

     Q-bus Devices

     o  Preston GM and EM series*[1]

     ___________________

   [1] indicates icon support

                                     3

 


     DEC Realtime Test Integrator for VMS, Version 2.0 SSA 28.30.07-A



     o  AAV11-DA*, AAV11-SA*, AAV11-SF*

     o  ADQ32*, ADQ32-SA*, ADQ32-SF*

     o  ADV11-DA*, ADV11-SA*, ADV11-SF*

     o  DRQ3B*, DRQ3B-SA*, DRQ3B-SF*

     o  IEQ11*, IEQ11-SA*, IEQ11-SF*

     o  KWV11-C*, KWV11-SA*, KWV11-SF*

     Serial I/O*

     o  Serial I/O is supported on all Q-bus, VAXBI and VAX 2000
        and 3000 series systems using the local serial ports or dis-
        tributed over the Ethernet using DECserver-series products.

     LIO Support Only

     o  AXV11-C, AXV11-SA, AXV11-SF

     o  DRV11-J, DRV1J-SA, DRV1J-SF

     o  DRV11-WA, DRV1W-SA, DRV1W-SF

     o  DRB32

     o  DRB32W

     o  Simpact RTC01

     LIO Support - Europe Only

     o  AAF01-A

     o  ADF01-B

     o  AMF01-A

     o  ASF01-A

     o  DRQ11-C

     o  IAV11-A, IAV11-AA, IAV11-B, IAV11-C, IAV11-CA

     o  IAV1S-A, IAV1S-AA, IAV1S-B, IAV1S-C, IAV1S-CA

                                     4

 


     DEC Realtime Test Integrator for VMS, Version 2.0 SSA 28.30.07-A



     o  IDV11-A, IDV11-B, IDV11-C, IDV11-D

     o  IDV1S-A, IDV1S-B, IDV1S-C, IDV1S-D

     UNIBUS Devices

     o  No UNIBUS devices are supported.

     Supported Pseudo Devices:

     LIO and Icon Support

     o  Fast file input and output

     o  Interprocess communication

     LIO Support Only

     o  Dynamic memory allocation

     o  Realtime plotting (VAXstation monitors only)

     Supported Graphics Output Devices

     o  HP7550

     o  LA12

     o  LA34

     o  LA50

     o  LA75

     o  LA100

     o  LA210

     o  LCG01

     o  LJ250

     o  LN03 PLUS

     o  LN03R

     o  LPS40

                                     5

 


     DEC Realtime Test Integrator for VMS, Version 2.0 SSA 28.30.07-A



     o  LVP16 (8 1/2 X 11)

     o  LVP16 (11 X 17)

     o  VAXstation 2000, VAXstation II, VAXstation II/GPX, VAXstation
        3100, VAXstation 3200, VAXstation 3500

     o  VT125

     o  VT240

     o  VT241

     o  VT330

     o  VT340

     o  VT4xx

     o  Tektronix 4014

     o  Tektronix 4107

     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration with the restric-
     tion that time-critical operations will be adversely affected by
     cluster state transitions. The HARDWARE REQUIREMENTS sections of
     this product's Software Product Description and System Support
     Addendum detail any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet and Mixed Interconnect configurations.




                                     6

 


     DEC Realtime Test Integrator for VMS, Version 2.0 SSA 28.30.07-A



     SOFTWARE REQUIREMENTS

     For Systems Using Terminals (No DECwindows Interface):

     o  VMS Operating System V5.4

     For Workstations Running VWS (Required to use the LIO realtime
     plotting device. The icon-based user interface is not available
     to customers who choose the VWS windowing system):

     o  VMS Operating System V5.4

     o  VMS Workstation Software V4.3

     For Workstations Running DECwindows (Required to use the icon-
     based user interface):

     o  VMS Operating Systems V5.4 (and necessary components of VMS
        DECwindows)

     o  DEC GKS for VMS V4.1

     o  VAX C V3.2 is required if the user is developing custom
        icons.

     DRB32 VMS Drivers V3.0 - prerequisite for LIO support of the
     DRB32 and DRB32W devices and I/O subsystems that interface to
     the VAXBI through the DRB32 and DRB32W.

     The RTC01 BI clock is a prerequisite to use BI devices through
     LIO I/O support.

     VMS DECwindows is part of the VMS Operating System but must
     be installed separately. Installation of VMS DECwindows gives
     users the option to install any or all of the following three
     components:

        VMS DECwindows Compute Server
           (Base kit; includes runtime support)
        VMS DECwindows Device Support
        VMS DECwindows Programming Support

                                     7

 


     DEC Realtime Test Integrator for VMS, Version 2.0 SSA 28.30.07-A



     For stand-alone execution, the following DECwindows components
     must be installed on the machine:

        VMS DECwindows Compute Server
        VMS DECwindows Device Support
        VMS DECwindows Programming Support

     For remote execution, the following DECwindows components must
     be installed on the machine:

     Server Machine

     VMS DECwindows Compute Server
     VMS DECwindows Device Support
     VMS DECwindows Programming Support

     Client Machine

     VMS DECwindows Compute Server
     VMS DECwindows Device Support
     VMS DECwindows Programming Support

     Either DECwindows (bundled with VMS Workstation Software (UIS
     V4.0)) is required to use the LGP or LIO plotting routines on
     any VAXstation system.

     VMS Tailoring

     For VMS V5.x systems, the following VMS classes are required for
     full functionality of this layered product:

     o  VMS Required Saveset

     o  Network Support

     o  Programming Support

     o  System Programming Support

     o  Secure User's Environment

     o  Utilities

                                     8

 


     DEC Realtime Test Integrator for VMS, Version 2.0 SSA 28.30.07-A



     o  RMS Journaling Files

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     OPTIONAL SOFTWARE

     Certain versions of these products depend upon a specific ver-
     sion of the operating system. Refer to the System Support Ad-
     dendum of the product in question to determine which version is
     required.

     The following high level languages are required if the user is
     developing applications using the LIO, LSP and LGP routines.
     They are not necessary if the user is building applications
     using DEC Realtime Test integrator.

     o  VAX Ada V2.2

     o  VAX BASIC V3.4

     o  VAX C V3.2

     o  VAX FORTRAN V5.6

     o  VAX PASCAL V4.2

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the requirements for
     the current version.

     DISTRIBUTION MEDIA

     TK50 Streaming Tape, 9-track 1600 BPI Magtape

     This product is also available as part of the VMS Consolidated
     Software Distribution on CDROM.

                                     9

 


     DEC Realtime Test Integrator for VMS, Version 2.0 SSA 28.30.07-A



     ORDERING INFORMATION

     Development Option

     The Development Kit allows the user to develop realtime applica-
     tions including data acquisition, IEEE-488 AND RS-232 instrument
     control, and test and measurement. After an application has been
     developed, the application can run on a system which has either
     the Development Kit or Runtime Kit.

     Software Licenses: QL-YWQA9-QB
     Software Media: QA-YWQAA-**
     Software Documentation: QA-YWQAA-GZ
     Software Product Services: QT-YWQA*-**

     Runtime Option

     The Runtime Kit allows the user to run an application, but not
     to develop an application.

     Software Licenses: QL-B15A9-J*
     Software Media: QA-B15A*-**
     Software Product Services: QT-B15A*-**

     *  Denotes variant fields. For additional information on li-
        censes, services, and media, refer to the appropriate price
        book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [R]  PostScript is a registered trademark of Adobe Systems,
          Incorporated.





                                    10

 


     DEC Realtime Test Integrator for VMS, Version 2.0 SSA 28.30.07-A




     [TM] The DIGITAL Logo, CI, DEC, DECserver, DECwindows, DRB32,
          LA, LA50, Q-bus, MicroVAX, RA, TK, VAXcluster, VAXserver,
          VAXstation, VAX, VAX Ada, VAX BASIC, VAXBI, VAX C, VAX FOR-
          TRAN, VAX Pascal, VMS, VT, VT330 and VT340 are trademarks
          of Digital Equipment Corporation.

































                                    11
