 













             DEC RT Integrator
             Installation Guide

             Order Number: AA-KN95D-TE



             February 1991

             This document describes the procedures for installing the DEC
             Realtime Test Integrator (DEC DEC RT Integrator) Development
             Kit and Runtime Kit on RISC ULTRIX and VMS systems.

                                               NOTE

                            DEC RT Integrator was formerly called
                            VAXlab Software Library.




             Revision/Update Information:  This is a revised document.

             Operating System and Version: ULTRIX Version 4.0 or higher
                                           VMS Version 5.3 or higher

             Software Version:             DEC RT Integrator Version 1.0
                                           (ULTRIX)
                                           DEC RT Integrator Version 2.0
                                           (VMS)
             digital equipment corporation
             maynard, massachusetts

 

             Revised,iAugust 1988mber 1987
             Revised, February 1990
             Revised, February 1991

             The information in this document is subject to change without
             notice and should not be construed as a commitment by Digital
             Equipment Corporation. Digital Equipment Corporation assumes
             no responsibility for any errors that may appear in this
             document.

             The software described in this document is furnished under a
             license and may be used or copied only in accordance with the
             terms of such license.

             No responsibility is assumed for the use or reliability
             of software on equipment that is not supplied by Digital
             Equipment Corporation or its affiliated companies.

             Restricted Rights: Use, duplication, or disclosure by the
             U.S. Government is subject to restrictions as set forth in
             subparagraph (c)(1)(ii) of the Rights in Technical Data and
             Computer Software clause at DFARS 252.227-7013.

             © Digital Equipment Corporation 1987, 1988, 1990, 1991.

             All rights reserved.
             Printed in U.S.A.

             The Reader's Comments form at the end of this guide requests
             your critical evaluation to assist in preparing future docu-
             mentation.

             The following are trademarks of Digital Equipment Corporation:
             CDA, DDIF, DECdecision, DECnet, DECstation, DECsystem,
             DECwindows, DECwrite, DRB32, DTIF, LA50, LN03, LN03 PLUS,
             LVP16, MicroVAX, MicroVAX II, Q-bus, RdB/VMS, ULTRIX, UWS,
             VAX, VAX C, VAX FORTRAN, VAX MACRO, VAX 6000, VAX 9000,
             VAXcluster, VAXlab, VAXstation, VMS, VT, VT330, and the
             DIGITAL logo.

             The following are third-party trademarks: HP7550 is a regis-
             tered trademark of Hewlett-Packard Corporation; PostScript
             is a registered trademark of Adobe Systems, Inc.; RS/1 is a
             registered trademark of BBN Software Product Corporation; and
             Tektronix is a registered trademark of Tektronix, Inc.

             This document was prepared with VAX DOCUMENT, Version 1.2.

             This document is available in both printed and CDROM ver-
             sions.

 















                                                                  Contents
          ________________________________________________________________

          Preface .........................................................   ix


          ________________________________________________________________
          Part I   Installing DEC RT Integrator on a RISC ULTRIX
                   System

          ________________________________________________________________
          Chapter 1  Preparing to Install DEC RT Integrator on RISC
                     ULTRIX

               1.1   Release Notes ......................................  1-2

               1.2   Development Kit Distinguished From Runtime
                     Kit..................................................   1-2

               1.3   Using RIS for Client Installations..............  1-2

               1.4   Installing DEC RT Integrator into a RIS Server
                     Area.................................................   1-3

               1.5   Installing DEC RT Integrator into a DMS Server
                     Area.................................................   1-3


               1.6   Checking the Media Software Distribution Kit ..   1-3


                                                                       iii

 






               1.7   Hardware Requirements............................. 1-4

               1.8   Software Requirements............................. 1-5
                     1.8.1 Optional Software.......................... 1-5

               1.9   Installation Procedure Requirements.............  1-5
                     1.9.1 Time......................................... 1-6
                     1.9.2 Privileges.................................. 1-6
                     1.9.3 Disk Space Required for DEC RT
                           Integrator.................................. 1-6
                     1.9.4 System Disk Backup......................... 1-8


          ________________________________________________________________
          Chapter 2  Installing DEC RT Integrator on RISC ULTRIX


               2.1   License Registration .............................. 2-2

               2.2   Aborting the Installation ........................ 2-3

               2.3   Installing DEC RT Integrator Locally............  2-3
                     2.3.1 Using TK50 Distribution Media............   2-3
                     2.3.2 Installing DEC RT Integrator from a RIS
                           Server....................................... 2-4

               2.4   Responding to Installation Procedure Prompts ..   2-5
                     2.4.1 Determining Which Development Kit
                           Subsets to Install......................... 2-5
                     2.4.2 Selecting Development Kit Subsets.......    2-6
                     2.4.3 Determining Which Runtime Kit Subsets
                           to Install.................................. 2-8
                     2.4.4 Selecting Runtime Kit Subsets............   2-9
                     2.4.5 Monitoring Displays During the Subset
                           Loading Process............................ 2-10

               2.5   Installing DEC RT Integrator into a Server
                     Environment ........................................   2-10

          iv

 






                     2.5.1 DMS Server Installations.................. 2-10
                     2.5.2 RIS Server Installations.................. 2-13

               2.6   Development Kit Installation Procedure ......... 2-17

               2.7   Runtime Kit Installation Procedure.............. 2-22

               2.8   Reconfiguring the Kernel to Support the ek
                     Driver...............................................    2-26
                     2.8.1 Editing the Configuration File...........  2-26
                     2.8.2 Computing Values in the Configuration
                           File.........................................  2-27
                     2.8.3 Building a New Kernel..................... 2-31

               2.9   Reconfiguring the Kernel to Delete the ek
                     Driver...............................................    2-31
                     2.9.1 Editing the Configuration File...........  2-31
                     2.9.2 Configuring the System to Delete the
                           Driver from a DMS Client  ................ 2-32
                     2.9.3 Building a New Kernel..................... 2-33

               2.10  Installation Verification Procedure (IVP)......  2-33

               2.11  Error Messages .....................................   2-33

               2.12  Determining the Files Added to the System......  2-34

               2.13  Reporting Problems.................................  2-34


          ________________________________________________________________
          Chapter 3  Running the IVP for ULTRIX







                                                                         v

 






          ________________________________________________________________
          Part II   Installing DEC RT Integrator on a VMS System


          ________________________________________________________________
          Chapter 4  Preparing to Install DEC RT Integrator on VMS


               4.1   Development Kit Distinguished From Runtime
                     Kit..................................................   4-1

               4.2   Prerequisite and Optional Software..............  4-2

               4.3   License Registration .............................. 4-2

               4.4   VAXcluster Considerations ........................ 4-3

               4.5   Installation Procedure Requirements.............  4-3
                     4.5.1 Privileges and Disk Space ................  4-4
                     4.5.2 System Parameters.......................... 4-4
                           4.5.2.1Checking System Parameter
                                  Values............................... 4-5
                           4.5.2.2Changing System Parameter Values
                                  with AUTOGEN........................ 4-6
                     4.5.3 VMSINSTAL Requirements....................  4-7
                     4.5.4 Backing Up Your System Disk..............   4-7

          ________________________________________________________________
          Chapter 5  Installing DEC RT Integrator on VMS

               5.1   Aborting the Installation ........................ 5-1

               5.2   Development Kit Installation Procedure .........  5-1

               5.3   Runtime Kit Installation Procedure.............. 5-16

               5.4   Error Recovery .....................................   5-30


          vi

 






          ________________________________________________________________
          Chapter 6  Postinstallation Tasks Under VMS

               6.1   Accessing the DEC RT Integrator Release
                     Notes................................................   6-2

               6.2   Editing the System Files.......................... 6-2

               6.3   Modifying System Parameters...................... 6-4

               6.4   Loading the DEC RT Integrator License for the
                     Other Nodes.........................................  6-5

               6.5   Loading the IEZ11 Device Driver in a Cluster ..   6-5

               6.6   Setting Quotas for User Accounts ................ 6-7

               6.7   Modifying the System Configuration Command
                     File.................................................   6-8

               6.8   Loading Device Drivers............................ 6-8

               6.9   Creating Pascal Environment Files...............  6-9

               6.10  Reporting Problems.................................  6-10


          ________________________________________________________________
          Chapter 7  Running the IVP for VMS

          ________________________________________________________________
          Appendix A ULTRIX Files Installed on Your System







                                                                       vii

 






          ________________________________________________________________
          Appendix B Sample ULTRIX Installation

               B.1   Sample Installation for RISC ULTRIX
                     Development Kit.................................... B-1

               B.2   Sample Installation for RISC ULTRIX Runtime
                     Kit..................................................   B-5


          ________________________________________________________________
          Appendix C Sample VMS Installation

               C.1   Sample Installation for VMS Development Kit ...   C-1

               C.2   Sample Installation for VMS Runtime Kit........   C-6

          ________________________________________________________________
          Index

          ________________________________________________________________
          Examples

               B-1   Sample Installation for RISC ULTRIX
                     Development Kit.................................... B-2

               B-2   Sample Installation for RISC ULTRIX Runtime
                     Kit..................................................   B-5

               C-1   Sample Installation for VMS Development Kit ...   C-2

               C-2   Sample Installation for VMS Runtime Kit........   C-6







          viii

 







          ________________________________________________________________
          Figures

               3-1   IVP Plot for DEC RT Integrator................... 3-3

               7-1   IVP Plot for DEC RT Integrator................... 7-2

          ________________________________________________________________
          Tables

               1-1   Disk Space Required by DEC RT Integrator.......   1-6

               2-1   ek Device Driver Configuration File............. 2-27

               4-1   Minimum Required System Parameter Values.......   4-5























                                                                        ix

 














                                                                   Preface
          ________________________________________________________________


          ____________________________________________________________

          Intended Audience

             This guide describes how to install the DEC RT Integrator
             Version 1.0 (ULTRIX) Development and Runtime Kits and the
             DEC RT Integrator Version 2.0 (VMS) Development and Runtime
             Kits. This guide is for ULTRIX or VMS system managers or the
             persons responsible for performing the system installation.

             For those installing DEC RT Integrator on RISC ULTRIX, this
             guides assumes experience with the following:

              o The setld ULTRIX utility

              o The fverify ULTRIX utility

              o Remote Installation Service (ris)

              o Diskless Management Services (dms)

             For those installing DEC RT Integrator on VMS, this guide
             assumes experience with VMSINSTAL.




                                                                        ix

 





          ____________________________________________________________

          Organization

             This guide has two parts. Part I describes how to install
             DEC RT Integrator on RISC ULTRIX. Part II describes how to
             install DEC RT Integrator on VMS. Parts I and II and their
             chapters follow:
































          x

 













































                                                                        xi

 





             _____________________________________________________________
             Chapter
             Number________Contents_______________________________________

             Part I        Installing DEC RT Integrator on a RISC ULTRIX
                           System

             Chapter 1     Discusses the preparations and requirements
                           necessary for installing DEC RT Integrator on
                           RISC ULTRIX.

             Chapter 2     Explains how to install DEC RT Integrator on
                           RISC ULTRIX and how to recover from errors.

             Chapter 3     Shows how to run the Installation Verification
                           Procedure (IVP) under ULTRIX.

             Part II       Installing DEC RT Integrator on a VMS System

             Chapter 4     Explains DEC RT Integrator installation prereq-
                           uisites for a VMS system.

             Chapter 5     Provides instructions for installing DEC RT
                           Integrator from a tape cartridge or magnetic
                           tape on a VMS system.

             Chapter 6     Describes procedures you perform after a suc-
                           cessful DEC RT Integrator installation on VMS,
                           such as editing the startup command files and
                           changing parameter settings.

             Chapter 7     Shows how to run the Installation Verification
                           Procedure (IVP) under VMS.

             Appendix A    Contains a list of the files created or modi-
                           fied by the ULTRIX installation procedure.

             Appendix B    Contains sample listings for an ULTRIX DEC RT
                           Integrator installation.

             Appendix C    Contains sample listings for a VMS DEC RT
          xii              Integrator installation.
             _____________________________________________________________

 





          ____________________________________________________________

          Associated Documentation

             The following is a complete list of the DEC RT Integrator
             documentation set:

             Basic manuals:

              o The DEC RT Integrator Installation Guide describes how to
                install DEC RT Integrator on RISC ULTRIX and VMS systems.

              o The DEC RT Integrator Master Index for ULTRIX lists the
                index entries in all the DEC RT Integrator documents for
                ULTRIX.

              o The DEC RT Integrator Master Index for VMS lists the index
                entries in all the DEC RT Integrator documents for VMS.

             DECwindows graphical user interface manuals:

              o The DEC RT Integrator User's Guide describes how to de-
                velop and run applications with the DECwindows graphical
                user interface.

              o The DEC RT Integrator Icon Developer's Guide describes
                how to develop icons for the DECwindows graphical user
                interface.

             Subroutine library manuals:

              o Getting Started with the Subroutine Libraries describes
                the subroutine library components of the product.

              o The DEC RT Integrator Laboratory Graphics Package (LGP)
                Reference Manual describes how to plot realtime data or
                data produced by calculations in two dimensions, three di-
                mensions, and 2-dimensional contours from a 3-dimensional
                view.

              o The DEC RT Integrator Laboratory Input/Output (LIO)
                Reference Manual for ULTRIX describes how to initiate,
                control, process, and terminate I/O to and from I/O de-
                vices on an ULTRIX system.

                                                                      xiii

 






              o The DEC RT Integrator Laboratory Input/Output (LIO)
                Reference Manual for VMS describes how to initiate, con-
                trol, process, and terminate I/O to and from I/O devices
                on a VMS system.

              o The DEC RT Integrator Laboratory Signal Processing (LSP)
                Reference Manual describes how to use the signal process-
                ing routines to perform Fourier transforms, correlation
                functions, and data filtering.

             See the following documents for more information about in-
             stalling software products on RISC ULTRIX systems:

              o ULTRIX-32 Introduction to System and Network Management

              o ULTRIX-32 Reference Pages Section 8: setld(8) command

              o ULTRIX-32 System Management Volume 2: Guide to System
                Configuration File Maintenance

              o ULTRIX-32 Installation Guide for your processor: in-
                stalling ULTRIX layered products

             See the following documents for more information about in-
             stalling software products on VMS systems:

              o Guide to Setting Up a VMS System

              o Introduction to VMS System Management

          ____________________________________________________________

          Conventions

             The DEC RT Integrator documentation set uses the following
             conventions:



          xiv

 





             _____________________________________________________________
             Convention_______Meaning_____________________________________

             Italics          Words in italics indicate one of the follow-
                              ing:

                               o Emphasis on a term or phrase

                               o The name of a manual

              . . .           Ellipses indicate that portions of a display
                              or example are excluded for presentation
                              purposes.

             Ctrl/X           A key combination indicating that you hold
                              down the first key while pressing the second
                              key. For example, Ctrl/C indicates that you
                              hold down the key labeled Ctrl while you
                              press the key labeled C.

             "Double quotes"  Double quotes enclose system messages or
                              screen prompts appearing in text.

             [Brackets]       Square brackets indicate a required argu-
                              ment.

             UPPERCASE TEXT   The ULTRIX system differentiates between
                              lowercase and uppercase letters. Enter
                              uppercase characters only when they are
                              specifically indicated by an example or
             _________________syntax_line.________________________________









                                                                        xv

 












                                                                    Part I
                      Installing DEC RT Integrator on a RISC ULTRIX System
          ________________________________________________________________



             Part I contains information about installing DEC RT
             Integrator on a RISC ULTRIX system.

 

















                                                                      Chapter 1


                          Preparing to Install DEC RT Integrator on RISC ULTRIX
               ________________________________________________________________


                  Chapter 1 discusses the preparations and requirements neces-
                  sary for installing DEC RT Integrator on RISC ULTRIX:

                   o Lists where the release notes can be found (see Section 1.1)

                   o Describes the difference between the Development Kit and
                     the Runtime Kit (see Section 1.2)

                   o Describes requirements for using RIS for client installa-
                     tions (see Section 1.3)

                   o Describes installing DEC RT Integrator into a RIS Server
                     area (see Section 1.4)

                   o Describes installing DEC RT Integrator into a DMS Server
                     area (see Section 1.5)

                   o Describes the media software distribution kit (see
                     Section 1.6)

                   o Lists the prerequisite hardware (see Section 1.7)

                   o Lists the prerequisite and optional software (see
                     Section 1.8)

                   o Lists the time, privileges required, disk space, and
                     backup procedures necessary to install DEC RT Integrator
                     (see Section 1.9)




                     Preparing to Install DEC RT Integrator on RISC ULTRIX  1-1

 











                  Your bill of materials (BOM) and indented bills report (BIL)
                  specify the number and contents of your media. Verify the
                  contents of your kit with this information. If your kit is
                  damaged or if you find that parts of it are missing, contact
                  your Digital representative.

               ____________________________________________________________

               1.1  Release Notes

                  DEC RT Integrator provides online release notes. Digital
                  strongly recommends that you read the release notes before
                  using the product. The release notes may contain information
                  about changes to the application.

                  After you install DEC RT Integrator, you can find online
                  release notes in the following file:

                    /usr/lib/X11/help/rti/rti100.release_notes

               ____________________________________________________________

               1.2  Development Kit Distinguished From Runtime Kit

                  The Development Kit allows the user to develop realtime
                  applications, including data acquisition, IEEE-488 and RS-232
                  instrument control, and test and measurement. The Runtime kit
                  allows the user to run an application but not to develop one.

                  Instructions for installing the Development Kit and the
                  Runtime Kit are similar. The Development Kit installation
                  procedure is described in Section 2.6. The Runtime Kit in-
                  stallation procedure is described in Section 2.7.

               ____________________________________________________________

               1.3  Using RIS for Client Installations

                  If you expect to install DEC RT Integrator subsets from a
                  Remote Installation Services (RIS) server area of a remote
                  system for installation on your local system, first check
                  with your site system administrator to make sure that:

                   o A DEC RT Integrator kit is installed in the RIS server
                     area and is available for use

                   o Your system is registered as a RIS client

               1-2  Preparing to Install DEC RT Integrator on RISC ULTRIX

 











                  If DEC RT Integrator subsets are available to you on a RIS
                  server system, you will need the name of that system to start
                  the installation procedure described in this guide.

               ____________________________________________________________

               1.4  Installing DEC RT Integrator into a RIS Server Area

                  If you manage a Remote Installation Services (RIS) server
                  area and intend to install DEC RT Integrator into your server
                  area, read the following sections of this guide:

                   o Section 1.6 for information about contents of the media
                     kit

                   o Section 1.7 for hardware requirements

                   o Section 1.8 for software requirements

                   o Section 2.4 for information about the displays and prompts
                     that are specific to DEC RT Integrator installations

               ____________________________________________________________

               1.5  Installing DEC RT Integrator into a DMS Server Area

                  If you manage a Diskless Management Services (DMS) server
                  area and intend to install DEC RT Integrator into your server
                  area, read the following sections of this guide:

                   o Section 1.6 for information about contents of the media
                     kit

                   o Section 1.7 for hardware requirements

                   o Section 1.8 for software requirements

                   o Section 1.9.3 for disk space requirements

                   o Section 2.4 for information about the displays and prompts
                     that are specific to DEC RT Integrator installations

               ____________________________________________________________

               1.6  Checking the Media Software Distribution Kit

                  For installations from media, use the Bill of Materials (BOM)
                  to check the contents of your software distribution kit.

                     Preparing to Install DEC RT Integrator on RISC ULTRIX  1-3

 











                  The kit includes this installation guide and the TK50 tape
                  cartridge, labeled DEC RT Integrator V1.0, for systems with
                  TK50 or TK70 tape cartridge drives.

               ____________________________________________________________

               1.7  Hardware Requirements

                  To perform the installation, you need the following hardware:

                   o Software distribution device (if installing from media)

                     You need a distribution device that corresponds with the
                     software distribution media. For example, if you have a
                     TK50 software kit, you need a TK50 or TK70 tape drive.
                     You must know how to load the media supplied with the
                     software distribution kit on the appropriate drive. The
                     documentation for the tape or disk drive that you are
                     using explains how to load media.

                   o Terminal

                     You can use either a hardcopy or video terminal to commu-
                     nicate with the operating system and respond to prompts
                     from the installation procedure for DEC RT Integrator.

                   o Processors

                     DEC RT Integrator requires one of the following proces-
                     sors:

                      _ DECstation 2100

                      _ DECstation 3100

                      _ DECstation 3100S

                      _ DECstation 5000 series

                      _ DECsystem 3100

                      _ DECsystem 5400

                      _ DECsystem 5810

                      _ DECsystem 5820

               1-4  Preparing to Install DEC RT Integrator on RISC ULTRIX

 










               ____________________________________________________________

               1.8  Software Requirements

                  DEC RT Integrator Version 1.0 requires that ULTRIX Version
                  4.0 or higher and ULTRIX/UWS Version 4.0 or higher be in-
                  stalled.

                  To use the DEC RT Integrator graphical user interface or the
                  LGP subroutine library, DEC GKS-3D for ULTRIX Version 1.1
                  must be installed on your system.

                  If you are using only the LIO or LSP subroutine libraries for
                  applications, you do not not need to install DEC GKS-3D for
                  ULTRIX Version 1.1.

                  To develop user-written icons for DEC RT Integrator, the
                  Worksystem Development Software ((UDWXDEV400) and the
                  Software Development Utilities (UDTPGMR400) subsets are
                  required from the ULTRIX Version 4.0 or higher software.

               ____________________________________________________________

               1.8.1  Optional Software

                  If you will be using the IEZ11 device, you can install
                  the IEZ11 driver either before or after installing DEC RT
                  Integrator.

                  To develop user-written icons for DEC RT Integrator, you must
                  have access to the compiler for the language in which you are
                  programming.

                  C for RISC is included with the ULTRIX operating system.
                  If you will be using FORTRAN for RISC, you must purchase it
                  separately.

                  Refer to the System Software Addendum (SSA) for a complete
                  list of compatible products and their required version num-
                  bers. The SSA is part of the Software Product Description
                  (SPD).

               ____________________________________________________________

               1.9  Installation Procedure Requirements

                  This section discusses time, privileges, disk space and
                  system disk backup for installing DEC RT Integrator.

                     Preparing to Install DEC RT Integrator on RISC ULTRIX  1-5

 










               ____________________________________________________________

               1.9.1  Time

                  A local DMS server or RIS server installation takes approxi-
                  mately 20 minutes, depending on your type of media and your
                  system configuration. A RIS client installation may take
                  longer because it is dependent on network activity at the
                  time you do the installation. If the network is not active,
                  you should expect an installation time roughly equal to a
                  local installation.

               ____________________________________________________________

               1.9.2  Privileges

                  To install DEC RT Integrator, you must be logged in to the
                  root or super user account.

               ____________________________________________________________

               1.9.3  Disk Space Required for DEC RT Integrator

                  To install the entire Development Kit for DEC RT Integrator
                  on RISC ULTRIX you must have 29,400 Kbytes available on your
                  /usr file system.

                  To install the entire Runtime Kit for DEC RT Integrator on
                  RISC ULTRIX you must have 14,400 Kbytes available on your
                  /usr file system.

                  Table 1-1 shows the disk space required for software subsets
                  in both the DEC RT Integrator Development Kit and DEC RT
                  Integrator Runtime Kit.

                  Table 1-1:  Disk Space Required by DEC RT Integrator
                  _____________________________________________________________
                  Description___________________Subset_Name___Kbytes___________

                  ___________________Development_Kit_Subsets___________________

                  Laboratory Graphics Package   RTILGP100      5000
                  (LGP)
                  Laboratory Input/Output       RTILIO100       400
                  (LIO)
                  _____________________________________________________________
                                                       (continued on next page)

               1-6  Preparing to Install DEC RT Integrator on RISC ULTRIX

 











                  Table 1-1 (Cont.):  Disk Space Required by DEC RT Integrator
                  _____________________________________________________________
                  Description___________________Subset_Name___Kbytes___________

                  ___________________Development_Kit_Subsets___________________

                  Laboratory Signal Processing  RTILSP100       200
                  (LSP)
                  DEC RT Integrator (DevelopmentRTIBASE100     6000
                  ULTRIX ek device driver       RTI488100      2100
                  DEC RT Integrator (Runtime)   RTIRTBASE100   6000
                  DEC RT Integrator Manual      RTIMAN100       400
                  Pages
                  DEC RT Integrator Examples    RTIEXA100       300
                  Icon Development              RTIICON100     9000

                  Total Development Kit Files                 29400

                  _____________________________________________________________
                  _____________________Runtime_Kit_Subsets_____________________

                  Laboratory Graphics Package   RTILGP100      5000
                  (LGP)
                  Laboratory Input/Output       RTILIO100       400
                  (LIO)
                  Laboratory Signal Processing  RTILSP100       200
                  (LSP)
                  DEC RT Integrator (Runtime)   RTIRUN100      6000
                  ULTRIX ek device driver       RTI488100      2100
                  DEC RT Integrator Manual      RTIRTMAN100     400
                  Pages
                  DEC RT Integrator Examples    RTIEXA100       300

                  Total_Runtime_Kit_Files_____________________14400____________

                  Use the following ULTRIX command to determine the amount of
                  space presently available in the /usr file system:

                    %df

                  If the disk does not have enough space, delete unnecessary
                  files to provide space.



                     Preparing to Install DEC RT Integrator on RISC ULTRIX  1-7

 










               ____________________________________________________________

               1.9.4  System Disk Backup

                  Digital recommends that you do a system disk backup before
                  installing any layered product. This backup protects your
                  files from being corrupted in case a system failure occurs
                  during the installation.

                  Install DEC RT Integrator on the backup disk. Use this backup
                  disk with DEC RT Integrator installed as your new system
                  disk.

                  For more information about backing up your system disk, refer
                  to the ULTRIX documentation.































               1-8  Preparing to Install DEC RT Integrator on RISC ULTRIX

 

















                                                                      Chapter 2


                                    Installing DEC RT Integrator on RISC ULTRIX
               ________________________________________________________________


                  Chapter 2 describes how to install DEC RT Integrator on RISC
                  ULTRIX:

                   o License registration (see Section 2.1)

                   o Aborting the installation (see Section 2.2)

                   o Installing DEC RT Integrator locally (see Section 2.3)

                   o Installation procedure prompts (see Section 2.4)

                   o Installing DEC RT Integrator into a server environment
                     (see Section 2.5)

                   o Development Kit installation procedure (see Section 2.6)

                   o Runtime Kit installation procedure (see Section 2.7)

                   o Reconfiguring the kernel to support the ek driver (see
                     Section 2.8)

                   o Reconfiguring the kernel to delete the ek driver (see
                     Section 2.9)

                   o Installation Verification Procedure (IVP) (see Section 2.10)

                   o Error messages (see Section 2.11)

                   o Determining the files added to the system (see Section 2.12)

                   o Reporting problems (see Section 2.13)

                               Installing DEC RT Integrator on RISC ULTRIX  2-1

 










               ____________________________________________________________

               2.1  License Registration

                  A License Product Authorization Key (License PAK) must be
                  registered in the License Database (LDB) in order to use
                  DEC RT Integrator on a newly-licensed node. The License PAK
                  may be shipped along with the kit if you ordered the license
                  and media together; otherwise, it is shipped separately to a
                  location based on your license order. If you are installing
                  DEC RT Integrator as an update on a node already licensed
                  for this software, you have already completed the License PAK
                  registration requirements.

                                               NOTE

                      You need to register the PAK before you install DEC RT
                      Integrator.

                      If you are installing in a DMS environment, you need
                      to register the PAK on the client, not the server.

                  To register a license under ULTRIX, first log in as supe-
                  ruser.

                  At the superuser prompt, edit an empty PAK template with the
                  lmf register command and include all the information on your
                  License PAK as follows:

                    # lmf register

                  After you register your license, use the following lmf reset
                  command to copy the license details from the License Database
                  (LDB) to the kernel cache:

                    # lmf reset

                  For complete information on using the ULTRIX License
                  Management Facility, see the ULTRIX Version 4.0 Guide to
                  Software Licensing or the lmf(8) reference page.






               2-2  Installing DEC RT Integrator on RISC ULTRIX

 










               ____________________________________________________________

               2.2  Aborting the Installation

                  To abort the installation procedure at any time, press the
                  interrupt character (usually Ctrl/C within a Digital environ-
                  ment). When you abort the installation procedure, it does not
                  delete files created up to that point. You must delete these
                  files interactively. See Appendix A for a list of files and
                  directories created during the installation procedure.

               ____________________________________________________________

               2.3  Installing DEC RT Integrator Locally

                  This installation procedure loads DEC RT Integrator files
                  on a disk that belongs to the system where you perform the
                  installation. When DEC RT Integrator is run, its executable
                  images are mapped into memory on this system.

                  This section explains how to start a local installation pro-
                  cedure and how to respond to installation procedure prompts.

                  If you are installing DEC RT Integrator from tape media,
                  start with Section 2.3.1.

                  If you are installing DEC RT Integrator on a client system
                  using a RIS kit, start with Section 2.3.2.

               ____________________________________________________________

               2.3.1  Using TK50 Distribution Media

                  If you are installing DEC RT Integrator from tape media,
                  start the installation procedure as follows:

                   1. Mount the media on the appropriate tape drive.

                   2. Log in as superuser (login name root) to the system where
                     you are installing DEC RT Integrator.

                   3. Make sure that you are at the root (/) directory by en-
                     tering the following command:

                       # cd /

                   4. Enter a setld command that specifies the -l (load) func-
                     tion and the device special file name for the tape drive
                     where the media is mounted. For example, if you load a
                     magnetic tape on tape unit 0, enter the following command:

                               Installing DEC RT Integrator on RISC ULTRIX  2-3

 











                       # setld -l /dev/rmt0h

                     The installation procedure displays the following informa-
                     tion and prompt:

                       Please make sure your installation tape is mounted and on-line.
                       Are you ready (y/n)?

                     After all tape rewind and wind operations are complete and
                     the tape drive indicates online status, enter y.

                  See Section 2.4 to continue the installation.

               ____________________________________________________________

               2.3.2  Installing DEC RT Integrator from a RIS Server

                  To install DEC RT Integrator from a Remote Installation
                  Services (RIS) server to a RIS client you must first install
                  DEC RT Integrator in your RIS server environment. See your
                  RIS manager if DEC RT Integrator is not already installed in
                  the RIS server.























               2-4  Installing DEC RT Integrator on RISC ULTRIX

 











                  To install DEC RT Integrator subsets that reside in a
                  /var/adm/ris distribution area on a remote system, start
                  the installation procedure as follows:

                   1. Log in as superuser (login name root) to the system where
                     you are installing DEC RT Integrator.

                   2. Make sure that you are at the root (/) directory by en-
                     tering the following command:

                       # cd /

                   3. Enter a setld command that requests the load function and
                     identifies the system where DEC RT Integrator subsets are
                     located. For example, if you are loading DEC RT Integrator
                     subsets from a RIS distribution area on node bigsys, enter
                     the following command:

                       # setld -l bigsys:

                  If you receive an error, verify that you correctly followed
                  the preparation steps in Section 1.3.

                  See Section 2.4 to continue the installation.

               ____________________________________________________________

               2.4  Responding to Installation Procedure Prompts

                  This section explains the installation procedure displays and
                  prompts. See Section 2.4.2 for prompts for the Development
                  Kit subsets. See Section 2.4.4 for prompts for the Runtime
                  Kit subsets.

               ____________________________________________________________

               2.4.1  Determining Which Development Kit Subsets to Install

                  All subsets are optional and will be installed only if you
                  choose them. In deciding whether to install a subset, con-
                  sider whether you will make use of it and how much disk space
                  you have available. Appendix A lists the files in each sub-
                  set.
                  The subsets are described as follows:

                   o Laboratory Graphics Package (LGP) (RTILGP100), 5000
                     Kbytes, is a set of subroutines used in the graphical
                     presentation of scientific and engineering applications.

                               Installing DEC RT Integrator on RISC ULTRIX  2-5

 











                   o Laboratory Input/Output (LIO) (RTILIO100), 400 Kbytes, is
                     a set of subroutines used to control realtime I/O devices.

                   o Laboratory Signal Processing (LSP) (RTILSP100), 200
                     Kbytes, is a set of subroutines designed to make standard
                     measurements and analyses common in the laboratory.

                   o DEC RT Integrator (Development) (RTIBASE100), 6000 Kbytes,
                     allows the user to develop realtime applications using
                     the DECwindows graphical user interface, including data
                     acquisition, IEEE-488 and RS-232 instrument control, and
                     test and measurement.

                   o ULTRIX ek device driver (RTI488100 Subset), 2100 Kbytes,
                     supports the IEZ11. The IEZ11 is an IEEE-488 bus-
                     controller for Digital workstations with a SCSI interface.
                     DEC RT Integrator manages all SCSI interactions, allowing
                     the user to communicate directly with the IEEE-488 bus.

                   o DEC RT Integrator (Runtime) (RTIRTBASE100), 6000 Kbytes,
                     runs the DEC RT Integrator applications that have already
                     been developed.

                   o DEC RT Integrator Manual Pages (RTIMAN100 Subset) for
                     ULTRIX, 400 Kbytes, provides online reference pages for
                     the subroutine libraries.

                   o DEC RT Integrator Examples (RTIEXA100 Subset), 300 Kbytes,
                     includes sample programs for LIO, LGP, LSP and DEC RT
                     Integrator applications.

                   o Icon Development (RTIICON100 Subset), 9000 Kbytes, pro-
                     vides tools for you to use to develop user-defined icons.
                     It also provides a library and tools to link the user-
                     defined icons into the DEC RT Integrator environment.

               ____________________________________________________________

               2.4.2  Selecting Development Kit Subsets

                  After you enter the setld command for local (node-specific)
                  installations or after you start the dms or ris utility for
                  server installations, the installation procedure displays the
                  names of DEC RT Integrator subsets and asks you to specify
                  the subsets that you want to load:

               2-6  Installing DEC RT Integrator on RISC ULTRIX

 











                    The subsets listed below are optional:
                     1) DEC RT Integrator (Development)      2) ULTRIX ek device driver
                     3) Laboratory Graphic Package (LGP)     4) Laboratory IO (LIO)
                     5) Laboratory Signal Processing (LSP)   6) Icon Development
                     7) DEC RT Integrator (Runtime)          8) DEC RT Integrator Manual Pages
                     9) DEC RT Integrator Examples

                    10) All of the Above
                    11) None of the Above
                    12) Exit without installing subsets

                    Enter your choice(s): 10

                  When installing from a RIS server, note that the subset
                  numbers may vary depending on what products are available
                  in the RIS area.

                                               NOTE

                      If you specify more than one number at the prompt,
                      separate each number with a space, not a comma.

                  Next, the installation lets you verify your choice. For
                  example, if you enter 10 in response to the previous prompt,
                  you will see the following list of optional subsets:

                    Enter your choice(s): 10

                    You are installing the following subsets:
                       DEC RT Integrator (Development)         ULTRIX ek device driver
                       Laboratory Graphic Package (LGP)        Laboratory IO (LIO)
                       Laboratory Signal Processing (LSP)      Icon Development
                       DEC RT Integrator (Runtime)             DEC RT Integrator Manual Pages
                       DEC RT Integrator Examples

                    Is this correct? (y/n): y

                  If the displayed subsets are not the ones you intended to
                  choose, enter n. In this case, the subset selection menu is
                  again displayed, and you can correct your choice of optional
                  subsets.

                  If the displayed subsets are the ones you want to load, enter
                  y.

                               Installing DEC RT Integrator on RISC ULTRIX  2-7

 










               ____________________________________________________________

               2.4.3  Determining Which Runtime Kit Subsets to Install

                  DEC RT Integrator (RTIRTBASE100 Subset) is used to run ap-
                  plications that have already been developed. This subset
                  will install the executable files necessary to run DEC RT
                  Integrator.

                  All subsets are optional and will be installed only if you
                  choose them. In deciding whether to install a subset, con-
                  sider whether you will make use of it and how much disk space
                  you have available. Appendix A lists the files in each sub-
                  set.

                  The subsets are described as follows:

                   o Laboratory Graphics Package (LGP) (RTILGP100), 5000
                     Kbytes, is a set of subroutines used in graphical pre-
                     sentation of scientific and engineering applications.

                   o Laboratory Input/Output (LIO) (RTILIO100), 400 Kbytes, is
                     a set of subroutines used to control realtime I/O devices.

                   o Laboratory Signal Processing (LSP) (RTILSP100), 200
                     Kbytes, is a set of subroutines designed to make standard
                     measurements and analyses common in the laboratory.

                   o ULTRIX ek device driver (RTI488100 Subset), 2100 Kbytes,
                     supports the IEZ11. The IEZ11 is an IEEE-488 bus-
                     controller for Digital workstations with a SCSI interface.
                     DEC RT Integrator manages all SCSI interactions, allowing
                     the user to communicate directly with the IEEE-488 bus.

                   o DEC RT Integrator (Runtime) (RTIRUN100), 6000 Kbytes, runs
                     the DEC RT Integrator applications that have already been
                     developed.

                   o DEC RT Integrator Manual Pages (RTIRTMAN100 Subset) for
                     ULTRIX, 400 Kbytes, provides online reference pages for
                     the subroutine libraries.

                   o DEC RT Integrator Examples (RTIEXA100 Subset), 300 Kbytes,
                     includes sample programs for LIO, LGP, LSP and DEC RT
                     Integrator applications.

               2-8  Installing DEC RT Integrator on RISC ULTRIX

 










               ____________________________________________________________

               2.4.4  Selecting Runtime Kit Subsets

                  After you enter the setld command for local (node-specific)
                  installations, or after you start the dms or ris utility for
                  server installations, the installation procedure displays the
                  names of DEC RT Integrator subsets and asks you to specify
                  the subsets that you want to load:

                    The subsets listed below are optional:
                     1) DEC RT Integrator (Runtime)          2) ULTRIX ek device driver
                     3) Laboratory Graphic Package (LGP)     4) Laboratory IO (LIO)
                     5) Laboratory Signal Processing (LSP)   6) DEC RT Integrator Manual Pages
                     7) DEC RT Integrator Examples

                     8) All of the Above
                     9) None of the Above
                    10) Exit without installing subsets

                    Enter your choice(s): 8

                  When installing from a RIS server, note that the subset
                  numbers may vary depending on what products are available
                  in the RIS area.

                                               NOTE

                      If you specify more than one number at the prompt,
                      separate each number with a space, not a comma.

                  Next, the installation lets you verify your choice. For
                  example, if you enter 8 in response to the previous prompt,
                  you will see the following display:

                    You are installing the following subsets:
                       DEC RT Integrator (Runtime)             ULTRIX ek device driver
                       Laboratory Graphic Package (LGP)        Laboratory IO (LIO)
                       Laboratory Signal Processing (LSP)      DEC RT Integrator Manual Pages
                       DEC RT Integrator Examples

                    Is this correct? (y/n): y

                  If the displayed subsets are not the ones you intended to
                  choose, enter n. In this case, the subset selection menu is
                  again displayed, and you can correct your choice of optional
                  subsets.

                  If the displayed subsets are the ones you want to load, enter
                  y.

                               Installing DEC RT Integrator on RISC ULTRIX  2-9

 










               ____________________________________________________________

               2.4.5  Monitoring Displays During the Subset Loading Process

                  The procedure displays messages about the status of the
                  installation as it progresses.

                  Sections 2.8 and 2.10 discuss the postinstallation require-
                  ments.

                  If, during the course of the installation, you encounter
                  errors from the setld utility, see the Diagnostics section of
                  the setld(8) manual reference page for an explanation of the
                  error and the appropriate action to take.

                  If the verification process fails, you can look in the file
                  /usr/var/adm/fverify to find information that can help you
                  diagnose the problem.

               ____________________________________________________________

               2.5  Installing DEC RT Integrator into a Server Environment

                  This section explains how to start the installation procedure
                  and load software subsets when you are installing DEC RT
                  Integrator into an environment controlled by DMS (Diskless
                  Management Services) or RIS (Remote Installation Services).

                  If installing from a TK50, mount it on the appropriate device
                  of the server node. You will later be prompted to enter the
                  name of the special file for that device.

                  Section 2.5.1 explains how to install DEC RT Integrator
                  into a DMS server environment. Section 2.5.2 explains how
                  to install DEC RT Integrator into a RIS server environment.

               ____________________________________________________________

               2.5.1  DMS Server Installations

                  In a local (node-specific) installation, the system on which
                  you are installing DEC RT Integrator will use its own disks
                  when DEC RT Integrator is run. A local (node-specific) in-
                  stallation procedure loads DEC RT Integrator files on the
                  disks that belong to the system where you perform the instal-
                  lation. When DEC RT Integrator is run, its executable files
                  are mapped into memory on the same system.

               2-10  Installing DEC RT Integrator on RISC ULTRIX

 











                  In a diskless client environment, the system on which you
                  are installing DEC RT Integrator is a server for Diskless
                  Management Services (DMS) and provides the disks for client
                  systems running DEC RT Integrator software. This installa-
                  tion environment is referred to as "diskless" because the
                  system uses DEC RT Integrator software accessed through
                  the network by Network File System (NFS) software. When DEC
                  RT Integrator is run by users logged into a client system,
                  DEC RT Integrator executables are mapped into memory on the
                  client system rather than the server system. From the per-
                  spective of the client node, DEC RT Integrator installation
                  is handled entirely by the manager of the DMS server area.

                                               NOTE

                      The diskless server area does not provide DEC RT
                      Integrator software to users logged in to the server
                      system itself. Installing DEC RT Integrator into the
                      diskless environment provides DEC RT Integrator soft-
                      ware only to client systems. Therefore, if users at
                      your site need to use DEC RT Integrator when logged in
                      to the local server system, you must perform a local
                      (node-specific) installation of DEC RT Integrator in
                      addition to the diskless installation.

                  The following procedure lets you install DEC RT Integrator
                  with the ULTRIX Version 4.0 dms utility into the diskless
                  server area. The examples in this section show how to install
                  the subsets to /dlenv0/root0.mips.

                                               NOTE

                      To start the installation procedure, use the dms util-
                      ity. Do not use the setld command.

                   1. Log in as superuser.

                   2. To invoke the dms utility, enter the following command:

                       # /etc/dms

                   3. Select the Install Software option from the following menu
                     by typing i:


                              Installing DEC RT Integrator on RISC ULTRIX  2-11

 











                       DISKLESS MANAGEMENT SERVICES (DMS) UTILITY MENU

                               a -  Add Client Processor
                               m -  Modify Client Parameters
                               r -  Remove Client Processor
                               l -  List Registered Clients
                               s -  Show Products in Diskless Environments
                               i -  Install Software
                               c -  Create Diskless Area on Disk
                               k -  Kernel Rebuild or Copy
                               e -  Exit

                       Enter your choice: i

                   4. Choose option 2 in the following menu:

                       The menu below offers you two software installation alternatives:

                          1)  You can install an operating system to a new diskless area.

                          2)  You can install additional software to an existing diskless
                              area that already contains an operating system.

                       Diskless Area Software Installation Menu:

                               1  Install Operating System to New Area
                               2  Add Software to Existing Area
                               3  Return to Previous Menu

                       Enter your choice: 2

                   5. The following message lists the available installation
                     directories:

                       You have chosen to install additional software into an existing diskless
                       environment.  These are the available installation directories:

                     If there is more than one installed rootn.mips direc-
                     tory in the diskless server area, choose the appropriate
                     directory from the menu that lists existing rootn.mips
                     directories. For example:

                       1.  /dlenv0/root0.mips
                       2.  /dlenv0/root1.mips
                       3.  /dlenv0/root0.vax

                       Enter your choice: 1

               2-12  Installing DEC RT Integrator on RISC ULTRIX

 











                   6. You are next prompted for an input device name:

                       Enter the device special name or mount point of the distribution
                       media, for example, /dev/rmt0h: /dev/rmt0h

                   7. If you want all registered clients to automatically have
                     access to DEC RT Integrator, enter y to the following
                     question:

                       The product software will automatically be propogated to every
                       registered client. Is this alright? (y/n):  y

                     If you answer n, DMS returns you to the main menu.

                   8. If your distribution media is tape, a message appears
                     asking you to confirm that the tape is ready and on line.
                     If it is, enter y.

                       Please make sure your installation tape is mounted and on-line.
                       Are you ready (y/n)?   y
                       Positioning Tape

                   9. The next message lists the software subsets you select for
                     automatic installation. See Section 2.4.5 to monitor the
                     displays during the subset load process and to complete
                     the installation procedure.

                   10.If diskless clients are registered to share this area, a
                     prompt asks you if you want to update the client_name.root
                     directories of those clients.

                     Enter yes to keep the diskless clients in a consistent
                     state.

                  Repeat these installation procedures for each rootn.mips area
                  you plan to set up.

                  The dms main menu appears for your next selection.

               ____________________________________________________________

               2.5.2  RIS Server Installations

                                               NOTE

                      To start the installation procedure, use the ris util-
                      ity. Do not use the setld command.

                              Installing DEC RT Integrator on RISC ULTRIX  2-13

 











                  The following sample session describes how to add the DEC RT
                  Integrator product to the ris0.mips area:

                   1. Log in as superuser.

                   2. Invoke the ris utility by entering the following command:

                       # /etc/ris

                   3. Select the Install Software option from the Remote
                     Installation Services (RIS) Menu by typing i:

                       REMOTE INSTALLATION SERVICES (RIS) MENU

                               a -  Add Client
                               r -  Remove Client
                               s -  Show Products in Remote Installation Environments
                               m -  Modify Client
                               i -  Install Software
                               e -  Exit

                       Enter your choice: i

                   4. Choose option 2 from the RIS Software Installation Menu:

                       The menu below offers you two software installation alternatives:

                           1) You can create a new area to serve either RISC or VAX clients
                              by installing a software product.  The ris utility automatically
                              creates the new area.

                           2) You can install additional software to an existing area
                              that serves either RISC or VAX clients.

                           RIS Software Installation Menu:

                           1  Install Software to a New Area.
                           2  Add Software to an Existing Area.
                           3  Return to Previous Menu

                       Enter your choice: 2

                   5. A list of available environments appears from which you
                     might select ris0.mips:

               2-14  Installing DEC RT Integrator on RISC ULTRIX

 











                       You have chosen to add a new product into an existing environment.

                       Select the remote installation environment:

                       1  /var/adm/ris/ris0.mips
                           ULTRIX V4.0/ULTRIX WS V4.0 MANDATORY SUPPORTED (RISC)

                       2  /var/adm/ris/ris0.vax
                           ULTRIX V4.0/ULTRIX WS V4.0 SUPPORTED (VAX)

                       Enter your choice: 1

                   6. You are next prompted for an input device name:

               Enter the device special file name or the path of the directory where the
               software is located, for example, /dev/rmt0h:
               /dev/rmt0h

                   7. If your distribution media is tape, a message appears
                     asking you to confirm that the tape is ready and on line.
                     If it is, enter y:

                       Please make sure your installation tape is mounted and on-line.
                       Are you ready (y/n)?  y
                       Positioning Tape

                   8. The next message lists the software subsets you select
                     for automatic installation. See Section 2.4.2 to spec-
                     ify the Development Kit subsets you want to load. See
                     Section 2.4.4 to specify the Runtime Kit subsets you want
                     to load. See Section 2.4.5 to monitor the displays during
                     the subset load process and to complete the installation
                     procedure.

                   9. After the subsets are installed, the following message
                     appears:

                       Media extraction complete.

                   10.Repeat steps a to f for each RIS client allowed to install
                     DEC RT Integrator.

                      a. The ris main menu appears for your next selection.
                        Select the Modify Client option from the Remote
                        Installation Services (RIS) Menu by typing m:

                              Installing DEC RT Integrator on RISC ULTRIX  2-15

 











                          REMOTE INSTALLATION SERVICES (RIS) MENU
                                  a -  Add Client
                                  r -  Remove Client
                                  s -  Show Products in Remote Installation Environments
                                  m -  Modify Client
                                  i -  Install Software
                                  e -  Exit

                          Enter your choice: m

                      b. Enter the name of the client to be modified from the
                        list of available clients:

                          The following clients are available to modify:

                          clienta clientb

                          Enter the client processor's hostname: clienta

                      c. Make sure the client processor's hardware Ethernet
                        address. Press Return to choose the default address,
                        the address assigned when the client was added to the
                        RIS environment.

                          Enter the client processor's hardware Ethernet address, for
                          example, 08-00-2b-02-67-e1 [08-00-2b-14-ac-d1]: <Return>

                      d. Choose the products you want this client to have access
                        to. You are shown the client's currently selected RIS
                        environment and the products the selected client al-
                        ready has access to. At the prompt, enter the products
                        you would like this client to be able to install in-
                        cluding DEC RT Integrator. Separate each choice with a
                        space.

                          The existing environment is /usr/var/adm/ris/ris0.mips.

                          The client currently can install the following products
                          from /usr/var/adm/ris/ris0.mips:

                              'ULTRIX V4.0/ULTRIX WS V4.0 MANDATORY SUPPORTED (RISC) '

                          Select one or more products for the client to install
                          from /usr/var/adm/ris/ris0.mips:

               2-16  Installing DEC RT Integrator on RISC ULTRIX

 











                          Product    Description
                           1    'ULTRIX V4.0/ULTRIX WS V4.0 MANDATORY SUPPORTED (RISC) '
                           2    'DEC RT Integrator '
                           3    'DEC GKS-3D for ULTRIX'

                          Enter one or more choices, for example, 1 2:  1 2

                      e. If the list of products available to this client is
                        correct, enter y. If the list is not correct, enter n
                        to return to step d and reenter the products.

                          You chose the following products:

                           1    'ULTRIX V4.0/ULTRIX WS V4.0 MANDATORY SUPPORTED (RISC) '
                           2    'DEC RT Integrator '
                           3    'DEC GKS-3D for ULTRIX'

                          Is that correct (y/n)? [y]: y

                      f. After modifying the client's records with the new
                        list of installable products available, the following
                        confirmation message appears:

                          clienta has been modified.

               ____________________________________________________________

               2.6  Development Kit Installation Procedure

                  To start the installation of ULTRIX, enter the following
                  command:

                    # setld -l /dev/rmt0h

                  The following prompt appears on your screen:

                    *** Enter Subset Selections ***

                    The subsets listed below are optional:
                     1) DEC RT Integrator (Development)      2) ULTRIX ek device driver
                     3) Laboratory Graphic Package (LGP)     4) Laboratory IO (LIO)
                     5) Laboratory Signal Processing (LSP)   6) Icon Development
                     7) DEC RT Integrator (Runtime)          8) DEC RT Integrator Manual Pages
                     9) DEC RT Integrator Examples

                    10) All of the Above
                    11) None of the Above
                    12) Exit without installing subsets

                              Installing DEC RT Integrator on RISC ULTRIX  2-17

 











                    Enter your choice(s): 10

                  You can choose all of the above (10), none of the above (11),
                  or exit the installation (12). If you want to install fewer
                  than all the subsets, choose the number(s) of the subsets and
                  separate them with a space. For example:

                    Enter your choice(s): 1  4

                  In the sample installation, we chose to install all the
                  subsets:

                    Enter your choice(s): 10

                  The following prompt appears, listing the subsets we chose to
                  install:

                    You are installing the following subsets:
                       DEC RT Integrator (Development)         ULTRIX ek device driver
                       Laboratory Graphic Package (LGP)        Laboratory IO (LIO)
                       Laboratory Signal Processing (LSP)      Icon Development
                       DEC RT Integrator (Runtime)             DEC RT Integrator Manual Pages
                       DEC RT Integrator Examples

                    Is this correct? (y/n): y

                  If you choose y, the installation continues. If you choose
                  n, the list of subsets reappears and the prompt asks you to
                  enter your choice(s).

                  Choose y and the installation continues as follows:

                    Copying DEC RT Integrator (Development) (RTIBASE100) from disk
                    Verifying DEC RT Integrator (Development) (RTIBASE100)

                    Copying ULTRIX ek device driver (RTI488100) from disk
                    Verifying ULTRIX ek device driver (RTI488100)

                    Copying Laboratory Graphic Package (LGP) (RTILGP100) from disk
                    Verifying Laboratory Graphic Package (LGP) (RTILGP100)

                    Copying Laboratory IO (LIO) (RTILIO100) from disk
                    Verifying Laboratory IO (LIO) (RTILIO100)

                    Copying Laboratory Signal Processing (LSP) (RTILSP100) from disk
                    Verifying Laboratory Signal Processing (LSP) (RTILSP100)

                    Copying Icon Development (RTIICON100) from disk
                    Verifying Icon Development (RTIICON100)

               2-18  Installing DEC RT Integrator on RISC ULTRIX

 











                    Copying DEC RT Integrator (Runtime) (RTIRTBASE100) from disk
                    Verifying DEC RT Integrator (Runtime) (RTIRTBASE100)

                    Copying DEC RT Integrator Manual Pages (RTIMAN100) from disk
                    Verifying DEC RT Integrator Manual Pages (RTIMAN100)

                    Copying DEC RT Integrator Examples (RTIEXA100) from disk
                    Verifying DEC RT Integrator Examples (RTIEXA100)

                    *************************************************************
                    * Installation of DEC RT Integrator V1.0 complete.          *
                    *                                                           *
                    * The IVP for DEC RT Integrator for ULTRIX can be run after *
                    * the installation has completed.                           *
                    *                                                           *
                    * To run the IVP, enter the following command:              *
                    *        setld -v RTIBASE100                                *
                    *************************************************************

                    Creating/Modifying necessary files for the ULTRIX ek Driver V1.0
                    For ULTRIX V40

                    Creating links to V40 objects...
                    Created scsi_asc.o...
                    Created scsi_sii.o...
                    Created scsi.o...
                    Created scsi_proc.o...
                    Created ekdriver.o...

                    Modifying appropriate driver files...
                    Modifying /sys/data/scsi_data.c

                    Modifying /sys/io/scsi/mips/scsireg.h

                    Modifying /sys/conf/mips/files.mips

                    Modifying /sys/machine/common/conf.c

                  If you are not installing in a DMS environment, the following
                  messages appear:

                    Configuring the system to run the ULTRIX ek Driver V1.0
                    For ULTRIX V40


                              Installing DEC RT Integrator on RISC ULTRIX  2-19

 











                    Creating /dev/ek0
                    Creating /dev/ek1
                    Creating /dev/ek2
                    Creating /dev/ek3
                    Creating /dev/ek4
                    Creating /dev/ek5
                    Creating /dev/ek6
                    Creating /dev/ek7
                    Creating /dev/ek8
                    Creating /dev/ek9
                    Creating /dev/ek10
                    Creating /dev/ek11
                    Creating /dev/ek12
                    Creating /dev/ek13
                    Creating /dev/ek14
                    Creating /dev/ek15

                    After verifying that the system is operating properly with the
                    ek  Driver installed you may wish to remove the following
                    saved files:
                    - /sys/conf/mips/files.mips.sav[n]
                    - /sys/machine/common/conf.c.sav[n]
                    - /sys/data/scsi_data.c.sav[n]
                    - /sys/conf/mips/MUNCHY.sav[n]

                    Reminder:
                       - Edit /sys/conf/mips/MUNCHY
                       - Rebuild your kernel
                       - Move the new kernel to /.
                       - Reboot your system.

                    Installation of the ULTRIX ek Driver V1.0 complete

                  After the files are copied and the IVP is run, ULTRIX veri-
                  fies that the procedures were successful by displaying the
                  ULTRIX prompt:

                    #

                  If you are installing DEC RT Integrator on a server in a
                  DMS environment, the messages on the screen stop after the
                  Modifying /sys/machine/common/conf.c message.



               2-20  Installing DEC RT Integrator on RISC ULTRIX

 











                  You must now reboot all clients before rebuilding the kernel.
                  Then the installation begins configuring the system to run
                  the ek driver. The following messages appear on the clients:

                    Configuring the system to run the ULTRIX ek Driver V1.0
                    For ULTRIX V40

                    Creating /dev/ek0
                    Creating /dev/ek1
                    Creating /dev/ek2
                    Creating /dev/ek3
                    Creating /dev/ek4
                    Creating /dev/ek5
                    Creating /dev/ek6
                    Creating /dev/ek7
                    Creating /dev/ek8
                    Creating /dev/ek9
                    Creating /dev/ek10
                    Creating /dev/ek11
                    Creating /dev/ek12
                    Creating /dev/ek13
                    Creating /dev/ek14
                    Creating /dev/ek15

                    After verifying that the system is operating properly with the
                    ek  Driver installed you may wish to remove the following
                    saved files:
                    - /sys/conf/mips/files.mips.sav[n]
                    - /sys/machine/common/conf.c.sav[n]
                    - /sys/data/scsi_data.c.sav[n]
                    - /sys/conf/mips/MUNCHY.sav[n]

                    Reminder:
                       - Edit /sys/conf/mips/MUNCHY
                       - Rebuild your kernel
                       - Move the new kernel to /.
                       - Reboot your system.

                    Installation of the ULTRIX ek Driver V1.0 complete

                  After the files are copied and the IVP is run, ULTRIX veri-
                  fies that the procedures were successful by displaying the
                  ULTRIX prompt:

                    #

                              Installing DEC RT Integrator on RISC ULTRIX  2-21

 










               ____________________________________________________________

               2.7  Runtime Kit Installation Procedure

                  To start the installation of ULTRIX, enter the following
                  command:

                    # setld -l  /dev/rmt0h

                  The following prompt appears on your screen:

                    *** Enter Subset Selections ***

                    The subsets listed below are optional:
                     1) DEC RT Integrator (Runtime)          2) ULTRIX ek device driver
                     3) Laboratory Graphic Package (LGP)     4) Laboratory IO (LIO)
                     5) Laboratory Signal Processing (LSP)   6) DEC RT Integrator Manual Pages
                     7) DEC RT Integrator Examples

                     8) All of the Above
                     9) None of the Above
                    10) Exit without installing subsets

                    Enter your choice(s): 8

                  You can choose all of the above (8), none of the above (9)
                  or exit the installation (10). If you want to install fewer
                  than all the subsets, choose the number(s) of the subsets and
                  separate them with a space. For example:

                    Enter your choice(s):  2 3

                  In the sample installation, we chose to install all the
                  subsets:

                    Enter your choice(s): 8

                  The following prompt appears, listing the subsets we chose to
                  install:

                    You are installing the following subsets:
                       DEC RT Integrator (Runtime)             ULTRIX ek device driver
                       Laboratory Graphic Package (LGP)        Laboratory IO (LIO)
                       Laboratory Signal Processing (LSP)      DEC RT Integrator Manual Pages
                       DEC RT Integrator Examples

                    Is this correct? (y/n): y

               2-22  Installing DEC RT Integrator on RISC ULTRIX

 











                  If you choose y, the installation continues. If you choose
                  n, the list of subsets reappears and the prompt asks you to
                  enter your choice(s).

                  Choose y and the installation continues as follows:

                    Copying DEC RT Integrator (Runtime) (RTIRUN100) from disk
                    Verifying DEC RT Integrator (Runtime) (RTIRUN100)

                    Copying ULTRIX ek device driver (RTI488100) from disk
                    Verifying ULTRIX ek device driver (RTI488100)

                    Copying Laboratory Graphic Package (LGP) (RTILGP100) from disk
                    Verifying Laboratory Graphic Package (LGP) (RTILGP100)

                    Copying Laboratory IO (LIO) (RTILIO100) from disk
                    Verifying Laboratory IO (LIO) (RTILIO100)

                    Copying Laboratory Signal Processing (LSP) (RTILSP100) from disk
                    Verifying Laboratory Signal Processing (LSP) (RTILSP100)

                    Copying DEC RT Integrator Manual Pages (RTIRTMAN100) from disk
                    Verifying DEC RT Integrator Manual Pages (RTIRTMAN100)

                    Copying DEC RT Integrator Examples (RTIEXA100) from disk
                    Verifying DEC RT Integrator Examples (RTIEXA100)

                    *************************************************************
                    * Installation of DEC RT Integrator V1.0 complete.          *
                    *                                                           *
                    * The IVP for DEC RT Integrator for ULTRIX can be run after *
                    * the installation has completed.                           *
                    *                                                           *
                    * To run the IVP, enter the following command:              *
                    *        setld -v RTIRUN100                                 *
                    *************************************************************

                    Creating/Modifying necessary files for the ULTRIX ek Driver V1.0
                    For ULTRIX V40

                    Creating links to V40 objects...
                    Created scsi_asc.o...
                    Created scsi_sii.o...
                    Created scsi.o...
                    Created scsi_proc.o...
                    Created ekdriver.o...

                              Installing DEC RT Integrator on RISC ULTRIX  2-23

 











                    Modifying appropriate driver files...
                    Modifying /sys/data/scsi_data.c

                    Modifying /sys/io/scsi/mips/scsireg.h

                    Modifying /sys/conf/mips/files.mips

                    Modifying /sys/machine/common/conf.c

                  If you are not installing in a DMS environment, the following
                  messages appear:

                    Configuring the system to run the ULTRIX ek Driver V1.0
                    For ULTRIX V40

                    Creating /dev/ek0
                    Creating /dev/ek1
                    Creating /dev/ek2
                    Creating /dev/ek3
                    Creating /dev/ek4
                    Creating /dev/ek5
                    Creating /dev/ek6
                    Creating /dev/ek7
                    Creating /dev/ek8
                    Creating /dev/ek9
                    Creating /dev/ek10
                    Creating /dev/ek11
                    Creating /dev/ek12
                    Creating /dev/ek13
                    Creating /dev/ek14
                    Creating /dev/ek15

                    After verifying that the system is operating properly with the
                    ek  Driver installed you may wish to remove the following
                    saved files:
                    - /sys/conf/mips/files.mips.sav[n]
                    - /sys/machine/common/conf.c.sav[n]
                    - /sys/data/scsi_data.c.sav[n]
                    - /sys/conf/mips/MUNCHY.sav[n]

                    Reminder:
                       - Edit /sys/conf/mips/MUNCHY
                       - Rebuild your kernel
                       - Move the new kernel to /.
                       - Reboot your system.

               2-24  Installing DEC RT Integrator on RISC ULTRIX

 











                    Installation of the ULTRIX ek Driver V1.0 complete

                  After the files are copied and the IVP is run, ULTRIX veri-
                  fies that the procedures were successful by displaying the
                  ULTRIX prompt:

                    #

                  If you are installing DEC RT Integrator on a server in a
                  DMS environment, the messages on the screen stop after the
                  Modifying /sys/machine/common/conf.c message.

                  You must now reboot all clients before rebuilding the kernel.
                  Then the installation begins configuring the system to run
                  the ek driver. The following messages appear on the clients:

                    Configuring the system to run the ULTRIX ek Driver V1.0
                    For ULTRIX V40

                    Creating /dev/ek0
                    Creating /dev/ek1
                    Creating /dev/ek2
                    Creating /dev/ek3
                    Creating /dev/ek4
                    Creating /dev/ek5
                    Creating /dev/ek6
                    Creating /dev/ek7
                    Creating /dev/ek8
                    Creating /dev/ek9
                    Creating /dev/ek10
                    Creating /dev/ek11
                    Creating /dev/ek12
                    Creating /dev/ek13
                    Creating /dev/ek14
                    Creating /dev/ek15

                    After verifying that the system is operating properly with the
                    ek  Driver installed you may wish to remove the following
                    saved files:
                    - /sys/conf/mips/files.mips.sav[n]
                    - /sys/machine/common/conf.c.sav[n]
                    - /sys/data/scsi_data.c.sav[n]
                    - /sys/conf/mips/MUNCHY.sav[n]


                              Installing DEC RT Integrator on RISC ULTRIX  2-25

 











                    Reminder:
                       - Edit /sys/conf/mips/MUNCHY
                       - Rebuild your kernel
                       - Move the new kernel to /.
                       - Reboot your system.

                    Installation of the ULTRIX ek Driver V1.0 complete

                  After the files are copied and the IVP is run, ULTRIX veri-
                  fies that the procedures were successful by displaying the
                  ULTRIX prompt:

                    #

               ____________________________________________________________

               2.8  Reconfiguring the Kernel to Support the ek Driver

                  This section describes how to reconfigure the kernel to add
                  the ULTRIX ek device driver.

                                               NOTE

                      When installing the ek device driver into a DMS area,
                      the client is responsible for reconfiguring the kernel
                      after the server installs the ULTRIX ek driver subset
                      (RTI488100) into the DMS area.

               ____________________________________________________________

               2.8.1  Editing the Configuration File

                  To add an ek device to your current system, you need to
                  perform the following steps:

                   1. Set your directory to your configuration area.

                       # cd /sys/conf/mips

                   2. Save a copy of the configuration file.

                       # cp HOSTNAME HOSTNAME.sav

                                                 NOTE

                         Use the name assigned to your system in place of
                         HOSTNAME.

               2-26  Installing DEC RT Integrator on RISC ULTRIX

 











                   3. Edit the configuration file.

                       # vi HOSTNAME

                   4. Add a line for each ek device you are installing on your
                     system. This line should be made up of four fields, as
                     shown in Table 2-1. You must supply the information within
                     the brackets ([]).

               Table 2-1:  ek Device Driver Configuration File
               ________________________________________________________________
                                            Fields
               1______2_______________3___________________4____________________

               device [device name,   at [SCSI bus        drive [SCSI device
                      logical unit    adapter name,       unit number]
                      number]         SCSI bus adapter
                                      unit number]
               ________________________________________________________________
               _____________________________Example____________________________

               device_ek12____________at_asc1_____________drive_4______________

               ____________________________________________________________

               2.8.2  Computing Values in the Configuration File

                  The values of fields 2, 3, and 4 change for each system,
                  depending on its configuration.

                  The values are dependent on one another. You have to calcu-
                  late the value of field 4 first and use that to calculate the
                  value of field 3, then field 2.












                              Installing DEC RT Integrator on RISC ULTRIX  2-27

 











                  Field 4. Drive [SCSI Device Unit Number]

                  In field 4, the [SCSI device unit number] is the address
                  of the ek device on the SCSI bus. The number of the address
                  is from 0 to 7. In Table 2-1, the ek device is at SCSI bus
                  address number 4.

                  You can select the address on the SCSI bus by manipulating
                  the switches on the back of the device. (See your appropriate
                  hardware manual for information on selecting the address of
                  the device.)

                  Field 3. at [SCSI Bus Adapter Name, SCSI Bus Adapter Unit
                  Number]

                  In field 3, the [bus name] is the SCSI bus adapter identi-
                  fier. It is made up of two parts:

                   o SCSI bus adapter name, asc or sii

                     The SCSI bus adapter uses different letters to identify
                     different DECstations. The DECstation 5000 letters are
                     "asc." The DECstation 2100 and the DECstation 3100 letters
                     are "sii."

                   o SCSI bus adapter unit number, 0 to 3

                     The SCSI bus adapter unit number indicates which SCSI bus
                     adapter the ek device connects to.

                     The SCSI bus adapter unit number for the DECstation 2100
                     and the DECstation 3100 is always 0. The full SCSI bus
                     adapter identifier, the letters followed immediately
                     by the adapter unit number, is always "sii0" for these
                     machines.

                     The DECstation 5000 can be configured with up to 4 SCSI
                     bus adapters. A SCSI bus adapter unit number is from 0
                     to 3. The SCSI bus adapter name and unit number for a
                     DECstation 5000 can range from "asc0" to "asc3."

                  Field 2. [Device Name, Logical Unit Number]

                  In field 2, the [device name] is the name of the driver and
                  its logical unit number. It is made up of two parts:

                   o Device Name

                     The device name for the ek device is "ek."

                   o Logical Unit Number

               2-28  Installing DEC RT Integrator on RISC ULTRIX

 











                     The logical unit number is derived from a formula using
                     the [unit number] from field 3 and the [bus name] from
                     field 4.










































                              Installing DEC RT Integrator on RISC ULTRIX  2-29

 











                     To obtain the logical unit number, follow these steps:

                      1. Multiply 8 (the maximum number of devices on the SCSI
                        bus) times the SCSI bus adapter unit number (1 in this
                        example, from the 1 in "asc1").

                      2. Add to this the SCSI device address [unit number] (4 in
                        this example from "drive 4").

                        The formula looks like the following:

                          (8 * SCSI bus adapter number) + SCSI Device Address

                                        (8 * 1)   +    4

                                                  12

                        In the example in Table 2-1, the value for field 2 is
                        ek12.

                        Examples:

                         _ An ek device installed on the SCSI bus of the

                           DECstation 3100 at SCSI address 4 would have the
                           following configuration:

                             device      ek4      at sii0      drive 4

                                       (8*0 +4)

                         _ The same ek device connected to the primary SCSI

                           bus of a DECstation 5000 would have the following
                           configuration:

                             device      ek4      at asc0      drive 4

                                       (8*0 +4)

                         _ The same ek device connected to a second SCSI bus of

                           a DECstation 5000 would have the following configu-
                           ration:

                             device      ek12      at asc1      drive 4

                                      (8*1 +4)

               2-30  Installing DEC RT Integrator on RISC ULTRIX

 










               ____________________________________________________________

               2.8.3  Building a New Kernel

                  After you edit the configuration file, process it and build a
                  new kernel:

                   1. Configure your kernel.

                       # doconfig -c HOSTNAME

                     See the doconfig(8) Manual Page for more information on
                     rebuilding your kernel.

                   2. Save your old kernel.

                       # cp /vmunix /vmunix.sav

                   3. Move your new kernel to the root directory.

                       # cp /sys/MIPS/HOSTNAME/vmunix /vmunix

                   4. Reboot your system with the new kernel.

                       # reboot

               ____________________________________________________________

               2.9  Reconfiguring the Kernel to Delete the ek Driver

                  You may for some reason need to delete the ek device driver
                  after it is installed. This section describes how to delete
                  the driver.

                                               NOTE

                      When deleting the ek device driver from a DMS area,
                      the client is responsible for reconfiguring the kernel
                      before the server deletes the ULTRIX ek driver subset
                      (RTI488100) from the DMS area.

               ____________________________________________________________

               2.9.1  Editing the Configuration File

                  To delete an ek device from your system, perform the follow-
                  ing steps:

                   1. Set your directory to your configuration area.

                       # cd /sys/conf/mips

                              Installing DEC RT Integrator on RISC ULTRIX  2-31

 











                   2. Save a copy of the configuration file.

                       # cp HOSTNAME HOSTNAME.sav

                                                 NOTE

                         Use the name assigned to your system in place of
                         HOSTNAME.

                   3. Edit the configuration file.

                       # vi HOSTNAME

                   4. Delete the line for each ek device that was installed on
                     your system. Refer to Section 2.8.2 for information on how
                     each device was added to the configuration file.

               ____________________________________________________________

               2.9.2  Configuring the System to Delete the Driver from a DMS
                      Client

                  This section describes an additional step that you must
                  perform to delete the ek driver from a DMS area.

                  You must do the following to configure the DMS client to
                  delete the ek driver:

                    # setld -c RTI488100 DELETE

                  The following message appears on your screen:

                    Configuring RTI488100

                    Configuring the system to delete the ULTRIX ek Driver V1.0
                            for ULTRIX V40









               2-32  Installing DEC RT Integrator on RISC ULTRIX

 











                            Deleting /dev/ek0
                            Deleting /dev/ek1
                            Deleting /dev/ek2
                            Deleting /dev/ek3
                            Deleting /dev/ek4
                            Deleting /dev/ek5
                            Deleting /dev/ek6
                            Deleting /dev/ek7
                            Deleting /dev/ek8
                            Deleting /dev/ek9
                            Deleting /dev/ek10
                            Deleting /dev/ek11
                            Deleting /dev/ek12
                            Deleting /dev/ek13
                            Deleting /dev/ek14
                            Deleting /dev/ek15

               ____________________________________________________________

               2.9.3  Building a New Kernel

                  After you edit the configuration file, process it and build a
                  new kernel, as described in Section 2.8.3.

               ____________________________________________________________

               2.10  Installation Verification Procedure (IVP)

                  The DEC RT Integrator Installation Verification Procedure
                  (IVP) verifies the installation by running a sample DEC RT
                  Integrator application.

                  You should run the IVP to verify that DEC RT Integrator is
                  installed correctly.

                  See Chapter 3 for information about running the IVP.

               ____________________________________________________________

               2.11  Error Messages

                  Errors can occur during the installation if any of the fol-
                  lowing conditions exist:

                   o The operating system version is incorrect.

                   o A prerequisite software version is incorrect.

                   o /usr file system space is insufficient.

                              Installing DEC RT Integrator on RISC ULTRIX  2-33

 











                   o The installation is being attempted on a non-RISC plat-
                     form.

                  For descriptions of the error messages generated by these
                  conditions, see the ULTRIX documentation on system messages,
                  recovery procedures, and installation.

                  For information on DEC RT Integrator installation require-
                  ments, see Chapter 1.

               ____________________________________________________________

               2.12  Determining the Files Added to the System

                  The DEC RT Integrator installation procedure creates or
                  modifies a number of files. Appendix A has a complete list of
                  these files.

               ____________________________________________________________

               2.13  Reporting Problems

                  If an error occurs while using DEC RT Integrator and you
                  believe that the error is caused by a problem with DEC RT
                  Integrator, take one of the following actions:

                   o If you have a basic or DECsupport Software Agreement, call
                     your Customer Support Center. The Customer Support Center
                     provides telephone support for high-level advisory and
                     remedial assistance.

                   o If you have a Self-Maintenance Software Agreement, submit
                     a Software Performance Report (SPR).

                   o If you purchased DEC RT Integrator within the past 90 days
                     and you think the problem is caused by a software error,
                     submit an SPR.

                  If you find an error in the DEC RT Integrator documentation,
                  fill out and submit the Reader's Comments form at the back of
                  the document in which the error occurred. Include the section
                  and page number where the error occurred.



               2-34  Installing DEC RT Integrator on RISC ULTRIX

 

















                                                                      Chapter 3


                                                     Running the IVP for ULTRIX
               ________________________________________________________________


                  The Installation Verification Procedure (IVP) confirms that
                  the DEC RT Integrator files are properly installed and opera-
                  tional.

                  To run the IVP for the Development Kit after installation,
                  enter the following command at the prompt:

                    # setld -v RTIBASE100

                  To run the IVP for the Runtime Kit after installation, enter
                  the following command at the prompt:

                    # setld -v RTIRUN100

                  The informational messages for the IVP are identical whether
                  you run setld for the Development Kit or the Runtime Kit,
                  except for the name of the kit. The following messages appear
                  for the Development Kit (RTIBASE100):

                    Checking setld data files.
                    The Installation Verification Procedure comes in two forms:
                         a DECwindows version or a non-DECwindows version.

                    The DECwindows version of the IVP can be chosen if you are
                    installing DEC RT Integrator from a system which has a
                    DECwindows display, such as a DECwindows terminal or a
                    workstation running DECwindows.

                    If you choose the DECwindows version of the IVP, a plot
                    will be displayed similar to the one shown in Chapter 3
                    of the DEC RT Integrator Installation Guide.

                                                Running the IVP for ULTRIX  3-1

 











                    If you choose the non-DECwindows version of the IVP, a
                    message stating:
                            DEC RT Integrator V1.0 IVP completed
                    will be displayed once the IVP has been performed.

                    Would you like to run the DECwindows version of the IVP?
                    (y/n) [y]:

                  If you enter n, the IVP is run and you receive the following
                  message:

                    Running the RTIBASE100 for RISC V1.0 IVP
                     - executing the IVP...

                    DEC RT Integrator V1.0 IVP completed

                    The installation verification of DEC RT Integrator V1.0
                    for RISC/ULTRIX completed successfully.

                  If you enter y, the IVP is run and you receive the following
                  message:

                    Running the RTIBASE100 for RISC V1.0 IVP
                     - executing the IVP...

                  Then the IVP plot is displayed, as shown in Figure 3-1.
                  When the plot finishes displaying, you receive the following
                  message:

                    The installation verification of DEC RT Integrator V1.0
                    for RISC/ULTRIX completed successfully.

                  If you enter y and your DISPLAY environment variable is not
                  set, you receive the following message:

                    The DECwindows version of the IVP cannot be
                    performed since the DISPLAY environment variable
                    isn't set.

                    Would you like to set DISPLAY? (y/n) [y]

                  If you enter y, you receive the following message:

                    Set DISPLAY using the following forms:
                         node:0 for Internet
                         node:=0 for shared memory connection
                         node::0 for DECnet

               3-2  Running the IVP for ULTRIX

 











                    Set DISPLAY :

                  After you set the DISPLAY environment variable, you receive
                  the following message:

                    Running the RTIBASE100 for RISC V1.0 IVP
                     - executing the IVP...

                  Then the IVP plot is displayed, as shown in Figure 3-1.
                  When the plot finishes displaying, you receive the following
                  message:

                    The installation verification of DEC RT Integrator V1.0
                    for RISC/ULTRIX completed successfully.

                  If you enter n to the question Would you like to set DISPLAY?
                  the IVP does not execute and you receive the following mes-
                  sage:

                    Exiting from the IVP...

                  Figure 3-1:  IVP Plot for DEC RT Integrator
                  _____________________________________________________________













                  _____________________________________________________________








                                                Running the IVP for ULTRIX  3-3

 

















                                                                        Part II
                                   Installing DEC RT Integrator on a VMS System
               ________________________________________________________________



                  Part II contains information about installing DEC RT
                  Integrator on a VMS system.

 

















                                                                      Chapter 4


                                  Preparing to Install DEC RT Integrator on VMS
               ________________________________________________________________


                  Chapter 4 discusses the following:

                   o Description of Development Kit and Runtime Kit (see
                     Section 4.1)

                   o Software prerequisites (see Section 4.2)

                   o License registration (see Section 4.3)

                   o Running DEC RT Integrator in a VAXcluster (see Section 4.4)

                   o Installation procedure requirements (see Section 4.5)

                  Your bill of materials (BOM) and indented bills report (BIL)
                  specify the number and contents of your media. Verify the
                  contents of your kit with this information. If your kit is
                  damaged or if you find that parts of it are missing, contact
                  your Digital representative.

                  The Release Notes are part of the software and are accessible
                  during the installation process. For information on accessing
                  the release notes, see Section 6.1.

               ____________________________________________________________

               4.1  Development Kit Distinguished From Runtime Kit

                  The Development Kit allows the user to develop realtime
                  applications, including data acquisition, IEEE-488 and RS-232
                  instrument control, and test and measurement. The Runtime kit
                  allows the user to run an application but not to develop one.

                             Preparing to Install DEC RT Integrator on VMS  4-1

 











                  Instructions for installing the Development Kit and the
                  Runtime Kit are similar. The Development Kit installation
                  procedure is described in Section 5.2. The Runtime Kit in-
                  stallation procedure is described in Section 5.3.

               ____________________________________________________________

               4.2  Prerequisite and Optional Software

                  The following software installations must be complete before
                  you install DEC RT Integrator:

                   o The VMS Version 5.3 operating system

                   o The graphics software package, DEC GKS Version 4.1. Either
                     the Runtime Kit or the Development Kit is acceptable,
                     though you must have the DEC GKS Development Kit if you
                     plan to use GKS calls directly in a Laboratory Graphics
                     Package (LGP) program.

                     You should install the DEC GKS software before installing
                     DEC RT Integrator. If the DEC GKS software is not in-
                     stalled, you receive the following warning message:

                       %RTI-W-NOGKS, DEC GKS V4.0 must be installed for DEC RT Integrator
                       V2.0 LGP

                   o VMS Workstation Software (VWS) Version 4.0 for VAXstations
                     that will not be using DECwindows to display LGP plots

                  The IEZ11, DRB32 or Preston devices can be installed either
                  before or after installing DEC RT Integrator.

               ____________________________________________________________

               4.3  License Registration

                  You must register and load your license for DEC RT Integrator
                  before you start the installation to run the Installation
                  Verification Procedure (IVP) and use the software.

                  To register a license under VMS, log in to the system man-
                  ager's account, SYSTEM. Now you can register in one of the
                  following ways:

                   o Invoke the SYS$UPDATE:VMSLICENSE.COM procedure. When it
                     prompts you for information, respond with data from your
                     License product authorization key (PAK).

               4-2  Preparing to Install DEC RT Integrator on VMS

 











                   o At the DCL prompt, enter the LICENSE REGISTER command with
                     the appropriate qualifiers that correspond to License PAK
                     information.

                  If you plan to use DEC RT Integrator on more than one node in
                  a VAXcluster, you need to perform a license load on the other
                  nodes after you complete this installation. See Section 6.4.

                  See the Guide to Setting Up a VMS System for information on
                  the license registration procedure.

               ____________________________________________________________

               4.4  VAXcluster Considerations

                  DEC RT Integrator fully supports VAXclusters. If you are
                  using DEC RT Integrator in a VAXcluster, DEC RT Integrator
                  and the DEC RT Integrator license must be installed on the
                  boot node.

                                               NOTE

                      Time-critical I/O operations may be adversely af-
                      fected by cluster operations. If your applications
                      are extremely time-critical, you should not use DEC RT
                      Integrator in a VAXcluster.

               ____________________________________________________________

               4.5  Installation Procedure Requirements

                  The installation takes the following approximate times:

                   o Tape cartridge-about 60 minutes on a MicroVAX II

                   o Magnetic tape-from about 15 minutes to about 40 minutes,
                     depending on your system

                  These times include the time required to execute the IVP.
                  However, they do not include the time required to in-
                  stall other layered products you plan to use with DEC RT
                  Integrator. For those installation times, see the appropriate
                  layered product installation guides.


                             Preparing to Install DEC RT Integrator on VMS  4-3

 










               ____________________________________________________________

               4.5.1  Privileges and Disk Space

                  To install DEC RT Integrator, you must be logged in to an
                  account that has SETPRV or at least the following privileges:

                   o CMKRNL

                   o WORLD

                   o SYSPRV

                  Note that VMSINSTAL turns off BYPASS privilege at the start
                  of the installation.

                  Development Kit Disk Space Requirements

                  To install the Development Kit, the system disk must contain
                  17,000 free blocks. If your system disk contains less than
                  17,000 free blocks, the following error message is generated:

                    %RTI-E-NOROOM, DEC RT Integrator V2.0 requires at least 17,000 free disk
                           blocks.

                  The Development Kit requires 16,200 blocks after it is in-
                  stalled.

                  Runtime Kit Disk Space Requirements

                  To install the Runtime Kit, the system disk must contain
                  11,000 free blocks. The Runtime Kit requires 10,000 blocks
                  after it is installed.

                  To determine the number of free disk blocks on the current
                  system disk, enter the following command at the DCL prompt:

                    $ SHOW DEVICE SYS$SYSDEVICE

               ____________________________________________________________

               4.5.2  System Parameters

                  Table 4-1 lists the minimum required system parameter values
                  for the installation. These values represent the number
                  of free global pages and free global sections required for
                  the installation, not the total number you need to run your
                  system and other software.

               4-4  Preparing to Install DEC RT Integrator on VMS

 











                  Table 4-1:  Minimum Required System Parameter Values
                  _____________________________________________________________
                  GBLPAGES              n + 450
                  GBLSECTIONS___________n_+_20_________________________________

               ____________________________________________________________

               4.5.2.1  Checking System Parameter Values

                  To check Global Pages (GBLPAGES) you have to subtract the
                  number used from the total number available. To get the
                  number of Global Sections and Global Pages Used enter the
                  install command at the DCL prompt:

                    $ INSTALL

                  At the prompt, enter the following command:

                    INSTALL> LIST/GLOBAL/SUMMARY

                  You will get information in the following form:

                        Summary of Local Memory Global Sections

                    397 Global Sections Used,  40714/9286 Global Pages Used/Unused

                  This command gives you Global Sections (GBLSECTIONS) Unused.
                  To get Global Pages Unused, you have to use the following
                  command at the DCL prompt to invoke the System Generation
                  Utility:

                    $ RUN SYS$SYSTEM:SYSGEN

                  At the SYSGEN> prompt, enter the SHOW command, for example:

                    SYSGEN> SHOW GBLPAGES

                  You will get information in the following form:

                    Parameter Name     Current   Default   Minimum   Maximum Unit    Dynamic
                    --------------     -------   -------   -------   ------- ----    -------
                    GBLPAGES           50000     10000       512        -1 Pages

                  To get the number of free Global Pages, subtract the num-
                  ber of Global Sections Used (397 in this example) from the
                  Current number (50000 in this example).

                  Enter the EXIT command at the SYSGEN> prompt to return to DCL
                  level.

                             Preparing to Install DEC RT Integrator on VMS  4-5

 










               ____________________________________________________________

               4.5.2.2  Changing System Parameter Values with AUTOGEN

                  Use the AUTOGEN command procedure to change system param-
                  eters. AUTOGEN automatically adjusts values for parameters
                  that are associated with the values you reset manually.

                  To change system parameters with AUTOGEN, edit the following
                  file:

                    SYS$SYSTEM:MODPARAMS.DAT

                  To modify incremental parameters such as GBLPAGES and
                  GBLSECTIONS, use ADD_. The following example increases the
                  global page setting by 2000:

                    ADD_GBLPAGES = 2000

                  Note that when you set the page file quota, do not use a
                  value that exceeds the amount of page file space available on
                  the system.

                  After you make your changes, exit from the editor and execute
                  the AUTOGEN procedure to recalculate your system parameters.
                  Enter the following command at the DCL prompt:

                    $ @SYS$UPDATE:AUTOGEN GETDATA REBOOT

                  When you specify REBOOT, AUTOGEN performs an automatic system
                  shutdown and then reboots the system. Any users logged on to
                  the system are immediately disconnected during the shutdown.
                  The automatic reboot puts the new parameter values into
                  effect.

                  The AUTOGEN Utility automatically adjusts some of the SYSGEN
                  parameters based on the consumption of resources since the
                  last reboot. If you do not want to take advantage of this
                  automatic adjustment, include the NOFEEDBACK qualifier on the
                  AUTOGEN command line.

                  For more information about using AUTOGEN, see VMS System
                  Management Subkit.



               4-6  Preparing to Install DEC RT Integrator on VMS

 










               ____________________________________________________________

               4.5.3  VMSINSTAL Requirements

                  When you invoke VMSINSTAL, it checks whether :

                   o You have logged in to the system account

                   o You are logged in to a privileged account

                   o You have adequate quotas for installation

                   o DECnet is running

                   o Any users are logged in to the system

                  Note that the VMSINSTAL requires that the installation ac-
                  count has a minimum of the following quotas:

                     ASTLM = 24
                     BIOLM = 18
                     BYTLM = 18,000
                     DIOLM = 18
                     ENQLM = 30
                     FILLM = 20

                  If VMSINSTAL detects any problems during the installation,
                  it notifies you and asks if you want to continue the instal-
                  lation. In some instances, you can enter yes to continue. To
                  stop the installation process and correct the situation, en-
                  ter no or press Return. Then, correct the problem and restart
                  the installation.

               ____________________________________________________________

               4.5.4  Backing Up Your System Disk

                  Before you begin the installation, verify that you have a
                  backup of your system disk. If your system disk fails for any
                  reason during installation, you need a copy of your previous
                  system disk to recover your disk files.

                  For information on backing up your system disk, see the
                  section on the Backup Utility in the VMS System Management
                  Subkit.

                             Preparing to Install DEC RT Integrator on VMS  4-7

 

















                                                                      Chapter 5


                                            Installing DEC RT Integrator on VMS
               ________________________________________________________________


                  Chapter 5 does the following:

                   o Tells how to abort the installation procedure (see
                     Section 5.1)

                   o Describes the Development Kit installation procedure step-
                     by-step (see Section 5.2)

                   o Describes the Runtime Kit installation procedure step-by-
                     step (see Section 5.3)

                   o Discusses error recovery (see Section 5.4)

               ____________________________________________________________

               5.1  Aborting the Installation

                  To abort the installation procedure at any time, press
                  Ctrl/Y. When you press Ctrl/Y, the installation procedure
                  deletes all files it has created up to that point and exits.
                  You can then start the installation again.

                  The termination process may take a few minutes depending on
                  where you are in the installation process.

               ____________________________________________________________

               5.2  Development Kit Installation Procedure

                  To install the DEC RT Integrator Development Kit on your VMS
                  system, perform the steps listed below.

                   1. Run VMSINSTAL.

                                       Installing DEC RT Integrator on VMS  5-1

 











                     Log in to the SYSTEM account. At the DCL prompt, set your
                     default directory to SYS$UPDATE:

                       $ SET DEFAULT SYS$UPDATE

                     Enter the following command line to run VMSINSTAL:

                       $ @VMSINSTAL

                     The system displays the following informational messages:

                         VAX/VMS Software Product Installation Procedure V5.4

                       It is dd-mmm-yyyy at hh:mm.
                       Enter a question mark (?) at any time for help.

                   2. Confirm system backup.

                       * Are you satisfied with the backup of your system disk [YES]?

                     If you have a current backup of your system disk, press
                     Return. If you do not have a current backup of your system
                     disk, enter No to stop the installation.

                     After you back up your system disk, you can restart the
                     installation.

                     VMSINSTAL then displays the following prompt:

                       * Where will the distribution volumes be mounted:

                     Enter a mnemonic for the tape, cartridge, or CDROM device
                     you are installing onto. For example:

                      o MUA0 (for a tape cartridge)

                      o MTA0 (for generic magnetic tape)

                     VMSINSTAL now prompts you for the product you are in-
                     stalling.

               Enter the products to be processed from the first distribution volume set.
               * Products:

                     Enter RTI020 after the "Products:" prompt.

                     VMSINSTAL prompts you for the Options parameter.

                       * Enter installation options you wish to use (none): N

               5-2  Installing DEC RT Integrator on VMS

 











                     Enter N after the "Options:" prompt. Specifying the N
                     parameter causes VMSINSTAL to prompt you later in the
                     installation procedure about the DEC RT Integrator Release
                     Notes.

                   3. Mount the media.

                     VMSINSTAL displays the following instruction and prompt:

                       Please mount the first volume of the set on MUA0:.
                       * Are you ready?

                     Enter Yes after the "Are you ready?" prompt when you have
                     loaded your DEC RT Integrator distribution medium and are
                     ready to continue.

                                     TAPE CARTRIDGE INSTALLATION

                         When you load or unload a tape cartridge from
                         the tape drive, make sure that the red light (the
                         LOAD/UNLOAD switch) on the right of, or above, the
                         tape drive is in the out position and not glowing,
                         and that the small green activity light on the left
                         of, or below, the tape drive is glowing steadily.
                         (The location of the lights in relation to the
                         drive depends on whether the drive is positioned
                         vertically or horizontally.)

                         When you have successfully loaded the tape car-
                         tridge, the red light button is in and glowing
                         steadily, and the green light is also glowing
                         steadily.

                     When your distribution medium is successfully loaded into
                     the drive, VMSINSTAL displays an informational message
                     telling you that the medium is mounted.

                   4. Select a release notes option.

                     VMSINSTAL displays the following informational messages
                     and prompts you to select a release notes option.

                       The following products will be processed:
                         RTI V2.0

                               Beginning installation of DEC RT Integrator V2.0 at hh:mm

                       %VMSINSTAL-I-RESTORE, Restoring product saveset A . . .

                           Release notes included with this kit are always copied to SYS$HELP.

                                       Installing DEC RT Integrator on VMS  5-3

 











                           Additional Release Notes Options:

                               1.  Display release notes
                               2.  Print release notes
                               3.  Both 1 and 2
                               4.  None of the above

                       * Select option [2]:

                     Print the DEC RT Integrator Release Notes and read them
                     before proceeding further with the installation. The
                     release notes may contain last-minute instructions or
                     changes to the installation procedures described in this
                     guide. For more information on accessing the release
                     notes, see Section 6.1.

                     If you want to continue the installation procedure, enter
                     yes after the following prompt:

                       Do you want to continue the installation [NO]? Yes
                       %VMSINSTAL-I-RELMOVED, The product's release notes have been
                        successfully moved to SYS$HELP
                       %RTI-I-VMSOK, Installing DEC RT Integrator V2.0 on VMS Version 5.3,
                       continuing . . .

                               Product:      RTI-V
                               Producer:     DEC
                               Version:      V2.0
                               Release Date: 20-JAN-91

                   5. Verify that your PAK is registered.

                     VMSINSTAL now asks you about required PAK registration. If
                     you have not registered your PAK, terminate the installa-
                     tion and register it. If your PAK is registered, enter yes
                     at the prompt.

                       * Does this product have an authorization key registered and loaded?

                     If DEC GKS is not installed, you receive the following
                     warning message:

               %RTI-W-NOGKS, DEC GKS V4.1 must be installed for DEC RT Integrator V2.0 LGP.

                     If a version of GKS is installed, VMSINSTAL does a GKS
                     license check. If no GKS license is found, you receive the
                     following warning message:

               5-4  Installing DEC RT Integrator on VMS

 











                       %RTI-W-NOGKSLIC, DEC GKS License not installed.
                       DEC RT Integrator V2.0 LGP facility will not work
                       until the GKS license is installed.

                     If you need to use LGP, terminate this installation and
                     install GKS V4.1. You can terminate the installation by
                     pressing Ctrl/Y. The termination process may take a few
                     minutes.

                   6. Select installation options.

                     If you continue installation, VMSINSTAL asks if you want
                     to purge the files replaced by this installation proce-
                     dure. Press Return.

                       * Do you want to purge files replaced by this installation [YES]?

                     VMSINSTAL prompts you to install the following DEC RT
                     Integrator standard software: LIO, LGP, LSP, and the
                     DECwindows user interface. Press Return.

               * Do you want to install the DEC RT Integrator V2.0 Standard Software [YES]?

                     VMSINSTAL now asks you if this is a European installation.
                     If you are not installing in Europe, press Return. If you
                     are installing DEC RT Integrator in Europe, enter Yes.

                       * Is this a European installation [NO]?

                     If you answer YES and you are installing on a Q-bus based
                     VAX, VMSINSTAL asks you to select the European boards
                     installed on your system. These questions are necessary
                     because some European boards are not autoconfigured.

               * Does your DEC RT Integrator system have an IEQ11 board installed [NO]?
               * Does your DEC RT Integrator system have an IXV11 board installed [NO]?
               * Does your DEC RT Integrator system have a DRQ11C board installed [NO]?

                                                 NOTE

                         For non-European installations, if you install DEC
                         RT Integrator with an IEQ11 device already in the
                         system, DEC RT Integrator automatically installs
                         the IEQ11 device driver.

                                       Installing DEC RT Integrator on VMS  5-5

 











                     VMSINSTAL now prompts you to install the optional soft-
                     ware: the Scientific Subroutines Package (SSP) and the
                     Peak Processing Package (PEAK). (Note that SSP and PEAK
                     are unsupported products.) If you want to install these
                     products, enter Yes after the following prompt:

               * Do you want to install the DEC RT Integrator V2.0 Optional Software [NO]?

                     Next, VMSINSTAL asks if you want to install the LIO ex-
                     ample programs in executable form. If you answer yes,
                     VMSINSTAL loads executable images of the LIO example
                     programs into the LIO$EXAMPLES directory.

                       * Do you want to install the LIO examples in executable form? [NO]?

                   7. Answer questions about the IEZ11 device driver.

                     The next prompt asks if you want to install the IEZ11
                     device driver:

                       * Does your DEC Realtime Test Integrator system have an
                       * IEZ11 SCSI to IEEE-488 converter [NO]? yes

                     If you enter No, the installation procedure skips to the
                     questions about the IVP.

                     If you answer Yes, the procedure tests to see if your
                     system is known to have a SCSI bus at the time DEC RT
                     Integrator was released. If the system is known to have a
                     SCSI bus, the procedure continues.

                     If the system does not have a SCSI bus, the following
                     information appears on the screen:

                       WARNING - The IEZ11 driver can only be installed on a system
                       that has a SCSI bus.  At the time that this kit was built, this
                       system was not a known SCSI system.  If this system DOES have
                       a SCSI bus, then the installation will succeed.  If this system
                       does not have a SCSI bus, then the installation will fail.

                       * Do you still want to install the IEZ11 driver [NO]?

                     If you enter No, the installation procedure skips to the
                     questions about the IVP.

                     If you enter Yes, and your system does not have a SCSI
                     bus, but the system is part of a cluster, the installation
                     procedure assumes that another node on your cluster has a
                     SCSI bus. The following information is displayed:

               5-6  Installing DEC RT Integrator on VMS

 











                       %SYSTEM-W-NOSUCHDEV, no such device available
                       %RTI-W-UNSUPCPU, the IEZ11 class driver is not supported on this CPU.
                       -RTI-W-UNSUPCPU, installation continues.
                           You must create a system specific startup command procedure for each
                           node in your VAXcluster which will use the IEZ11 IEEE488 Bus Converter.

                           You create this startup procedure for a specific node by running the
                           IEZ11$CONFIG.COM procedure interactively on the SPECIFIC node.
                           The required DCL command is:

                              $ @SYS$MANAGER:IEZ11$CONFIG

                     The installation continues to the questions about the IVP.

                     If you enter Yes, and your system does have a SCSI bus,
                     then the installation continues as follows:

               Your current SCSI device configuration, as known to VMS, contains:
                            (Pure internal SCSI buses not shown)

                  2 disks

               The current SCSI ID assignment is:

                  0        1        2        3        4        5        6        7
               unused   unused   DKA200   DKA300   unused   unused    *CPU*   unused
                                 >disk<   >disk<

               You may connect up to 5 IEZ11 SCSI488/D bus converters to the
               external SCSI connector of your VAXstation or MicroVAX.

               WARNING: Connecting more than two IEZ11 SCSI488/D bus converters
                        may conflict with future system hardware extensions.

               * How many IEZ11 bus converters will you connect to the SCSI port? [1]:
               * Use device EKA0:, SCSI ID 0 (currently unused)? [Y]:

                   The current SCSI ID assignment is:

                       0        1        2        3        4        5        6        7
                     EKA0    unused   DKA200   DKA300   unused   unused    *CPU*   unused
                     IEZ11            >disk<   >disk<

               A new version of SYS$SPECIFIC:[SYS$STARTUP]IEZ11$STARTUP.COM has been created.
               You may wish to purge this file.

                                       Installing DEC RT Integrator on VMS  5-7

 











                     If an IEZ11 driver is already installed (that is, if
                     there is an EKDRIVER.EXE in SYS$LOADABLE_IMAGES), then
                     the following information appears on the screen:

                       The IEZ11 Class Driver (EKDRIVER) is already installed on your
                       system. Replacement of this driver requires a system reboot.

                       You can defer this reboot to some later time without any problem,
                       however, the newly installed EKDRIVER will not be usable until
                       after the system reboot.

                       Do *not* try to simply reload the driver manually, the driver
                       data structures of the active and the newly installed driver
                       may not be compatible, which will cause a SYSTEM CRASH.

                   8. Answer questions about the IVP.

                     VMSINSTAL prompts you about installing and executing
                     the Installation Verification Procedure (IVP). The IVP
                     confirms that DEC RT Integrator is properly installed and
                     operational. If you choose to install and execute the IVP,
                     press Return after the prompt.

               * Do you want to install and execute the DEC RT Integrator V2.0 IVP [YES]?

                     The next prompt asks if you want to run the DECwindows
                     version of the IVP:

                       * Do you want to run the DECwindows version of the IVP [YES]?

                     If you enter Yes, a plot will be displayed on your screen
                     when you run the IVP.

                     If you enter No, your terminal bell will ring seven times
                     and a message will be displayed on your screen when you
                     run the IVP.

                     The next prompt lets you review your answers and change
                     them if necessary.

                       * Your selections are complete, do you want to proceed [YES]?

                     If your selections are correct, press Return and the
                     installation procedure continues.

                   9. Answer additional questions for European devices.

               5-8  Installing DEC RT Integrator on VMS

 











                     If you have European devices installed on your system,
                     VMSINSTAL prompts you for information about these devices.


                       The next question establishes the device name for the OPTIONAL
                       board(s). Please do one of the following:

                       (1) Enter an asterisk (*) to display a list of devices currently
                           known to your system.

                       (2) Enter a carriage return to select the default generic device
                           name for your board.

































                                       Installing DEC RT Integrator on VMS  5-9

 











                       (3) Enter a unique, two-letter, generic device name.  This device
                           name must be different from the two-letter device name of
                           all other devices known to your system.

                       * Enter the two-letter device name for your IXV11 board(s) [IV]:

                           ------------------------------------------------------------
                           Configuring a driver for IXV11 board number 1 (device IVA0).
                           ------------------------------------------------------------

                           The system treats each IXV11 board you install
                           as a separate controller within the same driver.
                           However, each board must be configured for a different
                           base address within the VAX I/O space, as well as
                           for a unique interrupt vector.  These two parameters are
                           set by DIP switches or jumpers on the interface board.
                           Please use the XCON sheet delivered with your system or
                           the SYSGEN/CONFIGURE option to determine the correct base
                           address and interrupt vector for your system.
                           The installation procedure asks you to supply these
                           parameters for each IXV11 board.

                       * Do you want to see a current system configuration list [YES]?

                                        System Device Information

                                Name: PUB  ) CSR: 760334  Vector1: 774  Vector2: 0
                                Name: PUA  ) CSR: 772150  Vector1: 154  Vector2: 0
                                Name: PTA  ) CSR: 774500  Vector1: 260  Vector2: 0
                                Name: XQA  ) CSR: 774440  Vector1: 120  Vector2: 0
                                Name: TXA  ) CSR: 760500  Vector1: 310  Vector2: 3
                                Name: AZA  ) CSR: 776410  Vector1: 330  Vector2: 3
                                Name: AYA  ) CSR: 776420  Vector1: 340  Vector2: 3
                                Name: KZA  ) CSR: 770420  Vector1: 320  Vector2: 3

                     The next two prompts request base and vector addresses
                     for the IXV11 board. The addresses you enter must be
                     valid octal numbers that are word-aligned on an even octal
                     boundary. The valid range for the base address is 760000
                     to 777776. The valid range for the vector address is 100
                     to 776. Use the XCON sheet delivered with your system or
                     the SYSGEN/CONFIGURE option to determine the correct CSR
                     and vector settings for your board.


               5-10  Installing DEC RT Integrator on VMS

 











                       * Enter the octal base address for your IXV11 board [771400]:
                       * Enter the octal vector address for your IXV11 board [400]:

                             IXV11 board number 1 is now fully specified (device IVA0).

                       * Do you want to specify additional IXV11 boards [NO]?

                     When your configuration is complete, VMSINSTAL asks if
                     you want to proceed with the installation. If you want to
                     proceed with the installation, press Return.

                       * Your configuration is complete, do you want to proceed [YES]?

































                                      Installing DEC RT Integrator on VMS  5-11

 











                   10.Read informational messages.

                     VMSINSTAL displays the following message:

                       No further questions will be asked.
                       The installation takes approximately 60 minutes on a MicroVAX II.
                       %VMSINSTAL-I-RESTORE, Restoring product saveset B . . .

                     VMSINSTAL continues displaying messages as it restores
                     product savesets C to M.

                     If you chose to install the DEC RT Integrator Optional
                     Software, VMSINSTAL displays brief messages about the
                     unsupported software: the Scientific Subroutines Package
                     (SSP) and the Peak Processing Package (PEAK).

                     Online documentation for SSP is located in SYS$SYSROOT:
                     [UNSUPPORTED.SSP]SSP_GUIDE.MEM.

                     DEC RT Integrator displays a message recommending that
                     you read the DEC RT Integrator Release Notes located in
                     SYS$HELP:RTI020.RELEASE_NOTES. Review the Release Notes
                     now if you have not done so already.

                     After the installation procedure is complete, see
                     Section 6.2, for instructions on editing the startup
                     command file, SYSTARTUP_V5.COM, the DEC RT Integrator
                     startup command file, RTI_STARTUP.COM, and the system
                     login command file, SYLOGIN.COM.

                     VMSINSTAL now displays the following message:

                       %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target
                        directories . . .

                     VMSINSTAL now moves all the DEC RT Integrator files for
                     the standard DEC RT Integrator software and selected
                     options from the VMSINSTAL working directory to their
                     target directories.

                   11.Observe the Installation Verification Procedure (IVP).

                     VMSINSTAL begins executing the IVP:


               5-12  Installing DEC RT Integrator on VMS

 











                       +------------------------------------------------------------------+
                       |                                                                  |
                       |        DEC Realtime Test Integrator  for VMS V2.0                |
                       |                                                                  |
                       |           Installation Verification Procedure                    |
                       |                                                                  |
                       +------------------------------------------------------------------+






































                                      Installing DEC RT Integrator on VMS  5-13

 











                     If you said that you did not want to run the DECwindows
                     version of the IVP, the following message is displayed:

                                                    NOTE:

                       You have either indicated that you are not on a DECwindows display
                       or GKS is not  installed.  Therefore  the  graphics section of the
                       Installation Verification Procedure will not be attempted.

                       Your terminal bell should ring seven times and the message

                          'DEC RT Integrator Installation Verification Program'

                       Should be printed on your terminal.

                     When the IVP has completed, the following message is
                     displayed:

                       DEC RT Integrator Installation Verification Program

                       +------------------------------------------------------------------+
                       |                                                                  |
                       |      DEC RT Integrator Installation Verification Procedure       |
                       |            successfully completed                                |
                       |                                                                  |
                       +------------------------------------------------------------------+

                     If you said that you did want to run the DECwindows ver-
                     sion of the IVP, a plot similar to Figure 7-1 is displayed
                     on your screen for about 60 seconds and the following
                     message appears:

                       +------------------------------------------------------------------+
                       |                                                                  |
                       |      DEC RT Integrator Installation Verification Procedure       |
                       |            successfully completed                                |
                       |                                                                  |
                       +------------------------------------------------------------------+

                   12.End the installation procedure.

                       Installation of DEC RT Integrator V2.0 completed at hh:mm

                       VMSINSTAL procedure done at hh:mm

                       $ LOGOUT
                         SYSTEM       logged out at dd-mmm-yyyy hh:mm:ss

               5-14  Installing DEC RT Integrator on VMS

 











                  Section C.1 contains a sample installation from a tape car-
                  tridge. The dialogue for a magnetic tape installation is
                  similar.

                  When you complete the installation, see Chapter 6 for postin-
                  stallation tasks.







































                                      Installing DEC RT Integrator on VMS  5-15

 










               ____________________________________________________________

               5.3  Runtime Kit Installation Procedure

                  To install DEC RT Integrator on your VMS system, perform the
                  steps listed below.

                   1. Run VMSINSTAL.

                     Log in to the SYSTEM account. At the DCL prompt, set your
                     default directory to SYS$UPDATE:

                       $ SET DEFAULT SYS$UPDATE

                     Enter the following command line to run VMSINSTAL:

                       $ @VMSINSTAL

                     The system displays the following informational messages:

                         VAX/VMS Software Product Installation Procedure V5.3

                       It is dd-mmm-yyyy at hh:mm.
                       Enter a question mark (?) at any time for help.

                   2. Confirm system backup.

                       * Are you satisfied with the backup of your system disk [YES]?

                     If you have a current backup of your system disk, press
                     Return. If you do not have a current backup of your system
                     disk, enter No to stop the installation.

                     After you back up your system disk, you can restart the
                     installation.

                     VMSINSTAL then displays the following prompt:

                       * Where will the distribution volumes be mounted:

                     Enter a mnemonic for the tape, cartridge, or CDROM device
                     you are installing onto. For example:

                      o MUA0 (for a tape cartridge)

                      o MTA0 (for generic magnetic tape)

                     VMSINSTAL now prompts you for the product you are in-
                     stalling.

               Enter the products to be processed from the first distribution volume set.
               * Products:

                     Enter RTIRT after the "Products:" prompt.

               5-16  Installing DEC RT Integrator on VMS

 











                     VMSINSTAL prompts you for the Options parameter.

                       * Enter installation options you wish to use (none): N

                     Enter N after the "Options:" prompt. Specifying the N
                     parameter causes VMSINSTAL to prompt you later in the
                     installation procedure about the DEC RT Integrator Release
                     Notes.

                   3. Mount the media.

                     VMSINSTAL displays the following instruction and prompt:

                       Please mount the first volume of the set on MUA0:.
                       * Are you ready?

                     Enter Yes after the "Are you ready?" prompt when you have
                     loaded your DEC RT Integrator distribution medium and are
                     ready to continue.

                                     TAPE CARTRIDGE INSTALLATION

                         When you load or unload a tape cartridge from
                         the tape drive, make sure that the red light (the
                         LOAD/UNLOAD switch) on the right of, or above, the
                         tape drive is in the out position and not glowing,
                         and that the small green activity light on the left
                         of, or below, the tape drive is glowing steadily.
                         (The location of the lights in relation to the
                         drive depends on whether the drive is positioned
                         vertically or horizontally.)

                         When you have successfully loaded the tape car-
                         tridge, the red light button is in and glowing
                         steadily, and the green light is also glowing
                         steadily.

                     When your distribution medium is successfully loaded into
                     the drive, VMSINSTAL displays an informational message
                     telling you that the medium is mounted.

                   4. Select a release notes option.

                     VMSINSTAL displays the following informational messages
                     and prompts you to select a release notes option.

                                      Installing DEC RT Integrator on VMS  5-17

 











                       The following products will be processed:
                         RTIRT V2.0

                               Beginning installation of RTIRT V2.0 at hh:mm

                       %VMSINSTAL-I-RESTORE, Restoring product saveset A . . .

                           Release Notes Options:

                               1.  Display release notes
                               2.  Print release notes
                               3.  Both 1 and 2
                               4.  None of the above

                       * Select option [2]:

                     Print the DEC RT Integrator Release Notes and read them
                     before proceeding further with the installation. The
                     release notes may contain last-minute instructions or
                     changes to the installation procedures described in this
                     guide. For more information on accessing the release
                     notes, see Section 6.1.

                     If you want to continue the installation procedure, enter
                     Yes after the following prompt:

                       Do you want to continue the installation [NO]? Yes
                       %VMSINSTAL-I-RELMOVED, The product's release notes have been
                        successfully moved to SYS$HELP
                       %RTI-I-VMSOK, Installing DEC RT Integrator V2.0 on VMS Version V5.3,
                       continuing . . .

                   5. Verify that your GKS is installed.

                     If DEC GKS is not installed, you receive the following
                     warning message:

                       %RTI-W-NOGKS, DEC GKS V4.1 must be installed for DEC RT Integrator V2.0 LGP.

                     If a version of GKS is installed, VMSINSTAL does a GKS
                     license check. If no GKS license is found, you receive the
                     following warning message:

                       %RTI-W-NOGKSLIC, DEC GKS License not installed.
                       DEC RT Integrator V2.0 LGP facility will not work
                       until the GKS license is installed.

               5-18  Installing DEC RT Integrator on VMS

 











                     If you need to use LGP, terminate this installation and
                     install GKS V4.1. You can terminate the installation by
                     pressing Ctrl/Y. The termination process may take a few
                     minutes. If you are going to run the IVP, you need to have
                     GKS V4.1 installed first.

                   6. Select installation options.

                     If you continue installation, VMSINSTAL asks if you want
                     to purge the files replaced by this installation proce-
                     dure. Press Return.

                       * Do you want to purge files replaced by this installation [YES]?

                     VMSINSTAL prompts you to install the following DEC RT
                     Integrator standard software: LIO, LGP, LSP, and the
                     DECwindows user interface. Press Return.

               * Do you want to install the DEC RT Integrator V2.0 Standard Software [YES]?

                     VMSINSTAL now asks you if this is a European installation.
                     If you are not installing in Europe, press Return. If you
                     are installing DEC RT Integrator in Europe, enter Yes at
                     the prompt.

                       * Is this a European installation [NO]?

                     If you answer yes and you are installing on a Q-bus based
                     VAX, VMSINSTAL asks you to select the European boards
                     installed on your system. These questions are necessary
                     because some European boards are not autoconfigured.

               * Does your DEC RT Integrator system have an IEQ11 board installed [NO]?
               * Does your DEC RT Integrator system have an IXV11 board installed [NO]?
               * Does your DEC RT Integrator system have a DRQ11C board installed [NO]?

                                                 NOTE

                         For non-European installations, if you install DEC
                         RT Integrator with an IEQ11 device already in the
                         system, DEC RT Integrator automatically installs
                         the IEQ11 device driver.

                     VMSINSTAL now prompts you to install the optional soft-
                     ware: the Scientific Subroutines Package (SSP) and the
                     Peak Processing Package (PEAK). (Note that SSP and PEAK
                     are unsupported products.) If you want to install these
                     products, enter Yes after the following prompt:

                                      Installing DEC RT Integrator on VMS  5-19

 











               * Do you want to install the DEC RT Integrator V2.0 Optional Software [NO]?

                     Next, VMSINSTAL asks if you want to install the LIO ex-
                     ample programs in executable form. If you enter Yes,
                     VMSINSTAL loads executable images of the LIO example
                     programs into the LIO$EXAMPLES directory.

                       * Do you want to install the LIO examples in executable form? [NO]?

                   7. Answer questions about the IEZ11 device driver.

                     The next prompt asks if you want to install the IEZ11
                     device driver.

                       * Does your DEC Realtime Test Integrator system have an
                       * IEZ11 SCSI to IEEE-488 converter [NO]? yes

                     If you enter No, the installation procedure skips to the
                     questions about the IVP.

                     If you answer Yes, the procedure tests to see if your
                     system is known to have a SCSI bus at the time DEC RT
                     Integrator was released. If the system is known to have a
                     SCSI bus, the procedure continues.

                     If the system does not have a SCSI bus, the following
                     information appears on the screen:

                       WARNING - The IEZ11 driver can only be installed on a system
                       that has a SCSI bus.  At the time that this kit was built, this
                       system was not a known SCSI system.  If this system DOES have
                       a SCSI bus, then the installation will succeed.  If this system
                       does not have a SCSI bus, then the installation will fail.

                       * Do you still want to install the IEZ11 driver [NO]?

                     If you enter No, the installation procedure skips to the
                     questions about the IVP.

                     If you enter Yes, and your system does not have a SCSI
                     bus, but the system is part of a cluster, the installation
                     procedure assumes that another node on your cluster has a
                     SCSI bus. The following information is displayed:

                       %SYSTEM-W-NOSUCHDEV, no such device available
                       %RTI-W-UNSUPCPU, the IEZ11 class driver is not supported on this CPU.
                       -RTI-W-UNSUPCPU, installation continues.
                           You must create a system specific startup command procedure for each
                           node in your VAXcluster which will use the IEZ11 IEEE488 Bus Converter.

               5-20  Installing DEC RT Integrator on VMS

 











                           You create this startup procedure for a specific node by running the
                           IEZ11$CONFIG.COM procedure interactively on the SPECIFIC node.
                           The required DCL command is:

                              $ @SYS$MANAGER:IEZ11$CONFIG

                     The installation continues to the questions about the IVP.

                     If you enter Yes, and your system does have a SCSI bus,
                     then the installation continues as follows:

               Your current SCSI device configuration, as known to VMS, contains:
                            (Pure internal SCSI buses not shown)

                  2 disks

               The current SCSI ID assignment is:

                  0        1        2        3        4        5        6        7
               unused   unused   DKA200   DKA300   unused   unused    *CPU*   unused
                                 >disk<   >disk<

               You may connect up to 5 IEZ11 SCSI488/D bus converters to the
               external SCSI connector of your VAXstation or MicroVAX.

               WARNING: Connecting more than two IEZ11 SCSI488/D bus converters
                        may conflict with future system hardware extensions.

               * How many IEZ11 bus converters will you connect to the SCSI port? [1]:
               * Use device EKA0:, SCSI ID 0 (currently unused)? [Y]:

                   The current SCSI ID assignment is:

                       0        1        2        3        4        5        6        7
                     EKA0    unused   DKA200   DKA300   unused   unused    *CPU*   unused
                     IEZ11            >disk<   >disk<

               A new version of SYS$SPECIFIC:[SYS$STARTUP]IEZ11$STARTUP.COM has been created.
               You may wish to purge this file.






                                      Installing DEC RT Integrator on VMS  5-21

 











                     If an IEZ11 driver is already installed (that is, if
                     there is an EKDRIVER.EXE in SYS$LOADABLE_IMAGES), then
                     the following information appears on the screen:

                       The IEZ11 Class Driver (EKDRIVER) is already installed on your
                       system. Replacement of this driver requires a system reboot.

                       You can defer this reboot to some later time without any problem,
                       however, the newly installed EKDRIVER will not be usable until
                       after the system reboot.

                       Do *not* try to simply reload the driver manually, the driver
                       data structures of the active and the newly installed driver
                       may not be compatible, which will cause a SYSTEM CRASH.

                   8. Answer questions about the IVP.

                     VMSINSTAL prompts you about installing and executing
                     the Installation Verification Procedure (IVP). The IVP
                     confirms that DEC RT Integrator is properly installed and
                     operational. If you choose to install and execute the IVP,
                     press Return after the prompt.

               * Do you want to install and execute the DEC RT Integrator V2.0 IVP [YES]?

                     The next prompt asks if you want to run the DECwindows
                     version of the IVP:

                       * Do you want to run the DECwindows version of the IVP [YES]?

                     If you enter Yes, a plot will be displayed on your screen
                     when you run the IVP.

                     If you enter No, your terminal bell will ring seven times
                     and a message will be displayed on your screen when you
                     run the IVP.

                     The next prompt lets you review your answers and change
                     them if necessary.

                       * Your selections are complete, do you want to proceed [YES]?

                     If your selections are correct, press Return and the
                     installation procedure continues.

                   9. Answer additional questions for European devices.

               5-22  Installing DEC RT Integrator on VMS

 











                     If you have European devices installed on your system,
                     VMSINSTAL prompts you for information about these devices.


                       The next question establishes the device name for the OPTIONAL
                       board(s). Please do one of the following:

                       (1) Enter an asterisk (*) to display a list of devices currently
                           known to your system.

                       (2) Enter a carriage return to select the default generic device
                           name for your board.

































                                      Installing DEC RT Integrator on VMS  5-23

 











                       (3) Enter a unique, two-letter, generic device name.  This device
                           name must be different from the two-letter device name of
                           all other devices known to your system.

                       * Enter the two-letter device name for your IXV11 board(s) [IV]:

                           ------------------------------------------------------------
                           Configuring a driver for IXV11 board number 1 (device IVA0).
                           ------------------------------------------------------------

                           The system treats each IXV11 board you install
                           as a separate controller within the same driver.
                           However, each board must be configured for a different
                           base address within the VAX I/O space, as well as
                           for a unique interrupt vector.  These two parameters are
                           set by DIP switches or jumpers on the interface board.
                           Please use the XCON sheet delivered with your system or
                           the SYSGEN/CONFIGURE option to determine the correct base
                           address and interrupt vector for your system.
                           The installation procedure asks you to supply these
                           parameters for each IXV11 board.

                       * Do you want to see a current system configuration list [YES]?

                                        System Device Information

                                Name: PUB  ) CSR: 760334  Vector1: 774  Vector2: 0
                                Name: PUA  ) CSR: 772150  Vector1: 154  Vector2: 0
                                Name: PTA  ) CSR: 774500  Vector1: 260  Vector2: 0
                                Name: XQA  ) CSR: 774440  Vector1: 120  Vector2: 0
                                Name: TXA  ) CSR: 760500  Vector1: 310  Vector2: 3
                                Name: AZA  ) CSR: 776410  Vector1: 330  Vector2: 3
                                Name: AYA  ) CSR: 776420  Vector1: 340  Vector2: 3
                                Name: KZA  ) CSR: 770420  Vector1: 320  Vector2: 3

                     The next two prompts request base and vector addresses
                     for the IXV11 board. The addresses you enter must be
                     valid octal numbers that are word-aligned on an even octal
                     boundary. The valid range for the base address is 760000
                     to 777776. The valid range for the vector address is 100
                     to 776. Use the XCON sheet delivered with your system or
                     the SYSGEN/CONFIGURE option to determine the correct CSR
                     and vector settings for your board.


               5-24  Installing DEC RT Integrator on VMS

 











                       * Enter the octal base address for your IXV11 board [771400]:
                       * Enter the octal vector address for your IXV11 board [400]:

                             IXV11 board number 1 is now fully specified (device IVA0).

                       * Do you want to specify additional IXV11 boards [NO]?

                     When your configuration is complete, VMSINSTAL asks if
                     you want to proceed with the installation. If you want to
                     proceed with the installation, press Return.

                       * Your configuration is complete, do you want to proceed [YES]?

































                                      Installing DEC RT Integrator on VMS  5-25

 











                   10.Read informational messages.

                     VMSINSTAL displays the following message:

                       No further questions will be asked.
                       The installation takes approximately 60 minutes on a MicroVAX II.
                       %VMSINSTAL-I-RESTORE, Restoring product saveset B . . .

                     VMSINSTAL continues displaying messages as it restores
                     product savesets C to L.

                     If you chose to install the DEC RT Integrator Optional
                     Software, VMSINSTAL displays brief messages about the
                     unsupported software: the Scientific Subroutines Package
                     (SSP) and the Peak Processing Package (PEAK).

                     Online documentation for SSP is located in SYS$SYSROOT:
                     [UNSUPPORTED.SSP]SSP_GUIDE.MEM.

                     DEC RT Integrator displays a message recommending that
                     you read the DEC RT Integrator Release Notes located in
                     SYS$HELP:RTIRT020.RELEASE_NOTES. Review the Release Notes
                     now if you have not done so already.

                     After the installation procedure is complete, see
                     Section 6.2, Editing the System Files, for instructions on
                     editing the startup command file, SYSTARTUP_V5.COM, the
                     DEC RT Integrator startup command file, RTI_STARTUP.COM,
                     and the system login command file, SYLOGIN.COM.

                     VMSINSTAL now displays the following message:

                       %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target
                        directories . . .

                     VMSINSTAL now moves all the DEC RT Integrator files for
                     the standard DEC RT Integrator software and selected
                     options from the VMSINSTAL working directory to their
                     target directories.

                   11.Observe the Installation Verification Procedure (IVP).

                     VMSINSTAL begins executing the IVP:


               5-26  Installing DEC RT Integrator on VMS

 











                       +------------------------------------------------------------------+
                       |                                                                  |
                       |        DEC Realtime Test Integrator  for VMS V2.0                |
                       |                                                                  |
                       |           Installation Verification Procedure                    |
                       |                                                                  |
                       +------------------------------------------------------------------+






































                                      Installing DEC RT Integrator on VMS  5-27

 











                     If you said that you did not want to run the DECwindows
                     version of the IVP, the following message is displayed:

                                                    NOTE:

                       You have either indicated that you are not on a DECwindows display
                       or GKS is not  installed.  Therefore  the  graphics section of the
                       Installation Verification Procedure will not be attempted.

                       Your terminal bell should ring seven times and the message

                          'DEC RT Integrator Installation Verification Program'

                       Should be printed on your terminal.

                     When the IVP has completed, the following message is
                     displayed:

                       DEC RT Integrator Installation Verification Program

                       +------------------------------------------------------------------+
                       |                                                                  |
                       |      DEC RT Integrator Installation Verification Procedure       |
                       |            successfully completed                                |
                       |                                                                  |
                       +------------------------------------------------------------------+

                     If you said that you did want to run the DECwindows ver-
                     sion of the IVP, a plot similar to Figure 7-1 is displayed
                     on your screen for about 60 seconds and the following
                     message appears:

                       +------------------------------------------------------------------+
                       |                                                                  |
                       |      DEC RT Integrator Installation Verification Procedure       |
                       |            successfully completed                                |
                       |                                                                  |
                       +------------------------------------------------------------------+

                   12.End the installation procedure.

                       Installation of DEC RT Integrator V2.0 completed at hh:mm

                       VMSINSTAL procedure done at hh:mm

                       $ LOGOUT
                         SYSTEM       logged out at dd-mmm-yyyy hh:mm:ss

               5-28  Installing DEC RT Integrator on VMS

 











                  Section C.2 contains a sample installation from a tape car-
                  tridge. The dialogue for a magnetic tape installation is
                  similar.

                  When you complete the installation, see Chapter 6 for postin-
                  stallation tasks.







































                                      Installing DEC RT Integrator on VMS  5-29

 










               ____________________________________________________________

               5.4  Error Recovery

                  If errors occur during the installation itself or when the
                  IVP is running, VMSINSTAL displays failure messages. If the
                  installation fails, you see the following message:

                    %VMSINSTAL-E-INSFAIL, The installation of DEC RT Integrator V2.0 has failed.

                  If the IVP fails, you see these messages:

                    The DEC RT Integrator V2.0 Installation Verification Procedure failed.

                    %VMSINSTAL-E-IVPFAIL, The IVP for DEC RT Integrator V2.0 has failed.

                  Errors can occur during the installation if any of the fol-
                  lowing conditions exist:

                   o The operating system version is incorrect.

                   o A prerequisite software version is incorrect.

                   o Quotas necessary for successful installation are insuffi-
                     cient.

                   o System parameter values for successful installation are
                     insufficient.

                   o The VMS help library is currently in use.

                   o The product license has not been registered and loaded.

                  For descriptions of the error messages generated by these
                  conditions, see the VMS documentation on system messages,
                  recovery procedures, and VMS software installation. For
                  information on installation requirements, see Section 4.5.









               5-30  Installing DEC RT Integrator on VMS

 

















                                                                      Chapter 6


                                               Postinstallation Tasks Under VMS
               ________________________________________________________________


                  Chapter 6 describes the tasks you need to perform after
                  successfully installing DEC RT Integrator. The tasks, in
                  the order in which you should perform them, are:

                   1. If you have not already done so, print a copy of the
                     online DEC RT Integrator Release Notes (see Section 6.1).

                   2. Edit the system startup command files to include the
                     DEC RT Integrator startup command procedures (see
                     Section 6.2).

                   3. Check the file SYS$SYSTEM:MODPARAMS.DAT and change parame-
                     ter settings if necessary (see Section 6.3).

                   4. If you are using DEC RT Integrator in a VAXcluster, load
                     the license for the satellite nodes (see Section 6.4).

                   5. If you are using DEC RT Integrator in a VAXcluster and you
                     plan to use the IEZ11 device, load the IEZ11 device driver
                     onto each node that has a SCSI bus (see Section 6.5).

                   6. When you create user accounts, set the user account quotas
                     (see Section 6.6).

                   7. For European installations, modify the system configura-
                     tion command file, SYCONFIG.COM, located in SYS$MANAGER,
                     by adding device-specific startup procedures for the
                     IEQ11, IXV11, or DRQ11-C. Modify the system configura-
                     tion command file only if you installed one or more of
                     these devices (see Section 6.7).

                   8. Shut down and reboot the system so that the system auto-
                     matically loads the device drivers (see Section 6.8).

                                          Postinstallation Tasks Under VMS  6-1

 











                   9. If you plan to use use the subroutine libraries to develop
                     Pascal programs, compile the symbolic definition files
                     into environment files (see Section 6.9).

                  For information on reporting problems, see Section 6.10,
                  Reporting Problems.

                  For instructions on running the IVP any time after installa-
                  tion, see Chapter 7.

               ____________________________________________________________

               6.1  Accessing the DEC RT Integrator Release Notes

                  The DEC RT Integrator Release Notes provide information
                  about software and documentation errors found late in the
                  development cycle.

                  When you select release notes option 1, 2, 3, or 4 during
                  the installation procedure, VMSINSTAL copies the release
                  notes to the directory SYS$HELP. You can access the release
                  notes at any time by entering the following command for the
                  Development Kit Release Notes:

                    $ TYPE SYS$HELP::RTI020.RELEASE_NOTES

                  You can access the release notes at any time by entering the
                  following command for the Runtime Kit Release Notes:

                    $ TYPE SYS$HELP::RTIRT020.RELEASE_NOTES

                  This example displays the release notes on your terminal
                  screen. You can substitute the PRINT command for the TYPE
                  command to print a copy of the release notes.

               ____________________________________________________________

               6.2  Editing the System Files

                  You need to edit the startup command files to include com-
                  mand lines that initialize the DEC RT Integrator software
                  properly. Do this by following these instructions:

                   o Edit SYS$STARTUP:SYSTARTUP_V5.COM to include the following
                     line to execute the DEC RT Integrator-specific startup
                     command file, RTI_STARTUP.COM:

                       $ @SYS$STARTUP:RTI_STARTUP.COM

               6-2  Postinstallation Tasks Under VMS

 











                     If there is a call to the VAXLAB startup command file
                     VSLSTARTUP.COM or VSL$STARTUP.COM, it should be deleted.
                     RTI_STARTUP.COM replaces these files.










































                                          Postinstallation Tasks Under VMS  6-3

 











                   o Edit your LOGIN.COM file, a groupwide LOGIN.COM file,
                     or the system logical names table to include the defi-
                     nitions of two logical names used by the GKS software,
                     GKS$WSTYPE and GKS$CONID. These logical names define the
                     terminal type and the serial port for printed LGP plots.
                     See the DEC RT Integrator Laboratory Graphics Package
                     (LGP) Reference Manual for the information you need to
                     include.

                   o Edit the files specified in the layered product guides
                     included with the layered products you installed on your
                     system. See the appropriate layered product installation
                     guides for the layered products you installed.

               ____________________________________________________________

               6.3  Modifying System Parameters

                  The file SYS$SYSTEM:MODPARAMS.DAT contains site-specific sys-
                  tem parameter settings. After DEC RT Integrator is installed,
                  display this file. If it does not contain the following
                  lines, add them to the file:

                    MAXBUF =8192
                    REALTIME_SPTS = 128
                    TTY_ALTYPAHD = 4096
                    TTY_TYPAHDSZ = 4096

                  MAXBUF is the parameter that sets the maximum size of a
                  buffered I/O transfer.

                  REALTIME_SPTS is the parameter that reserves a number of
                  system page table entries for mapping connect-to-interrupt
                  processes into system space. When DEC RT Integrator is in-
                  stalled, the REALTIME_SPTS parameter is set by default to
                  128, which is the appropriate value for one AXV11-C device.
                  If your system has more than one device, reset this parameter
                  to 128 times the number of AXV11-C devices your system has.

                  TTY_ALTYPAHD is the parameter that sets the size of the
                  alternate type-ahead buffer. TTY_TYPAHDSZ is the parameter
                  that sets the size of the terminal type-ahead buffer. These
                  parameters have been set to arbitrarily high values for
                  improved performance of the serial line device. For normal
                  operation, the default values are sufficient.

               6-4  Postinstallation Tasks Under VMS

 











                  For information on the procedure for making the modified
                  parameters take effect, see Section 4.5.2.2. In order to
                  conserve disk space, you should use the PURGE command to
                  delete some of the old system data files.

               ____________________________________________________________

               6.4  Loading the DEC RT Integrator License for the Other Nodes

                  If you are installing DEC RT Integrator in a VAXcluster, you
                  must load the license for each of the satellite nodes. If you
                  are installing the Runtime Kit, enter the following command
                  for each node:

                    $ LICENSE LOAD VAXLAB-SW-LIB

                  If you are installing the Development Kit, enter the follow-
                  ing command for each node:

                    $ LICENSE LOAD RTI-V

                  You can also run the IVP on the other nodes in the VAXcluster,
                  although running the IVP on the boot node should be suffi-
                  cient.

               ____________________________________________________________

               6.5  Loading the IEZ11 Device Driver in a Cluster

                  If you want to use the IEZ11 bus converter device in a
                  VAXcluster, you must create a system-specific startup com-
                  mand procedure for each node in the cluster that will use the
                  IEZ11 device (in other words, for each node that has a SCSI
                  bus).

                                               NOTE

                      This procedure is not necessary if you have only
                      one node with a SCSI bus and you installed DEC RT
                      Integrator on that node.

                  You create this startup procedure for a specific node by
                  running the IEZ11$CONFIG.COM procedure interactively on each
                  specific node.

                  To do this, set host to each node that has the SCSI bus:

                    $ SET HOST scsi_sys

                                          Postinstallation Tasks Under VMS  6-5

 











                  Then run the procedure:

                    $ @SYS$MANAGER:IEZ11$CONFIG

                  The following information is displayed for each node:

               Your current SCSI device configuration, as known to VMS, contains:
                            (Pure internal SCSI buses not shown)

                  2 disks



































               6-6  Postinstallation Tasks Under VMS

 











               The current SCSI ID assignment is:

                  0        1        2        3        4        5        6        7
               unused   unused   DKA200   DKA300   unused   unused    *CPU*   unused
                                 >disk<   >disk<

               You may connect up to 5 IEZ11 SCSI488/D bus converters to the
               external SCSI connector of your VAXstation or MicroVAX.

               WARNING: Connecting more than two IEZ11 SCSI488/D bus converters
                        may conflict with future system hardware extensions.

               * How many IEZ11 bus converters will you connect to the SCSI port? [1]:
               * Use device EKA0:, SCSI ID 0 (currently unused)? [Y]:

                   The current SCSI ID assignment is:

                       0        1        2        3        4        5        6        7
                     EKA0    unused   DKA200   DKA300   unused   unused    *CPU*   unused
                     IEZ11            >disk<   >disk<

               A new version of SYS$SPECIFIC:[SYS$STARTUP]IEZ11$STARTUP.COM has been created.
               You may wish to purge this file.

               ____________________________________________________________

               6.6  Setting Quotas for User Accounts

                  Use the SHOW WORKING_SET command at the DCL prompt to see the
                  working set quotas. The /Limit number refers to the working
                  set default value.

                  You can create accounts and make changes to them by using the
                  VMS Authorize Utility, as shown below:

                    $ SET DEFAULT SYS$SYSTEM
                    $ RUN AUTHORIZE

                  When you create user accounts, see that the following minimum
                  quotas are in effect for each account:

                   o AST limit (ASTLM): 64

                   o Buffered I/O count limit (BIOLM): 64

                   o Buffered I/O byte limit (BYTLM): 8192

                   o Direct I/O count limit (DIOLM): 64

                   o Working set default (WSDEF): 512

                   o Working set quota (WSQUO): 512

                                          Postinstallation Tasks Under VMS  6-7

 











                   o Working set extent (WSEXTENT): 1024

                  For information on the Authorize Utility, see the VMS
                  Authorize Utility Manual.

               ____________________________________________________________

               6.7  Modifying the System Configuration Command File

                  For European installations, VMSINSTAL generates command
                  procedures for loading the IEQ11, IXV11, and DRQ11-C de-
                  vice drivers. To load any of these device drivers, modify
                  SYS$MANAGER:SYCONFIG.COM by adding the following line to the
                  file for each of the devices you are using:

                    $ @SYS$MANAGER:xxLOAD.COM

                  where xx is the two-letter symbol for the device you are
                  using.

                  The following table lists the device names and their two-
                  letter symbols.

                  _____________________________________________________________
                  Device_Name___Symbol_________________________________________

                  IEQ11         IX
                  IXV11         IV
                  DRQ11-C_______UU_____________________________________________

                  During system startup, VMS executes this command procedure
                  from the SYCONFIG.COM file located in the SYS$MANAGER direc-
                  tory.

               ____________________________________________________________

               6.8  Loading Device Drivers

                  The device drivers load automatically when you shut down and
                  reboot your system.

                                               NOTE

                      If you do not plan to use the Laboratory I/O (LIO)
                      routines, you do not need to shut down and reboot the
                      system.

                  Use SYS$SYSTEM:SHUTDOWN.COM. to shut the system down. Then
                  halt the system to cause a system reboot.

               6-8  Postinstallation Tasks Under VMS

 











                  To halt the system, follow the instructions in the CPU
                  owner's guide accompanying your processor.

                  The system reexecutes the startup files you edited and recog-
                  nizes the changes you made to these files. When you see the
                  job-terminated message, press Return. The system displays the
                  "Username:" prompt. To log in to the new system, enter the
                  SYSTEM account name after the "Username:" prompt.

               ____________________________________________________________

               6.9  Creating Pascal Environment Files

                  If you plan to use use the subroutine libraries to develop
                  Pascal programs, you must compile the symbolic definition
                  files into environment files.

                  To create the appropriate environment files, take the follow-
                  ing steps:

                   1. Log in to a privileged account, such as the system man-
                     ager's account.

                   2. Set default to SYS$LIBRARY.

                   3. Enter the following command lines:

                       $ PASCAL/ENVIRONMENT/NOOBJECT LIO_DEF, LIO_SET
                       $ PASCAL/ENVIRONMENT/NOOBJECT LSP_DEF, LSP_SET
                       $ PASCAL/ENVIRONMENT/NOOBJECT LGP_DEF, LGP_ATTDEF
                       $ PASCAL/ENVIRONMENT/NOOBJECT RTI
                       $ SET PROT=(W:RE) *.PEN

                     The Pascal compiler creates an environment file, called
                     <filename>.PEN, for each symbolic definition file.

                  When you code an application program using Pascal, use the
                  following line to include a symbolic definition (environment)
                  file in a user program:

                    [INHERIT ('SYS$LIBRARY:filename')]

                  where <filename> is one of the symbolic definition files.

                  The following line contains the VAX PASCAL interface con-
                  struct that defines entry points for the DEC RT Integrator
                  routines. You must use it in every VAX PASCAL DEC RT
                  Integrator program:

                                          Postinstallation Tasks Under VMS  6-9

 











                    [INHERIT ('SYS$LIBRARY:RTI')]

               ____________________________________________________________

               6.10  Reporting Problems

                  If you encounter a problem while using DEC RT Integrator, do
                  one of the following:

                   o Call Digital if your software contract or warranty agree-
                     ment entitles you to telephone support.

                   o Submit a Software Performance Report (SPR).

                   o Fill out and submit a Reader's Comments form if the prob-
                     lem has to do with the documentation. Use the form from
                     the back of the manual in which you found the error.
                     Include the section and page number.



























               6-10  Postinstallation Tasks Under VMS

 

















                                                                      Chapter 7


                                                        Running the IVP for VMS
               ________________________________________________________________


                  Chapter 7 explains how to run the Installation Verification
                  Procedure (IVP).

                  You can run the IVP at any time after installation. Set your
                  default directory to SYS$TEST and then to the subdirectory
                  [.RTI_IVP]:

                    $ SET DEF SYS$TEST
                    $ SET DEF [.RTI_IVP]

                  To run the DECwindows IVP, use the following command:

                    $ RT_INTEGRATOR RTI_IVP

                  The following information is displayed on your terminal
                  screen:

                               +-------------------------------------------------------+
                               |                                                       |
                               |       DEC Realtime Test Integrator for VMS V2.0       |
                               |          Installation Verification Procedure          |
                               |                                                       |
                               +-------------------------------------------------------+









                                                   Running the IVP for VMS  7-1

 











                          +------------------------------------------------------------------+
                          |                                                                  |
                          | The  DEC  Realtime  Test  Integrator  Installation  Verification |
                          | Procedure will now draw an example plot on your screen.  See the |
                          | IVP  chapter  in  the  DEC Realtime Test Integrator Installation |
                          | Guide for a  sample  IVP plot.  The  plot  on  the screen should |
                          | be  similar to  the illustration  in the  installation guide and |
                          | remains  on  the  screen   for  approximately  one  (1)  minute. |
                          |                                                                  |
                          +------------------------------------------------------------------+

                  Figure 7-1 shows an IVP plot similar to the one that is
                  displayed on your screen if you run the DECwindows IVP.

                  Figure 7-1:  IVP Plot for DEC RT Integrator
                  _____________________________________________________________














                  _____________________________________________________________

                  If you do not have GKS installed on your system or you are
                  not on a DECwindows terminal, use the following command:

                    $ RUN RTI_IVP_NO_GKS

                  The following information is displayed on your terminal
                  screen:






               7-2  Running the IVP for VMS

 











                               +-------------------------------------------------------+
                               |                                                       |
                               |       DEC Realtime Test Integrator for VMS V2.0       |
                               |          Installation Verification Procedure          |
                               |                                                       |
                               +-------------------------------------------------------+

                                                         NOTE:

                            You have either indicated that you are not on a DECwindows display
                            or GKS is not  installed.  Therefore  the  graphics section of the
                            Installation Verification Procedure will not be attempted.

                            Your terminal bell should ring seven times and the message

                               'DEC RT Integrator Installation Verification Program'

                            Should be printed on your terminal.

                    DEC RT Integrator Installation Verification Program

                  After the IVP has finished, the following message appears:

                         +--------------------------------------------------------------------+
                         |                                                                    |
                         |        DEC RT Integrator Installation Verification Procedure       |
                         |                     successfully completed                         |
                         |                                                                    |
                         +--------------------------------------------------------------------+
















                                                   Running the IVP for VMS  7-3

 

















                                                                     Appendix A


                                          ULTRIX Files Installed on Your System
               ________________________________________________________________


                  The following subsets of files are installed when you install
                  DEC RT Integrator:

                  RTILGP100, Laboratory Graphics Package (LGP)

                  /usr/kits/RTI100/include/lgp_attdef.f
                  /usr/kits/RTI100/include/lgp_attdef.h
                  /usr/kits/RTI100/include/lgp_def.f
                  /usr/kits/RTI100/include/lgp_def.h
                  /usr/kits/RTI100/include/lgp_def_arg.f
                  /usr/kits/RTI100/include/lgp_def_arg.h
                  /usr/kits/RTI100/lib/liblgp.a
                  /usr/kits/RTI100/lib/liblgpgks.a
                  /usr/kits/RTI100/lib/liblgpgksbnd.a
                  /usr/kits/RTI100/lib/librticbnd.a

                  RTILIO100, Laboratory Input/Output (LIO)

                  /usr/kits/RTI100/include/lio_def.f
                  /usr/kits/RTI100/include/lio_def.h
                  /usr/kits/RTI100/include/lio_set.f
                  /usr/kits/RTI100/include/lio_set.h
                  /usr/kits/RTI100/lib/liblio.a

                  RTILSP100, Laboratory Signal Processing (LSP)

                  /usr/kits/RTI100/include/lsp_def.f
                  /usr/kits/RTI100/include/lsp_def.h
                  /usr/kits/RTI100/include/lsp_set.f
                  /usr/kits/RTI100/include/lsp_set.h
                  /usr/kits/RTI100/lib/liblsp.a
                  /usr/kits/RTI100/lib/librticbnd.a

                                     ULTRIX Files Installed on Your System  A-1

 











                  RTIBASE100, DEC RT Integrator (Development)

                  /usr/kits/RTI100/bin/rti
                  /usr/kits/RTI100/ivp/rti_ivp.rti
                  /usr/kits/RTI100/ivp/rti_nodecw_ivp.rti
                  /usr/lib/X11/help/rti/about
                  /usr/lib/X11/help/rti/csh_devs
                  /usr/lib/X11/help/rti/csh_menus
                  /usr/lib/X11/help/rti/csh_oso
                  /usr/lib/X11/help/rti/overview
                  /usr/lib/X11/help/rti/rti100.release_notes
                  /usr/lib/X11/help/rti/table_of_contents
                  /usr/lib/X11/help/rti/to_get_start
                  /usr/lib/X11/help/rti/to_work_em
                  /usr/lib/X11/uid/rti_library.uid
                  /usr/lib/X11/uid/rti_worksurface.uid

                  RTIRTBASE100, DEC RT Integrator (Runtime)

                  /usr/kits/RTI100/bin/rti_rt
                  /usr/kits/RTI100/ivp/rti_ivp.rti
                  /usr/kits/RTI100/ivp/rti_nodecw_ivp.rti
                  /usr/lib/X11/uid/rti_library.uid
                  /usr/lib/X11/uid/rti_worksurface.uid

                  RTI488100, ULTRIX ek device driver

                  /usr/sys/MIPS/BINARY/ekdriver.o.V40
                  /usr/sys/MIPS/BINARY/ekdriver.o.V41
                  /usr/sys/MIPS/BINARY/scsi.o.V40
                  /usr/sys/MIPS/BINARY/scsi.o.V41
                  /usr/sys/MIPS/BINARY/scsi_asc.o.V40
                  /usr/sys/MIPS/BINARY/scsi_asc.o.V41
                  /usr/sys/MIPS/BINARY/scsi_proc.o.V40
                  /usr/sys/MIPS/BINARY/scsi_proc.o.V41
                  /usr/sys/MIPS/BINARY/scsi_sii.o.V40
                  /usr/sys/MIPS/BINARY/scsi_sii.o.V41
                  /usr/sys/io/scsi/mips/ekioctl.h
                  /usr/sys/io/scsi/mips/ekvar.h






               A-2  ULTRIX Files Installed on Your System

 











                  RTIMAN100, DEC RT Integrator Development Kit Manual Pages

                  RTIRTMAN100, DEC RT Integrator Runtime Kit Manual Pages

                                               NOTE

                      The files in these two subsets are the same except
                      that /usr/man/man1/rti.1 is in the Development Kit
                      only.

                  /usr/man/man1/rti.1
                  /usr/man/man1/rti_rt.1
                  /usr/man/man3/lgp.3
                  /usr/man/man3/lgp_3d_simple.3
                  /usr/man/man3/lgp_change_plotting_logicals.3
                  /usr/man/man3/lgp_contour.3
                  /usr/man/man3/lgp_contour_shade.3
                  /usr/man/man3/lgp_contourm.3
                  /usr/man/man3/lgp_erase.3
                  /usr/man/man3/lgp_get_choice.3
                  /usr/man/man3/lgp_get_locator.3
                  /usr/man/man3/lgp_get_string.3
                  /usr/man/man3/lgp_get_stroke.3
                  /usr/man/man3/lgp_get_value.3
                  /usr/man/man3/lgp_hist.3
                  /usr/man/man3/lgp_info.3
                  /usr/man/man3/lgp_map_pen.3
                  /usr/man/man3/lgp_plot.3
                  /usr/man/man3/lgp_plot_3d.3
                  /usr/man/man3/lgp_plot_log.3
                  /usr/man/man3/lgp_plot_metafile.3
                  /usr/man/man3/lgp_plotc.3
                  /usr/man/man3/lgp_plotm.3
                  /usr/man/man3/lgp_point.3
                  /usr/man/man3/lgp_print_screen.3
                  /usr/man/man3/lgp_put_text.3
                  /usr/man/man3/lgp_scale.3
                  /usr/man/man3/lgp_scale_log.3
                  /usr/man/man3/lgp_set_3d_graph.3
                  /usr/man/man3/lgp_set_graph.3
                  /usr/man/man3/lgp_spline_qhc.3
                  /usr/man/man3/lgp_stndev.3
                  /usr/man/man3/lgp_table_modify.3
                  /usr/man/man3/lgp_table_read_value.3
                  /usr/man/man3/lgp_table_reset.3

                                     ULTRIX Files Installed on Your System  A-3

 











                  /usr/man/man3/lgp_terminate_plot.3
                  /usr/man/man3/lio.3
                  /usr/man/man3/lio_attach.3
                  /usr/man/man3/lio_dequeue.3
                  /usr/man/man3/lio_detach.3
                  /usr/man/man3/lio_enqueue.3
                  /usr/man/man3/lio_read.3
                  /usr/man/man3/lio_set_i.3
                  /usr/man/man3/lio_set_r.3
                  /usr/man/man3/lio_set_s.3
                  /usr/man/man3/lio_show.3
                  /usr/man/man3/lio_write.3
                  /usr/man/man3/lsp.3
                  /usr/man/man3/lsp_apply_window_table.3
                  /usr/man/man3/lsp_build_window_table.3
                  /usr/man/man3/lsp_correlation.3
                  /usr/man/man3/lsp_fft_complex.3
                  /usr/man/man3/lsp_fft_complex_2d.3
                  /usr/man/man3/lsp_fft_real.3
                  /usr/man/man3/lsp_filter_nonrec.3
                  /usr/man/man3/lsp_filter_poly.3
                  /usr/man/man3/lsp_filter_poly_1st_deriv.3
                  /usr/man/man3/lsp_filter_poly_2nd_deriv.3
                  /usr/man/man3/lsp_filter_poly_3rd_deriv.3
                  /usr/man/man3/lsp_format_translate_adc.3
                  /usr/man/man3/lsp_format_translate_dac.3
                  /usr/man/man3/lsp_hist_f.3
                  /usr/man/man3/lsp_hist_i.3
                  /usr/man/man3/lsp_phase_angle.3
                  /usr/man/man3/lsp_phase_angle_2d.3
                  /usr/man/man3/lsp_power_spectrum.3
                  /usr/man/man3/lsp_spectral_windows.3
                  /usr/man/man3/lsp_thermocouple_x.3

                  RTIEXA100, DEC RT Integrator Examples

                  /usr/kits/RTI100/examples/lgp/lgp_ex_3d.f
                  /usr/kits/RTI100/examples/lgp/lgp_ex_autoscale.f
                  /usr/kits/RTI100/examples/lgp/lgp_ex_contourm.f
                  /usr/kits/RTI100/examples/lgp/lgp_ex_erase.c
                  /usr/kits/RTI100/examples/lgp/lgp_ex_get_routines.f
                  /usr/kits/RTI100/examples/lgp/lgp_ex_plot_3d.f
                  /usr/kits/RTI100/examples/lgp/lgp_ex_plot_contour.f
                  /usr/kits/RTI100/examples/lgp/lgp_ex_plot_hist.f

               A-4  ULTRIX Files Installed on Your System

 











                  /usr/kits/RTI100/examples/lgp/lgp_ex_plot_log.c
                  /usr/kits/RTI100/examples/lgp/lgp_ex_plot_points.c
                  /usr/kits/RTI100/examples/lgp/lgp_ex_plot_sine.f
                  /usr/kits/RTI100/examples/lgp/lgp_ex_plotc.f
                  /usr/kits/RTI100/examples/lgp/lgp_ex_plotm_sine.f
                  /usr/kits/RTI100/examples/lgp/lgp_ex_scale_log.c
                  /usr/kits/RTI100/examples/lgp/lgp_ex_shade_contour.f
                  /usr/kits/RTI100/examples/lgp/lgp_ex_simple.c
                  /usr/kits/RTI100/examples/lgp/lgp_ex_stndev.f
                  /usr/kits/RTI100/examples/lgp/lgp_ex_write_text.f
                  /usr/kits/RTI100/examples/lio/lio_file_read.c
                  /usr/kits/RTI100/examples/lio/lio_file_write.c
                  /usr/kits/RTI100/examples/lio/lio_iez_example.c
                  /usr/kits/RTI100/examples/lio/lio_iez_srq_example.c
                  /usr/kits/RTI100/examples/lio/lio_mq_interproc_a.c
                  /usr/kits/RTI100/examples/lio/lio_mq_interproc_b.c
                  /usr/kits/RTI100/examples/lio/lio_serial_example.c
                  /usr/kits/RTI100/examples/lio/lio_serial_example.h
                  /usr/kits/RTI100/examples/lsp/lsp_autocor_rand_seq.f
                  /usr/kits/RTI100/examples/lsp/lsp_calc_comp_phse.f
                  /usr/kits/RTI100/examples/lsp/lsp_calc_phase_spec.f
                  /usr/kits/RTI100/examples/lsp/lsp_crosscor_sine_cosine.f
                  /usr/kits/RTI100/examples/lsp/lsp_fft_comp_forw.f
                  /usr/kits/RTI100/examples/lsp/lsp_fft_comp_inver.f
                  /usr/kits/RTI100/examples/lsp/lsp_fft_func.f
                  /usr/kits/RTI100/examples/lsp/lsp_fft_rand_dat.f
                  /usr/kits/RTI100/examples/lsp/lsp_filt_nonrec.f
                  /usr/kits/RTI100/examples/lsp/lsp_filt_poly.f
                  /usr/kits/RTI100/examples/lsp/lsp_filt_poly_1st_deriv.f
                  /usr/kits/RTI100/examples/lsp/lsp_form_trans_adc.f
                  /usr/kits/RTI100/examples/lsp/lsp_form_trans_dac.f
                  /usr/kits/RTI100/examples/lsp/lsp_histo_f.f
                  /usr/kits/RTI100/examples/lsp/lsp_histo_i.f
                  /usr/kits/RTI100/examples/lsp/lsp_phase_ang.f
                  /usr/kits/RTI100/examples/lsp/lsp_pow_spec_sine.f
                  /usr/kits/RTI100/examples/lsp/lsp_thermoc_b.f
                  /usr/kits/RTI100/examples/lsp/lsp_window_1.f
                  /usr/kits/RTI100/examples/lsp/lsp_window_2.f
                  /usr/kits/RTI100/examples/rti/fft_example.rti
                  /usr/kits/RTI100/examples/rti/loop_example.rti





                                     ULTRIX Files Installed on Your System  A-5

 











                  Icon Development, RTIICON100

                  /usr/kits/RTI100/examples/rti/edl.h
                  /usr/kits/RTI100/examples/rti/linkrti.sh
                  /usr/kits/RTI100/examples/rti/linkrti_rt.sh
                  /usr/kits/RTI100/examples/rti/mrld_def.h
                  /usr/kits/RTI100/examples/rti/mrld_filo.c
                  /usr/kits/RTI100/examples/rti/mrld_filo.h
                  /usr/kits/RTI100/examples/rti/mrld_filo_mods.h
                  /usr/kits/RTI100/examples/rti/mrld_filo_off.bit
                  /usr/kits/RTI100/examples/rti/mrld_filo_on.bit
                  /usr/kits/RTI100/examples/rti/mrld_hdr.h
                  /usr/kits/RTI100/examples/rti/mrld_sql.c
                  /usr/kits/RTI100/examples/rti/mrld_sql.h
                  /usr/kits/RTI100/examples/rti/mrld_sql_mods.h
                  /usr/kits/RTI100/examples/rti/mrld_sql_off.bit
                  /usr/kits/RTI100/examples/rti/mrld_sql_on.bit
                  /usr/kits/RTI100/examples/rti/mrld_rand.c
                  /usr/kits/RTI100/examples/rti/mrld_rand.h
                  /usr/kits/RTI100/examples/rti/mrld_rand_mods.h
                  /usr/kits/RTI100/examples/rti/mrld_rand_off.bit
                  /usr/kits/RTI100/examples/rti/mrld_rand_on.bit
                  /usr/kits/RTI100/examples/rti/mrld_rso.c
                  /usr/kits/RTI100/examples/rti/mrld_rso.h
                  /usr/kits/RTI100/examples/rti/mrld_rso_mods.h
                  /usr/kits/RTI100/examples/rti/mrld_rso_on.bit
                  /usr/kits/RTI100/examples/rti/mrld_rso_off.bit
                  /usr/kits/RTI100/examples/rti/mrld_rt_hdr.h
                  /usr/kits/RTI100/examples/rti/mrld_rt_shared.h
                  /usr/kits/RTI100/examples/rti/mrld_std_data_buff.h
                  /usr/kits/RTI100/examples/rti/mrld_tpl.c
                  /usr/kits/RTI100/examples/rti/mrld_tpl.h
                  /usr/kits/RTI100/examples/rti/mrld_tpl_mods.h
                  /usr/kits/RTI100/examples/rti/mrld_tpl_off.bit
                  /usr/kits/RTI100/examples/rti/mrld_tpl_on.bit
                  /usr/kits/RTI100/examples/rti/mrld_ui_shared.h
                  /usr/kits/RTI100/examples/rti/mrld_user_lib.c
                  /usr/kits/RTI100/examples/rti/replace.c
                  /usr/kits/RTI100/lib/liblgpgks.a
                  /usr/kits/RTI100/lib/liblgpgksbnd.a
                  /usr/kits/RTI100/lib/librti.a




               A-6  ULTRIX Files Installed on Your System

 











                  /usr/kits/RTI100/lib/librticbnd.a
                  /usr/kits/RTI100/lib/librtirt.a
                  /usr/lib/X11/uid/rti_library.uid
                  /usr/lib/X11/uid/rti_worksurface.uid

                  RTIRUN100, DEC RT Integrator (Runtime)

                  /usr/kits/RTI100/bin/rti_rt
                  /usr/kits/RTI100/ivp/rti_ivp.rti
                  /usr/kits/RTI100/ivp/rti_nodecw_ivp.rti
                  /usr/lib/X11/uid/rti_library.uid
                  /usr/lib/X11/uid/rti_worksurface.uid

































                                     ULTRIX Files Installed on Your System  A-7

 

















                                                                     Appendix B


                                                     Sample ULTRIX Installation
               ________________________________________________________________


                  Appendix B provides the following:

                   o An installation of DEC RT Integrator Development Kit on a
                     RISC system using tape media (see Example B-1)

                   o An installation of DEC RT Integrator Runtime Kit on a RISC
                     system using tape media (see Example B-2)

               ____________________________________________________________

               B.1  Sample Installation for RISC ULTRIX Development Kit

                  Example B-1 is a sample installation of the DEC RT Integrator
                  Development Kit. It assumes that DECnet has been shut down
                  and no users are logged in to your system.

















                                                Sample ULTRIX Installation  B-1

 











               Example B-1:  Sample Installation for RISC ULTRIX Development
                             Kit
               ________________________________________________________________

               # setld -l  /dev/rmt0h

               *** Enter Subset Selections ***

               The subsets listed below are optional:
                1) DEC RT Integrator (Development)      2) ULTRIX ek device driver
                3) Laboratory Graphic Package (LGP)     4) Laboratory IO (LIO)
                5) Laboratory Signal Processing (LSP)   6) Icon Development
                7) DEC RT Integrator (Runtime)          8) DEC RT Integrator Manual Pages
                9) DEC RT Integrator Examples

               10) All of the Above
               11) None of the Above
               12) Exit without installing subsets

               Enter your choice(s): 10

               You are installing the following subsets:
                  DEC RT Integrator (Development)         ULTRIX ek device driver
                  Laboratory Graphic Package (LGP)        Laboratory IO (LIO)
                  Laboratory Signal Processing (LSP)      Icon Development
                  DEC RT Integrator (Runtime)             DEC RT Integrator Manual Pages
                  DEC RT Integrator Examples

               Is this correct? (y/n): y

               Copying DEC RT Integrator (Development) (RTIBASE100) from disk
               Verifying DEC RT Integrator (Development) (RTIBASE100)

               Copying ULTRIX ek device driver (RTI488100) from disk
               Verifying ULTRIX ek device driver (RTI488100)

               Copying Laboratory Graphic Package (LGP) (RTILGP100) from disk
               Verifying Laboratory Graphic Package (LGP) (RTILGP100)

               Copying Laboratory IO (LIO) (RTILIO100) from disk
               Verifying Laboratory IO (LIO) (RTILIO100)

               Copying Laboratory Signal Processing (LSP) (RTILSP100) from disk
               Verifying Laboratory Signal Processing (LSP) (RTILSP100)

               Copying Icon Development (RTIICON100) from disk
               Verifying Icon Development (RTIICON100)

               ________________________________________________________________
                                                       (continued on next page)

               B-2  Sample ULTRIX Installation

 











               Example B-1 (Cont.):  Sample Installation for RISC ULTRIX
                                     Development Kit
               ________________________________________________________________

               Copying DEC RT Integrator (Runtime) (RTIRTBASE100) from disk
               Verifying DEC RT Integrator (Runtime) (RTIRTBASE100)

               Copying DEC RT Integrator Manual Pages (RTIMAN100) from disk
               Verifying DEC RT Integrator Manual Pages (RTIMAN100)

               Copying DEC RT Integrator Examples (RTIEXA100) from disk
               Verifying DEC RT Integrator Examples (RTIEXA100)

               *************************************************************
               * Installation of DEC RT Integrator V1.0 complete.          *
               *                                                           *
               * The IVP for DEC RT Integrator for ULTRIX can be run after *
               * the installation has completed.                           *
               *                                                           *
               * To run the IVP, enter the following command:              *
               *        setld -v RTIBASE100                                *
               *************************************************************

               Creating/Modifying necessary files for the ULTRIX ek Driver V1.0
               For ULTRIX V40

               Creating links to V40 objects...
               Created scsi_asc.o...
               Created scsi_sii.o...
               Created scsi.o...
               Created scsi_proc.o...
               Created ekdriver.o...

               Modifying appropriate driver files...
               Modifying /sys/data/scsi_data.c

               Modifying /sys/io/scsi/mips/scsireg.h

               Modifying /sys/conf/mips/files.mips

               Modifying /sys/machine/common/conf.c

               Configuring the system to run the ULTRIX ek Driver V1.0
               For ULTRIX V40

               ________________________________________________________________
                                                       (continued on next page)

                                                Sample ULTRIX Installation  B-3

 











               Example B-1 (Cont.):  Sample Installation for RISC ULTRIX
                                     Development Kit
               ________________________________________________________________

               Creating /dev/ek0
               Creating /dev/ek1
               Creating /dev/ek2
               Creating /dev/ek3
               Creating /dev/ek4
               Creating /dev/ek5
               Creating /dev/ek6
               Creating /dev/ek7
               Creating /dev/ek8
               Creating /dev/ek9
               Creating /dev/ek10
               Creating /dev/ek11
               Creating /dev/ek12
               Creating /dev/ek13
               Creating /dev/ek14
               Creating /dev/ek15

               After verifying that the system is operating properly with the
               ek  Driver installed you may wish to remove the following
               saved files:
               - /sys/conf/mips/files.mips.sav[n]
               - /sys/machine/common/conf.c.sav[n]
               - /sys/data/scsi_data.c.sav[n]
               - /sys/conf/mips/MUNCHY.sav[n]

               Reminder:
                  - Edit /sys/conf/mips/MUNCHY
                  - Rebuild your kernel
                  - Move the new kernel to /.
                  - Reboot your system.

               Installation of the ULTRIX ek Driver V1.0 complete

               ________________________________________________________________







               B-4  Sample ULTRIX Installation

 










               ____________________________________________________________

               B.2  Sample Installation for RISC ULTRIX Runtime Kit

                  Example B-1 is a sample installation of the DEC RT Integrator
                  Runtime Kit. It assumes that DECnet has been shut down and no
                  users are logged in to your system.

               Example B-2:  Sample Installation for RISC ULTRIX Runtime Kit
               ________________________________________________________________

               # setld -l  /dev/rmt0h

               *** Enter Subset Selections ***

               The subsets listed below are optional:
                1) DEC RT Integrator (Runtime)          2) ULTRIX ek device driver
                3) Laboratory Graphic Package (LGP)     4) Laboratory IO (LIO)
                5) Laboratory Signal Processing (LSP)   6) DEC RT Integrator Manual Pages
                7) DEC RT Integrator Examples

                8) All of the Above
                9) None of the Above
               10) Exit without installing subsets

               Enter your choice(s): 8

               You are installing the following subsets:
                  DEC RT Integrator (Runtime)             ULTRIX ek device driver
                  Laboratory Graphic Package (LGP)        Laboratory IO (LIO)
                  Laboratory Signal Processing (LSP)      DEC RT Integrator Manual Pages
                  DEC RT Integrator Examples

               Is this correct? (y/n): y

               Copying DEC RT Integrator (Runtime) (RTIRUN100) from disk
               Verifying DEC RT Integrator (Runtime) (RTIRUN100)

               Copying ULTRIX ek device driver (RTI488100) from disk
               Verifying ULTRIX ek device driver (RTI488100)

               Copying Laboratory Graphic Package (LGP) (RTILGP100) from disk
               Verifying Laboratory Graphic Package (LGP) (RTILGP100)

               Copying Laboratory IO (LIO) (RTILIO100) from disk
               Verifying Laboratory IO (LIO) (RTILIO100)

               ________________________________________________________________
                                                       (continued on next page)

                                                Sample ULTRIX Installation  B-5

 











               Example B-2 (Cont.):  Sample Installation for RISC ULTRIX
                                     Runtime Kit
               ________________________________________________________________

               Copying Laboratory Signal Processing (LSP) (RTILSP100) from disk
               Verifying Laboratory Signal Processing (LSP) (RTILSP100)

               Copying DEC RT Integrator Manual Pages (RTIRTMAN100) from disk
               Verifying DEC RT Integrator Manual Pages (RTIRTMAN100)

               Copying DEC RT Integrator Examples (RTIEXA100) from disk
               Verifying DEC RT Integrator Examples (RTIEXA100)

               *************************************************************
               * Installation of DEC RT Integrator V1.0 complete.          *
               *                                                           *
               * The IVP for DEC RT Integrator for ULTRIX can be run after *
               * the installation has completed.                           *
               *                                                           *
               * To run the IVP, enter the following command:              *
               *        setld -v RTIRUN100                                 *
               *************************************************************

               Creating/Modifying necessary files for the ULTRIX ek Driver V1.0
               For ULTRIX V40

               Creating links to V40 objects...
               Created scsi_asc.o...
               Created scsi_sii.o...
               Created scsi.o...
               Created scsi_proc.o...
               Created ekdriver.o...

               Modifying appropriate driver files...
               Modifying /sys/data/scsi_data.c

               Modifying /sys/io/scsi/mips/scsireg.h

               Modifying /sys/conf/mips/files.mips

               Modifying /sys/machine/common/conf.c

               Configuring the system to run the ULTRIX ek Driver V1.0
               For ULTRIX V40

               ________________________________________________________________
                                                       (continued on next page)

               B-6  Sample ULTRIX Installation

 











               Example B-2 (Cont.):  Sample Installation for RISC ULTRIX
                                     Runtime Kit
               ________________________________________________________________

               Creating /dev/ek0
               Creating /dev/ek1
               Creating /dev/ek2
               Creating /dev/ek3
               Creating /dev/ek4
               Creating /dev/ek5
               Creating /dev/ek6
               Creating /dev/ek7
               Creating /dev/ek8
               Creating /dev/ek9
               Creating /dev/ek10
               Creating /dev/ek11
               Creating /dev/ek12
               Creating /dev/ek13
               Creating /dev/ek14
               Creating /dev/ek15

               After verifying that the system is operating properly with the
               ek  Driver installed you may wish to remove the following
               saved files:
               - /sys/conf/mips/files.mips.sav[n]
               - /sys/machine/common/conf.c.sav[n]
               - /sys/data/scsi_data.c.sav[n]
               - /sys/conf/mips/MUNCHY.sav[n]

               Reminder:
                  - Edit /sys/conf/mips/MUNCHY
                  - Rebuild your kernel
                  - Move the new kernel to /.
                  - Reboot your system.

               Installation of the ULTRIX ek Driver V1.0 complete

               ________________________________________________________________







                                                Sample ULTRIX Installation  B-7

 

















                                                                     Appendix C


                                                        Sample VMS Installation
               ________________________________________________________________


                  Appendix C provides the following:

                   o An installation of DEC RT Integrator Development Kit on a
                     VMS system (see Section C.1)

                   o An installation of DEC RT Integrator Runtime Kit on a VMS
                     system (see Section C.2)

               ____________________________________________________________

               C.1  Sample Installation for VMS Development Kit

                  Example C-1 is a sample installation of the DEC RT Integrator
                  VMS Development Kit. It assumes that DECnet has been shut
                  down and no users are logged in to your system.

















                                                   Sample VMS Installation  C-1

 











               Example C-1:  Sample Installation for VMS Development Kit
               ________________________________________________________________

               $ @vmsinstal

                       VAX/VMS Software Product Installation Procedure V5.3

               It is 10-FEB-1991 at 16:53.

               Enter a question mark (?) at any time for help.

               * Are you satisfied with the backup of your system disk [YES]?
               * Where will the distribution volumes be mounted: dka200:

               Enter the products to be processed from the first distribution volume set.
               * Products: rti
               * Enter installation options you wish to use (none):

               The following products will be processed:

                 RTI V2.0

                       Beginning installation of RTI V2.0 at 16:53

               %VMSINSTAL-I-RESTORE, Restoring product save set A ...
               %VMSINSTAL-I-RELMOVED , The product's release notes have been successfully
               moved
                to SYS$HELP.
               %RTI-I-VMSOK, Installing DEC RT Integrator V2.0 on VMS Version V5.3, continuing
               ...

                       Product:      RTI-V
                       Producer:     DEC
                       Version:      V2.0
                       Release Date: 20-JAN-91

               * Does this product have an authorization key registered and loaded? yes
               * Do you want to purge files replaced by this installation [YES]?

               * Do you want to install the DEC RT Integrator V2.0 Standard Software [YES]?
               * Is this a European installation [NO]?
               * Do you want to install the DEC RT Integrator V2.0 Optional Software [NO]?
               * Do you want to install the LIO examples in executable form? [NO]?
               * Does your DEC Realtime Test Integrator system have an
               * IEZ11 SCSI to IEEE-488 converter [NO]? yes

               ________________________________________________________________
                                                       (continued on next page)

               C-2  Sample VMS Installation

 











               Example C-1 (Cont.):  Sample Installation for VMS Development
                                     Kit
               ________________________________________________________________

                   Your current SCSI device configuration, as known to VMS, contains:
                                (Pure internal SCSI buses not shown)

                      2 disks

                   The current SCSI ID assignment is:

                       0        1        2        3        4        5        6        7
                    unused   unused   DKA200   DKA300   unused   unused    *CPU*   unused
                                      >disk<   >disk<

                   You may connect up to 5 IEZ11 SCSI488/D bus converters to the
                   external SCSI connector of your VAXstation or MicroVAX.

                   WARNING: Connecting more than two IEZ11 SCSI488/D bus converters
                            may conflict with future system hardware extensions.

               * How many IEZ11 bus converters will you connect to the SCSI port [1]:
               * Use device EKA0:, SCSI ID 0 (currently unused) [Y]?

                   The current SCSI ID assignment is:

                       0        1        2        3        4        5        6        7
                     EKA0    unused   DKA200   DKA300   unused   unused    *CPU*   unused
                     IEZ11            >disk<   >disk<

                   The system specific IEZ11 driver startup commands are placed in:

                   SYS$SPECIFIC:[SYS$STARTUP]IEZ11$STARTUP.COM

               * Do you want to install and execute the DEC RT Integrator V2.0 IVP [YES]?
               * Do you want to run the DECwindows version of the IVP [YES]? no

               * Your selections are complete, do you want to proceed [YES]?

               ________________________________________________________________
                                                       (continued on next page)




                                                   Sample VMS Installation  C-3

 











               Example C-1 (Cont.):  Sample Installation for VMS Development
                                     Kit
               ________________________________________________________________

               No further questions will be asked.
               This installation takes approximately 60 minutes on a MicroVAX II.
               %VMSINSTAL-I-RESTORE, Restoring product save set B ...
               %VMSINSTAL-I-RESTORE, Restoring product save set C ...
               %VMSINSTAL-I-RESTORE, Restoring product save set D ...
               %VMSINSTAL-I-RESTORE, Restoring product save set E ...
               %VMSINSTAL-I-RESTORE, Restoring product save set F ...
               %VMSINSTAL-I-RESTORE, Restoring product save set G ...
               %VMSINSTAL-I-RESTORE, Restoring product save set H ...
               %VMSINSTAL-I-RESTORE, Restoring product save set I ...
               %VMSINSTAL-I-RESTORE, Restoring product save set L ...

                        +-----------------------------------------------------------+
                        |                                                           |
                        |                                                           |
                        |     Please read the Release Notes for this release of     |
                        |                                                           |
                        |                DEC Realtime Test Integrator               |
                        |                                                           |
                        |               which are located in the file:              |
                        |              SYS$HELP:RTI020.RELEASE_NOTES                |
                        |                                                           |
                        |         Please add the following line to the file         |
                        |               SYS$STARTUP:SYSTARTUP_V5.COM                |
                        |                                                           |
                        |             $ @SYS$STARTUP:RTI_STARTUP.COM                |
                        |                                                           |
                        +-----------------------------------------------------------+

               %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...

                          +-------------------------------------------------------+
                          |                                                       |
                          |       DEC Realtime Test Integrator for VMS V2.0       |
                          |          Installation Verification Procedure          |
                          |                                                       |
                          +-------------------------------------------------------+

                                                    NOTE:

               ________________________________________________________________
                                                       (continued on next page)

               C-4  Sample VMS Installation

 











               Example C-1 (Cont.):  Sample Installation for VMS Development
                                     Kit
               ________________________________________________________________

                       You have either indicated that you are not on a DECwindows display
                       or GKS is not  installed.  Therefore  the  graphics section of the
                       Installation Verification Procedure will not be attempted.

                       Your terminal bell should ring seven times and the message

                          'DEC RT Integrator Installation Verification Program'

                       Should be printed on your terminal.

               DEC RT Integrator Installation Verification Program

                    +--------------------------------------------------------------------+
                    |                                                                    |
                    |        DEC RT Integrator Installation Verification Procedure       |
                    |                     successfully completed                         |
                    |                                                                    |
                    +--------------------------------------------------------------------+

                       Installation of RTI V2.0 completed at 17:18

               Enter the products to be processed from the next distribution volume set.
               * Products:

               ________________________________________________________________
















                                                   Sample VMS Installation  C-5

 










               ____________________________________________________________

               C.2  Sample Installation for VMS Runtime Kit

                  Example C-2 is a sample installation of the DEC RT Integrator
                  VMS Runtime Kit. It assumes that DECnet has been shut down
                  and no users are logged in to your system.

               Example C-2:  Sample Installation for VMS Runtime Kit
               ________________________________________________________________

               $ @vmsinstal

                       VAX/VMS Software Product Installation Procedure V5.3

               It is 10-FEB-1991 at 16:53.

               Enter a question mark (?) at any time for help.

               * Are you satisfied with the backup of your system disk [YES]? yes
               * Where will the distribution volumes be mounted: dua1:

               Enter the products to be processed from the first distribution volume set.
               * Products: rtirt
               * Enter installation options you wish to use (none):

               The following products will be processed:

                 RTIRT V2.0

                       Beginning installation of RTIRT V2.0 at 12:31

               %VMSINSTAL-I-RESTORE, Restoring product save set A ...
               %VMSINSTAL-I-RELMOVED, Product's release notes have been moved to SYS$HELP.

               * Do you want to purge files replaced by this installation [YES]? yes

               * Do you want to install the DEC RT Integrator V2.0 Standard Software [YES]?
               * Is this a European installation [NO]?
               * Do you want to install the DEC RT Integrator V2.0 Optional Software [NO]?
               * Do you want to install the LIO examples in executable form? [NO]?
               * Does your DEC Realtime Test Integrator system have an
               * IEZ11 SCSI to IEEE-488 converter [NO]?
               * Do you want to install and execute the DEC RT Integrator V2.0 IVP [YES]?
               * Do you want to run the DECwindows version of the IVP [YES]? no

               * Your selections are complete, do you want to proceed [YES]?

               ________________________________________________________________
                                                       (continued on next page)

               C-6  Sample VMS Installation

 











               Example C-2 (Cont.):  Sample Installation for VMS Runtime Kit
               ________________________________________________________________

               No further questions will be asked.
               This installation takes approximately 60 minutes on a MicroVAX II.
               %VMSINSTAL-I-RESTORE, Restoring product save set B ...
               %VMSINSTAL-I-RESTORE, Restoring product save set C ...
               %VMSINSTAL-I-RESTORE, Restoring product save set D ...
               %VMSINSTAL-I-RESTORE, Restoring product save set E ...
               %VMSINSTAL-I-RESTORE, Restoring product save set F ...
               %VMSINSTAL-I-RESTORE, Restoring product save set G ...
               %VMSINSTAL-I-RESTORE, Restoring product save set H ...
               %VMSINSTAL-I-RESTORE, Restoring product save set I ...
               %VMSINSTAL-I-RESTORE, Restoring product save set L ...

                        +-----------------------------------------------------------+
                        |                                                           |
                        |                                                           |
                        |     Please read the Release Notes for this release of     |
                        |                                                           |
                        |                DEC Realtime Test Integrator               |
                        |                                                           |
                        |               which are located in the file:              |
                        |              SYS$HELP:RTIRT020.RELEASE_NOTES              |
                        |                                                           |
                        |         Please add the following line to the file         |
                        |               SYS$STARTUP:SYSTARTUP_V5.COM                |
                        |                                                           |
                        |             $ @SYS$STARTUP:RTI_STARTUP.COM                |
                        |                                                           |
                        +-----------------------------------------------------------+

               %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...

                          +-------------------------------------------------------+
                          |                                                       |
                          |       DEC Realtime Test Integrator for VMS V2.0       |
                          |          Installation Verification Procedure          |
                          |                                                       |
                          +-------------------------------------------------------+

                                                    NOTE:

               ________________________________________________________________
                                                       (continued on next page)

                                                   Sample VMS Installation  C-7

 











               Example C-2 (Cont.):  Sample Installation for VMS Runtime Kit
               ________________________________________________________________

                       You have either indicated that you are not on a DECwindows display
                       or GKS is not  installed.  Therefore  the  graphics section of the
                       Installation Verification Procedure will not be attempted.

                       Your terminal bell should ring seven times and the message

                          'DEC RT Intregrator Installation Verification Program'

                       Should be printed on your terminal.

               DEC RT Integrator Installation Verification Program

                    +--------------------------------------------------------------------+
                    |                                                                    |
                    |        DEC RT Integrator Installation Verification Procedure       |
                    |                     successfully completed                         |
                    |                                                                    |
                    +--------------------------------------------------------------------+

                       Installation of RTI V2.0 completed at 17:23

               Enter the products to be processed from the next distribution volume set.
               * Products:

               ________________________________________________________________

















               C-8  Sample VMS Installation

 




















                                                                      Index
               ________________________________________________________________


               A___________________________    Command files (Cont.)

               Abort installation                RTI_STARTUP.COM, 5-12,
                 ULTRIX, 2-3                       5-26, 6-2
                 VMS, 5-1                        startup, 6-2
               Adding ek device driver,          SYCONFIG.COM, 6-8
                  2-26                           SYLOGIN.COM, 5-12, 5-26
               ASTLM, 4-7, 6-7                   SYS$MANAGER:SYCONFIG.COM,
               Audience, ix                        6-8
               Authorize Utility, 6-7            SYS$STARTUP:RTI_
               AUTOGEN, 4-6                        STARTUP.COM, 6-2

               B                                 SYS$SYSTEM:SHUTDOWN.COM.,
               ____________________________        6-8
               Backup                            SYS$UPDATE:VMSINSTAL.COM,
                 system disk, ULTRIX, 1-8          5-2, 5-16
                 system disk, VMS, 4-7,          SYS$UPDATE:VMSLICENSE.COM,
                    5-2, 5-16                      4-2
               BIOLM, 4-7, 6-7                   SYSTARTUP_V5.COM, 5-12,
               Board                               5-26, 6-2
                 See Device                    Configuration file
               BYTLM, 4-7, 6-7                   adding a line, 2-26

               C                                 computing values, 2-27
               ____________________________      deleting a line, 2-31
               Cluster operations, 4-3, 6-5      fields, 2-27  to 2-30
               Command files                   Configuring Dms Client, 2-32
                 LOGIN.COM, 6-2, 6-4           Conventions, xiv

                                                                        Index-1

 






          D___________________________    Documentation

          Deleting Ek Driver, 2-32          associated, xiii
          Development Kit                 DRQ11-C
            ULTRIX                          device, 5-5, 5-19
               described, 1-2               device driver, 6-8
               disk space requirements
                  , 1-6                   E___________________________

               installation, 2-17         ek device driver
               selecting subsets, 2-6       adding, 2-26
                  to 2-7                    deleting, 2-31
               subsets, 2-5               EKDRIVER
            VMS                             installing for VMS, 5-6,
               described, 4-1                 5-20
               disk space requirements    ENQLM, 4-7
                  , 4-4                   Environment files
               installation, 5-2            Pascal, 6-9
          Device                          Error messages
            DRQ11-C, 5-5, 5-19              disk space, VMS, 4-4
            European, 5-5, 5-9, 5-19,       IVP for VMS, 5-30
               5-23                         ULTRIX, 2-33
            IEQ11, 5-5, 5-19                VMS, 5-30
            IXV11, 5-5, 5-9, 5-19,        European installation, 5-5,
               5-23                          5-19, 6-8
          Device driver                   Examples
            DRQ11-C, 6-8                    ULTRIX
            IEQ11, 6-8                         Development Kit
            IXV11, 6-8                           installation, 2-17
            loading for VMS, 6-8                 to 2-21, B-1  to B-4
          Device symbols, 6-8                  Runtime Kit installa-
          df, 1-7                                tion, 2-22  to 2-26,
          Dialogue                               B-5  to B-7
            See Example                     VMS
          DIOLM, 4-7, 6-7                      Development Kit
          Disk space                             installation, 5-2,
            df, 1-7
            ULTRIX requirements, 1-6             C-1  to C-5
            VMS requirements, 4-4              Runtime Kit installa-
            VMS Runtime Kit, 4-4                 tion, C-6  to C-8
          Distribution media, 2-3
          DMS server installation,        F___________________________
             ULTRIX, 1-3, 2-10  to        FILLM, 4-7
             2-13

          Index-2

 






          G___________________________    IXV11 (Cont.)

          GBLPAGES, 4-5                     device driver, 6-8
          GBLSECTIONS, 4-5
          GKS, 4-2, 5-4, 5-18             K___________________________
            logical names, 6-4            Kernel
          GKS$CONID, 6-4                    building, 2-31
          GKS$WSTYPE, 6-4                   ek device driver, 2-26

          H___________________________      ld driver, 2-26
          Hardware,ULTRIX                   reconfiguring, 2-26

            requirements, 1-4             L___________________________
            systems, 1-4                  Laboratory Graphics Package

          I___________________________      See LGP
          IEQ11                           ld driver, 2-26
            device, 5-5, 5-19             LGP, 2-5
            device driver, 6-8            License registration
          IEZ11$CONFIG.COM, 6-5             for VMS, 5-4, 5-18
          IEZ11 device driver               ULTRIX, 2-2
            installing for VMS, 5-6,        VMS, 4-2
               5-20                            for other nodes, 6-5
            loading in a VAXcluster,      Local area VAXcluster, 4-3,
               6-5                           6-5
          Installation                    Local installation, ULTRIX,
            European, 5-5, 5-19, 6-8         2-3
          Installation time,ULTRIX,       LOGIN.COM, 6-2, 6-4

             1-6                          M___________________________
          Installation Verification       MAXBUF parameter, 6-4
             Procedure                    Media
            See IVP                         ULTRIX, 2-3
          Installed files                      software distribution
            ULTRIX, A-1                          kit, 1-3
          IVP                               VMS, 5-3
            ULTRIX, 2-33                       loading the Development
               messages, 3-1                     kit, 5-3
               plot, 3-3                       loading the Runtime
               running, 3-1
            VMS, 5-8, 5-12, 5-22, 5-26           kit, 5-17
               plot, 7-1                       mounting the Runtime
               running, 7-1                      kit, 5-17
          IXV11                           Messages
            device, 5-9, 5-23

                                                                   Index-3

 






          Messages (Cont.)                Purging files
            IVP for ULTRIX, 3-1             VMS, 5-5, 5-19
          MODPARAMS.DAT, 4-6, 6-4         Q

          O                               ____________________________
          ____________________________    Quotas
          Operating system require-         system, 6-7
             ments                          user, 6-7

            ULTRIX, 1-5                   R
            VMS, 4-2                      ____________________________
          Optional software               REALTIME_SPTS parameter, 6-4
            ULTRIX, 1-5                   Reboot, 4-6
            VMS, 4-2                      Registration
          Organization, x                   See License registration

          P                               Release notes
          ____________________________      ULTRIX, 1-2
          PAK                               VMS, 5-3, 5-17
            for ULTRIX, 2-2                    accessing, 6-2
            for VMS, 4-2, 5-4, 5-18       Reporting problems
          Parameter settings                ULTRIX, 2-34
            See System parameters           VMS, 6-10
          Pascal                          Required hardware
            environment files, 6-9          ULTRIX, 1-4
          PEAK, 5-6, 5-12, 5-19, 5-26     Required software
          Peak Processing Package           ULTRIX, 1-5
            See PEAK                        VMS, 4-2
          Postinstallation                RIS
            VMS, 6-1  to 6-10               ULTRIX
          Preinstallation                      server installation,
            VMS, 4-1  to 4-7                     1-3
          Prerequisite software                to client, 1-2, 2-4
            ULTRIX, 1-5                   RISC ULTRIX
            VMS, 4-2                        See ULTRIX
          Privileges                      RIS server installation,
            ULTRIX, 1-6                      ULTRIX, 2-13  to 2-17
            VMS, 4-4                      RTI_STARTUP.COM, 5-12, 5-26,
          Problems                           6-2
            reporting, ULTRIX, 2-34       Runtime Kit
            reporting, VMS, 6-10            ULTRIX
          Processors                           described, 1-2
            ULTRIX, 1-4                        disk space requirements
          Programs                               , 1-6
            See Examples

          Index-4

 






          Runtime Kit                     SYS$STARTUP:RTI_STARTUP.COM,
            ULTRIX (Cont.)                   6-2
               subsets, 2-8  to 2-9       SYS$SYSROOT:[UNSUPPORTED.SSP]
            VMS                              , 5-12, 5-26
               described, 4-1             SYS$SYSTEM:MODPARAMS.DAT
               disk space requirements      See MODPARAMS.DAT
                  , 4-4                   SYS$SYSTEM:SHUTDOWN.COM.,
                                             6-8
          S___________________________    SYS$SYSTEM:SYSGEN, 4-5
          Sample programs                 SYS$UPDATE:AUTOGEN
            See Examples                    See AUTOGEN
          Scientific Subroutines          SYS$UPDATE:VMSINSTAL.COM,
             Package                         5-2, 5-16
            See SSP                       SYS$UPDATE:VMSLICENSE.COM,
          SCSI bus                           4-2
            for VMS systems, 5-6, 5-20    SYSGEN, 4-5
          setld, 2-17, 2-22, 3-1, B-1,    SYSTARTUP_V5.COM, 5-12,
             B-5                             5-26, 6-2
          Software                        System disk
            ULTRIX                          backup, ULTRIX, 1-8
               optional, 1-5                backup, VMS, 4-7, 5-2,
               required, 1-5                  5-16
            VMS                           System Generation Utility,
               optional, 5-12, 5-26          4-5
               required, 4-2              System parameters, 4-4
               unsupported, 5-12, 5-26      checking, 6-4
          SSP, 5-6, 5-12, 5-19, 5-26        GBLPAGES, 4-5
          Status display during subset      GBLSECTIONS, 4-5
             loading, 2-10                  MAXBUF, 6-4
          Stop installation                 modifying, 6-4
            ULTRIX, 2-3                     REALTIME_SPTS, 6-4
            VMS, 5-1                        TTY_ALTYPAHD, 6-4
          Subset loading                    TTY_TYPAHDSZ, 6-4

            Status display, 2-10          T
          Super user account, 1-6         ____________________________
          SYCONFIG.COM, 6-8               Tape cartridge
          SYLOGIN.COM, 5-12, 5-26           VMS
          SYS$HELP, 5-4, 5-12, 5-18,           loading the Development
             5-26, 6-2                           kit, 5-3
          SYS$MANAGER:SYCONFIG.COM,            loading the Runtime
             6-8                                 kit, 5-17

                                                                   Index-5

 






          Time                            VMS (Cont.)
            install on ULTRIX, 1-6          Authorize Utility, 6-7
            install on VMS, 4-3             Development Kit
          TK50 distribution media,             disk space requirements
             ULTRIX, 2-3                         , 4-4
          TTY_ALTYPAHD parameter, 6-4          installation, 5-2  to
          TTY_TYPAHDSZ parameter, 6-4            5-15, C-1

          U                                 IVP
          ____________________________         plot, 7-1
          ULTRIX                               running, 7-1
            Development Kit                 operating system
               disk space requirements        requirements, 4-2
                  , 1-6                     required software, 4-2
               installation, 2-17  to       Runtime Kit
                  2-21, B-1                    disk space, 4-4
               subsets, 2-5                    disk space requirements
            DMS server installation,             , 4-4
               1-3, 2-10                       installation, 5-16  to
            error messages, 2-34                 5-29, C-6
            files installed, A-1          VMSINSTAL
            IVP                             requirements, 4-7
               messages, 3-1                running, 5-1, 5-16
               plot, 3-3
               running, 3-1               W___________________________
            operating system              WSDEF, 6-7
               requirements, 1-5          WSEXTENT, 6-8
            reporting problems, 2-34      WSQUO, 6-7
            required software, 1-5
            RIS server installation,
               1-3, 2-13
            Runtime Kit
               disk space requirements
                  , 1-6
               installation, 2-22  to
                  2-26, B-5
               subsets, 2-8
            stopping installation, 2-3

          V___________________________

          VAXcluster, 4-3, 6-5
          VMS

          Index-6
