 






           System
           Support
           Addendum

           _________________________________________________________
           _________________________________________________________

           PRODUCT NAME:  DECnet/SNA Data Transfer Facility,     SSA
           27.85.03-A                Version 3.0

           HARDWARE REQUIREMENTS

           Processors Supported:

           VAX:       VAX 4000 Model 200,
                      VAX 4000 Model 300

                      VAX 6000 Model 200 Series,
                      VAX 6000 Model 300 Series,
                      VAX 6000 Model 400 Series,
                      VAX 6000 Model 500 Series

                      VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX
                      8500, VAX 8530, VAX 8550, VAX 8600, VAX 8650,
                      VAX 8700, VAX 8800, VAX 8810, VAX 8820, VAX
                      8830, VAX 8840

                      VAX 9000 Model 210,
                      VAX 9000 Model 400 Series

                      VAXft 3000 Model 310

                      VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

           MicroVAX:  MicroVAX II, MicroVAX 2000,
                      MicroVAX 3100, MicroVAX 3300,
                      MicroVAX 3400, MicroVAX 3500,
                      MicroVAX 3600, MicroVAX 3800,


                                    DIGITAL                June 1991

                                                         AE-MA18C-TE

 



           DECnet/SNA Data Transfer Facility,        SSA 27.85.03-A
           Version 3.0


                      MicroVAX 3900

           VAXstation:VAXstation II, VAXstation 2000,
                      VAXstation 3100 Series, VAXstation 3200,
                      VAXstation 3500, VAXstation 3520,
                      VAXstation 3540

           VAXserver: VAXserver 3100, VAXserver 3300, VAXserver
                      3400, VAXserver 3500, VAXserver 3600,
                      VAXserver 3602, VAXserver 3800, VAXserver
                      3900

                      VAXserver 4000 Model 200,
                      VAXserver 4000 Model 300

                      VAXserver 6000 Model 210,
                      VAXserver 6000 Model 220,
                      VAXserver 6000 Model 310,
                      VAXserver 6000 Model 320,
                      VAXserver 6000 Model 410,
                      VAXserver 6000 Model 420,
                      VAXserver 6000 Model 510,
                      VAXserver 6000 Model 520

           Processors Not Supported

           MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXsta-
           tion 8000

           Disk Space Requirements:

           VMS/DTF Server (Block Cluster Size = 1):

           Disk space required for     2,400 blocks
           installation:
                                       (1,200 Kbytes)




                                       2

 



           DECnet/SNA Data Transfer Facility,        SSA 27.85.03-A
           Version 3.0



           Disk space required for     2,000 blocks
           use (permanent):
                                       (1,000 Kbytes)

           VMS/DTF Utilities (Block Cluster Size = 1):

           Disk space required for     1,600 blocks
           installation:
                                       (800 Kbytes)

           Disk space required for     950 blocks
           use (permanent):
                                       (475 Kbytes)

           DTF for MVS (Listed in 3380 Tracks):

           Disk space required         185 tracks
           for installation and
           maintenance:

           Disk space required for     61 tracks
           use (permanent):

           DTF for VM (Listed in 4K Blocks):

           Disk space required         1,000 blocks
           for installation and
           maintenance:

           Disk space required for     3,000 blocks
           use (permanent):

           These counts refer to the disk space required on the sys-
           tem disk. The sizes are approximate; actual sizes may vary
           depending on the user's system environment, configuration,
           and software options.



                                       3

 



           DECnet/SNA Data Transfer Facility,        SSA 27.85.03-A
           Version 3.0

           CLUSTER ENVIRONMENT

           This layered product is fully supported when installed on
           any valid and licensed VAXcluster* configuration without re-
           strictions. The HARDWARE REQUIREMENTS sections of this prod-
           uct's Software Product Description and System Support Ad-
           dendum detail any special hardware required by this prod-
           uct.

           *  V5.x VAXcluster configurations are fully described in the
              VAXcluster Software Product Description (29.78.xx) and
              include CI, Ethernet, and Mixed Interconnect configura-
              tions.

           SOFTWARE REQUIREMENTS

           For VMS/DTF Server and VMS/DTF Utilities:

           VMS Operating System V5.2 - V5.4
           DECnet-VAX V5.2 - V5.4
           VMS/DTF Server V2 - V3

           The DECnet/SNA® Data Transfer Facility software requires one
           of the following products. Refer to the appropriate SPD for
           prerequisite hardware and software.

           o  VMS/SNA V2.1 (SPD 27.01.xx)

           o  DECnet/SNA Gateway-ST V1.2 (SPD 29.C6.xx)

           o  DECnet/SNA Gateway-CT V2.0 (SPD 29.76.xx)

           For VMS Clients:

           DECnet-VAX V5.4

           For ULTRIX Clients:

           ULTRIX Operating System V4.2
           DECnet-ULTRIX V4.2

           For MS-DOS® Clients:

                                       4

 



           DECnet/SNA Data Transfer Facility,        SSA 27.85.03-A
           Version 3.0

           PATHWORKS for DOS V4.0

           For OS/2® Clients:

           PATHWORKS for OS/2 V4.0

           For RSX-llM-PLUS Clients:

           DECnet-11M-PLUS V4.0

           For specific MS-DOS, OS/2, and RSX-11M-PLUS Operating Sys-
           tem Versions, refer to the PATHWORKS for DOS SPD (55.07.xx),
           PATHWORKS for OS/2 SPD (55.24.xx), and DECnet-11M-PLUS SPD
           (10.66.xx).

           For IBM® MVS Clients:

           VTAM V3.1, V3.2
           MVS/ESA V3.1 or MVS/XA V2.0
           DFP/ESA V3.1, V3.2 or DFP/XA V2.2, 2.3
           SMP/E V1.4, V1.5
           Assembler H V2.1, V2.2
           DTF for MVS V2, V3

           IBM VM Clients:

           VTAM V3.1, V3.2
           VM/SP5, VM/SP6, or VM/XA V2.2
           DTF for VM V3.0

           VMS Tailoring:

           For VMS V5.x systems, the following VMS classes are required
           for full functionality of this layered product:

           o  VMS Required Saveset

           o  Network Support

           o  Utilities

                                       5

 



           DECnet/SNA Data Transfer Facility,        SSA 27.85.03-A
           Version 3.0

           For more information on VMS classes and tailoring, refer to
           the VMS Operating System Software Product Description (SPD
           25.01.xx)


           OPTIONAL SOFTWARE

           For VMS/DTF Server:

           VAX Common Data Dictionary Plus V4.0
              (DMU format only)
           VAX DATATRIEVE V4.1
           DECnet/SNA Gateway Management V2.1

           For VMS Clients:

           VMS/DTF Utilities

           For IBM MVS Clients:

           TSO/E[1]
           ISPF
           JES2 or JES3
           CA-ACF2[TM], RACF, or CA-TOPSECRET[TM]

           For IBM VM Clients:

           ISPF
           Dirmaint
           CA-ACF2, RACF, or VMSECURE[TM]
           Assembler H[2]

           Refer to the SOFTWARE WARRANTY section of SPD 27.85.xx for
           the required versions of the VM-resident software.

           _________________
         [1] TSO with REXX needed for single-line interface.  Native

             node TSO can support DTF command processor only.

         [2] Assembler H is needed only to change sample exits.

                                       6

 



           DECnet/SNA Data Transfer Facility,        SSA 27.85.03-A
           Version 3.0

           GROWTH CONSIDERATIONS

           The minimum hardware/software requirements for any future
           version of this product may be different from the require-
           ments for the current version.

           DISTRIBUTION MEDIA

           For VMS Systems:

           9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

           For DTF for IBM MVS and VM Systems:

           9-track 6250 BPI Magtape

           ORDERING INFORMATION

           VMS/DTF Software:

           For VMS/DTF Server:

           Software Licenses: QL-VEBA*-**
           Software Media: QL-VEBA*-**
           Software Documentation: QL-VEBA*-GZ
           Software Product Services: QT-VEBA*-**

           For VMS/DTF Utilities:

           Software Licenses: QL-VEKA*-**
           Software Media: QA-VEKA*-**
           Software Documentation: QA-VEKA*-GZ
           Software Product Services: QA-VEKA*-**

           DTF for IBM Software:

           DTF for MVS:




                                       7

 



           DECnet/SNA Data Transfer Facility,        SSA 27.85.03-A
           Version 3.0

           Software License: QL-1GQA9-AA
           Software Media: QA-1GQAA-**
           Software Documentation: QA-1GQAA-GZ
           Software Product Services: QA-1GQA*-**

           DTF for VM:

           Software License: QL-GUYA9-AA
           Software Media: QA-GUYAA-**
           Software Documentation: QA-GUYAA-GZ
           Software Product Services: QA-GUYA*-**

           *  Denotes variant fields. For additional information on avail-
              able licenses, services, and media, refer to the appro-
              priate price book.

           The above information is valid at time of release. Please
           contact your local Digital office for the most up-to-date
           information.

           ®   IBM, OS/2, and SNA are registered trademarks of
               International Business Machines Corporation.

           ®   MS-DOS is a registered trademark of Microsoft Corpo-
               ration.

           [TM]CA-ACF2 and CA-TOPSECRET are trademarks of Computer
               Associates International, Inc.

           [TM]VMSECURE is a trademark of The Systems Center.

           [TM]The DIGITAL Logo, DATATRIEVE, DEC, DECnet, DECnet-DOS,
               MicroVAX, PATHWORKS, RSX-11M-PLUS, TK, ULTRIX, VAX,
               VAX CCD, VAXcluster, VAXft, VAXserver, VAXstation,
               and VMS are trademarks of Digital Equipment Corpora-
               tion.





                                       8
