 






          System
          Support
          Addendum

          ________________________________________________________________

          PRODUCT NAME:  DECnet/SNA VMS Gateway Management,   SSA 29.70.01-A
                         Version 2.1

          HARDWARE REQUIREMENTS

          Processors Supported:

          VAX:      VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840, VAX 8842,
                    VAX 8974, VAX 8978

                    VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

          MicroVAX: MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,
                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900

          VAXstation: VAXstation II, VAXstation 2000,
                      VAXstation 3100 Series, VAXstation 3200,
                      VAXstation 3500, VAXstation 3520,
                      VAXstation 3540




                                       DIGITAL                   July 1990

                                                               AE-LT51B-TE

 


          DECnet/SNA VMS Gateway Management, Version 2.1    SSA 29.70.01-A




          VAXserver: VAXserver 3100, VAXserver 3300,
                     VAXserver 3400, VAXserver 3500,
                     VAXserver 3600, VAXserver 3602,
                     VAXserver 3800, VAXserver 3900

                     VAXserver 6000-210, VAXserver 6000-310,
                     VAXserver 6000-410, VAXserver 6000-420

          Processors Not Supported:

          MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXstation
          8000

          Block Space Requirements (Block Cluster Size = 1):

          Disk space required for      1,700 blocks
          installation:
                                       (850K bytes)

          Disk space required for      1,500 blocks
          use (permanent):
                                       (750K bytes)

          These counts refer to the disk space required on the system
          disk. The sizes are approximations; actual sizes may vary de-
          pending on the user's system environment, configuration, and
          software options selected.

          OPTIONAL HARDWARE

          None

          CLUSTER ENVIRONMENT

          This layered product is fully supported when installed on any
          valid and licensed VAXcluster* configuration without restric-
          tions. The  HARDWARE REQUIREMENTS sections of this product's
          Software Product Description and System Support Addendum detail
          any special hardware required by this product.

                                          2

 


          DECnet/SNA VMS Gateway Management, Version 2.1    SSA 29.70.01-A



          * V5.x VAXcluster configurations are fully described in the
          VAXcluster Software Product Description (29.78.xx) and include
          CI, Ethernet, and Mixed Interconnect Configurations.

          SOFTWARE REQUIREMENTS

          o  VMS Operating System V5.2, V5.3

          Layered Product

          o  DECnet-VAX V5.2, V5.3

          VMS Tailoring

          For VMS V5.x systems, the following VMS classes are required for
          full functionality of this layered product:

          o  VMS required Saveset

          o  Network Support

          For more information on VMS classes and tailoring, refer to
          the VMS Operating System Software Product Description (SPD
          25.01.xx).

          OPTIONAL SOFTWARE

          o  DECnet/SNA Gateway-ST V1.1

          o  DECnet/SNA Gateway-CT V2.0

          For more information on other access routines available for use
          with the DECnet/SNA Gateway, refer to the appropriate DECnet/SNA
          Gateway SPD.

          GROWTH CONSIDERATIONS

          The minimum hardware/software requirements for any future ver-
          sion of this product may be different from the minimum require-
          ments for the current version.

          DISTRIBUTION MEDIA

                                          3

 


          DECnet/SNA VMS Gateway Management, Version 2.1    SSA 29.70.01-A



          Tape: 9-track 1600 BPI Magtape (PE), TK50 Tape Cartridge

          This product is also available as part of the VMS Consolidated
          Software Distribution on CDROM.

          ORDERING INFORMATION

          Software Licenses: QL-VCKAA-AA
          Software Media: QA-VCKAA-**
          Software Documentation: QA-VCKAA-GZ
          Software Product Services: QT-VCKA*-**

          *  Denotes variant fields. For additional information on avail-
             able licenses, services, and media, refer to the appropriate
             price book.

          The above information is valid at time of release. Please con-
          tact your local Digital office for the most up-to-date informa-
          tion.

          [R]  IBM is a registered trademark of International Business
               Machines, Inc.

          [R]  The DIGITAL Logo is a registered trademark of Digital
               Equipment Corporation.

          [TM] DECnet/SNA, DECnet-VAX, MicroVAX, VAXstation, VAXserver,
               VAXcluster, VAX and VMS are trademarks of Digital Equipment
               Corporation.










                                          4
