 















             _____________________________________________
             DECnet/SNA VMS APPC/LU6.2 Programming Interface
             Installation


                                                              AA-EV68D-TE




             This document tells the user how to install the DECnet/SNA
             VMS APPC/LU6.2 Programming Interface software.




             Revision/Update Information:  This is a revised manual.

             Operating System and Version: VMS Version 5.3

             Software Version:             DECnet/SNA VMS APPC/LU6.2
                                           Programming Interface Version
                                           2.2




             Digital Equipment Corporation
             Maynard, Massachusetts

 





             _____________________________________________
             October 1990

             The information in this document is subject to change without
             notice and should not be construed as a commitment by Digital
             Equipment Corporation. Digital Equipment Corporation assumes
             no responsibility for any errors that may appear in this
             document.

             The software described in this document is furnished under a
             license and may be used or copied only in accordance with the
             terms of such a license.

             No responsibility is assumed for the use or reliability
             of software on equipment that is not supplied by Digital
             Equipment Corporation or its affiliated companies.

             Restricted Rights: Use, duplication, or disclosure by the
             U.S. Government is subject to restrictions as set forth in
             subparagraph (c)(1)(ii) of the Rights in Technical Data and
             Computer Software clause at DFARS 252.227-7013.

                  Copyright ©1988, 1990 Digital Equipment Corporation
                                  All Rights Reserved
                                   Printed in U.S.A.

             The following are trademarks of Digital Equipment Corporation:

             DEC           ULTRIX        VAXcluster
             DECUS         UNIBUS        VMS
             DECnet        VAX           DIGITAL
             PDP

             IBM is a registered trademark of International Business
             Machines Corporation.


             This manual was produced by Telecommunications and Networks
	     Publications.

 















          ________________________________________________________________


                                                                  Contents




          About This Guide.........................................      v


          1  Preparing for Installation

                   Inspecting the Distribution Kit.................    1-1
                   Preparing the IBM SNA Environment...............    1-1
                   VMS System Requirements.........................    1-2
                   Verifying the Required VMS Version..............    1-3
                   Verifying Necessary Privileges..................    1-3
                   Verifying Required Disk Space...................    1-3
                   Determining Available Global Sections and Global
                   Pages...........................................    1-4
                   Registering and Loading the Product
                   Authorization Key...............................    1-4
                   Installing the Required Gateway Management
                   Software........................................    1-4
                   Installing the Required Transport Software......    1-4
                   Backing Up Your System Disk.....................    1-5





                                                                       iii

 






          2  Installing the APPC/LU6.2 Programming Interface

                   Installed Files.................................   2-10


          3  After the Installation

                   Verifying the Installation......................    3-1
                   Using the APPC/LU6.2 Software in a VAXcluster...    3-2
                   Installing the APPC/LU6.2 Programming Interface
                   as a Shareable Image............................    3-3
                   Adding the SNA_APPC HELP File to the HELP File
                   of an Editor....................................    3-3


          Index

          Tables

             1-1  Installation Requirements for the VMS APPC/LU6.2
                  Programming Interface............................    1-2



















          iv

 














          ________________________________________________________________


                                                          About This Guide




             The DECnet/SNA VMS APPC/LU6.2 Programming Interface enables
             VMS users to communicate with programs running on IBM
             systems. This manual is for system managers responsible for
             planning and installing the software.

          Document Structure

             This manual has the following chapters:

              _ Chapter 1, Preparing for Installation, provides in-

                structions on how to install the APPC/LU6.2 Programming
                Interface using the VMSINSTAL procedure.

              _ Chapter 2, Installing the APPC/LU6.2 Programming Interface

                software, provides a step-by-step process for installing
                the software.

              _ Chapter 3, After the Installation, describes steps you

                must take to verify the installation of the APPC/LU6.2
                Programming Interface software.

                                                                         v

 






          Related Documents

              _ DECnet/SNA VMS APPC/LU6.2 Programming Interface Programming

              _ DECnet/SNA VMS Gateway Management Installation

              _ DECnet/SNA VMS Gateway Management Management

              _ VMS/SNA Installation

              _ VMS/SNA Problem Solving

              _ VMS/SNA Guide to IBM Parameters

              _ Installing the DEC MicroServer

              _ Installing the DEC MicroServer-SP

              _ DECnet/SNA Gateway-ST Installation

              _ DECnet/SNA Gateway-ST Problem Solving

              _ DECnet/SNA Gateway-ST Guide to IBM Parameters

              _ DEC ChannelServer Hardware Installation Guide

              _ DEC ChannelServer Hardware Troubleshooting Guide

              _ DEC ChannelServer II Installation

              _ DEC ChannelServer II Problem Solving

              _ DECnet/SNA Gateway-CT Installation

              _ DECnet/SNA Gateway-CT Problem Solving

              _ DECnet/SNA Gateway-CT Guide to IBM Parameters

              _ VMS License Management Utility Manual

              _ VMS System Manager's Manual

          vi

 






          Conventions

             This manual uses the following conventions:

             Conventions         Meaning

             Special Type        Represents system input and output.
                                 System output prints in black; user input
                                 is in red.

             UPPERCASE LETTERS   Represent constant values or symbols.
                                 Code these exactly as they are specified.

             [  ]                Square brackets enclose optional values.
                                 Do not type the brackets in the command
                                 line.

             <Return>            Unless otherwise specified, terminate
                                 every command line by pressing <Return>.

             <Ctrl/x>            Control characters are shown as <Ctrl/x>,
                                 where x is an alphabetic character. Press
                                 <Ctrl> and the appropriate character key
                                 simultaneously.
















                                                                       vii

 

















                                                                              1
               ________________________________________________________________

                                                     Preparing for Installation




                  This chapter tells you how to prepare for installing the
                  APPC/LU6.2 Programming Interface on systems running either
                  VMS/SNA V2.0, DECnet/SNA Gateway-CT V2.0, or DECnet/SNA
                  Gateway-ST V1.1 software.



               Inspecting the Distribution Kit

                  The software Bill of Materials (BOM) included with your
                  distribution kit shows the contents of the kit. Carefully
                  compare the items you received against the BOM. Report
                  any missing or damaged components to Digital Equipment
                  Corporation before continuing with the installation.


               Preparing the IBM SNA Environment

                  Before you can use the APPC/LU6.2 Programming Interface
                  Software, you must prepare certain software components in
                  the IBM environment, as follows:

                   _ The VMS/SNA Guide to IBM Parameters explains the IBM

                     parameters to define for successful communication between
                     the IBM host and VMS/SNA.








                                                Preparing for Installation  1-1

 











                   _ The DECnet/SNA Gateway-ST Guide to IBM Parameters explains

                     the IBM parameters to define for successful communication
                     between the IBM host and your Gateway-ST.

                   _ The DECnet/SNA Gateway-CT Guide to IBM Parameters explains

                     the IBM parameters to define for successful communication
                     between the IBM host and your Gateway-CT.

                  You should view the Digital documentation as an adjunct
                  to the IBM documentation; the IBM documentation remains
                  the authoritative source for IBM software concepts and
                  procedures.

               Note Since IBM system programmers reconfigure and generate
                  their systems according to a set schedule, give them as much
                  advance notice as possible.

               VMS System Requirements

                  Table 1-1 shows the minimum VMS system requirements. More
                  detailed explanations follow the table.

                  Table 1-1    Installation Requirements for the VMS APPC/LU6.2
                               Programming Interface

                  _____________________________________________________________
                  Requirements          Specifications
		  _____________________________________________________________

                  Software Version      VMS Version 5.3 or Version 5.4

                  Privileges            System manager level (SYSPRV)

                  Disk space            4400 blocks minimum during installa-
                                        tion; 4400 blocks after installation

                  Global sections       4

                  Global pages          341

                  Approximate           6 to 30 minutes, depending on the type
                  installation time     of medium used

                                                       (continued on next page)



               1-2  Preparing for Installation

 











                  Table 1-1 (Cont.)    Installation Requirements for the VMS
                                       APPC/LU6.2 Programming Interface

                  _____________________________________________________________
                  Requirements		Specifications
		  _____________________________________________________________

                  Related documents	VMS System Manager's Manual
		  _____________________________________________________________

               Verifying the Required VMS Version

                  Your VMS system must be running VMS V5.3 or V5.4. Use the
                  SHOW SYSTEM command to determine the current version. If you
                  do not have the required version, you must install it before
                  you install the APPC/LU6.2 Programming Interface software.
                  The VMS System Manager's Manual explains how to install VMS
                  software.


               Verifying Necessary Privileges

                  To install the APPC/LU6.2 Programming Interface software,
                  you must be logged in to an account that has SYSPRV. Use the
                  SHOW PROCESS/PRIVILEGES command to check privileges.


               Verifying Required Disk Space

                  The APPC/LU6.2 Programming Interface software requires 4400
                  free blocks on the system disk during installation, and 4400
                  blocks after installation. Use the SHOW DEVICE command to
                  check available disk space.

                  The APPC/LU6.2 Programming Interface software supports VMS
                  tailoring for installation on systems that have limited
                  system disk space. The APPC/LU6.2 Programming Interface
                  Software Product Description (SPD) explains VMS tailoring and
                  lists the necessary VMS system classes. The VMS SPD provides
                  more information on classes and VMS tailoring.










                                                Preparing for Installation  1-3

 











               Determining Available Global Sections and Global Pages

                  The APPC/LU6.2 Programming Interface requires a minimum of
                  four (4) global sections and 341 global pages. To check the
                  number of global sections and global pages available on your
                  system, type the following command at the VMS prompt ($).

                  $ install list/summary/global

                  The VMSINSTAL utility will display the number of global
                  sections and global pages available on your system.

               Registering and Loading the Product Authorization Key

                  Make sure that you have registered and loaded the Product
                  Authorization Key (PAK) before your begin the installation.
                  Refer to the VMS License Management Utility Manual for this
                  information.


               Installing the Required Gateway Management Software

                  DECnet/SNA Gateway Management V2.1 software must be installed
                  before you can use the APPC/LU6.2 Programming Interface
                  software. Use Gateway Management software to configure and
                  manage the Gateway-CT or Gateway-ST.

                  DECnet/SNA VMS Gateway Management Installation explains how
                  to install the Gateway Management software.


               Installing the Required Transport Software

                  VMS/SNA V2.0, DECnet/SNA Gateway-ST V1.1, or DECnet/SNA
                  Gateway-CT V2.0 software must be installed before you can
                  use the APPC/LU6.2 Programming Interface software. Use the
                  transport software to communicate with the IBM host. See the
                  Software Product Description (SPD) for more information.










               1-4  Preparing for Installation

 











               Backing Up Your System Disk

                  Before you start an installation that involves writing to
                  your system disk, Digital Equipment Corporation recommends
                  that you make a backup copy of your system disk. The VMS
                  System Manager's Manual explains how to back up your system
                  disk.









































                                                Preparing for Installation  1-5

 

















                                                                              2
               ________________________________________________________________

                                Installing the APPC/LU6.2 Programming Interface




                  You install files on a VMS system through an automatic
                  question-and-answer session or dialog. You simply answer the
                  questions that are displayed as the procedure (VMSINSTAL)
                  runs. Most questions require a simple yes (Y) or no (N)
                  answer.

                  This manual supplies installation information in the
                  following format:

                  Default answers appear in brackets throughout the installa-
                  tion procedure. Press <Return> to accept a default answer.

                  Press <Ctrl/Y> to abort the installation procedure at any
                  time; later, you can restart the installation at 2 in the
                  dialog that follows.



















                           Installing the APPC/LU6.2 Programming Interface  2-1

 











               Username: SYSTEM   <Return>  1
               Password: password <Return>

               $ SET DEFAULT SYS$UPDATE <Return>

               $ @VMSINSTAL SNALU62022 ddcu:  [OPTIONS N] <Return>  2

                       VAX/VMS Software Product Installation Procedure V5.3

               It is dd-mmm-yyyy at hh:mm.

               Enter a question mark (?) at any time for help.

               %VMSINSTAL-W-ACTIVE, The following processes are still active:

                  JONES

               * Do you want to continue anyway [NO]?  3
               * Are you satisfied with the backup of your system disk [YES]?  4

               Please mount the first volume of the set on  MUA0:.
               * Are you ready? Y <Return> 5
               %MOUNT-I-MOUNTED, SNALU6 mounted on _MUA0:

























               2-2  Installing the APPC/LU6.2 Programming Interface

 





                   1 Digital Equipment Corporation recommends that you install
                     software from the system manager's account [SYSTEM] with
                     your default device and directory set to SYS$UPDATE.

                   2 VMSINSTAL prompts you if you do not supply the product and
                     device names. If you want to be prompted for the product
                     name, device name, and installation options, type the
                     following:

                       $ @SYS$UPDATE:VMSINSTAL <Return>

                     ddcu:
                     A device name where the distribution kit will be mounted
                     for the APPC/LU6.2 installation media, where dd is the
                     device, c is the controller, and u is the unit number.
                     MTA0: is the device name used in examples in this
                     document.

                     OPTIONS N
                     An optional parameter you should provide if you want to
                     be prompted to display or print the release notes. If you
                     do not include the OPTIONS N parameter, VMSINSTAL does
                     not prompt you to display or print the release notes,
                     but it does copy the release notes to SYS$HELP. VMSINSTAL
                     also permits the use of several other options. For more
                     information on options, see your processor-specific
                     installation/operations guide.

                   3 If users are logged in, you are asked whether you want to
                     continue the installation. To continue, type Y and press
                     <Return>. To stop the installation, press <Return>.

                   4 Before you proceed with the installation, make sure you
                     have a good backup copy. If you are satisfied with the
                     backup of your system disk, press <Return>. If you do not
                     have a good backup copy, type N and press <Return> to end
                     the installation.

                   5 Mount the distribution kit volume on the appropriate
                     drive. Type Y and press <Return> when you are ready.








	                Installing the APPC/LU6.2 Programming Interface 2-3

 



               The following products will be processed:

                   SNALU62 V2.2



                      Beginning installation of SNALU62 V2.2 at hh:mm


               %VMSINSTAL-I-RESTORE, Restoring product save set A...

               Release notes included with this kit are always copied to
	       SYS$HELP.

               Additional Release Notes Options:

                   1. Display release notes
                   2. Print release notes
                   3. Both 1 and 2
                   4. None of the above

               * Select option [2]:  6
               * Queue name [SYS$PRINT]:
               Job SNALU62022 (queue SYS$PRINT, entry 681) started on LPA0

               * Do you want to continue the installation? [NO] Y <Return> 7
               %VMSINSTAL-I-RELMOVED, The products release notes have been
	       successfully moved to SYS$HELP.

                       Product:      SNA-APPC-LU6.2
                       Producer:     DEC
                       Version:      V2.2
                       Release Date: 16-JUN-1990

               * Does this product have an authorization key registered and
	       loaded?Y <Return> 8
               * Do you want to purge files replaced by this installation
	       [YES]? <Return> 9






            2-4 Installing the APPC/LU6.2 Programming Interface

 











                   6 This step applies only if you specified OPTIONS N at 2.

                     If you select option 1, VMSINSTAL displays the release
                     notes. Press <Ctrl/C> to terminate the display.

                     If you select option 2, VMSINSTAL prompts you for a queue
                     name. Either type a queue name or press <Return> to send
                     the file to the default output print device.

                     If you select option 3, VMSINSTAL displays the release
                     notes and then prompts you for a queue name.

                     If you select option 4, VMSINSTAL does not display or
                     print the release notes.

                     Read the release notes carefully before continuing with
                     the VMSINSTAL procedure.

                   7 To continue the installation, type Y and press <Return>.
                     If you type N or press <Return>, VMSINSTAL moves the
                     release notes to SYS$HELP and ends the installation.

                   8 Use the VMS License Management Facility (LMF) to register
                     the product.

                     Check to see if this is the same information contained
                     in your Product Authorization Key (PAK). Type Y or N in
                     response to the question.

                     If you do not register and load your authorization key,
                     the product will not run. For more information on LMF,
                     refer to the VMS License Management Utility Reference
                     Manual.

                   9 If you answer Y to this prompt, VMSINSTAL deletes previous
                     versions of the distribution files.

                     Press <Return> after the following prompt if you want to
                     purge the files replaced during installation. If this is
                     your first APPC/LU6.2 software installation, type NO and
                     press <Return>.







            		Installing the APPC/LU6.2 Programming Interface 2-5

 











               * Do you want to run the IVP after the installation
	       [YES]? <Return> 10
               %SNALU62-I-NOQUEST, no further questions will be asked 11

                       To install the SNALU62SH.EXE and SNALU62MG.EXE images
		       as shareable each time the system reboots, you must add
		       the following line to your system startup procedure:

                               $ @SYS$STARTUP:SNALU62$STARTUP

                       On line release notes for this product can be found in
			       the file,
			       SYS$COMMON:[SYSHLP]SNALU62022.RELEASE_NOTES

               %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target
	       directories...

               ** DECnet/SNA VMS APPC/LU6.2 Programming Interface V2.2
		      Installation Test Beginning **

               .... Testing the APPC/LU6.2 Programming Interface V2.2

               ** DECnet/SNA VMS APPC/LU6.2 Programming Interface V2.2
		      Test Completed Successfully **
                       Installation of SNALU62 V2.2 completed at 14:50

                       VMSINSTAL procedure done at 14:50 12

               $ LOGOUT <Return> 13

               SYSTEM     logged out at dd-mmm-yyyy hh:mm




















            2-6 Installing the APPC/LU6.2 Programming Interface

 











                   10 The installation verification procedure (IVP) runs
                     tests to check whether the installation procedure was
                     successful. Press <Return> to run the IVP after the
                     installation. If you do not want to run the IVP, type
                     NO and press <Return>.

                     If you have not registered APPC/LU6.2 with LMF, the
                     following text appears:

                       ** DECnet/SNA VMS APPC/LU6.2 Programming Interface
                                     V2.2 Installation Test Beginning**

                       %LICENSE-F-NOAUTH, DEC SNA-APPC-LU6.2 use is not
                                     authorized on this node
                       -LICENSE-F-NOLICENSE, no license is active for this
                                     software product
                       -LICENSE-I-SYSMGR, please see your system manager
                       %Failed to test program with shareable image

                       ** DECnet/SNA VMS APPC/LU6.2 Programming Interface
                                     V2.2 Test FAILED **

                     Stop the installation and register APPC/LU6.2 with LMF as
                     described in step 8.

                   11 No more input is required. If you typed Y in response to
                     the prompt at 9, previous versions of the files are now
                     purged.

                     If the installation procedure is successful, the
                     executable files are moved to their target directory.

                   12 When the installation procedure is complete, VMSINSTAL
                     will finish and return you to the dollar sign ($) prompt.

                   13 VMSINSTAL deletes or changes entries in the process symbol
                     tables during the installation. Therefore, if you are
                     going to continue using the system manager's account and
                     want to restore those symbols, you should log out and log
                     in again.








            		Installing the APPC/LU6.2 Programming Interface 2-7

               Installed Files
                  VMSINSTAL installs the following files on your system:

                   _ SYS$SHARE:SNALU62SH.EXE

                          APPC/LU6.2 shareable image

                   _ SYS$MESSAGE:SNALU62MG.EXE

                          APPC/LU6.2 message file

                   _ SYS$LIBRARY:SNALU62DF.ADA

                          Symbol file for ADA

                   _ SYS$LIBRARY:SNALU62DF.BAS

                          Symbol file for BASIC

                   _ SYS$LIBRARY:SNALU62DF.FOR

                          Symbol file for FORTRAN

                   _ SYS$LIBRARY:SNALU62DF.H

                          Symbol file for C

                   _ SYS$LIBRARY:SNALU62DF.LIB

                          Library file

                   _ SYS$LIBRARY:SNALU62DF.MAR

                          Symbol file for MACRO

                   _ SYS$LIBRARY:SNALU62DF.PAS

                          Symbol file for Pascal

                   _ SYS$LIBRARY:SNALU62DF.PEN

                          Environment file for Pascal

                   _ SYS$LIBRARY:SNALU62DF.PLI

                          Symbol file for PLI

                   _ SYS$LIBRARY:SNALU62DF.R32

                          Symbol file for BLISS

                   _ SYS$STARTUP:SNALU62$STARTUP.COM

                          Startup command procedure

                   _ SYS$TEST:SNALU62$IVP.COM

                          Verification command procedure

                   _ SYS$HELP:SNALU62022.RELEASE_NOTES

                          Release notes
              2-8 Installing the APPC/LU6.2 Programming Interface

 

















                                                                              3
               ________________________________________________________________

                                                         After the Installation




                  This chapter describes some tasks to complete after you
                  install the Programming Interface software.

               Verifying the Installation

                  If you have chosen the IVP option, the IVP runs automatically
                  at the end of the installation. You can also run the IVP
                  after the installation to verify that the APPC/LU6.2
                  programming interface is installed and working properly.
                  To do so after the installation, type the following command
                  from your terminal:

                    $ @SYS$TEST:SNALU62$IVP.COM

                  The following message indicates that the software has been
                  successfully installed:

                    ** DECnet/SNA VMS APPC/LU6.2 Programming Interface V2.2
                                  Installation Test Beginning **

                    .... Testing the APPC/LU6.2 Programming Interface V2.2

                    ** DECnet/SNA VMS APPC/LU6.2 Programming Interface V2.2
                                  Test Completed Successfully **

               Note The IVP does not verify that the APPC/LU6.2 Programming
                  Interface can connect to an IBM system.

                  If the software was not installed properly, error messages
                  appear. Correct the problems indicated by the messages and
                  rerun the installation procedure. If you receive IVP errors,
                  you have a damaged kit; contact your Digital representative.


                                                    After the Installation  3-1

 











                  For information about configuring your IBM SNA software
                  components for logical unit (LU) type 6.2 communications,
                  see the VMS/SNA Guide to IBM Parameters.

                  If you have not registered APPC/LU6.2 with LMF, the following
                  text appears:

                    ** DECnet/SNA VMS APPC/LU6.2 Programming Interface V2.2
                                  Installation Test Beginning **

                    %LICENSE-F-NOAUTH, DEC SNA-APPC-LU6.2 use is not
                                  authorized on this node
                    -LICENSE-F-NOLICENSE, no license is active for this
                                  software product
                    -LICENSE-I-SYSMGR, please see your system manager
                    %Failed to test program with shareable image

                    ** DECnet/SNA VMS APPC/LU6.2 Programming Interface V2.2
                                  Test FAILED **

                  Stop the installation and register APPC/LU6.2 with LMF.

               Using the APPC/LU6.2 Software in a VAXcluster

                  After you have installed the APPC/LU6.2 software on one node
                  of a VAXcluster, you can install it on the other nodes by
                  executing the SNALU62$STARTUP.COM procedure on each node as
                  follows:

                    $@SYS$STARTUP:SNALU62$STARTUP.COM

                  You must activate an APPC/LU6.2 license for each node in the
                  VAXcluster that will execute and run the APPC/LU6.2 software.
                  You can activate the license in one of the following ways:

                   _ Log in to each VAXcluster node and enter the LICENSE LOAD

                     command.

                   _ Invoke the VMS SYSMAN Utility to execute the LICENSE

                     LOAD command on the desired VAXcluster nodes. See the
                     VMS SYSMAN Utility Manual for details on defining your
                     management environment, and executing commands on other
                     nodes.

                  For more information on the LICENSE LOAD command, refer to
                  the VMS License Management Utility Manual.

               3-2  After the Installation

 











               Installing the APPC/LU6.2 Programming Interface as a Shareable
               Image

                  SYS$STARTUP:SNALU62$STARTUP.COM contains the start-up command
                  procedure for the APPC/LU6.2 Programming Interface. To
                  install the APPC/LU6.2 Programming Interface as a shareable
                  image, execute the command procedure as follows:

                    $@SYS$STARTUP:SNALU62$STARTUP.COM

                  Include this command in your system start-up procedure to
                  automatically install the APPC/LU6.2 Programming Interface as
                  a shareable image when you boot the system.

               Adding the SNA_APPC HELP File to the HELP File of an Editor

                  You can insert the APPC/LU6.2 Programming Interface HELP
                  information (added to the HELPLIB file during installation)
                  into the HELP file of an editor, for programmers who use
                  editors to develop DECnet/SNA or VMS/SNA applications. You
                  need system manager privileges to perform this operation. Use
                  the following commands to insert the HELP information into
                  the HELP file of an editor:

                    $ LIBRARY/HELP/EXTRACT=SNA_APPC/OUTPUT=SNAAPPC -
                    _$ SYS$HELP:HELPLIB
                    $ LIBRARY/HELP/INSERT SYS$HELP:xxxHELP SNAAPPC
                    $ DELETE SNAAPPC.HLP;*

                  where xxx is the name of your editor, for example, EDT or
                  LSE.

















                                                    After the Installation  3-3

 




















               ___________________________________________________________


                                                                      Index



               B                               Gateway Management software

               Bill of Materials (BOM),           , 1-4
                  1-1                          Gateway-ST software, 1-4
                                               Global Pages requirement,
               C                                  1-4

               Configuring your IBM SNA        H

                  software components, 3-2     Help file installation, 3-3

               D                               I

               DECnet/SNA APPC/LU6.2           Image Sections requirement,
                  Programming Interface           1-4
                 defined, v, 1-1               Installation, preparing the
                 preparing for                    IBM environment for, 1-1
                    installation, 1-1          Installation problems, 3-1
               Disk space requirements for     Installation procedure, 2-1
                  installation, 1-3            Installation Verification
               Distribution kit, 1-1              Procedure (IVP), running

               G                                  during installation, 2-9

               Gateway-CT software, 1-4

                                                                    Index-1

 






          P                               V

          Preparing the IBM               VAXcluster use, 3-2
             environment for the          Verifying the installation,
             installation, 1-1               3-1
          Privileges                      VMS, installing a new

            See VMS system privileges        version of, 1-3
          Product Authorization Key       VMS, system requirement,
             registration and loading        1-3
             , 1-4                        VMSINSTAL utility

          S                                 running, 2-1

                                            specifying OPTIONS, 2-4
          Shareable image                 VMS system privileges, 1-3
             installation, 3-3























          Index-2
