


 

  
             DECnet/SNA VMS Remote Job Entry

             Installation

             AA-NF48A-TE


             This document describes how to install the
             DECnet/SNA VMS Remote Job Entry software.









             Revision/Update Information:  This is a new manual.

             Operating System and Version: VMS V5.0 or later
                                          

             Software Version:             DECnet/SNA VMS Remote Job
                                           Entry Version 1.4
                                           











             Digital Equipment Corporation

 





             ________________________
             June 1989

             __________
             The information in this document is subject to change without
             notice and should not be construed as a commitment by Digital
             Equipment Corporation. Digital Equipment Corporation assumes
             no responsibility for any errors that may appear in this
             document.

             The software described in this document is furnished under a
             license and may be used or copied only in accordance with the
             terms of such license.

             No responsibility is assumed for the use or reliability
             of software on equipment that is not supplied by Digital
             Equipment Corporation or its affiliated companies.

             __________
             Copyright © 1989 by Digital Equipment Corporation

             All Rights Reserved.
             Printed in U.S.A.

             __________
             The postpaid READER'S COMMENTS form on the last page of this
             document requests the user's critical evaluation to assist in
             preparing future documentation.

             The following are trademarks of Digital Equipment Corporation:

             DEC             DIBOL         UNIBUS
             DEC/CMS         EduSystem     VAX
             DEC/MMS         IAS           VAXcluster
             DECnet          MASSBUS       VMS
             DECsystem-10    PDP           VT
             DECSYSTEM-20    PDT
             DECUS           RSTS
             DECwriter       RSX           DIGITAL


             This document was prepared using VAX DOCUMENT, Version 1.1
                                                                      

 








                                                                  Contents
          ________________________________________________________________

                __________________________________________________________
                PREFACE                                                  v

          ________________________________________________________________
          CHAPTER 1  INSTALLATION                                      1-1


                1.1   RUNNING THE VMSINSTAL PROCEDURE                  1-3
                1.1.1     Logging In to the System Manager's
                          Account                                      1-4
                1.1.2     Making a Backup Copy of the System Disk      1-5
                1.1.3     Mounting the Distribution Kit Volume         1-6
                1.1.4     Confirming Your License                      1-7
                1.1.5     Purging the Distribution Files               1-8

                1.2   RUNNING THE INSTALLATION VERIFICATION
                      PROCEDURE                                        1-9


                1.3   LOCATING FILES AFTER INSTALLATION               1-12

                1.4   VERIFYING INSTALLATION OF THE RJE SOFTWARE      1-14


          ________________________________________________________________
          INDEX                                                    Index-1










                                                                       iii

 







          ________________________________________________________________
          TABLES

                1-1   Installation Specifications for VMS RJE
                      Software                                         1-1

                1-2   Location of RJE Files After Installation        1-13































          iv

 













                                                                   Preface
          ________________________________________________________________




          __________________________________________________________

          Objective of this Manual

             This manual provides the information you need to install the
             DECnet/SNA VMS Remote Job Entry access routine software.

          __________________________________________________________

          Intended Audience

             This manual assumes that you have user-level knowledge of the
             VMS operating system.

          __________________________________________________________

          Structure of this Manual

             This manual contains a brief explanation of how to install
             the DECnet/SNA VMS Remote Job Entry access routine software.

          __________________________________________________________

          Associated Documents

              o VMS/SNA Installation

              o VMS/SNA Management

              o VMS/SNA Problem Solving

              o DECnet/SNA VMS Remote Job Entry Problem Solving

                                                                         v

 






              o DECnet/SNA VMS Remote Job Entry Use

              o DECnet/SNA Gateway Installation Guide

              o DECnet/SNA Gateway Problem Determination Guide

              o DECnet/SNA Gateway Guide to IBM Parameters

              o Guide to DECnet/SNA VMS Gateway Management for DECSA

              o DECnet/SNA Gateway-ST Installation Guide

              o DECnet/SNA Gateway-ST Problem Determination Guide

              o DECnet/SNA Gateway-ST Guide to IBM Parameters

              o DECnet/SNA Gateway-CT Installation Guide

              o DECnet/SNA Gateway-CT Problem Determination Guide

              o DECnet/SNA Gateway-CT Guide to IBM Parameters

              o DECnet/SNA VMS Gateway Management Installation Guide

              o DECnet/SNA VMS Gateway Management Guide

              o VMS Network Control Program Manual

              o VMS Networking Manual

          __________________________________________________________

          Acronyms

             The following acronyms appear throughout this manual:

             DCL              Digital Command Language

             RJE              Remote Job Entry

             RJS              Remote Job Server

             SNA              IBM's Systems Network Architecture

             VMS              Virtual Memory System

          vi

 





          __________________________________________________________

          Graphic Conventions

             The following graphic conventions apply throughout this
             manual:

             _____________________________________________________________
             Convention          Meaning
             -------------------------------------------------------------

             $                   The dollar sign prompt precedes a command
                                 line for a VMS system.

             SNARJE>             The SNARJE angle bracket prompt indicates
                                 that you should use the SNARJE command
                                 language.

             monospaced type     Monospaced type indicates system input
                                 and output. System output is in black;
                                 user input is in red.

             Red type            Red type indicates user-entered commands
                                 or responses.

             UPPERCASE           Uppercase letters indicate that you must
                                 enter the characters exactly as shown.
                                 You can abbreviate command keywords to
                                 the first unique characters.

             lowercase italics   Lowercase italic type indicates variables
                                 in command lines. You must specify these
                                 variables.

             <RETURN>            This symbol indicates the RETURN key on
                                 the keyboard. Unless otherwise specified,
                                 terminate every command line by pressing
                                 the RETURN key.



                                                                       vii

 





             _____________________________________________________________
             Convention          Meaning
             -------------------------------------------------------------
         
             <CONTROL/x>         This symbol indicates a control charac-
                                 ter; x is an alphabetic character. Press
                                 the CONTROL key and the alphabetic key
                                 simultaneously.

             dd-mmm-yyyy         This is the required VMS format for spec-
                                 ifying a date, as in 21-Apr-1989. See the
                                 DCL Dictionary for further information.

             hh:mm:ss[.cc]       This is the required VMS format for
                                 specifying a time, as in 09:44:23.49.
                                 [.cc] represents hundredths of a second.
                                 These often appear in system messages,
                                 but you need not supply them when you are
                                 specifying a time. See the DCL Dictionary
                                 for further information.
             --------------------------------------------------------------
             All numbers are decimal unless otherwise noted.


















          viii

 











                                                                 Chapter 1


                                                              Installation
          ________________________________________________________________


             This manual refers to the base communications software as
             the "Gateway." Unless otherwise stated, the term "Gateway"
             applies to any or all of the following:

              o VMS/SNA

              o DECnet/SNA Gateway

              o DECnet/SNA Gateway-CT

              o DECnet/SNA Gateway-ST

             Before you begin to install the DECnet/SNA VMS Remote Job
             Entry software, you need to know what software, system priv-
             ileges, and disk space are required for your installation.
             The following table lists the preliminary requirements for
             installing the RJE software.

             Table 1-1:  Installation Specifications for VMS RJE Software
             ------------------------------------------------------------

             Software    VMS V5.0 or 5.1

             Privileges  System manager level

             Disk space  2200 blocks minimum during installation
                         1000 blocks minimum after installation

                                                         Installation  1-1

 






             Table 1-1 (Cont.):  Installation Specifications for VMS RJE
                                 Software
             -------------------------------------------------------------

             Approximate         6 to 30 minutes, depending on the 
             time                distribution media
             required for
             installation

             Associated          The VMS software installation guide for
             documents           your particular processor (contains general
                                 installation information.
             _____________________________________________________________
























          1-2  Installation

 






             In addition, the following VMS classes are required for full
             functionality of DECnet/SNA VMS Remote Job Entry:

              o VMS Required Saveset

              o Network Support

              o Secure User's Environment

             The installation process consists of five major tasks. You
             must complete each installation task before you begin the
             next task.

             1. Ensure that you have adequate disk space before you begin
                to install RJE.

             2. Check to make sure that you have a complete distribution
                kit. Each RJE distribution kit consists of one or more
                volume(s) of software and a set of documentation.

             3. Log in to the system manager's account, and execute the
                VMSINSTAL installation procedure.

             4. After you exit from the VMSINSTAL procedure, locate the
                RJE files on your system.

             5. Verify the successful installation of the RJE software.

          __________________________________________________________

          1.1  Running the VMSINSTAL Procedure

             The VMSINSTAL procedure allows you to install files onto your
             VMS system from the distribution kit. VMSINSTAL is automated
             and requires little input from you beyond responding to
             prompts displayed on your screen. Most of the prompts require
             only a YES (Y) or NO (N) response. Default answers to prompts
             are displayed within brackets, as shown in the following
             example:

                 [YES]:

             To select the default answer, press <RETURN>.

                                                         Installation  1-3

 





          __________________________________________________________

          1.1.1  Logging In to the System Manager's Account

             To begin the VMSINSTAL procedure you must log in to the
             system manager's account and enter a command, as in the
             following example, to install the distribution kit on your
             VMS host:

                 $ @SYS$UPDATE:VMSINSTAL SNARJE dduu:

             where

              o dduu: identifies the device on which the distribution kit
                is mounted.

              o SNARJE is the name of the distribution kit for the
                DECnet/SNA VMS RJE software.

             The VMSINSTAL sample shown in this manual describes a simple
             installation. Your installation might include additional
             prompts, depending on your configuration and whether you have
             other products already installed. For a full description of
             the VMSINSTAL procedure, refer to the VMS System Manager's
             Manual.

             After you log in to the system manager's account and load the
             volume(s) from your distribution kit, VMSINSTAL displays the
             following text:

                         VMS Software Product Installation Procedure

                 It is dd-mmm-yyyy at hh:mm.
                 Enter a question mark (?) at any time for help.
                 %VMSINSTAL-W-DECNET, Your DECnet network is up and running.

             Next, VMSINSTAL shows you the status of your current active
             processes and asks you if you want to continue with the
             installation.

          1-4  Installation

 






             %VMSINSTAL-W-ACTIVE, The following processes are still active:
                SMISERVER
              BATCH_601
              SERVER_002C
              _RTA3:
             * Do you want to continue anyway [NO]?

             If you continue with the installation procedure, the active
             processes might be affected, depending upon the utilities
             these processes are using. If you answer with the default
             NO, VMSINSTAL terminates. A YES answer causes VMSINSTAL to
             continue.

          __________________________________________________________

          1.1.2  Making a Backup Copy of the System Disk

             The VMSINSTAL procedure then prompts you as follows:

                * Are you satisfied with the backup of your system disk [YES]?

             Make sure that you have a backup copy of your system disk
             before you proceed with an installation that writes to your
             system disk. Having a backup copy is important because your
             disk could be corrupted during installation.

             If you do not have a backup copy of your system disk, en-
             ter N, and VMSINSTAL stops to allow you to create one. For
             instructions on how to back up a system disk, see the VMS
             Backup Utility Manual. After you have created a backup copy,
             start the VMSINSTAL procedure again. If you already have a
             backup copy of your system disk, press <RETURN> to continue
             the installation without interruption.






                                                         Installation  1-5

 





          __________________________________________________________

          1.1.3  Mounting the Distribution Kit Volume

             Next, VMSINSTAL tells you to mount the distribution kit
             volume on the the device you specified when you began the
             procedure. It then asks if you are ready to continue with the
             installation, as follows:

                 Please mount the first volume of the set on dduu
                 * Are you ready?

                                          NOTE

                 VMSINSTAL is a universal installation procedure, and
                 you can use it to install products with more than
                 one volume in the distribution kit. When you are in-
                 stalling a product that contains only one volume in
                 the kit, like RJE, the procedure still asks you to
                 mount "the first volume" but does not prompt you to
                 mount any additional volumes.

             After you have mounted the distribution kit volume, answer
             YES to the question * Are you ready?. VMSINSTAL responds with
             a message verifying that you mounted the volume correctly and
             the installation is continuing, as follows:

               %MOUNT-I-MOUNTED, SNARJE mounted on dduu:
                 The following products will be processed:

                   SNARJE V1.4

                    Beginning installation of SNARJE V1.4 at hh:mm

                 %VMSINSTAL-I-RESTORE, Restoring product saveset A ...
                 %VMSINSTAL-I-RELMOVED , The product's release notes have been
                 successfully moved to SYS$HELP.



          1-6  Installation

 





          __________________________________________________________

          1.1.4  Confirming Your License

             During the installation of the RJE software, the VMSINSTAL
             procedure asks you to confirm that you registered your
             Product Authorization Key (PAK) and are licensed to run RJE.

                         Product:      SNA-RJE

                         Producer:     DEC

                         Version:      V1.4

                         Release Date: dd-mmm-yyyy

           * Does this product have an authorization key registered and loaded?

             If you answer YES, VMSINSTAL continues with the installation.

             If you answer NO, VMSINSTAL displays the following message:

                     DECnet/SNA Remote Job Entry requires you to register your
                     Product Authorization Key (PAK).  You should have received
                     the PAK with your kit.

                     Register your PAK with...

                  $ @sys$update:vmslicense

                     after the installation completes.  The product will not
                     function until this is done.

             As the example indicates, if you have not registered your
             PAK, the installation will complete successfully, but you
             will not be able to run RJE. You can use the product only
             after registering your PAK.



                                                         Installation  1-7

 





          __________________________________________________________

          1.1.5  Purging the Distribution Files

             This installation creates new distribution files on your
             system. The VMSINSTAL procedure next asks if you want to
             delete the existing versions (if any) of these files that are
             superseded by the new files.

              * Do you want to purge files replaced by this installation [YES]?

             If this is your first RJE software installation, you will
             have no files to purge. Type NO and press <RETURN>. To delete
             the old files, answer with the default YES; VMSINSTAL auto-
             matically deletes the old files.

             At this point, VMSINSTAL describes the Installation
             Verification Procedure (IVP). The system message appears
             as follows:

                   You can verify the SNA-RJE installation using the IVP.  This
                   is recommended, and will help ensure that the installation has
                   completed correctly by:

                   o  Removing or renaming the V1.3 files, only if they exist.
                   o  Stopping the V1.3 processes, only if they exist.
                   o  Verifying the existence of the V1.4 files.
                   o  Initializing the V1.4 processes.
                   o  Verifying inter-process communication.

                   Once the installation is complete, you can execute the IVP
                   by using the command:

                       $ @sys$test:snarje$ivp.com

               NOTE:  Do NOT execute the IVP unless you have a PAK registered
                      for SNA-RJE V1.4.  The IVP will not complete successfully
                      due to the RJE components failing their license check.


          1-8  Installation

 






             Then the installation completes, and the following messages
             appear:

                       All installation questions have been asked.  No more
                       input from the terminal will be required.

               Your DECnet/SNA VMS RJE V1.4 installation is nearing completion.
               Remember to use..

                       $ @sys$startup:snarje$startup

                   to start the detached processes.

  %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...
   Installation of SNARJE V1.4 completed at hh:mm

             The procedure then prompts you for the next product you wish
             to install. If you have another product to install, enter
             the product name and respond to the prompts as they appear.
             Consult the installation manual for that product for further
             information. If you have no further products to install,
             press <RETURN>, and VMSINSTAL terminates with a confirmation
             message as follows:

     Enter the products to be processed from the next distribution volume set.
     * Products: <RETURN>
      VMSINSTAL procedure done at hh:mm

        __________________________________________________________

        1.2  Running the Installation Verification Procedure

             To run the Installation Verification Procedure (IVP), enter
             the following command at the DCL prompt:

                 @SYS$TEST:SNARJE$IVP.COM



                                                         Installation  1-9

 






             The following message appears:

                        Starting RJE Installation Verification Procedure (IVP)

           This procedure will first check for the existence of V1.3 processes
           and files.  This will take a moment.

             If the IVP finds files from Version 1.3 of RJE in your system
             directories, the procedure informs you that it has found
             these files. It then asks if you want to delete them.

      You currently have DECnet/SNA VMS Remote Job Entry V1.3 files in your
      system directories.  The naming convention for V1.4 has been updated, and
      the older files should either be DELETED, or RENAMED.

          * Delete the outdated files [Y/N]:

      To delete the outdated files, answer YES. VMSINSTAL deletes
      the files and sends you confirming messages, as in the fol-
      lowing example:

        The following outdated files are being DELETED.
        %DELETE-I-FILDEL, SYS$COMMON:[SYSEXE]SNAREADER.EXE;7 deleted (60 blocks)

      To keep the outdated files, answer NO. The outdated files
      will appear in the system directories with the designation
      "_V13" appended to the file name.

      Next, VMSINSTAL begins to initialize the RJE Version 1.4
      processes, as in the following example:

               Now the V1.4 processes will be initialized, using

                     @sys$startup:snarje$startup.com

         Creating detached process - SNARJE$MPX
         %RUN-S-PROC_ID, identification of created process is 24600957

         Creating detached process - SNARJE$SERVER
         %RUN-S-PROC_ID, identification of created process is 24600958

          1-10  Installation

 






               The process initialization may take a few moments.  The IVP
               will wait until both processes are fully declared, and will
               then proceed.

      When initialization of the Version 1.4 process is complete,
      the IVP creates a workstation and automatically executes
      a series of RJE commands to verify that RJE is correctly
      installed. The following is an example of normal IVP output:

               A workstation will now be created and some very basic
               tests will be performed.  This workstation will make use
               of the VMS based RJE Server.

       SNARJE> show workstation
          Workstations on  12-APR-1989 17:24:31.32
               Current IVP_TEST

       SNARJE> assign [] pr1
       SNARJE> assign snarje$reader rd1
       SNARJE> show status
         Status of workstation IVP_TEST on 12-APR-1989 17:24:43.95
           Server node:   MOUSSY    State:        OFF
           Access name:   IVP_A     Application:
           Circuit:                 Logon mode:
           Stream PR1  (Translate)
                       Assigned:  _MOUSSY::VMI$ROOT:[SYSUPD.SNARJE014]
                       Current:   none
           Stream RD1
                       Queue:     SNARJE$READER
                       Current:   none
       SNARJE> show counters
           Counters for workstation IVP_TEST on 12-APR-1989 17:24:51.19
                    24  Seconds since last zeroed
                     0  Maximum active files
                     0  Resource errors
                     0  Records read
                     0  Records written
                     0  Files accessed
                     0  File open errors

                                                        Installation  1-11

 






                    0  File read errors
                    0  File write errors
                    0  File close errors
                    0  Stream aborts
                    0  SNA protocol errors
            Stream PR1
                    0  Records written
                    0  Records written (active file)
                    0  Files accessed
                    0  File open errors
                    0  File write errors
                    0  File close errors
                    0  Stream aborts
                    0  SNA protocol errors
            Stream RD1
                    0  Records read
                    0  Records read (active file)
                    0  Files accessed
                    0  File open errors
                    0  File read errors
                    0  File close errors
                    0  Stream aborts
                    0  SNA protocol errors
         SNA RJE workstation IVP_TEST terminated on 12-APR-1989 17:24:58.48

                The SNARJE$IVP has completed successfully.  This IVP has
                tested out connections to the MPX and SERVER, but to ensure
                the correctness of the RJE system, please see DECnet/SNA
                VMS Remote Job Entry Installation and SUBMIT/SNA a test JCL.

          __________________________________________________________

       1.3  Locating Files After Installation

          After you run the VMSINSTAL procedure, you can find the RJE
          files in the following locations on your system:



          1-12  Installation

 







          --------------------------------------------------------------
          Table_1-2:  Location of RJE Files After Installation
          --------------------------------------------------------------
          File Name             Location      Description
          --------------------------------------------------------------
          SNARJE.EXE            SYS$SYSTEM    RJE operator utility

          SNARJE$MPX.EXE        SYS$SYSTEM    RJE control program

          SNARJE$SERVER.EXE     SYS$SYSTEM    RJE server

          SNARJE$RDR.EXE        SYS$SYSTEM    RJE reader stream processor

          SNASUBMIT.EXE         SYS$SYSTEM    RJE submit command processor

          SNARJE$RJEMSG.EXE     SYS$MESSAGE   RJE message file

          SNARJE$RJSMSG.EXE     SYS$MESSAGE   RJS message file

          SNARJE.HLB            SYS$HELP      RJE HELP library

          SNARJE$STARTUP.COM    SYS$STARTUP   RJE initialization command
                                              procedure

          SNARJE014.RELEASE_    SYS$HELP      RJE release notes
          NOTES

          SNARJE$MPX.COM        SYS$STARTUP   called in by SNARJE$STARTUP.COM

          SNARJE$SERVER.COM     SYS$STARTUP   called in by SNARJE$STARTUP.COM

          SNARJE$RJESYMBOL.COM  SYS$LIBRARY   RJE error symbols

          SNARJE$RJSSYMBOL.COM  SYS$LIBRARY   RJS error symbols




                                                        Installation  1-13

 





     
          Table_1-2_(Cont.):  Location of RJE Files After Installation

          ----------------------------------------------------------------
          File_Name             Location      Description
          ----------------------------------------------------------------
          SNARJE$IVP.COM        SYS$TEST      RJE installation verifica-
                                              tion procedure
          ----------------------------------------------------------------


             When you install RJE, VMSINSTAL automatically creates an
             RJE server, SNARJE$SERVER.EXE., on your VMS system. If your
             Gateway resources are limited because your Gateway is sup-
             porting multiple tasks, you can try to increase throughput by
             running RJE through the RJE server on your VMS system.


                                          NOTE

                 HELP information for the DECnet/SNA RJE has been added
                 to the SYS$HELP:HELPLIB.HLB library.

          __________________________________________________________

          1.4  Verifying Installation of the RJE Software

             After you have installed the DECnet/SNA VMS RJE software, you
             should verify that it can communicate with the appropriate
             IBM application subsystem. You should be able to verify
             communication provided the following conditions exist:

              o All other components in your configuration are properly
                installed.

              o You have a link from your system to the IBM host.

             This section provides sample procedures for accessing an
             IBM Job Entry Subsystem by using two commonly available
             IBM utilities: JES2 and JES3. If you need more information
             about any command variables used in the following samples,
             see DECnet/SNA VMS Remote Job Entry Use. To verify that you

          1-14  Installation

 






             have successfully installed the DECnet/SNA VMS RJE software,
             complete the following steps:

             1. Run the SNARJE$STARTUP.COM file.

             2. Verify that the RJE software is installed on your system
                and that all other necessary components are installed and
                running.

             3. Set up your terminal by entering the following VMS com-
                mand:

                    $ SET TERMINAL/BROADCAST

             4. Enter the following commands to invoke RJE and to identify
                the workstation:

                    $ RUN SYS$SYSTEM:SNARJE
                    SNARJE> USE workstation-name

                where workstation-name is a one- to eight-character name
                you assign to the workstation you are creating.

             5. Configure or set up the workstation using the following
                sequence of commands:

                    SNARJE> SET WORKSTATION/GATEWAY=gateway-node-name
                    SNARJE> SET WORKSTATION/ACCESS=access-name/DATA=logon-data
                    SNARJE> SET MONITOR

             6. Assign the default queue SNARJE$READER to the reader
                stream:

                    SNARJE> ASSIGN SNARJE$READER RD1

             7. Configure a print stream:

                    SNARJE> ASSIGN disk:[directory] PR1

             8. Set the workstation ON:

                    SNARJE> SET WORKSTATION/STATE=ON

                                                        Installation  1-15

 






                Setting the workstation ON enables messages from the IBM
                host to be displayed on your screen.

             9. Enter interactive console mode:

                    SNARJE> SET CONSOLE

             10. TypeIBM RJE console commands to send data to your ter-
                 minal. For example, for JES2 type the following command:

                    $DU,JES workstation

                where JES workstation is a valid JES workstation designa-
                tion.

                For JES3, type the following command:

                    I,Q,N=ALL

                These commands cause JES2 or JES3 to display data on your
                screen.

             11. Press<CTRL/Z> to return to SNARJE. Then type EXIT to
                 return to DCL.

             At this point your RJE software is installed correctly.













          1-16  Installation

 












                                                                Index
          __________________________________________________________

          ___________________________
          A                              Default queue,  1-15
          ___________________________    Deleting old files,  1-8
          Active processes,  1-4         Digital Command Language,
          ASSIGN command,  1-15             vi
          Authorization to run RJE,      Displaying data,  1-16
             1-7                         Distribution files,  1-8
          ___________________________      purging,  1-8
          B                              Distribution kit
          ___________________________      installing,  1-4
          Backing up system disk,        Distribution kit volume,
             1-5                            1-6
          ___________________________    ___________________________
          C                              E
          ___________________________    ___________________________
          Configuring a workstation,     Exiting from RJE,  1-16
             1-15                        ___________________________
          Console                        G
            commands,  1-16              ___________________________
            mode,  1-16                  Gateway,  1-1
          ___________________________      -CT,  1-1
          D                                DECnet/SNA,  1-1
          ___________________________      -ST,  1-1
          DCL,  vi                       ___________________________
          DCL commands                   H
            RUN SYS$SYSTEM:SNARJE,       ___________________________
               1-15                      HELP information,  1-14
            SET TERMINAL/BROADCAST,
               1-15
          DECnet/SNA Gateway,  1-1
          DECnet/SNA Gateway-CT,  1-1
          DECnet/SNA Gateway-ST,  1-1
          Default answers,  1-3

                                                              Index-1

 






          ___________________________    ___________________________
          I                              R
          ___________________________    ___________________________
          Initialization of process,     Reader stream,  1-15
             1-11                        Remote Job Entry,  vi
          Installation                   Remote Job Server,  vi
            process,  1-3                RJE,  vi
            requirements,  1-1           RJE commands
            verifying,  1-14               ASSIGN,  1-15
          Installing other products,       SET CONSOLE,  1-16
             1-9                           SET MONITOR,  1-15
          Interactive mode,  1-16          SET WORKSTATION/ACCESS,
          ___________________________        1-15
          J                                SET WORKSTATION/GATEWAY,
          ___________________________        1-15
          JES2,  1-15                      SET WORKSTATION/STATE=ON,
          JES3,  1-15                        1-15
          ___________________________      USE,  1-15
          L                              RJE files,  1-12
          ___________________________    RJE server on VMS system,
          License,  1-7                     1-14
          Link,  1-14                    RJS,  vi
          Locating RJE files,  1-12      RUN SYS$SYSTEM:SNARJE
          ___________________________
          M                                 command,  1-15
          ___________________________    ___________________________
          Mounting distribution kit      S
             volume,  1-6                ___________________________
          ___________________________    SET CONSOLE command,  1-16
          P                              SET MONITOR command,  1-15
          ___________________________    SET TERMINAL/BROADCAST
          PAK,  1-7                         command,  1-15
          Print stream,  1-15            SET WORKSTATION/ACCESS
          Process initialization,           command,  1-15
             1-11                        SET WORKSTATION/GATEWAY
          Product Authorization Key,        command,  1-15
             1-7                         SET WORKSTATION/STATE=ON
          Purging distribution files,       command,  1-15
             1-8                         SNA,  vi
          Purging files,  1-8            System disk backup,  1-5

                                         System manager
                                           account,  1-4
                                           privileges,  1-1

          2-Index

 






          Systems Network                Virtual Memory System,  vi
             Architecture,  vi           VMS,  vi
          ___________________________    VMS/SNA,  1-1
          U                              VMSINSTAL,  1-3
          ___________________________      sample text,  1-4
          USE command,  1-15             ___________________________
          ___________________________    W
          V                              ___________________________
          ___________________________    Workstation,  1-11
          Verifying installation,          configuring,  1-15
             1-14                          setting ON,  1-15




























                                                              Index-3
