VAX Software Performance Monitor, Version 3.4			SSA 27.56.09-A

HARDWARE REQUIREMENTS 

Processors Supported

VAX:	 VAX 6000 Model 200 Series, VAX 6000 Model 300 Series, VAX 6000 
         Model 400 Series

	 VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500, VAX 8530, VAX 
         8550, VAX 8600, VAX 8650, VAX 8700, VAX 8800, VAX 8810, VAX 8820, 
         VAX 8830, VAX 8840, VAX 8842, VAX 8974, VAX 8978

	 VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785 

MicroVAX:	   MicroVAX II,   MicroVAX 2000, MicroVAX 3100, MicroVAX 
                   3300, MicroVAX 3400, MicroVAX 3500, MicroVAX 3600, 
                   MicroVAX 3800, MicroVAX 3900

VAXstation:	   VAXstation II,   VAXstation 2000, VAXstation 3100 Series,
                   VAXstation 3200, VAXstation 3500, VAXstation 3520, 
                   VAXstation 3540

VAXserver:	   VAXserver 3100, VAXserver 3300, VAXserver 3400, 
                   VAXserver 3500, VAXserver 3600, VAXserver 3602, 
                   VAXserver 3800, VAXserver 3900, VAXserver 6000-210, 
                   VAXserver 6000-310, VAXserver 6000-410, VAXserver 
                   6000-420

Processors Not Supported

		   VAXstation I, VAXstation 8000, MicroVAX I, VAX 11/725, 
                   VAX 11/782

Processor Restrictions

MicroVAX 2000 and VAXstation 2000 systems require a TK50 drive for software 
distribution and updates.

Other Hardware Requirements

A minimum system configuration includes:

oo   2MB of physical memory for a single node and 4MB of physical memory for 
    a VAXcluster

oo   Console terminal

oo   10,000 pages of page file quota

oo   250 pages of working set quota (1,000 pages for cluster reporting)

Block Space Requirements (Block Cluster Size = 1):

Full VAX SPM Facility including the Collector:

Disk space required for installation:
						      18,000 blocks
						      (9.2M bytes)

Disk space required for use (permanent):

						      11,000 blocks
						      (7.0M bytes)

For VAX SPM Collector:

Disk space required for installation:
						      5,000 blocks
						      (2.6M bytes)

Disk space required for use (permanent):

						      2,000 blocks
						      (1.0M bytes)

These counts refer to the disk space required on the system disk.  The 
sizes are approximate; actual sizes may vary depending on the user's system 
environment, configuration and software options.

OPTIONAL HARDWARE

Some of the advanced video displays require a VT125, VT240, VT241, VT340, 
VT341 or PRO 350 terminal.  The PRO 350 terminal must be equipped with a 
VC241-A extended bit map graphic option and the PRO/Communications Software 
Package.

CLUSTER ENVIRONMENT 

This layered product is fully supported when installed on any valid   and 
licensed VAXcluster* configuration without restrictions. The HARDWARE 
REQUIREMENTS sections of this product's Software Product Description and 
System Support Addendum detail any special hardware required by this 
product.

*   V5.x VAXcluster configurations are fully described in the VAXcluster 
    Software Product Description (29.78.xx) and include CI, Ethernet and 
    Mixed Interconnect configurations.


SOFTWARE REQUIREMENTS 

VMS Operating System Version 5.0 - 5.3

Prerequisite for Collector Licensing

At least one Full Function VAX SPM License is required in a multi-CPU or 
VAXcluster environment

VMS Tailoring

For VMS V5.x, the following VMS classes are required for full functionality 
of this layered product:

oo   VMS Required Saveset

oo   Network Support

oo   Programming Support

oo   System Programming Support

oo   Secure User's Environment

oo   Utilities

For more information on VMS classes and tailoring, refer to the VMS 
Operating System Software Product Description (SPD 25.01.xx).

OPTIONAL SOFTWARE

None

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of this 
product may be different from the minimum requirements for the current 
version.

DISTRIBUTION MEDIA

Tape:	 9-track 1600 BPI Magtape, TK50 Streaming Tape 

This product is also available as part of the VMS Consolidated Software 
Distribution on CDROM.

ORDERING INFORMATION 

Full VAX SPM Facility

Software Licenses: QL-850A*-**
Software Media: QA-850A*-**
Software Documentation: QA-850AA-GZ
Software Product Services: QT-850A*-**

VAX SPM Collector Facility

Software Licenses: QL-VUPA*-**
Software Media: QA-VUPA*-**
Software Documentation: QA-VUPAA-GZ
Software Product Services: QT-VUPA*-**

*   Denotes variant fields. For additional information on available 
    licenses, services and media, refer to the appropriate price book.

The above information is valid at time of release. Please contact your 
local Digital office for the most up-to-date information.


(R)  The DIGITAL Logo is a registered trademark of Digital Equipment 
     Corporation.
(TM) MicroVAX, PRO, VAX, VAX SPM, VAXstation, VAXserver, VMS, and VT are 
     trademarks of Digital Equipment Corporation.


