 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  VAX Disk Striping Driver for VMS, Version 2.0 SSA
     31.66.01-A

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:        VAXft 3000-310

                 VAX 4000 Model 200,
                 VAX 4000 Model 300

                 VAX 6000 Model 200 Series,
                 VAX 6000 Model 300 Series,
                 VAX 6000 Model 400 Series,
                 VAX 6000 Model 500 Series

                 VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500,
                 VAX 8530, VAX 8550, VAX 8600, VAX 8650, VAX 8700,
                 VAX 8800, VAX 8810, VAX 8820, VAX 8830, VAX 8840

                 VAX 9000-210, VAX 9000 Model 400 Series

                 VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX:   MicroVAX II, MicroVAX 2000,
                 MicroVAX 3100, MicroVAX 3300,
                 MicroVAX 3400, MicroVAX 3500,
                 MicroVAX 3600, MicroVAX 3800,
                 MicroVAX 3900


                                  DIGITAL                  April 1991

                                                          AE-NZ30B-TE

 


     VAX Disk Striping Driver for VMS, Version 2.0     SSA 31.66.01-A




     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100 Series, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540

     VAXserver:  VAXserver 3100, VAXserver 3300, VAXserver 3400,
                 VAXserver 3500, VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900

                 VAXserver 4000 Model 300

                 VAXserver 6000-210, VAXserver 6000-220, VAXserver
                 6000-310, VAXserver 6000-320, VAXserver 6000-410,
                 VAXserver 6000-420, VAXserver 6000-510, VAXserver
                 6000-520

     Processors Not Supported

     MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXstation
     8000

     Disk Space Requirements (Block Cluster Size = 1):

     Disk space required for      2,500 blocks
     installation:
                                  (1.3 Mbytes)

     Disk space required for      1,500 blocks
     use (permanent):
                                  (0.8 Mbytes)

     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.



                                     2

 


     VAX Disk Striping Driver for VMS, Version 2.0     SSA 31.66.01-A



     OPTIONAL HARDWARE

     The following disk drives and controllers are supported up
     to the maximum supported by VMS and the specific processor
     configuration:

     Disk Drives

     RA-series, RF-series, RZ-series

     Electronic Storage Element

     ESE20 drives

     Controllers

     HSC controllers, KDA50, KDB50, KDM70, KFMSA, KFQSA, RQDX3, UDA50

     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet, and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     For Systems Using Terminals (No DECwindows Interface):

     VMS Operating System V5.2 - V5.4, standalone,
        VAXcluster support with MSCP-served nodes
     VMS Operating System V5.4, for full VAXcluster support

     VMS Tailoring

                                     3

 


     VAX Disk Striping Driver for VMS, Version 2.0     SSA 31.66.01-A



     For VMS V5.x systems, the following VMS class is required for
     full functionality of this layered product:

     VMS Required Saveset

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     OPTIONAL SOFTWARE

     None

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the requirements for
     the current version.

     DISTRIBUTION MEDIA

     TK50 Streaming Tape, 1600 BPI Magnetic Tape

     This product is also available as part of the VMS Consolidated
     Software Distribution on CDROM.

     ORDERING INFORMATION

     Software Licenses: QL-YELA*-**
     Software Media: QA-YELA9-**
     Software Documentation: QA-YELAA-GZ
     Software Product Services: QT-YELA*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services, and media, refer to the appropriate
        price book.



                                     4

 


     VAX Disk Striping Driver for VMS, Version 2.0     SSA 31.66.01-A



     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [TM] The DIGITAL Logo, DECwindows, MicroVAX, VAX, VAXcluster,
          VAXft, VAXserver, VAXstation, and VMS are trademarks of
          Digital Equipment Corporation.
































                                     5
