












                       SYSTEM SUPPORT ADDENDUM



PRODUCT NAME:  VAX TEAMDATA/DANSK Version 1.3
SSA 25.G4.00-A
January 1989
BH-MS97A-TE



HARDWARE REQUIREMENTS

Processor Support


VAX: VAX 6210, VAX 6220, VAX 6230, VAX 6240, VAX 8200, VAX 8250, 
     VAX 8300, VAX 8350, VAX 8500, VAX 8530, VAX 8550, VAX 8600, VAX
     8650, VAX 8700, VAX 8800, VAX 8810, VAX 8820, VAX 8830, VAX 8840,
     VAX 8842, VAX 8974, VAX 8978

     VAX-11/750, VAX-11/780, VAX-11/785, VAX-11/782

MicroVAX:   MicroVAX II, MicroVAX 2000, MicroVAX 3300, MicroVAX 3400, 
            MicroVAX 3500, MicroVAX 3600

VAXstation: VAXstation II, VAXstation 2000, VAXstation 3200, 
            VAXstation 3500, VAXstation 8000

VAXserver:  VAXserver 3300, VAXserver 3400, VAXserver 3500, 
            VAXserver 3600, VAXserver 3602, VAXserver 6210, 
            VAXserver 6220

Not supported:  VAX-11/725, VAX-11/730, MicroVAX I, VAXstation I



Processor Restrictions

The VAX-11/782 processor is not supported by VMS Operating System V5.0
or later.



                                - 1 -

SYSTEM SUPPORT ADDENDUM


A minimum of four megabytes of memory.  Typical configurations will
require more than four megabytes of memory.

Mass storage with a minimum of 13.000 disk blocks for VAX TEAMDATA
system software and sufficient space for database storage areas.

For MicroVAX and VAXstation Systems:

     TK50 tape drive for installation of the software 

For all other VAX Systems:

     One 9-track 1600 BPI magnetic tape unit for installation of the
     software   



Terminals

VAX TEAMDATA may be run on VT220, VT240/241, or VT320/330/340
terminals.

Graphics can be displayed on VT240/241, or VT330/340 terminals.



Printers

VAX TEAMDATA reports can be printed on any DIGITAL text printer.

Graphics can be printed on DIGITAL devices which support either the
SIXEL (e.g, LN03, LA75) or ReGIS (e.g., LCP01) protocols.



Block Space Requirements (Block Cluster Size =1):


Disk space required for installation: 13,000 blocks (6.5 Mbytes)

Disk space required for use (permanent): 11,000 blocks (5.5 Mbytes)

These counts refer to the disk space required on the system disk.  The
sizes are approximations; actual sizes may vary depending on the
users' system environment, configuration and software options
selected.



CLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid


                                - 2 -

SYSTEM SUPPORT ADDENDUM


and licensed VAXcluster* configuration without restrictions.  The
HARDWARE REQUIREMENTS sections of this product's Software Product
Description and System Support Addendum detail any special hardware
required by this product.

* V5.x VAXcluster configurations are fully described in the VAXcluster
Software Product Description (29.78.xx) and include CI, Ethernet and
Mixed Interconnect configurations.



SOFTWARE REQUIREMENTS

Operating System

VMS Operating System V4.7 - V5.0

MicroVMS Operating System V4.7



Layered Products:

VAX Rdb/VMS V2.2 - V3.0 (Run-Time, Development or Interactive Option)

VMS Workstation Software V3.0 - V4.0



VMS Tailoring

For VMS V5.x systems, the following VMS classes are required for full
functionality of this layered product:

      o  Required Save Set

      o  Network Support

      o  Programming Support

      o  Secure Users Environment


For more information on VMS classes and tailoring, refer to the VMS
Operating System Software Product Description (SPD 25.01.xx).



MicroVMS Tailoring

For MicroVMS V4.x systems, the following components of MicroVMS are
required for full functionality of this layered product:


                                - 3 -

SYSTEM SUPPORT ADDENDUM


      o  Base System

      o  Program Development




Restrictions

VAX TEAMDATA/DANSK cannot be installed or run on the same system as
VAX TEAMDATA US version or any other language versions.



OPTIONAL SOFTWARE

ALL-IN-1 V2.1

VAX RALLY V1.1 - V2.0

VAX DATATRIEVE V4.0 - V4.2

VAX Common Data Dictionary V3.4

VAX Common Data Dictionary/Plus V4.0

VAX DBMS V3.0 - V4.0

VAX Xway V1.1

VIDA with IDMS/R (tm) V2.0

IDMS/R is a trademark of Cullinet Software, Inc.



GROWTH CONSIDERATIONS

The minimum hardware requirements for any future version of this
product may be different than the minimum hardware requirements for
the current version.



DISTRIBUTION MEDIA

Tape:  9-track 1600 BPI Magtape (PE), TK50 Streaming Tape







                                - 4 -

SYSTEM SUPPORT ADDENDUM


ORDERING INFORMATION


Software Licenses:         QL-741D*-** 
Software Media:            QA-741D*-** 
Software Documentation:    QA-741DA-GZ 
Software Product Services: QT-741D*-** 

The above information is valid at time of release.  Please contact
your local DIGITAL office for the most up-to-date information.








































* Denotes variant fields.  For additional information on available
licenses, services and media, refer to the appropriate price book.


                                - 5 -
