 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  Terminal Server Manager, Version 1.4          SSA
     27.64.05-A

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:        VAXft 3000-310

                 VAX 4000 Model 200,
                 VAX 4000 Model 300

                 VAX 6000 Model 200 Series,
                 VAX 6000 Model 300 Series,
                 VAX 6000 Model 400 Series,
                 VAX 6000 Model 500 Series

                 VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500,
                 VAX 8530, VAX 8550, VAX 8600, VAX 8650, VAX 8700,
                 VAX 8800, VAX 8810, VAX 8820, VAX 8830, VAX 8840

                 VAX 9000-210, VAX 9000 Model 400 Series

                 VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX:   MicroVAX II, MicroVAX 2000,
                 MicroVAX 3100, MicroVAX 3300,
                 MicroVAX 3400, MicroVAX 3500,
                 MicroVAX 3600, MicroVAX 3800,
                 MicroVAX 3900


                                  DIGITAL                  March 1991

                                                          AE-LT59C-TE

 


     Terminal Server Manager, Version 1.4              SSA 27.64.05-A




     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100 Series, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540

     VAXserver:  VAXserver 3100, VAXserver 3300, VAXserver 3400,
                 VAXserver 3500, VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900

                 VAXserver 4000 Model 300

                 VAXserver 6000-210, VAXserver 6000-220, VAXserver
                 6000-310, VAXserver 6000-320, VAXserver 6000-410,
                 VAXserver 6000-420, VAXserver 6000-510, VAXserver
                 6000-520

     Processors Not Supported

     MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXstation
     8000

     Processor Restrictions

     VT1300 color terminal

     A TK50 Tape Drive is required for stand-alone MicroVAX 2000 and
     VAXstation 2000 systems.

     Disk Space Requirements (Block Cluster Size = 1):

     Disk space required for      3,700 blocks
     installation:
                                  (1,895 Kbytes)

     Disk space required for      1,700 blocks
     use (permanent):
                                  (871 Kbytes)

                                     2

 


     Terminal Server Manager, Version 1.4              SSA 27.64.05-A



     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.


     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet, and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     VMS Operating System V5.4

     Layered Products:
        DECnet-VAX V5.0 - V5.4
        DECserver 100 for VMS V1.2 - V2.0
        Ethernet Terminal Server V3.0
        DECserver 200 for VMS V1.0 - V3.1
        DECserver 250 for VMS V1.0 - V2.0
        DECserver 300 for VMS V1.0 - V2.0
        DECserver 500 for VMS V1.0 - V2.1
        MUXserver 100 Remote Terminal Server
           for VMS V2.3
        MUXserver 300 Remote Terminal Server
           for VMS V1.1

     VMS Tailoring

     For VMS V5.x systems, the following VMS classes are required for
     full functionality of this layered product:

                                     3

 


     Terminal Server Manager, Version 1.4              SSA 27.64.05-A



     o  VMS Required Saveset

     o  Network Support

     o  Programming Support

     o  Utilities

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the requirements for
     the current version.

     DISTRIBUTION MEDIA

     Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     ORDERING INFORMATION

     Software Licenses: QL-VDHA*-**
     Software Media: QA-VDHA*-**
     Software Documentation: QA-VDHAA-GZ
     Software Product Services: QT-VDHA*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services, and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.



                                     4

 


     Terminal Server Manager, Version 1.4              SSA 27.64.05-A




     [TM] The DIGITAL Logo, DEC, DECnet, DECnet-VAX, DECserver,
          MicroVAX, MUXserver, VAX, VAXcluster, VAXft, VAXserver,
          VAXstation, and VMS are trademarks of Digital Equipment
          Corporation.


































                                     5
