 






     4

     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  VAXELN Ada, Version 2.2            SSA 27.22.05-A

     HARDWARE REQUIREMENTS

     Processor Support - Host

     VAX:      VAXft 3000-310
               VAX 4000 Model 300,
               VAX 6000 Model 200 Series
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840

               VAX 9000-210, VAX 9000-410

               VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX: MicroVAX II, MicroVAX 2000,
               MicroVAX 3100, MicroVAX 3300,
               MicroVAX 3400, MicroVAX 3500,
               MicroVAX 3600, MicroVAX 3800,
               Microvax 3900



                                  DIGITAL               February 1991

                                                          AE-LT57C-TE

 


     VAXELN Ada, Version 2.2                           SSA 27.22.05-A




     VAXstationVAXstation II, VAXstation 2000,
               VAXstation 3100 Series, VAXstation 3200,
               VAXstation 3500, VAXstation 3520
               VAXstation 3540

     Processors Not Supported

     VAX-11/725, VAX-11/782, MicroVAX I, VAXstation I, VAXstation
     8000

     Processor Support - Target

     Any valid target environment supported by VAXELN. Supported
     processors include:

     VAX:      VAX 4000 Model 300 Series,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series

               VAX 8200, VAX 8250, VAX 8500, VAX 8530,
               VAX 8550, VAX 8700, VAX 8800, VAX 8810

               VAX-11/730, VAX-11/750

               VAX RTA

     MicroVAX: MicroVAX II, MicroVAX 2000,
               MicroVAX 3100, MicroVAX 3300,
               MicroVAX 3400, MicroVAX 3500,
               MicroVAX 3600, MicroVAX 3800,
               MicroVAX 3900

     Board     KA620-BA, KA800-M, rtVAX 630
     Prod-
     ucts:


                                     2

 


     VAXELN Ada, Version 2.2                           SSA 27.22.05-A




     rtVAX     rtVAX 1000, rtVAX 3200, rtVAX 3300,
     Products: rtVAX 3400, rtVAX 3500, rtVAX 3600,
               rtVAX 3800, rtVAX 4000 Model 300,
               rtVAX 6000 Models 200, 300, and 400,
               Series, rtVAX 8550, rtVAX 8700,
               rtVAXstation 3100 Models 30 and 38,
               rtVAX 3305

     IVAX      IVAX 620, IVAX 630
     Prod-
     ucts:



























                                     3

 


     VAXELN Ada, Version 2.2                           SSA 27.22.05-A




     VAXstationVAXstation 2000, VAXstation 3100 Series,
               VAXstation 3150, VAXstation 3200,
               VAXstation 3500, VAXstation II/GPX

     VAXserver:VAXserver 3100, VAXserver 3300,
               VAXserver 3400, VAXserver 3500,
               VAXserver 3600, VAXserver 3602,
               VAXserver 3800, VAXserver 3900

               VAXserver 6000-210, VAXserver 6000-220,
               VAXserver 6000-310, VAXserver 6000-320,
               VAXserver 6000-410, VAXserver 6000-420

     Processors Not supported as targets:

     VAX:      VAX 6312, VAX 6333, VAX 8300, VAX 8350,
               VAX 8600, VAX 8650, VAX 8820, VAX 8830,
               VAX 8840, VAX 8842, VAX 8974, VAX 8978

               VAX-11/780, VAX-11/782, VAX-11/785

               VAXstation II, VAXstation 3520,
               VAXstation 3540, VAXstation 8000

     Note: A device capable of reading a TK50 is required to install
     VAXELN Ada on MicroVAX 2000 and VAXstation 2000 systems.

     Disk Space Requirements (Block Cluster Size = 1):

     Disk space required for      5000 Blocks
     installation:
                                  (2.6M bytes)

     Disk space required for      5000 Blocks
     permanent use:



                                     4

 


     VAXELN Ada, Version 2.2                           SSA 27.22.05-A




                                  (2.6M bytes)

     These block counts refer to the disk space required on the
     system disk. The sizes are approximate; actual sizes may vary
     depending on the user's system environment, configuration and
     software options selected.

     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet and Interconnect configurations.

     SOFTWARE REQUIREMENTS

     For Systems Using Terminals:

     o  VMS Operating System V5.4

     o  VAX Ada V2.0 - V2.2

     o  VAXELN Toolkit V4.1

     o  DECnet-VAX V5.4

     For Workstations Running VMS Workstation Software:

     o  VMS Operating System V5.4

     o  VMS Workstation Software V4.1 - V4.2

     o  VAX Ada V2.0 - V2.2

     o  VAXELN Toolkit V4.1

                                     5

 


     VAXELN Ada, Version 2.2                           SSA 27.22.05-A



     o  DECnet-VAX V5.4

     VMS Tailoring

     For VMS V5.x systems, the following VMS classes are required for
     full functionality of this product:

     o  VMS Required Saveset

     o  Network Support

     o  Programming Support

     o  Utilities

     For more information on VMS classes and tailoring, refer to the
     VMS Operating System (SPD 25.01.xx).

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the minimum require-
     ments for the current version.

     DISTRIBUTION MEDIA

     Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     This product is also available as part of the VMS Consolidated
     Software Distribution on CDROM.









                                     6

 


     VAXELN Ada, Version 2.2                           SSA 27.22.05-A



     ORDERING INFORMATION

     Software Licenses: QL-A97A*-**
     Software Media: QA-A97A*-**
     Software Documentation: QA-A97AA-GZ
     Software Product Services: QT-A97A*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [TM]  The DIGITAL Logo, DECnet, VMS, DECwindows, VAX, MicroVAX,
           VAXstation, VAXserver, VAXELN and VAXset are trademarks of
           Digital Equipment Corporation.





















                                     7
