 






          System
          Support
          Addendum

          ________________________________________________________________

          PRODUCT NAME:  VAX DEC/MMS, Version 2.6           SSA 26.03.13-A

          HARDWARE REQUIREMENTS

          Processors Supported

          VAX:      VAX 4000 Model 300,
                    VAXft 3000 Model 310,
                    VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840, VAX 8842,
                    VAX 8974, VAX 8978

                    VAX 9000-210, VAX 9000-410

                    VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

          MicroVAX: MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,
                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900






                                       DIGITAL              September 1990

                                                               AE-LT64D-TE

 


          VAX DEC/MMS, Version 2.6                          SSA 26.03.13-A




          VAXstationVAXstation II, VAXstation 2000,
                    VAXstation 3100 Series, VAXstation 3200,
                    VAXstation 3500, VAXstation 3520,
                    VAXstation 3540

          VAXserver:VAXserver 3100, VAXserver 3300,
                    VAXserver 3400, VAXserver 3500,
                    VAXserver 3600, VAXserver 3602,
                    VAXserver 3800, VAXserver 3900,

                    VAXserver 6000-210, VAXserver 6000-310,
                    VAXserver 6000-410, VAXserver 6000-420

          Processors Not Supported

          VAX-11/725, VAX-11/782, MicroVAX I, VAXstation I, VAXstation
          8000 Processor Restrictions

          A TK50 Tape Drive is required for standalone MicroVAX 2000 and
          VAXstation 2000 systems.

          Block Space Requirements (Block Cluster Size = 1):

          Disk space required for      2,300 blocks
          installation:
                                       (1.1M bytes)

          Disk space required for      800 blocks
          use (permanent):
                                       (0.4M bytes)

          These counts refer to the disk space required on the system
          disk. The sizes are approximate; actual sizes may vary depending
          on the user's system environment, configuration, and software
          options.

          OPTIONAL HARDWARE

                                          2

 


          VAX DEC/MMS, Version 2.6                          SSA 26.03.13-A



          None

          CLUSTER ENVIRONMENT

          This layered product is fully supported when installed on any
          valid and licensed VAXcluster* configuration without restric-
          tions. The HARDWARE REQUIREMENTS sections of this product's
          Software Product Description and System Support Addendum detail
          any special hardware required by this product.

          *  V5.x VAXcluster configurations are fully described in the
             VAXcluster Software Product Description (29.78.xx) and in-
             clude CI, Ethernet and Mixed Interconnect configurations.

          SOFTWARE REQUIREMENTS

          o  VMS Operating System V5.2 - V5.4

          On VMS workstations running windowing software, VAX DEC/MMS may
          be used in terminal emulator (for example, from DECterm). VAX
          DEC/MMS does not have a DECwindows user interface.

          Refer to the System Support Software Addendum (SSA 26.03.13-
          x) for availability and versions of required software. VMS
          Tailoring

          The following VMS classes are required for full functionality of
          this layered product:

          o  VMS Required Saveset

          o  Programming Support

          o  Utilities

          For more information on VMS classes and tailoring, refer to
          the VMS Operating System Software Product Description (SPD
          25.01.xx).

          OPTIONAL SOFTWARE

                                          3

 


          VAX DEC/MMS, Version 2.6                          SSA 26.03.13-A



          VAX CDD/Plus V4.2
          VAX FMS V2.4
          VAX DEC/CMS V3.3- V3.4
          VAX Language-Sensitive Editor/Source Code Analyzer V3.1

          Certain versions of these products depend upon a specific ver-
          sion of the Operating System. Please see the System Software
          Addendum of the product in question to determine which version
          you need.

          GROWTH CONSIDERATIONS

          The minimum hardware/software requirements for any future ver-
          sion of this product may be different from the minimum require-
          ments for the current version.

          DISTRIBUTION MEDIA

          Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

          This product is also available as part of the VMS Consolidated
          Software Distribution on CDROM.

          The software documentation for this product is also available as
          part of the VMS Online Documentation Library on CDROM.

          ORDERING INFORMATION

          Software Licenses: QL-VADA*-**
          Software Media: QA-VADA*-**
          Software Documentation: QA-VADAA-GZ
          Software Product Services: QT-VADA*-**

          *  Denotes variant fields. For additional information on avail-
             able licenses, services and media refer to the appropriate
             price book.



                                          4

 


          VAX DEC/MMS, Version 2.6                          SSA 26.03.13-A



          The above information is valid at time of release. Please con-
          tact your local Digital office for the most up-to-date informa-
          tion.

          [TM]  The DIGITAL Logo, VAX, MicroVAX, VAXstation, VAXserver and
                VMS are trademarks of Digital Equipment Corporation.

































                                          5
