 






          System
          Support
          Addendum

          ________________________________________________________________

          PRODUCT NAME:  VAXset Package, Release 10         SSA 27.07.09-A

          1  HARDWARE REQUIREMENTS

          Processors Supported

          VAX:      VAX 4000 Model 300,
                    VAXft 3000 Model 310,
                    VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840, VAX 8842,
                    VAX 8974, VAX 8978

                    VAX 9000-210, VAX 9000-410

                    VAX-11/780, VAX-11/785

          MicroVAX: MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,
                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900






                                       DIGITAL              September 1990

                                                               AE-LT84F-TE

 


          VAXset Package, Release 10                        SSA 27.07.09-A




          VAXstationVAXstation II, VAXstation 2000,
                    VAXstation 3100 Series, VAXstation 3200,
                    VAXstation 3500, VAXstation 3520,
                    VAXstation 3540

          VAXserver:VAXserver 3100, VAXserver 3300,
                    VAXserver 3400, VAXserver 3500,
                    VAXserver 3600, VAXserver 3602,
                    VAXserver 3800, VAXserver 3900

                    VAXserver 6000-210, VAXserver 6000-310,
                    VAXserver 6000-410, VAXserver 6000-420

          Processors Not Supported

          VAX-11/725, VAX-11/730, VAX-11/750, VAX-11/782, MicroVAX I,
          VAXstation I, VAXstation 8000. Processor Restrictions

          o  A TK50 tape drive is required for MicroVAX 2000 and VAXsta-
             tion 2000 systems.

          o  VAXset requires sufficient on-line mass storage to accommo-
             date the components of this package and the libraries created
             by VAX DEC/CMS and VAX Language-Sensitive Editor/Source Code
             Analyzer.

          o  VAXset requires a valid VAX, MicroVAX or VAXstation configu-
             ration. For more information on valid system configuration,
             please refer to the VMS Operating System Software Product
             Description (SPD 25.01.xx).

          Terminals

          Some components of VAXset require the following terminals for
          Character Cell Interface:

          o  A VT1xx, VT2xx, VT3xx, or ANSI CRT

                                          2

 


          VAXset Package, Release 10                        SSA 27.07.09-A



          Some components of VAXset require the following configuration
          for DECwindows Interface:

          o  A valid DECwindows workstation configuration. Please refer to
             the individual component's Software Product Description for
             valid configuration.

          Block Space Requirements (Block Cluster Size = 1):

          Disk space required for      33,700 blocks
          installation:
                                       (17.5M bytes)

          Disk space required for      28,200 blocks
          permanent use:
                                       (14.5M bytes)

          Note: Approximately 275 blocks should be added for each language
          you choose to have supported by the Editor component of the VAX
          Language-Sensitive Editor/Source Code Analyzer.

          For installation of the Language-Sensitive Editor component
          of the VAX Language-Sensitive Editor/Source Code Analyzer with
          support for all the languages:

          Disk space required for      36,725 blocks
          installation:
                                       (18.9M bytes)

          Disk space required for      31,225 blocks
          permanent use:
                                       (16.0M bytes)

          These counts refer to the disk space required on the system
          disk. The sizes are approximate; actual sizes may vary depending
          on the user's system environment, configuration, and software
          options selected.

          Memory Requirements for DECwindows Support

                                          3

 


          VAXset Package, Release 10                        SSA 27.07.09-A



          The minimum supported memory for this application running in
          a standalone DECwindows environment with both the client and
          server executing on that same system is 8 MB.

          The performance and memory usage of DECwindows applications are
          particularly sensitive to system configuration. Less memory may
          be required on the client system (the system where the software
          is installed and executed) if the server (the component that
          displays the application) resides on another system. More memory
          may be required on a system with several applications running or
          may be desirable to improve the performance of an application.

          2  OPTIONAL HARDWARE

          None

          3  CLUSTER ENVIRONMENT

          This layered product is fully supported when installed on any
          valid and licensed VAXcluster* configuration without restric-
          tions. The HARDWARE REQUIREMENTS sections of this product's
          Software Product Description and System Support Addendum detail
          any special hardware required by this product.

          *  V5.x VAXcluster configurations are fully described in the
             VAXcluster Software Product Description (28.78.xx) and in-
             clude CI, Ethernet and Mixed Interconnect configurations.

          4  SOFTWARE REQUIREMENTS

          For systems using terminals: (No DECwindows interface)

          o  VMS Operating System V5.3 - V5.4

          Note: VMS DECwindows Compute Server Component must be installed
          to use VAX Performance and Coverage Analyzer.



                                          4

 


          VAXset Package, Release 10                        SSA 27.07.09-A



          For workstations running VWS:

          o  VMS Operating System V5.3 - V5.4

          o  VMS Workstation Software V4.2

          For workstations running DECwindows:

          o  VMS Operating System (and necessary components of VMS DECwin-
             dows) V5.3 - V5.4

          VAXset may run in either of the following ways:

          o  Stand-alone execution - Running the X11 display server and
             the client application on the same machine.

          o  Remote execution - Running the X11 display server and the
             client application on different machines.

          VMS DECwindows is part of the VMS Operating System but must
          be installed separately. Installation of VMS DECwindows gives
          you the option to install any or all of the following three
          components:

          o  VMS DECwindows Compute Server (Base kit; provides runtime
             support)

          o  VMS DECwindows Device Support

          o  VMS DECwindows Programming Support

          For stand-alone execution, the following DECwindows components
          must be installed on the machine:

          o  VMS DECwindows Compute Server (Base Kit; provides runtime
             support)

          o  VMS DECwindows Device Support

          o  VMS DECwindows Programming Support

          For remote execution, the following DECwindows components must
          be installed on the machines:

                                          5

 


          VAXset Package, Release 10                        SSA 27.07.09-A



          Server Machine

          o  VMS DECwindows Compute Server (Base Kit; provides runtime
             support)

          o  VMS DECwindows Device Support

          o  VMS DECwindows Programming Support

          Client Machine

          o  VMS DECwindows Compute Server (Base Kit; provides runtime
             support)

          o  VMS DECwindows Device Support

          o  VMS DECwindows Programming Support

          VMS Tailoring

          For VMS V5.x, the following classes of VMS are required for full
          functionality of this layered product.

          o  VMS Required Saveset

          o  Programming Support

          o  Utilities

          o  Secure User's Environment

          For more information on VMS classes and tailoring, refer to
          the VMS Operating System Software Product Description (SPD
          25.01.xx).

          OPTIONAL SOFTWARE

          VAX Ada V2.1
          VAX BASIC V3.4
          VAX BLISS-32 Implementation Language V4.6
          VAX C V3.1
          VAX COBOL V4.3
          VAX CDD/Plus V4.2
          VAX DIBOL V4.1

                                          6

 


          VAXset Package, Release 10                        SSA 27.07.09-A



          VAX FORTRAN V5.4 - V5.5
          VAX FORTRAN High-Performance Option V1.0
          VAX FMS V2.4
          VAX PASCAL V4.0 - V4.1
          VAX PL/I V3.3 - V3.4
          VAX RPG II V2.1
          VAX SCAN V1.2


          5  GROWTH CONSIDERATIONS

          The minimum hardware/software requirements for any future ver-
          sion of this package may be different from the minimum require-
          ments for the current version.

          6  DISTRIBUTION MEDIA

          Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

          This product is also available as part of the VMS Consolidated
          Software Distribution on CDROM.

          7  ORDERING INFORMATION

          Software License: QL-965A*-**
          Software Media: QA-965A*-**
          Software Documentation: QA-965AA-GZ
          Software Product Services: QT-965A*-**

          *  Denotes variant fields. For additional information on avail-
             able licenses, services and media, refer to the appropriate
             price book.

          The above information is valid at time of release. Please con-
          tact your local Digital office for the most up-to-date informa-
          tion.



                                          7

 


          VAXset Package, Release 10                        SSA 27.07.09-A




          [TM]  The DIGITAL Logo, VMS, DECwindows, VAX, MicroVAX, VAXs-
                tation, VAXserver and VAXset are trademarks of Digital
                Equipment Corporation.



































                                          8
