 
















             VAX Performance and Coverage Analyzer Installation
             VAX Performance and Coverage Analyzer Installation
             VAX Performance and Coverage Analyzer Installation
             Guide
             Guide
             Guide

             Order Number: AA-EB57E-TE



             August 1990
             August 1990
             August 1990

             This document contains instructions for installing VAX PCA on
             the VMS operating system. It also explains how to read the
             online release notes before or after installing the product.
             This document applies to VAX PCA Version 3.0.





                                           This revised manual supersedes
             Revision/Update Information:
             Revision/Update Information:
             Revision/Update Information:
                                           the
                                               ___ ___ ____________ _____
                                               VAX PCA Installation Guide
                                           (Order number AA-EB57D-TE).

                                           VMS Version 5.3 or higher and
             Operating System and Version:
             Operating System and Version:
             Operating System and Version:
                                           DECwindows
                                           Version 2.0

                                           VAX PCA Version 3.0
             Software Version:
             Software Version:
             Software Version:

             Digital Equipment Corporation
             Digital Equipment Corporation
             Digital Equipment Corporation

 





             ________________________
             First Printing, June 1985
             First Printing, June 1985
             First Printing, June 1985
             Revised, October 1985
             Revised, October 1985
             Revised, October 1985
             Revised, August 1987
             Revised, August 1987
             Revised, August 1987
             Revised, April 1989
             Revised, April 1989
             Revised, April 1989
             Revised, December 1989
             Revised, December 1989
             Revised, December 1989
             Revised, August 1990
             Revised, August 1990
             Revised, August 1990

             The information in this document is subject to change without
             notice and should not be construed as a commitment by Digital
             Equipment Corporation. Digital Equipment Corporation assumes
             no responsibility for any errors that may appear in this
             document.

             The software described in this document is furnished under a
             license and may be used or copied only in accordance with the
             terms of such license.

             No responsibility is assumed for the use or reliability
             of software on equipment that is not supplied by Digital
             Equipment Corporation or its affiliated companies.

             Restricted Rights: Use, duplication, or disclosure by the
             U.S. Government is subject to restrictions as set forth in
             subparagraph (c)(1)(ii) of the Rights in Technical Data and
             Computer Software clause at DFARS 252.227-7013.

             __________
             Copyright ©1985, 1987, 1989, 1990 Digital Equipment
             Corporation

             All Rights Reserved.
             Printed in U.S.A.

             The postpaid Reader's Comments forms at the end of this docu-
             ment request your critical evaluation to assist in preparing
             future documentation.

             The following are trademarks of Digital Equipment Corporation:

             CDD/Plus        VAX Document  VAXstation
             DATATRIEVE      VAX MACRO     VMS
             DECforms        VAX Notes     VT
             DECwindows      VAX SCAN
             VAX             VAXcluster
             VAX DIBOL       VAXset
                                           DIGITAL
                                           DIGITAL
                                           DIGITAL

                                                                    ZK5284

 







                                                                  Contents
                                                                  Contents
                                                                  Contents
          ________________________________________________________________

                __________________________________________________________
                PREFACE                                                  v
                PREFACE                                                  v
                PREFACE                                                  v

                1     PREPARING TO INSTALL VAX PCA                       1
                1     PREPARING TO INSTALL VAX PCA                       1
                1     PREPARING TO INSTALL VAX PCA                       1
                1.1       Required Operating System Components           1
                1.1       Required Operating System Components           1
                1.1       Required Operating System Components           1
                1.2       Prerequisite Software                          1
                1.2       Prerequisite Software                          1
                1.2       Prerequisite Software                          1
                1.3       Optional Software                              2
                1.3       Optional Software                              2
                1.3       Optional Software                              2
                1.4       Accessing the Online Release Notes             3
                1.4       Accessing the Online Release Notes             3
                1.4       Accessing the Online Release Notes             3
                1.5       Installation Procedure Requirements            3
                1.5       Installation Procedure Requirements            3
                1.5       Installation Procedure Requirements            3
                1.6       User Account Quotas and Privileges             5
                1.6       User Account Quotas and Privileges             5
                1.6       User Account Quotas and Privileges             5
                1.7       VMS License Management Facility                6
                1.7       VMS License Management Facility                6
                1.7       VMS License Management Facility                6
                1.8       Using VMSINSTAL                                7
                1.8       Using VMSINSTAL                                7
                1.8       Using VMSINSTAL                                7


                2     INSTALLING VAX PCA                                 9
                2     INSTALLING VAX PCA                                 9
                2     INSTALLING VAX PCA                                 9
                2.1       Installing VAX PCA on a VAXcluster            16
                2.1       Installing VAX PCA on a VAXcluster            16
                2.1       Installing VAX PCA on a VAXcluster            16

                3     AFTER THE INSTALLATION                            17
                3     AFTER THE INSTALLATION                            17
                3     AFTER THE INSTALLATION                            17


                4     RUNNING THE INSTALLATION VERIFICATION
                4     RUNNING THE INSTALLATION VERIFICATION
                4     RUNNING THE INSTALLATION VERIFICATION
                      PROCEDURE SEPARATELY                              17
                      PROCEDURE SEPARATELY                              17
                      PROCEDURE SEPARATELY                              17

                5     ERROR CONDITIONS                                  18
                5     ERROR CONDITIONS                                  18
                5     ERROR CONDITIONS                                  18


                6     MAINTENANCE UPDATES                               19
                6     MAINTENANCE UPDATES                               19
                6     MAINTENANCE UPDATES                               19

                7     IMPROVING PRODUCT PERFORMANCE                     19
                7     IMPROVING PRODUCT PERFORMANCE                     19
                7     IMPROVING PRODUCT PERFORMANCE                     19


                8     DETERMINING AND REPORTING PROBLEMS                20
                8     DETERMINING AND REPORTING PROBLEMS                20
                8     DETERMINING AND REPORTING PROBLEMS                20

                9     SAMPLE INSTALLATION                               20
                9     SAMPLE INSTALLATION                               20
                9     SAMPLE INSTALLATION                               20


                                                                       iii

 






                9.1       Sample 1 for Installation with PCA
                9.1       Sample 1 for Installation with PCA
                9.1       Sample 1 for Installation with PCA
                          Authorization Key and the IVP                 21
                          Authorization Key and the IVP                 21
                          Authorization Key and the IVP                 21
                9.2       Sample 2 for Installation with PCA
                9.2       Sample 2 for Installation with PCA
                9.2       Sample 2 for Installation with PCA
                          Authorization Key without the IVP             23
                          Authorization Key without the IVP             23
                          Authorization Key without the IVP             23
                9.3       Sample 3 for Installation without PCA
                9.3       Sample 3 for Installation without PCA
                9.3       Sample 3 for Installation without PCA
                          Authorization Key                             25
                          Authorization Key                             25
                          Authorization Key                             25

































          iv

 














                                                                   Preface
                                                                   Preface
                                                                   Preface
          ________________________________________________________________



             This document describes how to install the VAX Performance
             and Coverage Analyzer (PCA) on the VMS operating system. It
             is intended for system managers. This document applies to VAX
             PCA Version 3.0 and all maintenance updates in that version.
             A major version number is represented by the digits to the
             left of the decimal point, and the maintenance update version
             number is indicated by the digits to the right of the decimal
             point.

             Keep this document with your distribution kit. You will need
             it to install maintenance updates or to reinstall VAX PCA for
             any other reason.

             At the back of this document are two Reader's Comments forms.
             If you have any comments about this document, fill out one
             form and mail it; your comments will be considered for the
             next revision of the installation guide.

             For more information about installing VAX PCA on VMS systems,
             see your processor-specific installation/operations guide.

             The installation procedure is described step-by-step and is,
             for the most part, self-explanatory. The system prompts you
             to answer questions and to change volumes, and waits for you
             to tell it to continue.

                                                                         v

 






             Defaults appear in brackets ([])  throughout the installation
             procedure. Text you type is indicated in red.





































          vi

 





          __________________________________________________________

          1  Preparing to Install VAX PCA
          1  Preparing to Install VAX PCA
          1  Preparing to Install VAX PCA

             Your bill of materials (BOM) and indented bills report (BIL)
             specify the number and contents of your media. Be sure to
             check the contents of your kit against this information.
             If your kit is damaged or if you find that parts of it are
             missing, call your Digital representative.

             Distribution media must be mounted in numerical order. The
             installation procedure prompts you to mount the volumes. For
             more information on how to mount distribution media, see your
             processor-specific installation/operations guide, which also
             details several options to the installation procedure.

          __________________________________________________________

          1.1  Required Operating System Components
          1.1  Required Operating System Components
          1.1  Required Operating System Components

             The VMS operating system comes with a variety of support op-
             tions, or classes. Classes include such features as network-
             ing and RMS journaling. For a complete list of the required
             classes, see the Software Support Addendum (SSA), which comes
             with the Software Product Description (SPD).

          __________________________________________________________

          1.2  Prerequisite Software
          1.2  Prerequisite Software
          1.2  Prerequisite Software

             VAX PCA Version 3.0 requires VMS Version 5.3 or higher. If
             you are using the PCA DECwindows interface, VMS DECwindows
             Version 2.0 is also required.

             The VMS DECwindows Compute Server component must be in-
             stalled before the VAX Performance and Coverage Analyzer
             is installed. The DECwindows compute server consists of
             the RTL images: DECW$DWTLIBSHR.EXE, DECW$XLIBSHR.EXE, and
             DECW$TRANSPORT_COMMON.EXE.

                                                                         1

 





          __________________________________________________________

          1.3  Optional Software
          1.3  Optional Software
          1.3  Optional Software

             The following optional software can be used with VAX PCA
             Version 3.0:

              o VAX Ada Version 1.5 and 2.0

              o VAX BASIC Version 3.2 and Version 3.3

              o VAX BLISS-32 Implementation Language Version 4.5

              o VAX C Version 2.4 through Version 3.0

              o VAX COBOL Version 4.2

              o VAX DIBOL Version 4.0

              o VAX FORTRAN Version 5.4 and 5.5

              o VAX FORTRAN HPO Version 1.0

              o VAX PASCAL Version 3.9 and 4.0

              o VAX PL/I Version 3.2

              o VAX RPG II Version 2.1

              o VAX SCAN Version 1.1

              o VAX DEC/Test Manager Version 3.2

              o VAX Language-Sensitive Editor Version 3.0 and 3.1

              o VAX Source Code Analyzer Version 2.0 and 2.1

             All features of PCA are available to each of these languages.
             The VAX DEC/Test Manager, the VAX Language-Sensitive Editor,
             and the VAX Source Code Analyzer can be used in conjunction
             with VAX PCA.

          2

 





          __________________________________________________________

          1.4  Accessing the Online Release Notes
          1.4  Accessing the Online Release Notes
          1.4  Accessing the Online Release Notes

             VAX PCA provides online release notes. The prompt to display
             or print the release notes during the installation appears
             in step 5 of the installation procedure when you invoke
             VMSINSTAL with the OPTIONS N parameter.

             To obtain the release notes after the installation, type or
             print the file SYS$HELP:PCA030.RELEASE_NOTES. Online help
             also directs you to the the release notes file. After the
             installation, type the following command:

               $ HELP PCA RELEASE_NOTES <RETURN>

          __________________________________________________________

          1.5  Installation Procedure Requirements
          1.5  Installation Procedure Requirements
          1.5  Installation Procedure Requirements

             The installation takes approximately 5 to 25 minutes, de-
             pending on the type of media and your system configuration.
             Before installing VAX PCA, you must have the following privi-
             leges and resources:

              o SETPRV privileges, or CMKRNL, WORLD, and SYSPRV privileges

              o A minimum of 11000 blocks of free disk space during in-
                stallation; 5500 blocks are used after installation; 6500
                blocks are used after installation with the demo package

              o A minimum of 40 free global pages plus the size (in number
                of disk blocks) of the file SYS$LIBRARY:DCLTABLES.EXE
                at installation; for most efficient operation, you will
                need a total of 40 free global pages plus the size of
                SYS$LIBRARY:DCLTABLES.EXE after installation

              o A minimum of 4 free global sections at installation

                                          NOTE
                                          NOTE
                                          NOTE

                 You must ensure that your system has the necessary
                 global page and global section SYSGEN quotas for the

                                                                         3

 






                 installation. Failure to do so could cause the DCL
                 tables to be corrupted in some situations.

             To determine the number of available global pages on your
             system, invoke the VMS Install Utility by typing the follow-
             ing commands:

               $ INSTALL <RETURN>

             Then type the following command:

               INSTALL> LIST/GLOBAL/SUMMARY <RETURN>

                       Summary of Local Memory Global Sections

               100 Global Sections Used,  300/400 Global Pages Used/Unused

               INSTALL> EXIT <RETURN>

             When you issue these commands, the system displays a summary
             of the number of global sections used, the number of global
             pages used, and the number of global pages unused. To exit
             from the VMS Install Utility, type the EXIT command.

             VAX PCA requires approximately 40 global pages. If there
             are fewer than 40 pages available, you can delete an ex-
             isting known image with the VMS Install Utility, or you
             can increase the GBLPAGES system parameter with the VMS
             System Generation Utility (SYSGEN) by editing the file
             SYS$SYSTEM:MODPARAMS.DAT and then invoking the AUTOGEN com-
             mand procedure, SYS$UPDATE:AUTOGEN.COM. For more information
             on the AUTOGEN command procedure, see your processor-specific
             installation/operations guide.

             You can determine the number of available global sections by
             invoking SYSGEN as follows:

               $ RUN SYS$SYSTEM:SYSGEN <RETURN>
               SYSGEN> USE CURRENT <RETURN>
               SYSGEN> SHOW GBLSECTIONS <RETURN>

               SYSGEN> EXIT <RETURN>

          4

 






             The last number displayed is the maximum number of global
             sections. Compare this number to the number of global sec-
             tions in use displayed by the VMS Install Utility. VAX PCA
             requires 4 global sections. Therefore, if the number of
             global sections used plus 2 exceeds the maximum number of
             global sections, you must increase the number of available
             global sections before you can install VAX PCA. To increase
             the number, you must increase the GBLSECTIONS system parame-
             ter with SYSGEN by editing the file SYS$SYSTEM:MODPARAMS.DAT
             and then invoking the SYS$UPDATE:AUTOGEN.COM procedure.
             For more information on the AUTOGEN.COM procedure, see your
             processor-specific installation/operations guide.

             If the number of global sections used plus 2 is less than the
             maximum number of global sections, you can exit from SYSGEN
             and continue.

          __________________________________________________________

          1.6  User Account Quotas and Privileges
          1.6  User Account Quotas and Privileges
          1.6  User Account Quotas and Privileges

             To use VAX PCA, it is recommended that each account have
             TMPMBX and NETMBX privileges and the following requirements:

              o AST limit (ASTLM) 30 (minimum)

              o Buffered I/O byte count quota (BYTLM) 4096 (minimum)

              o Open file limit (FILLM) 20 (minimum)

             Use the VMS Authorize Utility (AUTHORIZE) to compare the
             current values of these quotas with the requirements for VAX
             PCA. For example, the account used in the following example
             is the SYSTEM account:

               $ SET DEFAULT SYS$SYSTEM <RETURN>
               $ RUN AUTHORIZE <RETURN>
               UAF> SHOW SYSTEM <RETURN>

                                                                         5

 






             To change the values of these quotas, use the VMS Authorize
             Utility's MODIFY command. For more information, see the
                                                                     ___
                                                                     VMS
                                     .
             _________ _______ ______
             Authorize Utility Manual

          __________________________________________________________

          1.7  VMS License Management Facility
          1.7  VMS License Management Facility
          1.7  VMS License Management Facility

             The VMS License Management Facility (LMF) is available with
             Version 5.0 of the VMS operating system. To install VAX PCA
             on a VMS V5.3 system, you must register your VAX PCA software
             license.

             The license registration information you need is contained in
             the Product Authorization Key (PAK) that is shipped with VAX
             PCA. The PAK is a paper certificate that contains information
             about the license you have to run a particular piece of
             software.

             During the installation, you are asked if you have registered
             the VAX PCA license and loaded the appropriate authoriza-
             tion key. You must register and load your license for VAX
             PCA        you start the installation in order to run the
                 ______
                 before
             Installation Verification Procedure (IVP) and use the soft-
             ware.

             To register a license under VMS Version 5.3, first log in to
             the system manager's account, SYSTEM. You then have a choice
             of two ways to perform the registration:

              o Invoke the SYS$UPDATE:VMSLICENSE.COM procedure. When it
                prompts you for information, respond with data from your
                Product Authorization Key (PAK).

              o Issue the LICENSE REGISTER DCL command with the appro-
                priate qualifiers that correspond to information on the
                PAK.


          6

 






             For complete information on using LMF, see the
                                                            ___ _______
                                                            VMS License
                                       in the VMS documentation set.
             __________ _______ ______
             Management Utility Manual
             Register the information contained in the Product Authorization
             Key (PAK) that is shipped with VAX PCA by using either the
             VMS License command procedure (VMSLICENSE) or the LICENSE
             REGISTER and LICENSE LOAD commands.

          __________________________________________________________

          1.8  Using VMSINSTAL
          1.8  Using VMSINSTAL
          1.8  Using VMSINSTAL

             After you log in to a privileged account to install VAX PCA,
             invoke VMSINSTAL, the command procedure that installs this
             product. An example of this procedure is shown in steps 1 and
             2 of the Installing VAX PCA section.

             The VMSINSTAL command procedure has the following syntax:

               $ @SYS$UPDATE:VMSINSTAL PCA030 ddcu: [OPTIONS N]

             _____
             ddcu:
             ddcu:
             ddcu:
             Represents a device name where the distribution volumes
             will be mounted for the VAX PCA installation media, where
                is the device code,   is the controller code, and   is the
             __                     _                             _
             dd                     c                             u
             unit number. It is not necessary to use the console drive to
             install VAX PCA. If you do use the console drive, you should
             replace any media you removed from the drive. CSA1: is the
             device name used in examples in this document.

             _______ _
             OPTIONS N
             OPTIONS N
             OPTIONS N
             Is an optional parameter you should provide if you want to be
             prompted to display or print the release notes. If you do not
             include the OPTIONS N parameter, VMSINSTAL does not prompt
             you to display or print the release notes. VMSINSTAL permits
             the use of several other options. For more information on
             the other options, see your processor-specific installation
             /operations guide.


                                                                         7

 






             If you do not supply the first two parameters, VMSINSTAL
             prompts you for the product and device names. If you wish to
             be prompted for the product and device names and to display
             or print the release notes, type the following:

               $ @SYS$UPDATE:VMSINSTAL <RETURN>

             When you invoke VMSINSTAL, it checks the following:

              o Whether you logged in to a privileged account. Digital
                recommends that you install software from the system
                manager's account with your default device and directory
                set to SYS$UPDATE.

              o Whether you have adequate quotas for installation.
                VMSINSTAL checks for the following quota values:

                 - ASTLM = 24

                 - BIOLM = 18

                 - BYTLM = 18000

                 - DIOLM = 18

                 - ENQLM = 30

                 - FILLM = 20

                VMSINSTAL then checks whether the following conditions
                exist. If so, discontinue the conditions before resuming
                the installation procedure.

                 o Whether DECnet is up and running

                 o Whether any users are logged in to the system

                If VMSINSTAL detects either of these conditions, you will
                be asked whether you want to continue the installation. If
                you want to continue, type YES. If you want to stop the
                installation, press RETURN.

          8

 





          __________________________________________________________

          2  Installing VAX PCA
          2  Installing VAX PCA
          2  Installing VAX PCA

             This section contains excerpts from the installation pro-
             cedure and explains each step. Defaults appear in brackets
             throughout the installation procedure.

             To abort the installation procedure at any time, press
             CTRL/Y. When you press CTRL/Y, the installation procedure
             deletes all files it has created up to that point and then
             returns you to DCL level. If you want to retry the installa-
             tion procedure after pressing CTRL/Y, you must proceed from
             step 2.

             Step 1: Log in to a privileged account and set your default
             Step 1: Log in to a privileged account and set your default
             Step 1: Log in to a privileged account and set your default
             device and directory to SYS$UPDATE.
             device and directory to SYS$UPDATE.
             device and directory to SYS$UPDATE.

          <RETURN>

               Username: SYSTEM  <RETURN>
               Password:         <RETURN>
               $ SET DEFAULT SYS$UPDATE <RETURN>

             Step 2: Invoke VMSINSTAL.
             Step 2: Invoke VMSINSTAL.
             Step 2: Invoke VMSINSTAL.

               $ @VMSINSTAL PCA030 CSA1: OPTIONS N <RETURN>

                     VAX/VMS Software Product Installation Procedure V5.3

               It is dd-mmm-yyyy at hh:mm.
               Enter a question mark (?) at any time for help.

               * Are you satisfied with the backup of your system disk [YES]? <RETURN>

             If you are satisfied with the backup of your system disk,
             press RETURN. Otherwise, type NO and press RETURN to discon-
             tinue the installation.


                                                                         9

 






             Step 3: Insert the first installation kit volume.
             Step 3: Insert the first installation kit volume.
             Step 3: Insert the first installation kit volume.

               Please mount the first volume of the set on CSA1:.
               * Are you ready? YES <RETURN>
               The following products will be processed:

                 VAX PCA V3.0

                   Beginning installation of VAX PCA V3.0 at 12:30

               %VMSINSTAL-I-RESTORE, Restoring product saveset A...

             To indicate that you want to continue the installation, mount
             volume 1, type YES, and press RETURN.


             Step 4: Insert the subsequent installation kit volumes.
             Step 4: Insert the subsequent installation kit volumes.
             Step 4: Insert the subsequent installation kit volumes.

               %BACKUP-I-READYREAD, mount volume 2 on _CSA1: for reading

               Enter "YES" when ready: YES<RETURN>

             VMSINSTAL prompts you to insert the next volume and waits for
             you to type YES after inserting it. If you type NO, VMSINSTAL
             displays the prompt again. This prompt is displayed only if
             your installation kit contains more than one volume.

             Step 5: Select a release notes option.
             Step 5: Select a release notes option.
             Step 5: Select a release notes option.

             This step applies only if you specified OPTIONS N in step 2.

               Release Notes Options:

                   1. Display release notes
                   2. Print release notes
                   3. Both 1 and 2
                   4. Copy release notes to SYS$HELP
                   5. Do not display, print or copy release notes

          10

 






               * Select option [3]: <RETURN>

             If you select option 1, VMSINSTAL displays the release notes
             on line immediately. You can terminate the display at any
             time by pressing CTRL/C.

             If you select option 2, VMSINSTAL prompts you for a queue
             name. Either type a queue name or press RETURN to send the
             file to the default output print device.

               * Queue name [SYS$PRINT]: <RETURN>

             If you select option 3, VMSINSTAL displays the release notes
             on line immediately. You can terminate the display at any
             time by pressing CTRL/C. VMSINSTAL then prompts you for a
             queue name. Either type a queue name or press RETURN to send
             the file to the default output print device. The VAX PCA
             release notes are then copied to SYS$HELP:PCA030.RELEASE_
             NOTES.

             If you select option 4, VMSINSTAL copies the release notes to
             SYS$HELP immediately.

             If you selected release note option 5 which specified that
             the release notes be copied to SYS$HELP, you will not be able
             to access the release notes without installing the product
             kit again.

                                          NOTE
                                          NOTE
                                          NOTE

                 This version of the release notes file installed by
                 VMSINSTAL is labeled with the current product name and
                 version number. Take care not to delete release notes
                 for previous versions of VAX PCA.

             Next, VMSINSTAL displays the following prompt:

               * Do you want to continue the installation [N]?: Y <RETURN>
               %VMSINSTAL-I-RELMOVED, The product release notes have been
                     successfully moved to SYS$HELP.

                                                                        11

 






             If you want to continue the installation, type YES and press
             RETURN. If you type NO or press RETURN, VMSINSTAL discon-
             tinues the installation. In either case, VMSINSTAL moves the
             release notes to SYS$HELP.


             Step 6: Respond to License Registration Queries.
             Step 6: Respond to License Registration Queries.
             Step 6: Respond to License Registration Queries.

             VAX PCA supports the VMS License Management Facility (LMF).
             The installation procedure displays license information about
             your product and then asks if you have registered and loaded
             your authorization key for VAX PCA. The following is an
             example of such information:

               Product:       PCA
               Producer:      DEC
               Version:       3.0
               Release Date:  10-AUG-1990

               * Does this product have an authorization key registered and loaded?

             You must have a PCA license installed and loaded on the
             system. If you do not have a license installed, answer NO.
             The installation of PCA will continue but the Installation
             Verification Procedure (IVP) will not be executed. The IVP
             will be placed on the system. It is recommended that you
             execute the IVP upon completion of installation once you have
             registered and loaded the PCA license. See step 10 on how to
             execute the IVP.


             Step 7: Select installation options.
             Step 7: Select installation options.
             Step 7: Select installation options.

               * Do you want to run the IVP after the installation [YES]? <RETURN>





          12

 






             The Installation Verification Procedure (IVP) runs tests
             to check whether the installation procedure was successful.
             Press RETURN to run the IVP after the installation. If you do
             not want to run the IVP, type NO in response to the prompt.

               * Do you want to purge files replaced by this installation [YES]? <RETURN>

             The directories SYS$EXAMPLES, SYS$HELP, SYS$LIBRARY,
             SYS$MANAGER, and SYS$SYSTEM may contain previous versions of
             VAX PCA files. These files are replaced during the installa-
             tion with new files, but the old files are not automatically
             purged. Purging is recommended. In response to the purging
             prompt, press RETURN to purge the files or type NO to keep
             them.


             Step 8: Install the PCA demo package.
             Step 8: Install the PCA demo package.
             Step 8: Install the PCA demo package.

               * Do you want to install the PCA demo package [YES]? Y<RETURN>
               %VMS-I-SYSDIR, This product creates system directory
                     [SYSHLP.EXAMPLES.PCA]

             VMSINSTAL asks you if you want to install the optional
             PCA demo package. If you type YES (the default), then the
             SYS$COMMON:[SYSHLP.EXAMPLES.PCA] directory is created, and
             all the demo files are copied into it. The system logical
             name PCA$EXAMPLES, pointing to this directory, is also de-
             fined. After the installation, you will be able to run the
             demos with @PCA$EXAMPLES:PCA_DEMO.

             Step 9: Read informational messages.
             Step 9: Read informational messages.
             Step 9: Read informational messages.

             The VAX PCA installation procedure produces a number of
             informational messages that report on the progress of the
             installation.




                                                                        13

 






             The success of the installation is indicated by the following
             message:

               %VMSINSTAL-I-MOVEFILES, files will now be moved to their target
                     directories...

             If the installation procedure is successful, the new or
             modified files are moved to their target directories.

             The SYS$HELP:HELPLIB.HLB and SYS$LIBRARY:DCLTABLES.EXE files
             are updated to include the new versions of the VAX PCA HELP
             text and the PCA command line definition.

             This installation will add the following files:

              o SYS$SYSTEM:PCA$ANALYZER.EXE

              o SYS$LIBRARY:PCA$COLLECTOR.EXE

              o SYS$LIBRARY:PCA$OBJ.OBJ

              o SYS$HELP:PCA030.RELEASE_NOTES

              o SYS$HELP:PCA$HELP.HLB

              o DECW$SYSTEM_DEFAULTS:PCAC$UID.UID

              o DECW$SYSTEM_DEFAULTS:PCAA$UID.UID

              o SYS$HELP:PCA$DWHELP.HLB

              o SYS$MESSAGE:PCA$MSG.MSG

              o SYS$STARTUP:PCA$STARTUP.COM

              o SYS$COMMON:[SYSTEST]PCA.DIR

              o VUE$LIBRARY:*.COM (PCA VUE Files)

              o SYS$COMMON:[SYSTEST.PCA]*.*

              o SYS$TEST:PCA$IVP.COM

             The VAX PCA Version 3.0 installation optionally adds or
             replaces the SYS$COMMON:[SYSHLP.EXAMPLES.PCA] directory and
             its contents.

          14

 






             If you typed YES in response to the prompt that requests a
             file purge at step 7, previous versions of the VAX PCA files
             are now purged.


             Step 10: Observe the Installation Verification Procedure.
             Step 10: Observe the Installation Verification Procedure.
             Step 10: Observe the Installation Verification Procedure.

             If you chose to run the IVP in step 7, VMSINSTAL now calls
             the IVP to verify that VAX PCA was successfully installed.

             If VAX PCA has been successfully installed, the IVP displays
             the following:

               Running the IVP...

               The IVP ran successfully for VAX PCA Version V3.0

             If you answered NO to the LMF question in step 6, you can run
             the IVP after installation, and after loading and registering
             the PCA license.

             To execute the IVP command procedure, enter the following
             command:

               $ @SYS$TEST:PCA$IVP<RETURN>

             Step 11: End the installation procedure.
             Step 11: End the installation procedure.
             Step 11: End the installation procedure.

                  Installation of VAX PCA V3.0 completed at hh:mm

                  VMSINSTAL procedure done at hh:mm

               $ LOGOUT <RETURN>
               SYSTEM     logged out at dd-mmm-yyyy hh:mm:ss.ss

             When the product installation procedure is complete, you
             can choose to install more products or to log out (as shown
             here.) If you removed any media from the console drive before
             beginning the installation, you should replace it now.

                                                                        15

 






             VMSINSTAL deletes or changes entries in the process symbol
             tables during the installation. Therefore, if you are going
             to continue using the system manager's account and you want
             to restore these symbols, you should log out and log in
             again.

          __________________________________________________________

          2.1  Installing VAX PCA on a VAXcluster
          2.1  Installing VAX PCA on a VAXcluster
          2.1  Installing VAX PCA on a VAXcluster

             If you want to run VAX PCA on multiple nodes of a VAXcluster,
             first check to see that you have the appropriate software
             license. Then, follow these steps after installing VAX PCA:

              1. Issue the LICENSE LOAD command to activate the license
                on each node in the VAXcluster on which VAX PCA is to
                be executed as described in the
                                                ___ _______ __________
                                                VMS License Management
                              .
                _______ ______
                Utility Manual

              2. Execute PCA$STARTUP.COM on each node of the cluster that
                has a software license.

              3. To use the product on other nodes in the VAXcluster,
                you must replace the version of the DCL tables that is
                installed on the other VAXcluster nodes. To do this,
                perform the following steps:

                 a. Log in to a node on the cluster.

                 b. Run INSTALL and enter the following command at the
                   INSTALL> prompt:

                             INSTALL> REPLACE SYS$LIBRARY:DCLTABLES.EXE <RETURN>

                 c. Repeat steps a and b for each node of the cluster.




          16

 





          __________________________________________________________

          3  After the Installation
          3  After the Installation
          3  After the Installation

             VAX PCA is now installed and can be invoked by all users with
             the PCA command.

             The installation procedure modifies the DCL command table so
             that the PCA command is recognized and processed. However,
             the previous command table is still in effect for those users
             who are currently logged in. All logged-in users who want
             to use the PCA command must log out of the system and log in
             again.

             To reinstall VAX PCA at system boot time, modify the system-
             specific startup procedure. Include the following line in the
             SYS$STARTUP:SYSTARTUP_V5.COM file:

               @SYS$STARTUP:PCA$STARTUP.COM

             The PCA$STARTUP.COM file contains commands to install
             PCA$COLLECTOR.EXE. The VAX PCA installation procedure puts
             the PCA$STARTUP.COM file in the SYS$STARTUP directory.

          __________________________________________________________

          4  Running the Installation Verification Procedure Separately
          4  Running the Installation Verification Procedure Separately
          4  Running the Installation Verification Procedure Separately

             The Installation Verification Procedure (IVP) is usually run
             at installation. If you want to run the IVP separately to
             ensure the integrity of installed files if system problems
             occur, execute the following command procedure:

               $  @SYS$TEST:PCA$IVP<RETURN>

             If the IVP fails for any reason, the following messages are
             displayed:

               The VAX PCA V3.0 Installation Verification Procedure failed.

               %VMSINSTAL-E-IVPFAIL, The IVP for VAX PCA V3.0 has failed.

                                                                        17

 





          __________________________________________________________

          5  Error Conditions
          5  Error Conditions
          5  Error Conditions

             If the installation procedure fails for any reason, a message
             like the one following is displayed:

               %VMSINSTAL-E-INSFAIL, The installation of VAX PCA V3.0 has failed.

             An error during the installation can occur if one or more of
             the following conditions exist:

              o Operating system version is incorrect.

              o Prerequisite software version is incorrect.

              o Quotas necessary for successful installation are in-
                sufficient (see the Installation Procedure Requirements
                section).

              o Process quotas required by VMSINSTAL are incorrect (see
                the Using VMSINSTAL section).

              o The VMS HELP library is currently in use.

              o The product license was registered incorrectly or not
                registered.

             For descriptions of the error messages generated by these
             conditions, see the
                                 ___ ______ ________ ___ ________
                                 VMS System Messages and Recovery
                                        , your processor-specific in-
             __________ _________ ______
             Procedures Reference Volume
             stallation/operations guide, or the
                                                 ___ _______ __________
                                                 VMS License Management
                           .
             _______ ______
             Utility Manual

             If you are notified that any of these conditions exist, you
             should take the appropriate action as described in the mes-
             sage. You may need to change a system parameter or increase
             an authorized quota value.

             If the installation fails, you must restart the installation
             procedure from step 2. If the installation fails due to an
             IVP failure, contact a Digital field service representative.

          18

 





          __________________________________________________________

          6  Maintenance Updates
          6  Maintenance Updates
          6  Maintenance Updates

             Digital may periodically issue maintenance updates of VAX
             PCA. Each update consists of an installation kit. You should
             install this kit as described in this document or in any
             documentation that may accompany the maintenance update.

             Each time a maintenance update is released, the version
             number changes. For example, if the current version is 1.0,
             the version number of the first maintenance update will
             be 1.1. In addition, each maintenance update includes new
             release notes. The release notes describe the changes that
             have been made to VAX PCA since the previous release.

             The update release notes are provided on line. You should
             read the release notes when you first install VAX PCA;
             they are also accessible at any time after the product is
             installed. For information on reading the release notes
             at the time that you install VAX PCA, follow the instal-
             lation procedure through step 5. To locate the release
             notes after VAX PCA is installed, display or print the file
             SYS$HELP:PCA030.RELEASE_NOTES, or type the following command
             :

               $ HELP PCA RELEASE_NOTES <RETURN>

          __________________________________________________________

          7  Improving Product Performance
          7  Improving Product Performance
          7  Improving Product Performance

             The PCA Collector uses memory resources to gather the speci-
             fied data. To minimize the effect of this memory usage on the
             behavior of the program, especially paging behavior, you can
             add 600 pages to the process working set. This is approxi-
             mately the number of pages the Collector uses while gathering
             data. Further, you can also increase the virtual page count
             by 1800 pages.

                                                                        19

 





          __________________________________________________________

          8  Determining and Reporting Problems
          8  Determining and Reporting Problems
          8  Determining and Reporting Problems

             If an error occurs while you are using VAX PCA and you be-
             lieve that the error is caused by a problem with VAX PCA,
             take one of the following actions:

              o If you purchased VAX PCA within the past 90 days and you
                think the problem is caused by a software error, you can
                submit a Software Performance Report (SPR).

              o If you have a Basic or DECsupport Software Agreement,
                you should call your Customer Support Center. With these
                services, you receive telephone support that provides
                high-level advisory and remedial assistance. For more
                information, contact your local Digital representative.

              o If you have a Self-Maintenance Software Agreement, you can
                submit a Software Performance Report (SPR).

             If you find an error in the VAX PCA documentation, you should
             fill out and submit a Reader's Comments form from the back
             of the document in which the error was found. Include the
             section and page number where the error was found.

          __________________________________________________________

          9  Sample Installation
          9  Sample Installation
          9  Sample Installation

             This section contains three sample installations of VAX PCA:
             the first sample is an installation with PCA's authorization
             key registered and loaded and running the IVP; the second
             sample is an installation with PCA's authorization key reg-
             istered and loaded and without running the IVP; the third
             sample is an installation without PCA's authorization key
             registered and loaded.

             Note that these are only samples. Sometimes the installation
             procedure is modified in maintenance updates of this prod-
             uct. Because this installation guide is not usually revised
             for maintenance updates, be sure to read the
                                                          ____ ______
                                                          Read Before
                                         letter before you install this
             __________ __ _____ ___ ___
             Installing or Using VAX PCA

          20

 






             product. This letter notes any significant changes in the
             installation that vary from this sample.

          __________________________________________________________

          9.1  Sample 1 for Installation with PCA Authorization Key and
          9.1  Sample 1 for Installation with PCA Authorization Key and
          9.1  Sample 1 for Installation with PCA Authorization Key and
               the IVP
               the IVP
               the IVP

          $  @SYS$UPDATE:VMSINSTAL PCA030 PCA$KIT

                VAX/VMS Software Product Installation Procedure V5.3

           VAX/VMS Software Product Installation Procedure V5.3

          It is 15-MAR-1990 at 13:48.

          Enter a question mark (?) at any time for help.
          %VMSINSTAL-W-NOTSYSTEM, You are not logged in to the SYSTEM account.
          %VMSINSTAL-W-ACTIVE, The following processes are still active:
           DECW$WM_1
          * Do you want to continue anyway [NO]? y
          * Are you satisfied with the backup of your system disk [YES]?

          The following products will be processed:

            PCA V3.0

           Beginning installation of PCA V3.0 at 13:49

          %VMSINSTAL-I-RESTORE, Restoring product save set A ...
          %VMSINSTAL-I-RELMOVED , The product's release notes have been successfully
                    moved to SYS$HELP.

              *** PCA V3.0 installation procedure. ***

                  Product:      PCA
                  Producer:     DEC
                  Version:      3.0
                  Release Date: 10-AUG-1990

                                                                        21

 






          * Does this product have an authorization key registered and loaded? Yes
          * Do you want to run the IVP after the installation [YES]?
          * Do you want to purge files replaced by this installation [YES]?
          * Do you want to install the PCA demo package [YES]:

              You have answered all the questions required for this installation.
              The installation will now continue for about 5 to 25 minutes without
              further intervention, depending on your system's configuration, the
              installation media, and the options you have selected.

          %VMSINSTAL-I-RESTORE, Restoring product save set B ...
          %VMSINSTAL-I-RESTORE, Restoring product save set C ...
          %VMSINSTAL-I-SYSDIR, This product creates system disk directory
                       VMI$ROOT:[SYSTEST.PCA].
          %VMSINSTAL-I-RESTORE, Restoring product save set D ...
          %VMSINSTAL-I-SYSDIR, This product creates system directory
                  [SYSHLP.EXAMPLES.PCA].

              If you intend to execute this layered product on other nodes in your
              VAXcluster, and you have the appropriate software license, you must
              prepare the system-specific roots on the other nodes by issuing the
              following command on each node (using a suitably privileged account):

           $ CREATE /DIRECTORY SYS$SPECIFIC:[SYSHLP.EXAMPLES.PCA]

          The name of the PCA startup command file is: PCA$STARTUP.COM in the
          SYS$STARTUP directory area.

          In order to start up PCA when your system boots, you should add the
          following line to your system startup procedure:

           $ @SYS$STARTUP:PCA$STARTUP.COM

          The release notes are available online by typing HELP PCA RELEASE_NOTES.

          %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...

              Starting the IVP procedure for VAX PCA Version V3.0

              The IVP procedure is complete for VAX PCA Version V3.0

                The IVP ran successfully for VAX PCA Version V3.0

           Installation of PCA V3.0 completed at 14:08

          22

 






           VMSINSTAL procedure done at 14:09

          __________________________________________________________

          9.2  Sample 2 for Installation with PCA Authorization Key
          9.2  Sample 2 for Installation with PCA Authorization Key
          9.2  Sample 2 for Installation with PCA Authorization Key
               without the IVP
               without the IVP
               without the IVP

          $  @SYS$UPDATE:VMSINSTAL PCA030 PCA$KIT

                VAX/VMS Software Product Installation Procedure V5.3

           VAX/VMS Software Product Installation Procedure V5.3

          It is 15-MAR-1990 at 14:09.

          Enter a question mark (?) at any time for help.

          %VMSINSTAL-W-NOTSYSTEM, You are not logged in to the SYSTEM account.
          %VMSINSTAL-W-ACTIVE, The following processes are still active:
           DECW$WM_1
          * Do you want to continue anyway [NO]? y
          * Are you satisfied with the backup of your system disk [YES]?

          The following products will be processed:

            PCA V3.0

           Beginning installation of PCA V3.0 at 14:09

          %VMSINSTAL-I-RESTORE, Restoring product save set A ...
          %VMSINSTAL-I-RELMOVED , The product's release notes have been successfully
                   moved to SYS$HELP.

              *** PCA V3.0 installation procedure. ***

                  Product:      PCA
                  Producer:     DEC
                  Version:      3.0
                  Release Date: 10-AUG-1990

          * Does this product have an authorization key registered and loaded? Yes
          * Do you want to run the IVP after the installation [YES]? No
          * Do you want to purge files replaced by this installation [YES]?
          * Do you want to install the PCA demo package [YES]:

                                                                        23

 






              You have answered all the questions required for this installation.
              The installation will now continue for about 5 to 25 minutes without
              further intervention, depending on your system's configuration, the
              installation media, and the options you have selected.

          %VMSINSTAL-I-RESTORE, Restoring product save set B ...
          %VMSINSTAL-I-RESTORE, Restoring product save set C ...
          %VMSINSTAL-I-SYSDIR, This product creates system disk directory
                       VMI$ROOT:[SYSTEST.PCA].
          %VMSINSTAL-I-RESTORE, Restoring product save set D ...
          %VMSINSTAL-I-SYSDIR, This product creates system directory
                       [SYSHLP.EXAMPLES.PCA].

              If you intend to execute this layered product on other nodes in your
              VAXcluster, and you have the appropriate software license, you must
              prepare the system-specific roots on the other nodes by issuing the
              following command on each node (using a suitably privileged account):

           $ CREATE /DIRECTORY SYS$SPECIFIC:[SYSHLP.EXAMPLES.PCA]

          The name of the PCA startup command file is: PCA$STARTUP.COM in the
          SYS$STARTUP directory area.

          In order to start up PCA when your system boots, you should add the
          following line to your system startup procedure:

           $ @SYS$STARTUP:PCA$STARTUP.COM

          The release notes are available online by typing HELP PCA RELEASE_NOTES.

          %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...
           Installation of PCA V3.0 completed at 14:32

           VMSINSTAL procedure done at 14:32





          24

 





          __________________________________________________________

          9.3  Sample 3 for Installation without PCA Authorization Key
          9.3  Sample 3 for Installation without PCA Authorization Key
          9.3  Sample 3 for Installation without PCA Authorization Key

               $  @SYS$UPDATE:VMSINSTAL PCA030 PCA$KIT

                     VAX/VMS Software Product Installation Procedure V5.3

               It is 15-MAR-1990 at 14:45.

               Enter a question mark (?) at any time for help.

               %VMSINSTAL-W-NOTSYSTEM, You are not logged in to the SYSTEM account.
               %VMSINSTAL-W-ACTIVE, The following processes are still active:
                DECW$WM_1
               * Do you want to continue anyway [NO]? y
               * Are you satisfied with the backup of your system disk [YES]? y

               The following products will be processed:

                 PCA V3.0

                Beginning installation of PCA V3.0 at 14:46

               %VMSINSTAL-I-RESTORE, Restoring product save set A ...
               %VMSINSTAL-I-RELMOVED , The product's release notes have been successfully
                         moved to SYS$HELP.

                   *** PCA V3.0 installation procedure. ***

                       Product:      PCA
                       Producer:     DEC
                       Version:      3.0
                       Release Date: 10-AUG-1990

               * Does this product have an authorization key registered and loaded? No

               %PCA-W-PCA$NOIVP, PCA's IVP will not be run, because license not registered.

               %PCA-I-PCA$IVP, It is recommended that the IVP be run after the license has
                             been registered.

               %PCA-I-PCA$IVP,               Installation continuing

               * Do you want to purge files replaced by this installation [YES]?
               * Do you want to install the PCA demo package [YES]:

                                                                        25

 






                   You have answered all the questions required for this installation.
                   The installation will now continue for about 5 to 25 minutes without
                   further intervention, depending on your system's configuration, the
                   installation media, and the options you have selected.

               %VMSINSTAL-I-RESTORE, Restoring product save set B ...
               %VMSINSTAL-I-RESTORE, Restoring product save set C ...
               %VMSINSTAL-I-SYSDIR, This product creates system disk directory
                         VMI$ROOT:[SYSTEST.PCA].

               The name of the PCA IVP Procedure is: PCA$IVP.COM in the
               SYS$TEST directory area.

               In order to execute the IVP enter the command:

                                  @SYS$TEST:PCA$IVP.COM

               %VMSINSTAL-I-RESTORE, Restoring product save set D ...
               %VMSINSTAL-I-SYSDIR, This product creates system directory
                               [SYSHLP.EXAMPLES.PCA].

                   If you intend to execute this layered product on other nodes in your
                   VAXcluster, and you have the appropriate software license, you must
                   prepare the system-specific roots on the other nodes by issuing the
                   following command on each node (using a suitably privileged account):

                $ CREATE /DIRECTORY SYS$SPECIFIC:[SYSHLP.EXAMPLES.PCA]

               The name of the PCA startup command file is: PCA$STARTUP.COM in the
               SYS$STARTUP directory area.

               In order to start up PCA when your system boots, you should add the
               following line to your system startup procedure:

                $ @SYS$STARTUP:PCA$STARTUP.COM

               The release notes are available online by typing HELP PCA RELEASE_NOTES.

               %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...
                Installation of PCA V3.0 completed at 15:08

                VMSINSTAL procedure done at 15:08

          26
