 















             VAX VTX
             Installation Guide

             Order Number: AA-FS81F-TE



             This guide explains how to install VAX VTX and run the
             Installation Verification Procedure.





             Revision/Update Information:  This is a revised manual.

             Operating System:             VMS

             Software Version:             VAX VTX Version 4.1








             digital equipment corporation
             maynard, massachusetts

 



             ___________________________________________________

             April 1990

             The information in this document is subject to change without
             notice and should not be construed as a commitment by Digital
             Equipment Corporation. Digital Equipment Corporation assumes
             no responsibility for any errors that may appear in this
             document.

             The software described in this document is furnished under a
             license and may be used or copied only in accordance with the
             terms of such license.

             © Digital Equipment Corporation 1989.

             All Rights Reserved.
             Printed in U.K.

             The postpaid Reader's Comments forms at the end of this docu-
             ment request your critical evaluation to assist in preparing
             future documentation.

             The following are trademarks of Digital Equipment Corporation:

             ALL-IN-1         PDP              VMS
             DEC              Professional     VT
             DECmate          Rainbow          VTX20
             DECnet           ReGIS            WPS-PLUS
             DECtalk          UNIBUS
             DECUS            VAX
             DECwindows       VAX VTX
             DECwrite         VAXstation       DIGITAL

             IBM[R] is a registered trademark of International Business
             Machines Corporation.
             CROSSTALK XVI[TM] is a trademark of MicrosTuf, Inc.
             Mark IV[TM] is a trademark of Norpak Corporation, Ontario,
             Canada.
             SONY[TM] is a trademark of Sony Corporation.
             Minitel[TM] is a trademark of Intelmatique, France.
             MS-DOS[TM] is a registered trademark of MicroSoft Corporation.

 















                                                                  Contents
          ________________________________________________________________

          Preface .........................................................    
vii


          ________________________________________________________________
          Chapter 1  Preparing to Install VAX VTX

               1.1   Required Operating System Components............  1-1

               1.2   Prerequisite Software............................. 1-2

               1.3   Optional Software.................................. 1-2

               1.4   Prerequisite Hardware............................. 1-2

               1.5   VAX VTX Licensing.................................. 1-3
                     1.5.1 License Management......................... 1-3

               1.6   Installation Procedure Requirements.............  1-4
                     1.6.1 Media........................................ 1-4
                     1.6.2 Time......................................... 1-4
                     1.6.3 Privileges.................................. 1-4
                     1.6.4 Disk Space.................................. 1-5
                     1.6.5 System Parameters.......................... 1-6
                           1.6.5.1VIRTUALPAGECNT ..................... 1-6
                           1.6.5.2CTLPAGES ............................ 1-6



                                                                       iii

 






                     1.6.6 GBLPAGES and GBLSECTIONS..................  1-7
                           1.6.6.1Checking System Parameter
                                  Values............................... 1-8
                           1.6.6.2Changing System Parameter Values
                                  with AUTOGEN........................ 1-9
                     1.6.7 Page File Quota............................ 1-10
                     1.6.8 Process Account Quotas.................... 1-10
                     1.6.9 VMSINSTAL Requirements.................... 1-12
                     1.6.10 Backing Up Your System Disk.............. 1-13
                     1.6.11 VAX VTX Requirements ...................... 1-13
                     1.6.12 IVP Requirements........................... 1-13
                     1.6.13 The VAX VTX VISTA Utility ................ 1-14
                     1.6.14 Converting Previous VTX Files to VAX
                           VTX Version 4.0 Format.................... 1-14


          ________________________________________________________________
          Chapter 2  Installing VAX VTX

               2.1   General Information ............................... 2-1
                     2.1.1 Accessing the Online Release Notes......    2-1
                     2.1.2 Running the Installation Verification
                           Procedure (IVP)............................ 2-2
                     2.1.3 Aborting the Installation ................  2-2

               2.2   The Installation Procedure ....................... 2-2
                     2.2.1 Invoking VMSINSTAL......................... 2-3
                     2.2.2 Installation Questions....................  2-4
                     2.2.3 Informational Messages.................... 2-17
                     2.2.4 Running the Installation Verification
                           Procedure................................... 2-17
                     2.2.5 Completing the Installation Procedure ..   2-18

               2.3   Installing the MS-DOS TCP on Your Personal
                     Computer ............................................    
2-18

               2.4   Error Recovery .....................................   2-23


          iv

 






          ________________________________________________________________
          Chapter 3  After Installing VAX VTX

               3.1   Establishing a VAX VTX Print Queue..............  3-1
                     3.1.1 Editing the System Startup File .........   3-2
                     3.1.2 Configuring Print Tables for
                           VTX$QUEUE................................... 3-2
                     3.1.3 DCLTABLES................................... 3-5

               3.2   Cluster Considerations............................ 3-5

               3.3   Subscriber Account Privileges and Quotas.......   3-6
                     3.3.1 Privileges.................................. 3-6
                     3.3.2 Account Quotas ............................. 3-6

               3.4   Defining System Logicals.......................... 3-7

               3.5   DECnet...............................................   3-8
                     3.5.1 Establishing a DECnet Node ...............  3-8
                     3.5.2 Starting DECnet............................ 3-8

               3.6   Creating a VTX Operator Account ................. 3-10

               3.7   Using Search Lists.................................  3-12

               3.8   Enhancing VAX VTX Performance.................... 3-12
                     3.8.1 Tuning Your System......................... 3-13
                     3.8.2 Installing VAX VTX as a Shared Image....   3-13

               3.9   Deleting the [.VTX$VISTA] Subdirectory ......... 3-17

               3.10  Print Queue and Workbench Output Files
                     Directory...........................................   3-17

               3.11  Workbench Server Command Procedure Changes.....  3-18

               3.12  VAS Command Procedure Changes.................... 3-18


                                                                         v

 






               3.13  Determining and Reporting Problems.............. 3-18


          ________________________________________________________________
          Chapter 4  Installation Verification Procedure

               4.1   Running the VAX VTX IVP........................... 4-2

               4.2   Performing the Optional Part of the IVP........   4-3

               4.3   Conclusion..........................................  4-5

          ________________________________________________________________
          Appendix A Sample Installation


          ________________________________________________________________
          Appendix B VTX Files and Logical Names Installed on Your
                     System

               B.1   File Names..........................................  B-1
                     B.1.1 SYS$COMMON:[ELKLIB] ....................... B-1
                     B.1.2 SYS$COMMON:[RUSLLIB] ...................... B-2
                     B.1.3 SYS$COMMON:[SYS$STARTUP]..................  B-3
                     B.1.4 SYS$COMMON:[SYSEXE] ....................... B-3
                     B.1.5 SYS$COMMON:[SYSHLP] ....................... B-4
                     B.1.6 SYS$COMMON:[SYSLIB] ....................... B-5
                     B.1.7 SYS$COMMON:[SYSMSG] ....................... B-6
                     B.1.8 SYS$COMMON:[SYSTEST.VTX]..................  B-6
                     B.1.9 SYS$COMMON:[SYSTEST] ...................... B-7
                     B.1.10 SYS$COMMON:[TCPLIB] ....................... B-7
                     B.1.11 SYS$COMMON:[VASLIB] ....................... B-11
                     B.1.12 SYS$COMMON:[VTX$LIBRARY].................. B-12

               B.2   Logical Names ......................................   B-13




          vi

 






          ________________________________________________________________
          Index

          ________________________________________________________________
          Tables

               1-1   Disk Space Requirements........................... 1-5

               1-2   Process Account Quotas for the Installing
                     Account .............................................    
1-11

               2-1   Files Made Obsolete by Installation
                     Procedure...........................................   2-15

               3-1   Subscriber Account Quotas for Using VAX VTX ...   3-6

               3-2   Required System Parameter Values ................ 3-13

               3-3   Workbench Server Command Procedure Changes.....  3-18




















                                                                       vii

 














                                                                   Preface
          ________________________________________________________________


          ____________________________________________________________

          Purpose of This Manual

             This manual explains how to install and verify VAX VTX
             Version 4.1. The installation procedure uses VMSINSTAL.

          ____________________________________________________________

          Intended Audience

             This manual is intended for anyone responsible for installing
             and maintaining a VAX VTX system. To install this product,
             you must have access to a privileged system manager account.

          ____________________________________________________________

          Operating System Information

             To verify which versions of your operating system are compat-
             ible with this version of VAX VTX, check the Software Product
             Description (SPD) which is included in the VAX VTX kit.





                                                                       vii

 





          ____________________________________________________________

          Structure of This Manual

             This manual is organized as follows:

             Chapter 1        Describes the preparations you must complete
                              before you can install VAX VTX Version 4.1.

             Chapter 2        Describes the VAX VTX Version 4.1 installa-
                              tion procedure and how to install the MS-DOS
                              TCP on a Personal Computer.

             Chapter 3        Describes the tasks you must complete after
                              you install VAX VTX Version 4.1.

             Chapter 4        Contains more detailed information about
                              running the Installation Verification
                              Procedure (IVP).

             Appendix A       Contains a sample VAX VTX Version 4.1 in-
                              stallation.

             Appendix B       Lists the files and system logicals in-
                              stalled on the system during the VAX VTX
                              installation.

          ____________________________________________________________

          Related Documentation

             The documentation set for VAX VTX consists of:

                VAX VTX Installation Guide
                VAX VTX Guide to Designing and Implementing an Infobase
                VAX VTX Information Provider's Guide
                VAX VTX Operator's Guide
                VAX VTX Guide to Modifying the Terminal Control Program
                (TCP)
                VAX VTX Subscriber's Booklet
                VAX VTX/VALU Summary Description

          viii

 






                VAX VTX/VALU Guide to Using VAS
                VAX VTX/VALU Guide to Using RUSL
                VAX VTX/VALU Guide to Using ELK

             VAX VTX Version 4.1 also comes with online release notes,
             which you can access in SYS$HELP:VTX041.RELEASE_NOTES.

             A glossary for all the VAX VTX manuals is contained in the
             VAX VTX Guide to Designing and Implementing an Infobase. A
             glossary for all the VAX VTX/VALU manuals is contained in the
             VAX VTX/VALU Summary Description.

             For more information about the License Management Utility
             (LMF), VMSINSTAL, or modifying account quotas see the VMS
             documentation set. For more information about using AUTOGEN,
             see the VMS System Management Subkit.

          ____________________________________________________________

          Conventions

             $             The system prompt. It indicates that the VMS
                           command interpreter is ready for command input.

             .
             .             Information not directly related to the example
             .             has been omitted.

             <Return>      Press the Return key.

                           Shows user input. All characters the system
                           prints or displays are in black.
             Red print

             <Ctrl/x>      Indicates that you press the Ctrl key and
                           another key.



                                                                        ix

 

















                                                                      Chapter 1


                                                   Preparing to Install VAX VTX
               ________________________________________________________________


                  This chapter discusses the preparations and requirements
                  necessary for installing VAX VTX.

                  Your bill of materials (BOM) and indented bills report (BIL)
                  specify the number and contents of your media. Be sure to
                  verify the contents of your kit with this information. If
                  your kit is damaged or if parts are missing, contact your
                  Digital representative.

                  VAX VTX provides online release notes. Digital strongly
                  recommends that you read the release notes before you proceed
                  with the installation.

               ____________________________________________________________

               1.1  Required Operating System Components

                  Before you attempt to install VAX VTX, you must be running
                  VMS Version 5.1 (or higher) on your system. The following VMS
                  tailoring classes are required to enable the full capabili-
                  ties of VAX VTX:

                   o VMS Required Saveset

                   o NETWORK Support

                   o PROGRAMMING Support





                                              Preparing to Install VAX VTX  1-1

 











                   o Secure User's Environment

                   o Utilities

                  DECwindows is required only if you will be using VAX VTX
                  through the DECwindows interface.

               ____________________________________________________________

               1.2  Prerequisite Software

                  If you are using the VAS component of VAX VTX in an IBM or
                  IBM-compatible environment, you must install DECnet/SNA VMS
                  APPL/LU6.2 Version 2.0 (or higher) before you install VAX
                  VTX.

               ____________________________________________________________

               1.3  Optional Software

                  The following Digital software products are compatible with
                  VAX VTX Version 4.1 and can be used with it:

                   o DECnet-VAX V5.3

                   o WPS-PLUS Version 3.1

                   o ALL-IN-1 Version 2.3

                   o VAX BLISS-32 V4.6

                   o VAX P.S.I. Access Version 4.2

                   o DECnet/SNA VMS APPL/LU6.2 Version 2.0

                   o DECnet/SNA VMS 3270 Data Stream Programming Interface
                     Version 1.4

                  See the System Software Addendum (SSA) for a complete list of
                  compatible products and their required version numbers. The
                  SSA is part of the Software Product Description (SPD).

               ____________________________________________________________

               1.4  Prerequisite Hardware

                  The VAX VTX Installation Verification Procedure (IVP) is
                  provided in two parts. You need only a hardcopy terminal to
                  run the first part, but you must use a video terminal to run
                  the second part. See Chapter 4 for additional information on
                  the IVP.

               1-2  Preparing to Install VAX VTX

 










               ____________________________________________________________

               1.5  VAX VTX Licensing

                  The terms and conditions of your license agreement determine
                  your legal use of the VAX VTX software; the License Managment
                  Facility (LMF) is a management tool that helps you to comply
                  with this license agreement. This section describes the
                  types of licenses offered for VAX VTX, the things you need to
                  consider when deciding which VTX licenses to purchase, and
                  how to use LMF to register and manage your VTX licenses.

                  Two types of licensing are offered for VAX VTX: Activity
                  licensing and Availability licensing. With either type of
                  licensing, you obtain the right to run one or more VAX VTX
                  Servers and Update Servers on a system. In some special con-
                  figurations, you may also need one of the forms of licensing
                  to run an ELK application on a system.

               ____________________________________________________________

               1.5.1  License Management

                  With the VMS License Management Facility (LMF), you can do
                  the
                  following:

                   o Register a VTX software license Product Authorization Key
                     (PAK) in the LICENSE database

                   o Register additional availability or activity license PAKs

                   o Activate the license information to authorize a product
                     for use

                   o Display current and previous license data

                   o Include and exclude product access on nodes in a
                     VAXcluster
                     environment

                   o Move a software license to another system

                  Refer to the VMS License Management Utility Manual for more
                  information on these operations.

                                              Preparing to Install VAX VTX  1-3

 










               ____________________________________________________________

               1.6  Installation Procedure Requirements

                  The following subsections discuss various requirements for
                  installing VAX VTX.

               ____________________________________________________________

               1.6.1  Media

                  VAX VTX ships on either one TK50 or one magtape, depending on
                  your system configuration.

               ____________________________________________________________

               1.6.2  Time

                  The installation takes approximately 20 minutes to 4 hours
                  20 minutes, depending on the type of media you are using and
                  your system configuration.

                  Installing the complete VAX VTX kit, including the TCP
                  sources, and running the IVP on a standalone VAX 8820 system
                  takes 20 minutes.

               ____________________________________________________________

               1.6.3  Privileges

                  To install VAX VTX, you must log into an account that has
                  SETPRV or an account with at least the following privileges:

                     CMKRNL
                     WORLD
                     SYSPRV
                     SYSNAM
                     GROUP
                     GRPNAM
                     NETMBX
                     TMPMBX

                                               NOTE

                      VMSINSTAL turns off the BYPASS privilege at the start
                      of the installation.

               1-4  Preparing to Install VAX VTX

 










               ____________________________________________________________

               1.6.4  Disk Space

                  Installing VAX VTX requires a certain amount of free storage
                  disk space during the installation. After you install VAX
                  VTX, the product requires less storage space. Table 1-1
                  summarizes the storage requirements for each of the VAX VTX
                  installation options.

                  Table 1-1:  Disk Space Requirements
                  _____________________________________________________________
                                          Blocks During    Blocks After
                  Kit_____________________Installation_____Installation________

                  Subscriber Interface    10800            4700
                  only

                  Full VAX VTX kit        21500            8700

                  Full VAX VTX kit with   41000            22000
                  TCP_source_code______________________________________________

                  For additional information on the TCP source code option,
                  see the Installing the TCP source code part of step 5 in
                  Section 2.2.2.

                  If you choose to do the conversational installation, the
                  following disk space is needed:

                   o Front-End only (4700 blocks)

                   o Information Provider Tools (2200 blocks)

                   o Information Provider Conversion Tools (200 blocks)

                   o VTX Servers (1000 blocks)

                   o VAS and ELK (600 blocks)

                   o TCP source code (13000 blocks)

                  To determine the number of free disk blocks on the current
                  system disk, enter the following command at the DCL prompt:

                    $ SHOW DEVICE SYS$SYSDEVICE <Return>

                                              Preparing to Install VAX VTX  1-5

 










               ____________________________________________________________

               1.6.5  System Parameters

                  Installing VAX VTX requires certain system parameters. The
                  following subsections describe the system parameters that you
                  may need to update.

               ____________________________________________________________

               1.6.5.1  VIRTUALPAGECNT

                  This must be set to at least 35,000 on your system. Please
                  refer to Section 1.6.6.1 for information on how to verify and
                  update a system parameter.

               ____________________________________________________________

               1.6.5.2  CTLPAGES

                  The process from which you plan to install VTX must have at
                  least 42 free CTLPAGES. You can verify the number of free
                  CTLPAGES by issuing the following command at the DCL prompt:

                    $ SHOW PROCESS/MEMORY <Return>

                  The following information is displayed:

                    26-APR-1990 11:23:25.55  User: USER1      Process ID:   
27C004E5
                                             Node: NODE1      Process name: 
"USER1_8"
                    Process Dynamic Memory Area
                       Current Size (bytes)      768000   Current Total Size 
(pages)  1500
                       Free Space (bytes)        755736   Space in Use (bytes)   
    12264
                       Size of Largest Block     755664   Size of Smallest Block 
       24
                       Number of Free Blocks          3   Free Blocks LEQU 32 
Bytes      1

                  The value of interest is "Free Space". In the example shown,
                  the process has 755736 bytes free which is equivalent to
                  755736/512 = 1476 full pages. If you have 42 or more free
                  pages (21504 bytes) you do not need to change anything. If
                  you have less than 42 free pages, you need to increase the
                  value of your CTLPAGES. The value you need on your CTLPAGES
                  is:

                        ((Your_free_space + 511) / 512) + 42.

                  Refer to Section 1.6.6.2 for information on how to update a
                  system parameter.

               1-6  Preparing to Install VAX VTX

 











                       IF YOUR CTLPAGES IS VERY CLOSE TO THE REQUIRED VALUE

                      CTLPAGES are used, for example, when defining process
                      logical names. If you are close to the required value,
                      log in to a new process and verify your free CTLPAGES.
                      If the value from the new process is also close to the
                      required value, you should perform the installation
                      from a new process.

               ____________________________________________________________

               1.6.6  GBLPAGES and GBLSECTIONS

                  The installation updates your DCLTABLES and requires at
                  least n + 40 free GBLPAGES, where n is the size of your
                  DCLTABLES.EXE which you can display by typing:

                    $ DIRECTORY/SIZE SYS$SHARE:DCLTABLES.EXE <Return>

                  In the following example, the value of n is 786. Therefore,
                  you need at least 786 + 40 = 826 GBLPAGES free. You will also
                  need at least 1 GBLSECTIONS free.

                    Directory SYS$COMMON:[SYSLIB]

                    DCLTABLES.EXE;439       786

                    Total of 1 file, 786 blocks.

                  The GBLPAGES and GBLSECTIONS parameters can be checked with
                  the INSTALL utility. In the following example, there are
                  19690 free GBLPAGES:

                    $ INSTALL LIST /GLOBAL /SUMMARY <Return>

                        Summary of Local Memory Global Sections

                        380 Global Sections Used,  35310/19690 Global Pages 
Used/Unused
                    $

                  Use the SYSGEN utility (see Section 1.6.6.1) to verify that
                  the GBLSECTIONS value is sufficient; that is, GBLSECTIONS is
                  at least 1 greater than the value shown for Global Sections
                  Used.

                                              Preparing to Install VAX VTX  1-7

 










               ____________________________________________________________

               1.6.6.1  Checking System Parameter Values

                  To check the values of your system parameters, invoke the
                  System Generation Utility by entering the following command
                  at the DCL prompt:

                    $ RUN SYS$SYSTEM:SYSGEN <Return>
                    SYSGEN>

                  At the SYSGEN> prompt, enter the SHOW command to display
                  the value of a system parameter. The values the SHOW command
                  displays should equal or exceed the value of the parameter
                  listed in Section 1.6.5.1. The following command displays the
                  value for the VIRTUALPAGECNT system parameter:

                    SYSGEN> SHOW VIRTUALPAGECNT <Return>

                  After you check the VIRTUALPAGECNT parameter with the SHOW
                  command, enter the EXIT command at the SYSGEN> prompt to
                  return to DCL level.
























               1-8  Preparing to Install VAX VTX

 










               ____________________________________________________________

               1.6.6.2  Changing System Parameter Values with AUTOGEN

                  You use the AUTOGEN command procedure to change system param-
                  eters. AUTOGEN automatically adjusts values for parameters
                  that are associated with the ones you reset manually. To
                  change system parameters with AUTOGEN, you must edit the
                  following file:

                    SYS$SYSTEM:MODPARAMS.DAT

                  Use an editor to access the file. If you need to change a
                  parameter value in the SYS$SYSTEM:MODPARAMS.DAT file, delete
                  the current value associated with that parameter and enter
                  the new value.

                  To add a new value, add a line to the MODPARAMS.DAT file. The
                  line contains the name of the parameter and its value. For
                  example:

                    WSMAX = 1024

                  You can also modify incremental parameters in the 
MODPARAMS.DAT
                  file. The following example increases the global page setting
                  by 2000:

                    ADD_GBLPAGES = 2000

                  After you complete all your changes, run the AUTOGEN pro-
                  cedure to recalculate your system parameters. Enter the
                  following command at the DCL prompt:

                    $ @SYS$UPDATE:AUTOGEN GETDATA REBOOT <Return>

                  AUTOGEN performs an automatic system shutdown and then re-
                  boots your system. Rebooting your system activates the new
                  parameter values.

                  When you reboot a system under VMS Version 5.0, the Autogen
                  Utility
                  automatically adjusts some of the SYSGEN parameters based on
                  the
                  consumption of resources since the last reboot. If you do not
                  want to take
                  advantage of this automatic adjustment, include the
                  NOFEEDBACK qualifier on the AUTOGEN command line.

                                              Preparing to Install VAX VTX  1-9

 











                  For more information about using AUTOGEN, see the instruc-
                  tions on modifying system parameters in the documentation on
                  the VMS System Management Subkit.

               ____________________________________________________________

               1.6.7  Page File Quota

                  You must provide a value of at least 35,000 for the process
                  parameter PGFLQUO (page file quota). To check the current
                  value of PGFLQUO, type the following:

                    $ SHOW PROCESS/ALL <Return>

                  The item Paging file quota: shows the value of PGFLQUO.
                  If the value is below 35,000, run the Authorize Utility to
                  modify it. For example:

                    $ RUN SYS$SYSTEM:AUTHORIZE <Return>
                    UAF> MODIFY OPER/PGFLQUO=35000 <Return>

                  Substitute the name of the account from which you are in-
                  stalling VTX for OPER.

                  You can change the quota even though you are logged into the
                  account.

                                               NOTE

                      You must log out and log back in again for the quota
                      to become active.

               ____________________________________________________________

               1.6.8  Process Account Quotas

                  The account you use to install VAX VTX must have sufficient
                  quotas to enable you to perform the installation. Table 1-2
                  summarizes the process quotas VAX VTX requires for the in-
                  stallation account.





               1-10  Preparing to Install VAX VTX

 











                  Table 1-2:  Process Account Quotas for the Installing Account
                  _____________________________________________________________
                  Account_Quota____Value_______________________________________

                  ASTLM              240

                  BIOLM              230

                  BYTLM            65,000

                  DIOLM               50

                  ENQLM              300

                  FILLM              200

                  PGFLQUO          35,000

                  TQELM_______________20_______________________________________

                  VMS stores user account quotas in the file SYSUAF.DAT. Use
                  the VMS Authorize Utility to verify and change user account
                  quotas. First set your directory to SYS$SYSTEM and then run
                  AUTHORIZE.

                    $ SET DEFAULT SYS$SYSTEM <Return>
                    $ RUN AUTHORIZE <Return>
                    UAF>

                  At the Authorize Utility prompt (UAF>), use the SHOW command
                  with an account name to check a particular account. For
                  example:

                    UAF> SHOW SMITH <Return>

                  To change a quota, use the MODIFY command at the UAF> prompt.
                  MODIFY has the following format:

                        MODIFY account-name /quota-name=NNN

                  The following example changes the FILLM quota for the SMITH
                  account and then exits from the Authorize Utility:

                    UAF> MODIFY SMITH /FILLM=50 <Return>
                    UAF> EXIT <Return>

                                             Preparing to Install VAX VTX  1-11

 











                  After you exit from the utility, the VMS system displays
                  messages indicating whether or not changes were made. After
                  you make the changes, you must log out and log in again to
                  enable the new quotas.

                  For more information on modifying account quotas, see the
                  description of the Authorize Utility in the VMS documentation
                  set.

               ____________________________________________________________

               1.6.9  VMSINSTAL Requirements

                  Before you invoke VMSINSTAL, you should complete the follow-
                  ing steps:

                   1. Log into a privileged account

                   2. Set your default device and directory to SYS$UPDATE

                   3. Ensure the system has adequate quotas for installation

                  When you invoke VMSINSTAL, the procedure first checks to
                  be sure you meet these requirements and then displays the
                  following information:

                   o Whether DECnet is up and running on the system

                   o Which, if any, users are logged into the system

                  Some software products may require you to disconnect DECnet
                  before you begin an installation. You can install VAX VTX
                  whether or not DECnet is running. However, DECnet must be
                  running to use the Installation Verification Procedure (IVP).

                  You can install VAX VTX when users are logged into the sys-
                  tem, although the installation could fail if a user and the
                  VAX VTX installation procedure try to access a file at the
                  same time. Therefore, you should have all users log off the
                  system to ensure that the installation does not fail.

                  If VMSINSTAL detects a problem during the installation, it
                  notifies you and asks if you want to continue the installa-
                  tion. In some instances, you can enter YES to continue. To
                  stop the installation process and correct the situation, en-
                  ter NO or press RETURN, then correct the problem and restart
                  the installation.

               1-12  Preparing to Install VAX VTX

 










               ____________________________________________________________

               1.6.10  Backing Up Your System Disk

                  At the beginning of the installation, VMSINSTAL asks if you
                  have backed up your system disk. Digital recommends that you
                  do a system disk backup before installing any software in
                  addition to the operating system.

                  Use the backup procedures that have been established at your
                  site. For details on performing a system disk backup, see the
                  section on the Backup Utility in the VMS documentation set.

               ____________________________________________________________

               1.6.11  VAX VTX Requirements

                  VAX VTX checks for the following conditions during the in-
                  stallation
                  procedure:

                   o VMS Version 5.3 (or higher) is running on the system

                   o The appropriate number of free blocks are available on the
                     system disk (required for a complete installation)

                   o System parameters and account quotas meet required mini-
                     mums

                  See the documentation on the VMS System Management Subkit for
                  more information.

               ____________________________________________________________

               1.6.12  IVP Requirements

                  Before you run the Installation Verification Procedure (IVP)
                  as part of the VAX VTX installation or separately, you must
                  stop all VTX, Workbench, and Update Servers, as well as
                  all VAS run-time images. The VAX VTX Version 4.1 IVP starts
                  servers using the default object numbers and could fail if
                  these numbers are already being used.




                                             Preparing to Install VAX VTX  1-13

 










               ____________________________________________________________

               1.6.13  The VAX VTX VISTA Utility

                  For VAX VTX Version 4.0, the VISTA Utility was enhanced and
                  renamed the VAX VTX Workbench. The VISTA menu structure files
                  that were created with VTX Version 3.1 are not compatible
                  with the Workbench Utility in VAX VTX Version 4.0 or Version
                  4.1.

                  If you are upgrading directly from Version 3.1 to Version 4.1
                  and you want to do additional work on menu structures saved
                  in Version 3.1 files (menu structure files named structure-
                  name_MENUSTR.VTX in your VTX$VISTA subdirectory), follow the
                  steps listed below:

                   1. Update your infobase with the menu structures before you
                     install VAX VTX Version 4.1

                   2. After you install VAX VTX Version 4.1, convert your VISTA
                     library files to Workbench library files (see the VAX
                     VTX Operator's Guide for information on the conversion
                     process)

                   3. Use the LOCATE option (provided through the Workbench
                     interactive graphical interface, WBGI) to recreate the
                     menu structure

                   4. Save the menu structure to a Version 4.1 menu structure
                     file

                  If you fail to follow this procedure, you will receive an
                  error message when you try to open Version 3.1 menu structure
                  files.

                  For additional information on the Workbench Utility, see the
                  online release notes.

               ____________________________________________________________

               1.6.14  Converting Previous VTX Files to VAX VTX Version 4.0
                       Format

                  If you used a version of VTX prior to installing VAX VTX
                  Version 4.0, you must convert certain files to Version 4.0
                  format. See the VAX VTX Operator's Guide for more infor-
                  mation on page file conversion using the VTXPFC utility.
                  If you used VTX prior to Version 4.0, you should review
                  the conversion procedures carefully before you install VAX
                  VTX.

               1-14  Preparing to Install VAX VTX

 

















                                                                      Chapter 2


                                                             Installing VAX VTX
               ________________________________________________________________


                  This chapter describes how to install VAX VTX. Section 2.2
                  contains a step-by-step description of the installation
                  procedure.

               ____________________________________________________________

               2.1  General Information

                  This section includes information about accessing release
                  notes, determining files and logical names added to your
                  system, running the Installation Verification Procedure
                  (IVP), and aborting the installation. It also describes how
                  to install the MS-DOS Terminal Control Program (TCP) on a
                  Personal Computer.

               ____________________________________________________________

               2.1.1  Accessing the Online Release Notes

                  VAX VTX provides online release notes. You must specify
                  OPTIONS N when you invoke VMSINSTAL to access the release
                  notes. VMSINSTAL provides a list of options near the begin-
                  ning of the installation that allows you to decide how you
                  want to view the release notes during the installation.

                  You should review the release notes in case they contain
                  any information about changes in the installation procedure.
                  If you are restarting the installation procedure and you
                  have already reviewed the release notes, you do not need to
                  specify OPTIONS N.


                                                        Installing VAX VTX  2-1

 











                  After you install VAX VTX, your system stores the release
                  notes in the following file:

                    SYS$HELP:VTX041.RELEASE_NOTES

               ____________________________________________________________

               2.1.2  Running the Installation Verification Procedure (IVP)

                  The Installation Verification Procedure (IVP) for VAX VTX
                  verifies the installation. When you install VAX VTX, the
                  VMSINSTAL procedure asks you if you want to run the IVP as
                  part of the installation. If you respond YES, VMSINSTAL runs
                  the IVP.

                  There are three different IVPs for VAX VTX. The IVP you run
                  depends on the installation option you choose. The VTX full
                  kit installation option requires a two-part IVP. See the
                  instructions in Chapter 4 to determine the IVP you need to
                  run and whether you need to execute a second part of the IVP
                  after you complete the installation.

                  After you install VAX VTX, you can run the IVP independently
                  to verify that the software is available on your system. You
                  can also run the IVP after a system failure to be sure that
                  users can access VAX VTX.

                  See Chapter 4 for more detailed information on the IVP.

               ____________________________________________________________

               2.1.3  Aborting the Installation

                  You can abort the installation procedure at any time by
                  pressing CTRL/Y. When you press CTRL/Y, the installation
                  procedure deletes all files it creates up to that point and
                  exits. You can then restart the installation.

               ____________________________________________________________

               2.2  The Installation Procedure

                  The VAX VTX installation procedure consists of a series of
                  questions and informational messages.

               2-2  Installing VAX VTX

 










               ____________________________________________________________

               2.2.1  Invoking VMSINSTAL

                  To start the installation, invoke the VMSINSTAL command
                  procedure from a privileged account, such as the SYSTEM
                  account. VMSINSTAL is in the SYS$UPDATE directory. Use the
                  following syntax to invoke VMSINSTAL:

                        @SYS$UPDATE:VMSINSTAL product-name device-name OPTIONS
               N

                  product-name
                  The installation name for the component. For VAX VTX, use the
                  following installation name:

                    VTX041

                  device-name
                  The name of the device on which you plan to mount the media.
                  For example, MTA0: is the device name for a tape drive. It is
                  not necessary to use the console drive for this installation.
                  However, if you do use the console drive, you should replace
                  any media you remove once you complete the installation.

                  OPTIONS N
                  An optional parameter that gives you the option of accessing
                  the release notes during the installation. If you do not
                  include the OPTIONS N parameter, VMSINSTAL does not provide
                  this option. You should always review the release notes
                  before you proceed with the installation in case they contain
                  new information about the installation.

                  Note that there are several other options you can select when
                  you invoke VMSINSTAL. See the VMS documentation on software
                  installation for information on these options.

                  The following example displays the command you use to invoke
                  VMSINSTAL to install VAX VTX from tape drive MTA0: and shows
                  the system response. This example uses the OPTIONS N release
                  note parameter.





                                                        Installing VAX VTX  2-3

 











                    $ @SYS$UPDATE:VMSINSTAL VTX041 POLO$MUA6: <Return>

                          VAX/VMS Software Product Installation Procedure V5.3


                    It is 14-APR-1990 at 11:55.
                    Enter a question mark (?) at any time for help.

                  If you do not supply either the product name or the device
                  name, VMSINSTAL prompts you for this information later in
                  the installation procedure. Because VMSINSTAL does not prompt
                  for options, be sure to include OPTIONS N on the VMSINSTAL
                  command line if you want to access the release notes during
                  the installation.

               ____________________________________________________________

               2.2.2  Installation Questions

                  This section describes the questions that appear during
                  the installation. Appendix A contains a sample installation
                  procedure that explains how to answer the questions.

                  VMSINSTAL marks each question in the installation with an
                  asterisk (*) at the beginning of the line. Some questions
                  show the default response in brackets, for example [YES]. To
                  use the default response, press the RETURN key.

                  The following list outlines the steps in the installation
                  procedure:

                   1. DECnet status

                     VMSINSTAL displays a list of all active processes on
                     the system and tells you whether your DECnet network
                     is running. It then asks if you want to continue the
                     installation. You should install VAX VTX on a standalone
                     system or cluster with your DECnet network shut down. NO
                     is the default response to the question.

                       %VMSINSTAL-W-DECNET, Your DECnet network is up and 
running.
                          .
                          .
                          .
                       * Do you want to continue anyway [NO]?

                   2. System backup

               2-4  Installing VAX VTX

 











                     VMSINSTAL asks if you are satisfied with your system
                     backup. You should always back up your system disk before
                     performing an installation. If you are satisfied with the
                     backup of your system disk, press RETURN. Otherwise, enter
                     NO to discontinue the installation. After you back up your
                     system disk, you can restart the installation.

                       * Are you satisfied with the backup of your system disk 
[YES]?

                   3. Release notes

                     If you specify OPTIONS N when you invoke VMSINSTAL, the
                     procedure now asks you to choose one of the five options
                     for reviewing the release notes.

                       Release Notes Options:

                        1.  Display release notes
                        2.  Print release notes
                        3.  Both 1 and 2
                        4.  Copy release notes to SYS$HELP
                        5.  Do not display, print or copy release notes

                       * Select option [2]:

                     The following list describes each selection and its corre-
                     sponding result:

                      o Option 1

                        VMSINSTAL displays the release notes immediately on the
                        console terminal. You can terminate the display at any
                        time by pressing CTRL/C.

                        If you choose this option, VMSINSTAL copies the release
                        notes to the SYS$HELP directory.

                      o Option 2

                        VMSINSTAL prompts you for the name of the print queue
                        that you want to use:

                          * Queue name [SYS$PRINT]:

                        Press RETURN to send the file to the default output
                        print device or enter another queue name.

                        This option also prompts VMSINSTAL to copy the release
                        notes to the SYS$HELP directory.

                                                        Installing VAX VTX  2-5

 











                      o Option 3

                        VMSINSTAL displays the release notes immediately on the
                        console terminal and then prompts you for a queue name
                        for the printed version.

                        This option also prompts VMSINSTAL to copy the release
                        notes to the SYS$HELP directory.

                      o Option 4

                        VMSINSTAL copies the release notes to the help direc-
                        tory.

                      o Option 5

                        VMSINSTAL takes no action. Select this option if
                        you have already reviewed the release notes and are
                        restarting the installation.

                                                  NOTE

                            For a typical installation, you should select
                            either option 2 or option 4.





















               2-6  Installing VAX VTX

 











                   4. Continuing the installation

                     The installation procedure now asks if you want to con-
                     tinue the installation. To continue, enter YES. Otherwise,
                     press RETURN.

                     In either case, VMSINSTAL copies the release notes to a
                     file in the SYS$HELP directory. For example:

                       * Do you want to continue the installation [N]?: YES
                       %VMSINSTAL-I-RELMOVED, The product's release notes have 
been
                           successfully moved to SYS$HELP.

                     VMSINSTAL copies the release notes to the following file:

                       SYS$HELP:VTX041.RELEASE_NOTES

                                                 NOTE

                         The name of the release notes file installed by
                         VMSINSTAL consists of the current product name and
                         version number. Do not delete the release notes for
                         previous versions of VAX VTX.

                   5. Selecting VAX VTX components

                     VMSINSTAL gives you the option of installing the entire
                     kit, or just the kits or components you require. You can
                     also exit the installation procedure.

                       1) Install Subscriber interface only

                       2) Conversational installation

                       3) Install Full VTX kit

                       4) Install Full VTX kit with TCP source code

                       5) Exit from the installation procedure

                       * Enter option [2]:

                     The default is option 2 which is the conversational mode
                     of VTX installation. You are asked to select the VTX
                     options that you want to install.

                                                        Installing VAX VTX  2-7

 











                     Depending on the option you select, the following instal-
                     lation takes place:

                      o Selecting Subscriber Interface only (option 1)

                        If you select option 1 from the installation menu, only
                        the Subscriber environment is installed on your system.
                        See the first item under the installation procedure
                        for a conversational installation for details of the
                        component parts of the Subscriber interface.



































               2-8  Installing VAX VTX

 











                      o Selecting Conversational Installation (option 2)

                        If you choose to do a conversational installation, you
                        are prompted whether or not you want to install each
                        part of the full VTX kit.

                         * Installing the Subscriber environment

                           You have the option to install the VTX Subscriber
                           environment which includes the following parts:

                           VTXPAD    Subscriber's interface for VTX

                           VTXCON    Concentrator for VTX Subscriber sessions

                           MSDOS     Subscriber's interface to VTX for MS-DOS
                                     (reference kit)

                           The Subscriber environment is installed if you enter
                           YES in response to the question:

                             * Would you like to install the VTX Subscriber 
environment
                               [YES]?

                         * Installing the Information Provider tools

                           You have the option to install the Information
                           Provider tools which are required if you want to
                           update a VTX infobase. This option requires that the
                           Subscriber environment is installed.

                             * Would you like to install the VTX Information 
Provider tools
                               [YES]?

                         * Installing the VTX V3.x IP conversion tools

                           A few file formats for Information Provider tools
                           changed between VTX V3.x and V4.0; to upgrade your
                           V3.x files you need the following components:

                           PFC       The Page File Conversion tool

                           VLC       Converts a VISTA library to a Workbench
                                     library

                           IAF       Converts an APMS Index

                                                    NOTE

                               No file conversions are needed if you go from

                                                        Installing VAX VTX  2-9

 











                               VTX V4.0 to V4.1.

                           If you need to convert your VTX V3.x files, answer
                           YES to the question, otherwise NO:

                             * Would you like to install VTX V3.x IP Conversion 
tools [YES]?







































               2-10  Installing VAX VTX

 











                         * Installing the VTX Servers

                           You have the option to install the VTX Server envi-
                           ronment which has the following parts:

                           SRV       Allows local and remote VTX Subscribers to
                                     access a VTX infobase on this system.

                           UPDSRV    Allows remote VTX Information Providers to
                                     update VTX infobases on this system.

                           WBSRV     Allows remote VTX Information Providers to
                                     access Workbench libraries on this system.

                           ACU       VTX infobase access Authorization and
                                     Accounting utility.

                           To install the Server environment, answer YES to the
                           following question:

                             * Would you like to install the VTX Servers [YES] ?

                         * Installing the VTX Back-End environment.

                           VTX Back-End applications are programs that are
                           started when a subscriber references a page in a VTX
                           infobase. This option includes the following parts:

                           VAS       A high-level programming interface for
                                     writing VTX Back-End applications.

                           ELK       A low-level programming interface to
                                     writing VTX Back-End applications.

                           Both the components include their programming inter-
                           faces and can be installed by answering YES to the
                           following question"

                             * Would you like to install the VTX Back End 
environment [YES] ?






                                                       Installing VAX VTX  2-11

 











                         * Installing the TCP source code

                           The VTX Subscriber interface can be customized
                           by modifying the source code. Refer to your VTX
                           Warranty Exclusion for details on what can be
                           changed without violating your standard VTX support
                           contract.

                                                    NOTE

                               You need access to a BLISS32 compiler in
                               order to compile any changes that you make.

                           If you want this option, answer YES to the following
                           question:

                             * Would you like to install the TCP source code 
[NO] ?

                           You are then asked where you want the TCP source
                           files to be put. You must specify a directory in
                           response to the following question:

                             * Where do you want the TCP sources 
[SYS$SYSROOT:TCPLIB]:

                         * Installing the Common keypad

                           The Common keypad is a superset of the traditional
                           VTX default keypad and the ALL-IN-1 keypad except
                           where there are conflicting mappings. Refer to the
                           VAX VTX Subscriber's Booklet for more details of the
                           Common keypad.

                           If you want to use the Common keypad, answer YES to
                           the following question:

                             * Would you like to install the new keypad [NO]?

                      o Selecting to install the full VTX kit (option 3)

                        If you select option 3 from the installation menu, the
                        full VAX VTX kit is installed on your system. The full
                        VTX kit consists of:

                         * Subscriber environment

                         * Information Provider tools

                         * Information Provider Conversion tools

                         * VTX Servers

               2-12  Installing VAX VTX

 











                        See the conversational installation for details of
                        installing these components.











































                                                       Installing VAX VTX  2-13

 











                      o Selecting to install the full VTX kit with TCP source
                        code (option 4)

                        If you select option 4 from the installation menu, the
                        full VTX kit plus the TCP source code is installed on
                        your system as follows:

                         * Subscriber environment

                         * Information Provider tools

                         * Information Provider Conversion tools

                         * VTX Servers

                        See the conversational installation for details of
                        installing these components.

                      o Selecting to exit from the installation procedure
                        (option 5)

                        If you select option 5 from the installation menu, you
                        exit from the installation procedure without installing
                        anything on your system.

                   6. Choosing to purge files

                     You have the option to purge files from previous versions
                     of VAX VTX that are superseded by this installation.
                     Purging is recommended; however, if you need to keep files
                     from the previous version, enter NO in response to the
                     question.

                       * Do you want to purge files replaced by this 
installation [YES]?

                   7. Deleting obsolete files

                     The installation procedure asks you if you want to delete
                     all files made obsolete by this installation. The default
                     answer is NO. To delete the obsolete files, answer YES.

                     Table 2-1 provides a list of the files made obsolete by
                     the installation.


               2-14  Installing VAX VTX

 











                  Table 2-1:  Files Made Obsolete by Installation Procedure
                  _____________________________________________________________
                  ______Directory_and_Filename_________________________________

                        SYS$COMMON:[SYSLIB]VTX$TERMSHR.EXE

                        SYS$HELP:VTXCTLVSRV.HLB

                        SYS$LIBRARY:VTXIAF.FDL

                        SYS$LIBRARY:VTXIAF_CONVERT.CLD

                        SYS$LIBRARY:VTXKFC.FDL

                        SYS$LIBRARY:VTXPAF.FDL

                        SYS$LIBRARY:VTXPAF_CONVERT.CLD

                        SYS$SYSROOT:[RUSLLIB]RUSLLIB.OLB

                        SYS$SYSROOT:[SYSTEST]VTX$IVP_UPDATE.COM

                        SYS$SYSROOT:[SYSTEST]VTX$IVP_VAS.COM

                        SYS$SYSTEM:VASCTL.EXE

                        SYS$SYSTEM:VTXIAF_CONVERT.EXE

                        SYS$SYSTEM:VTXKFC.EXE

                        SYS$SYSTEM:VTXPAF_CONVERT.EXE

                        SYS$SYSTEM:VTXVISTA.EXE

                        SYS$SYSTEM:VTXVISTASRV.EXE

                        SYS$UPDATE:SAMPLE_STYLE.VTX

                        SYS$UPDATE:VTXBASE.TXT
                  _____________________________________________________________
                                                       (continued on next page)




                                                       Installing VAX VTX  2-15

 











                  Table 2-1 (Cont.):  Files Made Obsolete by Installation
                                      Procedure
                  _____________________________________________________________
                  ______Directory_and_Filename_________________________________

                        SYS$UPDATE:VTXCON.COM

                        SYS$UPDATE:VTXIAF_CONVERT.COM

                        SYS$UPDATE:VTXMAIN.VTU

                        SYS$UPDATE:VTXPAF_CONVERT.COM

                        SYS$UPDATE:VTXSERVER.COM

                        SYS$UPDATE:VTXUPDSRV.COM

                        SYS$UPDATE:VTXVISASRV.COM

                        SYS$UPDATE:VTX_INTERNALS.VTU

                        VTX$TCPLIB:CON.OLB

                        VTX$TCPLIB:DECTERMLIB.OLB

                        VTX$TCPLIB:DSLLIB.OLB

                        VTX$TCPLIB:NOREGISLIB.OLB

                        VTX$TCPLIB:STRINGS.OBJ

                        VTX$TCPLIB:VTXCON.OPT

                        VTX$TCPLIB:VTXCTLCMD.OBJ

                  ______VTX$TCPLIB:VTXPAD.OPT__________________________________









               2-16  Installing VAX VTX

 











                   8. Choosing to run the Installation Verification Procedure
                     (IVP)

                     The installation procedure now asks if you want to run the
                     Installation Verification Procedure (IVP), which checks
                     that the installation is successful.

                       * Do you want to run the IVP after the installation 
[YES]?

                     It is recommended that you run the IVP. See Chapter 4 for
                     information on how to do this.

               ____________________________________________________________

               2.2.3  Informational Messages

                  At this point, there are no further questions. The installa-
                  tion procedure displays a number of informational messages
                  that report on the progress of the installation.

                  For example, VMSINSTAL notifies you that it is restoring
                  various savesets, building command and message files, and
                  creating system and component libraries.

                  If the installation procedure is successful up to this point,
                  VMSINSTAL moves the new or modified files to their target
                  directories, updates help files, and updates DCL tables, if
                  necessary. If you asked for files to be purged, that work is
                  done now. VMSINSTAL displays the following message:

                    %VMSINSTAL-I-MOVEFILES, files will be moved to their target 
directories...

               ____________________________________________________________

               2.2.4  Running the Installation Verification Procedure

                  If you chose to run the IVP, VMSINSTAL runs it now. When the
                  IVP runs successfully, you see the following message:

                       * * * * *   S U C C E S S   * * * * *

                      VAX VTX V4.1 IVP completed successfully

                       * * * * *   S U C C E S S   * * * * *

                                                       Installing VAX VTX  2-17

 










               ____________________________________________________________

               2.2.5  Completing the Installation Procedure

                  The following messages indicate that the entire installation
                  procedure is complete:

                       Installation of VTX V4.1 completed at 10:16

                       VMSINSTAL procedure done at 10:17

                  When the optional portion of the VAX VTX IVP is completed,
                  you must stop the servers. To so so, follow these steps:

                   1. Run the VTXCTL Utility using the following command:

                       $ Run SYS$SYSTEM:VTXCTL <Return>

                   2. Type the STOP commands and the EXIT command at the CTL>
                     prompt; for example:

                       CTL> STOP SERVER/NAME=IVP <Return>
                       CTL> STOP VAS/NAME=IVP <Return>
                       CTL> EXIT <Return>
                       $

                  You can now log out of the privileged account:

                    $ LOGOUT <Return>
                    SYSTEM     logged out at 20-APR-1990 10:44:00.00

                  Note that VMSINSTAL deletes or changes entries in the process
                  symbol tables during the installation. Therefore, if you are
                  going to continue using the system manager's account and you
                  want to restore these symbols, you should log out and log in
                  again.

               ____________________________________________________________

               2.3  Installing the MS-DOS TCP on Your Personal Computer

                  If you want to access VAX VTX on a PC running MS-DOS, you
                  must have the MS-DOS Terminal Control Program (TCP) installed
                  on the PC. To install the MS-DOS TCP on your PC:

                   o You must be a DECnet node and have DECnet running.
                     You need access to two VMS systems: the VMS sys-
                     tem you install the kit from, which needs to access
                     SYS$COMMON:[VTX$LIBRARY], and the system that runs your
                     home server which only needs to be defined, as follows:

               2-18  Installing VAX VTX

 











                           C:> NCP DEFINE node area.nodenum name nodename

                     You can define the VMS system for your home server after
                     the
                     installation if you prefer.

                   o You must have write access to the destination disk on your
                     PC.

                   o You must have 125KB free on the destination disk.

                   o Copy the installation (.BAT) file and program from the VMS
                     system by typing the following command:

                       C:> NFT COPY node::SYS$COMMON:[vtx$library]:vtxdosin.bat,
                           vtxdosq.exe *.*

                     The following messages will be displayed:

                       Copying file: 
nodename::SYS$COMMON:[vtx$library]:vtxdosin.bat to
                       C:\VTX\vtxdosin.bat  [n bytes at m bytes/second]

                       Copying file: 
nodename::SYS$COMMON:[vtx$library]:vtxdosq.exe to
                       C:\VTX\vtxdosq.exe  [n bytes at m bytes/second]

                   o Execute the .BAT file by typing the following command:

                       C:> vtxdosin

                     You are now prompted for some information: you must spec-
                     ify the destination disk and nodename, otherwise you may
                     take all the default responses if they meet your require-
                     ments. The default responses appear in brackets.

                  The installation procedure creates two files of interest
                  in the VTX library: the VTXENV.BAT file and the VTX.SYS
                  (configuration) file.

                  The VTXENV.BAT file defines the environment variable VTXLIB
                  which points to the VTX library.

                                               NOTE

                      The VTXENV.BAT file should be called or executed from
                      your AUTOEXEC.BAT file at boot time.

                                                       Installing VAX VTX  2-19

 











                  Also, the VTXENV.BAT file contains the command to add the
                  VTX library to your search path. If you need to move the VTX
                  library to a different disk, you must edit the VTXENV.BAT
                  file to point to the new location and change the command in
                  your AUTOEXEC.BAT file that calls the VTXENV.BAT file.

                  The VTX.SYS file specifies parameters to the TCP such as the
                  server to connect to, and the language, protocol and keypad
                  to be used. You should edit this file if your default server
                  name or object number changes or if you want to access the
                  server with a different language or protocol.


































               2-20  Installing VAX VTX

 











                  The following items are in the configuration (VTX.SYS) file:

                     SERVER=node_name
                     OBJECT=n
                     PROTOCOL=valid-vtx-protocol
                     LANGUAGE=valid-vtx-language
                     DEVICE_TYPE=valid-vtx-device-type
                     KEYPAD={NUMERIC|APPLICATION}
                     KEYBOARD={EPC|AT|XT|LK250}

                  where:

                   o node_name is the DECnet node name of the server, without
                     trailing colons

                   o n is the DECnet object number of the server

                   o valid-vtx-protocol defaults to ASCII

                   o valid-vtx-language defaults to ENGLISH

                   o valid-vtx-device-type defaults to IBMPC

                   o KEYPAD defaults to APPLICATION

                   o KEYBOARD can be explicitly set, although the MS-DOS TCP
                     tries to determine which type of keyboard is being used.
                     The default value is EPC.

                                               NOTE

                      In a PCSA environment, when one disk can be shared
                      by many PCs, you do not need to install VAX VTX on
                      each PC. Simply install the VTX MS-DOS TCP on one PC,
                      which must have write access to the destination disk
                      during installation. Then add the VTXENV file to the
                      AUTOEXE.BAT file of each PC that will be sharing the
                      disk that has the MS-DOS TCP installed.







                                                       Installing VAX VTX  2-21

 











                  The following is a sample MS-DOS TCP installation:

                    C> vtxdosin

                    
=======================================================================
                    |                                                            
          |
                    |             VTX V4.1 Installation Procedure for MS-DOS     
          |
                    | Copyright 1986, 1987, 1988, 1989, 1990 Digital Equipment 
Corporation |
                    |                                                            
          |
                    
=======================================================================

                    What disk would you like to copy the VTX kit to? >>

                    What VMS node is the VTX kit located on? >> vax1

                    What is the node name of your home server? >> vax2

                    What is the object number of your home server? [43] >> 143

                    What keypad would you like to use? [NUMERIC] >>

                    What language would you like to connect as? [ENGLISH] >>
                    Creating VTX directory...
                    Copying file: vax1::sys$common:[vtx$library]vtx$pchlpat.txt 
to
                    C:\VTX\vtxhlpat.txt  [9450 bytes at m bytes/second]
                    Copying file: 
vax1::sys$common:[vtx$library]vtx$pchlpatap.txt to
                    C:\VTX\vtxhlpatap.txt  [9450 bytes at m bytes/second]
                    Copying file: vax1::sys$common:[vtx$library]vtx$pchlpxt.txt 
to
                    C:\VTX\vtxhlpxt.txt  [9458 bytes at m bytes/second]
                    Copying file: vax1::sys$common:[vtx$library]vtx$pchlplk.txt 
to
                    C:\VTX\vtxhlpxtap.txt  [9458 bytes at m bytes/second]
                    Copying file: vax1::sys$common:[vtx$library]vtx$pchlplk.txt 
to
                    C:\VTX\vtxhlplk.txt  [9845 bytes at m bytes/second]
                    Copying file: 
vax1::sys$common:[vtx$library]vtx$pchlplkap.txt to
                    C:\VTX\vtxhlplkap.txt  [9845 bytes at m bytes/second]
                    Copying file: vax1::sys$common:[vtx$library]vtx$pchlpep.txt 
to
                    C:\VTX\vtxhlpep.txt  [9510 bytes at m bytes/second]
                    Copying file: 
vax1::sys$common:[vtx$library]vtx$pchlpepap.txt to
                    C:\VTX\vtxhlpepap.txt  [9510 bytes at m bytes/second]
                    Copying file: vax1::sys$common:[vtx$library]vtx$dostcp.exe 
to
                    C:\VTX\vtx.exe [89472 bytes at m bytes/second]
                         1 File(s) copied
                         1 File(s) copied

                        NOTE: Append the execution of the file \VTX\VTXENV.BAT 
in
                              your VTX library directory on the target disk to 
your
                              autoexec.bat and reboot to use VTX.

               2-22  Installing VAX VTX

 











                    
====================================================================
                    |                                                            
       |
                    |                 End of VTX V4.1 Installation               
       |
                    |                                                            
       |
                    
====================================================================

               ____________________________________________________________

               2.4  Error Recovery

                  If errors occur during the installation procedure or when the
                  IVP is running, VMSINSTAL displays failure messages. If the
                  installation fails, you see the following message:

                    %VMSINSTAL-E-INSFAIL, The installation of VTX V4.1 has 
failed.

                  If the IVP fails, you see these messages:

                    The VTX V4.1 Installation Verification Procedure failed.

                    %VMSINSTAL-E-IVPFAIL, The IVP for VTX V4.1 has failed.

                  Errors can occur during the installation if any of the fol-
                  lowing conditions exist:

                   o The operating system version is incorrect

                   o A prerequisite software version is incorrect

                   o Quotas necessary for successful installation are insuffi-
                     cient

                   o System parameter values for successful installation are
                     insufficient

                   o The VMS help library is currently in use

                   o The product license is not registered and loaded

                  For descriptions of the error messages generated by these
                  conditions, see the VMS documentation on system messages,
                  recovery procedures, and VMS software installation. If you
                  are notified that any of these conditions exist, you should
                  take the appropriate action as described in the message.
                  You might need to change a system parameter or increase
                  an authorized quota value. For information on installation
                  requirements, see Chapter 1.

                                                       Installing VAX VTX  2-23

 

















                                                                      Chapter 3


                                                       After Installing VAX VTX
               ________________________________________________________________


                  After installing VAX VTX, you need to perform the following
                  tasks:

                   o Edit the system startup file to establish a VTX print
                     queue

                   o Start VAX VTX on other nodes in your VAXcluster

                   o Set subscriber account privileges and quotas

                   o Define the appropriate system logicals

                   o Set up DECnet

                   o Create a VTX operator's account

                  This chapter also describes how to use search lists.

               ____________________________________________________________

               3.1  Establishing a VAX VTX Print Queue

                  To establish a VAX VTX print queue, you must modify your
                  system startup file. There is no automatic startup procedure
                  for VAX VTX; however, if you want to use an editor to create
                  VAX VTX documents, you must edit the system startup file to
                  provide for automatic startup of the VAX VTX print queue when
                  you reboot your system.




                                                  After Installing VAX VTX  3-1

 










               ____________________________________________________________

               3.1.1  Editing the System Startup File

                  Add the command line that starts the VAX VTX print queue to
                  the system startup file, SYS$MANAGER:SYSTARTUP_V5.COM. The
                  following example displays the network startup command line
                  followed by the startup command line for the VAX VTX print
                  queue:

                    $ @SYS$MANAGER:STARTNET.COM
                         .
                         .
                         .
                    $ @SYS$STARTUP:VTXWPS_STARTUP.COM

                  Place the command line to start the VAX VTX print queue
                  in the system startup file at a position that meets the
                  requirements of your site.

                                               NOTE

                      If you create an automatic startup procedure for
                      VAX VTX, you must add the command line that starts
                      that procedure to the system startup file after the
                      @SYS$MANAGER:STARTNET.COM command line entry. However,
                      it does not have to be after the @SYS$STARTUP:VTXWPS_
                      STARTUP.COM command line entry.

               ____________________________________________________________

               3.1.2  Configuring Print Tables for VTX$QUEUE

                  To use WPS-PLUS with VTX$QUEUE, you must configure the WPS-
                  PLUS or ALL-IN-1 print tables so that WPS-PLUS recognizes
                  VTX$QUEUE. This subsection describes how to configure print
                  tables for VTX$QUEUE if your system is running WPS-PLUS
                  Version 3.1 under ALL-IN-1 Version 2.3 or as a standalone.

                  If you are running WPS-PLUS Version 3.1 under ALL-IN-1
                  Version 2.3, follow these steps to configure print tables
                  for VTX$QUEUE:

                   1. Log in to a privileged account, preferably SYSTEM.

                   2. Locate the device on which the [ALLIN1] directory is
                     located.

               3-2  After Installing VAX VTX

 











                   3. Copy the files VTX.PRA and VTX.PRC from
                     SYS$COMMON:[VTX$LIBRARY] to the directory
                     DEVICE:[ALLIN1.PRINT].

                   4. Log in to the ALL-IN-1 manager's account.

                   5. Establish the VTX print table in ALL-IN-1:

                      o Select the menu option MPR (Manage printers). ALL-IN-1
                        displays the two options of the Manage Printers menu,
                        PR and PT.

                      o Select menu option PT (Printer types). ALL-IN-1 dis-
                        plays the Manage Printer Types menu.

                      o Select menu option C (Create). ALL-IN-1 displays the
                        following form. Fill in the information listed to the
                        right of each field as it appears below. Be sure to
                        leave the last field (Print Form:) blank.

                              Printer Type:            VTX
                              Foreground function:     DO WPPSYSTEM
                              Background function:     DO WPPBGFORMAT
                              Printer Device:          VTX
                              Print Form:

                      o Return to the Manage Printers menu.

                      o Select the Manage Printers menu option PR (Site print-
                        ers).
                        ALL-IN-1 displays Manage Site Printers menu.

                      o Select the SEL menu option. ALL-IN-1 prompts you for a
                        name. Enter VTX$QUEUE and press the RETURN key.

                      o If ALL-IN-1 cannot find VTX$QUEUE, select menu option C
                        (Create).

                      o If ALL-IN-1 finds VTX$QUEUE, select menu option E
                        (Edit).

                      o Whether you select menu option C or E, ALL-IN-1 dis-
                        plays the following form. If the form is blank, fill in
                        the fields with the information listed to the right of
                        each field. If the fields contain information that dif-
                        fers from the information seen below, edit the form and
                        change the appropriate fields to those listed below.

                                                  After Installing VAX VTX  3-3

 











                              Printer Name:                VTX$QUEUE
                              Description:                 Format document and 
send to VTX
                              Format Printer Type:         VTX
                              Destination Printer Type:    VTX
                              Print Queue:                 VTX$QUEUE

                  If you are running WPS-PLUS Version 3.1 in a standalone
                  environment, follow these steps to configure print tables
                  for VTX$QUEUE:

                   1. Log in to a privileged account, preferably SYSMGR.

                   2. Locate the device on which the [WPSPLUS] directory is
                     located.

                   3. Copy the files VTX.PRA and VTX.PRC from
                     SYS$COMMON:[VTX$LIBRARY] to the directory
                     DEVICE:[WPSPLUS.PRINT].



























               3-4  After Installing VAX VTX

 










               ____________________________________________________________

               3.1.3  DCLTABLES

                  This version of VTX contains slight changes to the DCL com-
                  mand. Please refer to the VAX VTX Subscriber's Booklet for
                  details of the new COMMON device type.

                                               NOTE

                      If you are in a VAX Cluster, you must re-install
                      DCLTABLES on all nodes in the cluster except the node
                      that you performed the installation from.

                  Failure to re-install DCLTABLES will cause the following
                  error message to be displayed:

                    %CLI-F-SYNTAX, error parsing 'PIC1'
                    -CLI-E-ENTNF, specified entity not found in command tables

                  In addition to this error, VTXPAD will refuse to start.

                  You can reinstall DCLTABLES with the following command:

                    $ RUN SYS$SYSTEM:INSTALL <Return>
                    INSTALL> SYS$SHARE:DCLTABLES/REPLACE <Return>
                    INSTALL> <Ctrl/Z>
                    $

               ____________________________________________________________

               3.2  Cluster Considerations

                  You must perform the following actions on each node that
                  supports VAX VTX, before VAX VTX starts on other nodes in a
                  VAXcluster.

                   1. Replace DCL tables using the VMS INSTALL utility.

                   2. Run VTXWPS_STARTUP.COM (if you will be using the VTX print
                     queue).

                   3. Load the license.

                   4. Run the IVP.

                                                  After Installing VAX VTX  3-5

 










               ____________________________________________________________

               3.3  Subscriber Account Privileges and Quotas

                  To work with VAX VTX, subscriber accounts on your system must
                  have certain privileges and quotas.

               ____________________________________________________________

               3.3.1  Privileges

                  To use VAX VTX, each account must have at least the TMPMBX
                  and NETMBX privileges. Use the VMS Authorize Utility to
                  determine if subscribers have the privileges they require.

               ____________________________________________________________

               3.3.2  Account Quotas

                  You must ensure that the appropriate subscriber accounts have
                  sufficient quotas to use VAX VTX. Table 3-1 summarizes the
                  quotas user accounts require.

                  Table 3-1:  Subscriber Account Quotas for Using VAX VTX
                  _____________________________________________________________
                  Account_Quota____Value_______________________________________

                  ASTLM                8

                  BIOLM                8

                  BYTLM            10,000

                  DIOLM                6

                  ENQLM               10

                  FILLM                3

                  TQELM                8

                  PCFLQUOTA_________8000_______________________________________

                  VAX VTX stores subscriber account quotas in the file
                  SYSUAF.DAT. Use the VMS Authorize Utility to verify and
                  change subscriber account quotas. First set your directory to
                  SYS$SYSTEM and then run AUTHORIZE:

               3-6  After Installing VAX VTX

 











                    $ SET DEFAULT SYS$SYSTEM <Return>
                    $ RUN AUTHORIZE <Return>
                    UAF>

                  At the Authorize Utility prompt (UAF>), enter the SHOW com-
                  mand with an account name to check that particular account.
                  For example:

                    UAF> SHOW SMITH <Return>

                  To change a quota, use the MODIFY command at the UAF> prompt.
                  MODIFY has the following syntax:

                        MODIFY account-name /quota-name=???

                  The following example shows how to change the FILLM quota for
                  the SMITH account and then exit from the utility:

                    UAF> MODIFY SMITH /FILLM=50 <Return>
                    UAF> EXIT <Return>

                  After you exit from the utility, the VMS system displays
                  messages indicating whether or not changes were made. After
                  you finish making the changes, the subscriber must log out
                  and log in again for the new quotas to take effect.

                  For more information on modifying account quotas, see the
                  description of the Authorize Utility in the VMS documentation
                  set.

               ____________________________________________________________

               3.4  Defining System Logicals

                  If you install the TCP files for future modification, you
                  should define two system logicals at startup time. The fol-
                  lowing example shows the DEFINE command lines you should
                  enter in the SYS$MANAGER:SYSTARTUP_V5.COM file for TCP files
                  stored in the default directory.

                    $ DEFINE/SYSTEM/EXECUTIVE VTX$REQUIRE SYS$SYSROOT:[TCPLIB]
                    $ DEFINE/SYSTEM/EXECUTIVE DSL$REQUIRE SYS$SYSROOT:[TCPLIB]

                  VAX VTX does not require that you define these logicals in
                  order for it to run; however, the logicals are useful when
                  you want to modify the TCP.

                                                  After Installing VAX VTX  3-7

 










               ____________________________________________________________

               3.5  DECnet

                  You must have DECnet running on your VMS system to run VAX
                  VTX. The VMS operating system comes with a single node DECnet
                  license, so even if you have a single node system, you can
                  run DECnet. If DECnet is already running on your VMS system,
                  you can create a VTX operator's account. If your site is not
                  running DECnet, you must execute two command procedures in
                  order to establish your VMS system as a DECnet node.

               ____________________________________________________________

               3.5.1  Establishing a DECnet Node

                  To establish a DECnet node, set your default directory to
                  SYS$MANAGER and then identify your VMS system as a DECnet
                  node by executing the command procedure NETCONFIG.COM as
                  follows:

                    $ SET DEFAULT SYS$MANAGER <Return>
                    $ @NETCONFIG <Return>

                  The command procedure is interactive and self-explanatory.
                  The procedure asks you to supply a DECnet node name and
                  DECnet address for your node, and whether you want a de-
                  fault DECnet account. Follow the instructions that appear on
                  your terminal. Your node name can be any 6-character alphanu-
                  meric name. If you do not have a multinode DECnet license,
                  a node address of 1 is recommended. If you are configuring
                  a multinode network, you should first read the VMS DECnet
                  documentation. This is the only time you should have to run
                  NETCONFIG in order to use VAX VTX.

               ____________________________________________________________

               3.5.2  Starting DECnet

                  After you add your node to the DECnet database, you must
                  start DECnet. This procedure activates the changes that
                  you made to the DECnet database and makes your VMS system a
                  recognized DECnet node. To start DECnet, execute the command
                  procedure STARTNET.COM as follows:

                    $ @STARTNET  <Return>

               3-8  After Installing VAX VTX

 











                  If your site does not have a multinode DECnet license,
                  your terminal displays a series of error messages while
                  STARTNET.COM is executing. You can ignore these. You must
                  execute STARTNET.COM every time you boot your VMS system, but
                  not every time you start VAX VTX. For convenience, you can
                  insert the @STARTNET command in the SYS$MANAGER:SYSTARTUP_
                  V5.COM file so that DECnet starts automatically every time
                  you boot your VMS system.





































                                                  After Installing VAX VTX  3-9

 










               ____________________________________________________________

               3.6  Creating a VTX Operator Account

                  Create a VTX operator account that allows you to run a VTX
                  Server. The operator account requires certain privileges and
                  quotas. To add an operator account to your VMS system, run
                  the VMS Authorize Utility, as described in the documentation
                  on the VMS System Management Subkit. Assign the following
                  privileges as authorized privileges and default privileges to
                  the VTX operator's account:

                     GROUP
                     SYSNAM
                     GRPNAM
                     TMPMBX
                     NETMBX

                  In addition, assign the following quotas to the account:

                  _____________________________________________________________
                  ____________Account_Quota____Value___________________________

                              ASTLM              240

                              BIOLM              230

                              BYTLM            65,000

                              DIOLM               50

                              ENQLM              300

                              FILLM              200

                  ____________TQELM_______________20___________________________

                  After you create an account for the VTX operator, you need
                  to create a directory for that account. Assign the same UIC
                  to the directory as the Authorize Utility assigned to the
                  operator account.

                  If you need to run VTX Workbench from the VTX operator ac-
                  count, set the PGFLQUO value to at least 12,000 (see the VAX
                  VTX Operator's Guide.)

               3-10  After Installing VAX VTX

 











                  The Operator's account must have GROUP and GRPNAM privileges
                  so that VTX utilities can manage group logical names. Since
                  these privileges also allow the operator account to define
                  group logical names at the DCL level, Digital recommends that
                  you assign group UICs for operator accounts that differ from
                  user accounts on your system.







































                                                 After Installing VAX VTX  3-11

 










               ____________________________________________________________

               3.7  Using Search Lists

                  When you define the default device and directory names
                  for the VTX operator account with the ADD command in the
                  Authorize Utility, the utility combines these names to become
                  the definition of the logical name SYS$LOGIN when you log in
                  to that account. The format for the command is:

                        ADD new-username 
/DEVICE=device-name/DIRECTORY=[directory-
               name]

                  At VMS system startup, if you define the default device name
                  as a system logical name which has an equivalence string that
                  is a VMS search list, you must be sure to create the default
                  directory ([directory-name]) for the VTX account on the first
                  device in the search list that is the translation for the
                  default device logical name (device-name).

                  For example, if your system defines SYS$SYSROOT as follows,
                  you can use the DCL command SHOW LOGICAL SYS$SYSROOT to
                  display the definition at your terminal:

                    "SYS$SYSROOT" = "DISK1:[SYS0.]" (LNM$SYSTEM_TABLE) = 
"SYS$COMMON"
                    "SYS$COMMON" = "DISK1:[SYS0.SYSCOMMON.]" (LNM$SYSTEM_TABLE)

                  Now, suppose you create the VTX account to have the following
                  SYS$LOGIN definition:

                    "SYS$LOGIN" = "SYS$SYSROOT:[VTX]"

                  You must be sure that the VTX directory ([VTX] in the preced-
                  ing example, or whatever name you have chosen) is a subdirec-
                  tory of DISK1:[SYS0]; for example:

                    DISK1:[SYS0.VTX]

                  If your default directory is set to the SYS$LOGIN equivalence
                  name rather than to SYS$LOGIN, you will be unable to start
                  the VTX Server or create any files.

               ____________________________________________________________

               3.8  Enhancing VAX VTX Performance

                  This section includes information on system tuning and ex-
                  plains how to install VAX VTX as a shared image.

               3-12  After Installing VAX VTX

 










               ____________________________________________________________

               3.8.1  Tuning Your System

                  After you install VAX VTX, you should adjust your system
                  to enhance performance or lower the use of some system re-
                  sources. See the VAX VTX Operator's Guide for information
                  that may be useful in tuning your system.

               ____________________________________________________________

               3.8.2  Installing VAX VTX as a Shared Image

                  The most frequently used images of VAX VTX are:

                     VTXPAD.EXE
                     VTX$MSCSHR.EXE

                  While you do not need to install any VAX VTX components as
                  shared images, you can reduce the system overhead and memory
                  requirements by installing it as a shared image, particularly
                  if you expect VAX VTX to be used extensively on your system.
                  To install VAX VTX as a shared image on a system that is
                  currently running, use the VMS Install Utility (INSTALL).
                  You should perform the install operation on a newly rebooted
                  system because the available space in the global page table
                  is less likely to be fragmented.

                  To install VAX VTX as a shared image, first determine the
                  number of available global pages and global sections on your
                  system. Table 3-2 shows correct values for the GBLPAGES and
                  GBLSECTIONS system parameters.

                  Table 3-2:  Required System Parameter Values
                  _____________________________________________________________
                  System_Parameter___________Value_____________________________

                  GBLPAGES[1]                n + 1300

                  GBLSECTIONS[1]             n + 5
                  [1]The_n_variable_refers_to_the_system_parameter_values_that_

                  are currently in use. To install VAX VTX, you must raise
                  those values by the number indicated.
                  _____________________________________________________________

                  The n + 1300 value for GBLPAGES and the n + 5 value for
                  GBLSECTIONS in Table 3-2 indicate that you must have at least

                                                 After Installing VAX VTX  3-13

 











                  1300 unused pages and 5 unused sections available on your
                  system for the installation to process successfully.











































               3-14  After Installing VAX VTX

 











                  To calculate how many unused global pages and global sections
                  your system has, perform the following steps:

                   1. Run the VMS Install Utility (INSTALL) using the following
                     DCL command:

                       $ INSTALL LIST /GLOBAL /SUMMARY <Return>

                     The Install Utility displays a summary of global pages
                     and global sections used by your system, as well as the
                     current number of unused global pages. For example:

                                        Summary of Local Memory Global Sections

                       258 Global Sections Used,  22580/3420 Global Pages 
Used/Unused

                   2. Determine if the number of unused global pages (3420 in
                     the example) is equal to or greater than 1300. If the
                     number of unused pages is less than 1300, you need to
                     increase the value for GBLPAGES.

                   3. Run the System Generation Utility and use the SHOW command
                     to determine how many global sections have been allocated.
                     For example:

                       $ RUN SYS$SYSTEM:SYSGEN <Return>
                       SYSGEN> SHOW GBLSECTIONS <Return>

                       Parameter Name    Current   Default   Minimum   Maximum 
Unit  Dynamic
                       --------------    -------   -------   -------   ------- 
----  -------
                       GBLSECTIONS           512       250        20      4095 
Sections

                   4. Subtract the amount shown in the summary (258 in the
                     example) from the amount allocated. If the difference
                     is less than 5, you need to increase the value of the
                     GBLSECTIONS parameter.

                  Section 1.6.6.2 describes the procedures for increasing these
                  values as well as those of other system parameters. See the
                  documentation on the VMS System Management Subkit for more
                  information.

                  After you reset the system parameter values, invoke the VMS
                  Install Utility from a privileged account and then install
                  VAX VTX as a shared image:

                                                 After Installing VAX VTX  3-15

 











                    $ INSTALL <Return>
                    INSTALL> ADD SYS$SHARE:VTXPAD.EXE /OPEN /SHARED /REPLACE 
<Return>
                    INSTALL> ADD SYS$SHARE:VTX$MSGSHR.EXE /OPEN /SHARED /REPLACE 
<Return>
                    INSTALL> EXIT <Return>

                  You must add the following lines to the appropriate system
                  startup command file so that each time you start the system,
                  VAX VTX is available as a shared image. If your site modu-
                  larizes its startup procedures, be sure you add the lines to
                  the correct file. The default startup command file for VMS
                  Version 5.n systems is SYS$MANAGER:SYSTARTUP_V5.COM.


































               3-16  After Installing VAX VTX

 











                                               NOTE

                      If you have previously used installed VTX images, make
                      sure you use REPLACE when you install VAX VTX. This
                      command has the following format:

                        $ INSTALL <Return>
                        INSTALL> REPLACE SYS$SYSTEM:VTXPAD.EXE /OPEN /SHARED 
<Return>

                  If you install VAX VTX as a shared image, you need to
                  increase the value of the global page and global sec-
                  tion parameters. Increase global pages (GBLPAGES) by 1300
                  pages and global sections (GBLSECTIONS) by 5 sections. See
                  Section 1.6.5 for information on changing these parameters.

               ____________________________________________________________

               3.9  Deleting the [.VTX$VISTA] Subdirectory

                  After Workbench information providers (IPs) start us-
                  ing the Workbench Utility, VAX VTX no longer requires the
                  [.VTX$VISTA] subdirectory. If you followed the procedure
                  specified in Section 1.6.13, the [.VTX$VISTA] subdirectory
                  should be empty and you can now delete it.

               ____________________________________________________________

               3.10  Print Queue and Workbench Output Files Directory

                  The print queue no longer uses the SYS$SYSROOT:[VISTA_FILES]
                  directory. When the VTXWPS_STARTUP.COM procedure starts
                  the VAX VTX Version 4.1 print queue, the system creates a
                  new directory, SYS$SYSROOT:[VTX$WB_FILES]. After the system
                  creates this directory, you can move all the files from the
                  [VISTA_FILES] directory to the [VTX$WB_FILES] directory using
                  the following command:

                    $ RENAME SYS$SYSROOT:[VISTA_FILES]*.* 
SYS$SYSROOT:[VTX$WB_FILES]*.* <Return>

                  After you move the files, the SYS$SYSROOT:[VISTA_FILES]
                  directory is empty and you can delete it.




                                                 After Installing VAX VTX  3-17

 










               ____________________________________________________________

               3.11  Workbench Server Command Procedure Changes

                  If your site previously used VISTA Version 3.n to create VTX
                  infobases, you must modify any command procedures you use
                  to start and stop the VTX Servers. Change the commands and
                  logical definitions as noted in Table 3-3.

                  Table 3-3:  Workbench Server Command Procedure Changes
                  _____________________________________________________________
                  Current:____________Change_to:_______________________________

                  START VISTA_SERVER  START WORKBENCH_SERVER

                  DEFINE VISTA$SERVER DEFINE VTX$WB_SERVER

                  DEFINE VISTA$STYLE  DEFINE VTX$WB_STYLEFILES

                  STOP_VISTA_SERVER___STOP_WORKBENCH_SERVER____________________

               ____________________________________________________________

               3.12  VAS Command Procedure Changes

                  Prior to VTX Version 4.0, the VAS runtime system was started
                  using VASCTL. If you have any existing procedures that use
                  VASCTL, they must be modified to use VTXCTL. All VASCTL
                  functionality has been merged into VTXCTL.

               ____________________________________________________________

               3.13  Determining and Reporting Problems

                  If an error occurs while using VAX VTX and you believe that
                  VAX VTX is causing the error, take one of the following
                  actions:

                   o Call your Customer Support Center if you have a BASIC or
                     DECsupport Software Agreement. With these services, you
                     receive telephone support that provides both high-level
                     advisory and remedial assistance.

                   o Submit a Software Performance Report (SPR) if you have a
                     Self-Maintenance Software Agreement.

               3-18  After Installing VAX VTX

 











                   o Submit a Software Performance Report (SPR) if you pur-
                     chased VAX VTX within the past 90 days and you think the
                     problem is caused by a software error.

                  If you find an error in the VAX VTX documentation, you should
                  fill out and submit the Reader's Comments form at the back of
                  the appropriate VAX VTX manual. Include the section and page
                  number that best describes where the error occurred.





































                                                 After Installing VAX VTX  3-19

 

















                                                                      Chapter 4


                                            Installation Verification Procedure
               ________________________________________________________________


                  Use the VAX VTX Installation Verification Procedure (IVP) to
                  verify the installation of the product. This procedure takes
                  about 15 minutes. For the most part, the instructions in this
                  chapter assume that you are verifying a new installation of
                  VAX VTX.

                  There are three different IVPs for VAX VTX. The IVP you run
                  depends on the VTX option you choose. The IVP for the full
                  kit consists of two parts, while the IVP for the VALU runtime
                  kit and the remote update kit have only one part each.

                  Even though you can install VAX VTX and run the IVP using
                  either a hardcopy or a video terminal, you must have a video
                  terminal to run the second part of the IVP for the full VTX
                  kit.

                                               NOTE

                      If you install only the TCP and the terminal concen-
                      trator, you cannot run the IVP. Also, if you have a
                      previous version of VAX VTX, certain files will al-
                      ready be in place. Therefore, you may need to slightly
                      modify some of these instructions.









                                       Installation Verification Procedure  4-1

 










               ____________________________________________________________

               4.1  Running the VAX VTX IVP

                  This section describes how to run the VAX VTX IVP. See
                  Section 4.2 for instructions on how to run the optional
                  portion of the IVP for the full VTX kit.

                  You can run the IVP during the VAX VTX installation proce-
                  dure. To run the IVP independent of the installation pro-
                  cedure, you must have VAX VTX Version 4.1 installed on your
                  system and you must log in to an account with privileges de-
                  scribed in Section 3.6. Before you run either the IVP or its
                  optional supplement (for the full VTX kit), you must have
                  DECnet running on your system.

                  Run the IVP command procedure using the command procedure:

                    $ @SYS$SYSROOT:[SYSTEST]VTX$IVP.COM <Return>

                  After you enter the command, a message appears indicating
                  that the IVP has begun:

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *

                      VAX VTX V4.1 Installation Verification Procedure

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *

                  The VTX$IVP.COM command procedure does the following:

                   o Creates a VAX VTX infobase

                   o Starts a VAX VTX server

                   o Starts a Workbench server

                   o Creates a Workbench library

                   o Stops the Workbench server

                   o Starts a VAS server

                   o Builds and loads VAS transaction definitions

                  See Appendix A for a sample installation of VAX VTX.

                  These operations verify the installation of the complete VAX
                  VTX kit.

               4-2  Installation Verification Procedure

 











                  The next message introduces the optional part of the IVP:

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * * *

                        You can now run the optional part of the IVP.  See
                        the "VTX Installation Guide" for instructions.

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * * *

                  The automated portion of the IVP is now complete. Assuming it
                  detected
                  no errors, the IVP displays the following message, regardless
                  of the
                  command procedures you chose to run the IVP:

                     * * * * *   S U C C E S S   * * * * *

                    VAX VTX V4.1 IVP completed successfully

                    * * * * *   S U C C E S S   * * * * *

               ____________________________________________________________

               4.2  Performing the Optional Part of the IVP

                  This section describes how to run the optional part of the
                  VAX VTX IVP for the full VTX kit. You must use a video termi-
                  nal to run this part of the IVP. You must also have VAX VTX
                  Version 4.1 installed on your system.

                  To perform this part of the VAX VTX IVP, follow these steps:

                   1. Enter the following command to start your VTX session:

                       $ VTX <Return>

                     A VTX menu with only one choice appears on the screen.

                   2. Enter 1 at the CHOICE: prompt and press RETURN:

                       Choice: 1 <Return>

                     VAX VTX displays a form with three fields on the screen.

                   3. Fill in each field with any string of text of no more than
                     five characters, and press the FORM ENTER function key
                     sequence (PF1-ENTER for Digital terminals).

                     A VTX display page appears on the screen. This is the last
                     page in the VAX VTX IVP.

                                       Installation Verification Procedure  4-3

 











                   4. Exit from VTX, using the EXIT function key sequence (PF1-.
                     for Digital terminals).

                     That completes the optional portion of the VAX VTX IVP.
                     Next you must stop the servers. To so so, follow these
                     steps:

                   1. Run the VTXCTL Utility using the following command:

                       $ Run SYS$SYSTEM:VTXCTL <Return>

                   2. Type the STOP commands and the EXIT command at the CTL>
                     prompt; for example:

                       CTL> STOP SERVER/NAME=IVP <Return>
                       CTL> STOP VAS/NAME=IVP <Return>
                       CTL> EXIT <Return>
                       $

                  Next, verify that the information you typed on the VAX VTX
                  form was accepted correctly. Enter the following command to
                  display the VAS log file, VASIVP.ASL:

                    $ TYPE VASIVP.ASL <Return>

                  Check that the text you entered in the three fields on the
                  VAX VTX form appends to the first line in the log file.

                  The log should also include two additional lines. The first
                  of those lines should contain the following text:

                    Installation Verification Procedure

                  The next line should indicate that the IVP has been success-
                  fully completed:

                    Installation Verification Procedure Successfully Completed

                  If you see this last line in the VAS.ASL file, you know that
                  the optional part of VAX VTX IVP processed correctly.





               4-4  Installation Verification Procedure

 










               ____________________________________________________________

               4.3  Conclusion

                  After you successfully perform all the IVP tasks, you have
                  installed your VAX VTX system correctly.

                  If you encounter any difficulties, first verify that the
                  appropriate files for starting VTX are in the expected direc-
                  tories. Next, make sure you have followed the procedures
                  in this manual, including setting up the correct quotas
                  and privileges. Then reinstall VTX. If failures still oc-
                  cur, submit an SPR or contact your local support office for
                  assistance.
































                                       Installation Verification Procedure  4-5

 

















                                                                     Appendix A


                                                            Sample Installation
               ________________________________________________________________


                  This appendix contains a sample installation for the VAX VTX
                  full development kit, using VMSINSTAL. This sample was run on
                  a system that had no previous version of VAX VTX installed.

                  If you do not install the full kit, you will not see all of
                  the following messages and questions when you perform your
                  installation. If you have other layered products on your
                  system, you may see additional messages and questions when
                  you perform your VAX VTX installation.


                    $ @SYS$UPDATE:VMSINSTAL VTX041 POLO$MUA6:

                     VAX/VMS Software Product Installation Procedure T5.4-4ET

                    It is 25-APR-1990 at 11:55.

                    Enter a question mark (?) at any time for help.
                    %VMSINSTAL-W-NOTSYSTEM, You are not logged in to the SYSTEM 
account.
                    %VMSINSTAL-W-ACTIVE, The following processes are still 
active:
                     VTXTEST
                     DECW$WM_1
                     DECW$WM_4
                     _TWA7:
                     VTXSRV_IVP
                     DECW$TE_1
                     VASIVP
                     _TWA6:
                    * Do you want to continue anyway [NO]? Y
                    * Are you satisfied with the backup of your system disk 
[YES]?


                                                       Sample Installation  A-1

 











                    The following products will be processed:
                      VTX V4.1

                     Beginning installation of VTX V4.1 at 11:55

                    %VMSINSTAL-I-RESTORE, Restoring product save set A ...
                    %VMSINSTAL-I-RELMOVED, Product's release notes have been 
moved to SYS$HELP.

                     
***************************************************************
                     *                                                           
  *
                     *                VAX VTX V4.1                               
  *
                     *                                                           
  *
                     *                  Installation Procedure                   
  *
                     *                                                           
  *
                     *        Copyright 1990, Digital Equipment Corporation      
  *
                     *                                                           
  *
                     
***************************************************************

                         1. Install Subscriber interface only

                         2. Conversational installation

                         3. Install Full VTX kit

                         4. Install Full VTX kit with TCP source code

                         5. Exit from this installation procedure

                    * Enter option [2]: ?

                        Please choose one of the 5 alternatives. The meaning of 
the
                        alternatives are:

                            1. Installs the VTX Subscriber interface only. This 
is
                               what you need to access a local or remote VXT 
Infobase.

                            2. Choice 2 takes you through a conversational 
installation,
                               where you can select the parts that you want to 
install.

                            3. Installs a complete VTX system, with all its
                               options, except for the TCP sources.

                               You do not need the TCP sources unless you are 
planning
                               to customize the VTX subscriber interface through 
source
                        code modifications.

                            4. Same as Choice 3 except that it also installs the 
TCP
                        sources.

                            5. Choice 5 exits from this installation procedure.

               A-2  Sample Installation

 











                    * Enter option [2]:

                        This is the conversational mode of VTX installation. You 
will
                        be asked to select the VTX options that you want to 
install.

                        If you are not sure about what a question means, please 
type a
                        question-mark (?) at the prompt. This will cause a more
                        detailed description to be displayed.

                        At the end of the questions you have the option of 
confirming
                        your selection or going back to this procedure's main 
menu.

                        
****************************************************************
































                                                       Sample Installation  A-3

 











                        You have the option of installing the VTX subscriber
                        environment. This option permits VTX users to access a
                        VTX infobase.

                    * Would you like to install the VTX subscriber environment 
[YES]? ?

                        SUBSCRIBER ENVIRONMENT
                        ----------------------

                        You have the option of installing the VTX subscriber
                        environment. This option includes the following parts:

                            #  VTXPAD; Subscriber's interface to VTX

                            #  VTXCON; Concentrator for VTX Subscriber sessions

                            #  MSDOS; Subscriber's interface to VTX for MS-DOS
                               (reference kit)

                        Please answer YES or NO.

                    * Would you like to install the VTX subscriber environment 
[YES]?

                        You have the option of installing the Information 
Provider tools
                        part of VTX. They are required in order to update a VTX 
infobase.

                        This option requires the VTX Subscriber Environment.

                    * Would you like to install the VTX Information Provider 
tools [YES]? ?

                        INFORMATION PROVIDER TOOLS
                        --------------------------

                        The Information Provider's tools are required in order 
to update
                        a VTX Infobase. This installation option includes the 
following
                        tools:

                            #  APMS; Automatic Page Management System

                            #  WPSSMB; A tool for paginating WPS-PLUS documents 
for use
                                in VTX

                            #  PAGER; A tool for paginating DDIF documents and 
text files

                            #  WBGI; Workbench graphical interface.

                            #  WBCLU; Workbench command language.

                            #  UPD; A command language updating a VTX infobase

                            #  RUSL; A callable interface for remote updates of 
VTX infobases

                            #  IVU; Infobase Verification Utility.

                        This option implies that the VTX Subscriber environment 
be installed.

               A-4  Sample Installation

 











                        Please answer YES or NO.

                    * Would you like to install the VTX Information Provider 
tools [YES]?

                        A few file formats for information provider tools 
changed between
                        VTX V3.x and V4.0. However, nothing has changed between 
V4.0 and
                        V4.1. If you plan to convert VTX files from a VTX V3.x 
system then
                        this option is of value to you, otherwise not.





































                                                       Sample Installation  A-5

 











                    * Would you like to install VTX V3.x IP Conversion tools 
[YES]? ?

                        V3.X CONVERSIONS
                        ----------------

                        A few file formats for Information Provider tools 
changed between
                        VTX V3.x and V4.0. This option includes the following 
conversion
                        tools:

                            #  PFC; Page File conversion tool

                            #  VLC; Converts a VISTA library to a Workbench 
library

                            #  IAF; Converts a APMS Index

                        If you plan to convert any VTX V3.x files associated 
with any of
                        the above three tools to V4.0 format then you should 
answer YES
                        to this option.

                        Please note that there are no file conversions needed if 
you go from
                        V4.0 to V4.1.

                    * Would you like to install VTX V3.x IP Conversion tools 
[YES]?

                        You have the option of installing the files needed to 
run any of
                        the VTX servers on this system.

                    * Would you like to install the VTX Servers [YES]? ?

                        SERVERS
                        -------

                        The VTX Server environment contains the following parts:

                            #  SRV; Allows local and remote VTX Subscribers to 
access a
                               VTX infobase on this system

                            #  UPDSRV; Allows remote VTX Information Providers 
to update
                               VTX infobases on this system.

                            #  WBSRV; Allows remote VTX Information Providers to 
access
                               Workbench libraries on this system.

                            #  ACU; VTX infobase access Authorization and 
Accounting utility

                        Please answer YES or NO.

                    * Would you like to install the VTX Servers [YES]?

                        You have the option of installing the VTX tools required 
to create
                        and run a VTX Back End Application.

                    * Would you like to install the VTX Back End environment 
[YES]? ?

               A-6  Sample Installation

 











                        BACK END APPLICATIONS
                        ---------------------

                        VTX Back End applications are programs that are started 
in
                        response to a subscriber referencing a specific page in 
a
                        VTX Infobase. The Back End Application can dynamically 
create
                        the actual VTX page from private data or by asking a 
remote
                        computer, such as an IBM Mainframe.  It can also guide 
the
                        VTX Server that is connected to it, to display pages 
already
                        in its infobase.

                        This option includes the following parts:

                            #  VAS; A high level programming interface for 
writing VTX
                               Back End applications.

                            #  ELK; A low level programming interface to writing 
a VTX
                               Back End applications

                        Both components include their programming interface and 
their
                        associated run-time environment.

                        Please answer YES or NO.

                    * Would you like to install the VTX Back End environment 
[YES]?

                        The VTX Subscriber interface can be customized somewhat 
by
                        changing the source code. Please refer to your VTX 
Warranty
                        Exclusion for details on what can be changed without 
violating
                        your standard VTX support contract.

                        You need access to a BLISS32 compiler in order to 
compile the
                        changes.

                    * Would you like to install the TCP source code [NO]? ?

                        MODIFIED TSMs
                        -------------

                        The VTX Subscriber interface can be customized somewhat 
by
                        changing the source code. Please refer to your VTX 
Warranty
                        Exclusion for details on what can be changed without 
violating
                        your standard VTX support contract.

                        This option will install the files you may need when you
                        customize the Front End as well as related files to 
relink
                        the PAD, CON and CTL.

                        You need access to a BLISS32 compiler in order to 
compile the
                        changes.

                                                       Sample Installation  A-7

 











                        Please answer YES or NO.

                    * Would you like to install the TCP source code [NO]?

                        This version has added a new keypad. The new keypad is a
                        superset of the traditional VTX default keypad and the
                        ALL-IN-1 keypad, except where there were conflicting 
mappings.

                        You have the option of making the new keypad the default 
keypad,
                        instead of the one that was default in previous versions 
of VTX.

                    * Would you like to install the new keypad [NO]? ?

                        DEFAULT DEVICE/KEYPAD
                        ---------------------

                        This version has added a new keypad, the COMMON keypad.
                        The COMMON keypad is a superset of the traditional VTX
                        default keypad and the ALL-IN-1 keypad, except where 
there
                        were conflicting mappings. The Subscriber's Booklet 
describes
                        the exact layout of the new keypad.

                        This installation option allows you to make the new 
keypad
                        the default keypad on your system. The default can be
                        overriden by a logical name (VTX$DEFAULT_DEVICE) and 
also by
                        the user explicitly stating desired keypad at command 
line.

                        If you answer YES the COMMON keypad will be your system
                        default keypad. If you answer NO the traditional VTX 
keypad
                        will be your system default keypad.

                    * Would you like to install the new keypad [YES]?
                    %VTX-I-ENDCONV, end of questions in conversational part
                    * Do you want to purge files replaced by this installation 
[YES]?
                    * Do you want files made obsolete by this installation 
deleted [YES]?

                     This kit contains an Installation Verification Procedure
                     to verify the correct installation of VAX VTX.

                    * Do you want to run the IVP after the installation [YES]?
                    * Are you satisfied with all your answers for this 
installation [YES]?

                     All questions regarding the installation of VAX VTX have 
now
                     been asked.

                     Depending on your configuration, current system activity 
and
                     options you selected during this installation, it will
                     continue from 20 minutes to 4 hours and 20 minutes.

               A-8  Sample Installation

 











                     It takes 4 hours and 20 minutes to install the complete
                     VTX kit, including the optional TCP sources followed by
                     running the IVP, on a VAXstation 2000. It takes 
approximately
                     20 minutes to install the complete kit on a VAX 8800.

                    %VMSINSTAL-I-RESTORE, Restoring product save set B ...
                    %VMSINSTAL-I-RESTORE, Restoring product save set C ...
                    %VMSINSTAL-I-RESTORE, Restoring product save set D ...
                    %VTX-I-BUILD, building core files
                    %VTX-I-LINK, linking VTX$MSGSHR ..
                    %VTX-I-LINK, linking VTX$DSLSHR ..
                    %VTX-I-LINK, linking VTXCTL ..
                    %VTX-I-BUILD, building files for IVP
                    %VTX-I-BUILD, building subscriber environment
                    %VTX-I-LINK, linking VTXPAD ..
                    %VTX-I-LINK, linking VTXCON ..
                    %VTX-I-LINK, linking VTX$PANESHR ..
                    %VTX-I-BUILD, building IP tools
                    %VTX-I-LINK, linking VTXAPMS ..
                    %VTX-I-LINK, linking VTXWPSSMB ..
                    %VTX-I-LINK, linking VTX$PAGER ..
                    %VTX-I-LINK, linking VTX$WBCLU ..
                    %VTX-I-LINK, linking VTX$WBGI ..
                    %VTX-I-LINK, linking RUSLSHR ..
                    %VTX-I-LINK, linking VTXUPD ..
                    %VTX-I-LINK, linking VTXIVU ..
                    %VTX-I-BUILD, building IP conversion tools
                    %VTX-I-LINK, linking VTXPFC ..
                    %VTX-I-LINK, linking VTXVLC_V4 ..
                    %VTX-I-LINK, linking VTXIAF_V4_CONVERT ..
                    %VTX-I-BUILD, building servers
                    %VTX-I-LINK, linking VTXSRV ..
                    %VTX-I-LINK, linking VTXUPDSRV ..
                    %VTX-I-LINK, linking VTX$WBSRV ..
                    %VTX-I-LINK, linking VTXACU ..
                    %VTX-I-BUILD, building backend environment
                    %VTX-I-LINK, linking ELKSHR ..
                    %VTX-I-LINK, linking VASMSGSHR ..
                    %VTX-I-LINK, linking VAS ..
                    %VTX-I-DELOBS, Deleting obsolete files
                    %VMSINSTAL-I-MOVEFILES, Files will now be moved to their 
target
                    directories...

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *

                                                       Sample Installation  A-9

 











                      VAX VTX V4.1 Installation Verification Procedure

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *
                        This part of the IVP leaves the following files
                        in your SYS$LOGIN:

                     VTX$IVPVTD.VTD
                     VTX$IVPWORKBENCH.VTD

                        You may want to delete these files after the IVP
                        has completed.

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *
                    %VTXIVP-I-UPD, running VTXUPD to create IVP infobase
                    VAX VTX Infobase Update Utility V4.1
                    %VTX-I-RNGMSG1, Your current range is 0 to 9~~~~~~~~~~~~~
                    %VTX-I-RNGMSG2, The range for page file SYS$LOGIN:VTX$IVPVTD 
is
                    0 to 9~~~~~~~~~~~~~
                    Total of 4 pages added
                    %VTX-I-RNGMSG1, Your current range is 0 to 9~~~~~~~~~~~~~
                    %VTX-I-RNGMSG2, The range for page file 
SYS$LOGIN:VTX$IVPWORKBENCH is
                    0 to 9~~~~~~~~~~~~~
                    %VTX-I-PAGFILCLS, Page file SYS$LOGIN:VTX$IVPWORKBENCH 
closed
                    %VTX-I-PAGFILCLS, Page file SYS$LOGIN:VTX$IVPVTD closed
                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *

                        This part of the IVP leaves the following files
                        in your SYS$LOGIN:

                     VTXBASE.TXT     VTXACF.VTA
                     VTXSERVER.COM     VTX$WBSRV.COM
                     VTXSRV_IVP.VTE

                        You may want to delete these files after the IVP
                        has completed.

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *"

                        This part of the IVP uses DECnet objects 43 and 59.
                        If these objects are currently being used on
                        this system, this IVP may signal success even
                        though not all components have been tested.

               A-10  Sample Installation

 











                        If extraneous errors occur while executing this
                        procedure, stop all existing VTX, Workbench,
                        and Update servers, as well as VAS runtime images
                        and execute this procedure again.

                        Refer to the VAX VTX Installation Guide for further
                        details on the Installation Verification Procedure.

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *




































                                                      Sample Installation  A-11

 











                    Ignore any ACU_ERROPNACF and FNF error messages, they are 
normal.

                                         VAX VTX Account Control Utility V4.1

                    %VTX-W-ACU_ERROPNACF, VTXACF.VTA Account file could not be 
opened
                    -RMS-E-FNF, file not found
                    Account file VTXACF.VTA has been created.

                    Account successfully added
                    VTXACF.VTA account file modified
                    %VTXIVP-I-SRV, starting a VTX infobase server
                                            VAX VTX Control Program V4.1

                    ...Working...
                    ...Working...

                    %VTXIVP-I-WORKBENCH, starting a VTX Workbench server

                    Ignore any ERROPNLIB and INVLIBFIL messages
                    They simply mean that old library files exist
                    for this account, and are normal.

                                            VAX VTX Control Program V4.1

                    ...Working...

                    %VTX-I-LIBCREATED, new Workbench library created

                                            VAX VTX Control Program V4.1

                    ...Working...
                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *

                        This part of the IVP leaves the following files
                        in your SYS$LOGIN:

                         VTX$IVPTDS.TDS VAS.COM
                         VTX$IVPTDS.TDI VASIVP.ASL
                         VTX$IVPTDS.LIS VASIVP.ASE

                        You may want to delete these files after the IVP
                        has completed.

                    * * * * * * * * * * * * * * * * * * * * * * * * * * * *
                    %VTXIVP-I-VAS, starting a VAS server
                                            VAX VTX Control Program V4.1

                    ...Working...

               A-12  Sample Installation

 











                    Known VAS status as of 25-APR-1990 10:16:12.63
                    VAS started:       25-APR-1990 10:16:09.50
                    Communication  ENABLED  DECNET object number: 59
                    Oper notification DISABLED
                    Logging for log channel VAS$LOG_CHANNEL
                     written to log file SYS$SYSDEVICE:[VTXTEST]VASIVP.ASL;1
                    Transactions loaded from: 
SYS$SYSDEVICE:[VTXTEST]VTX$IVPTDI.TDI;1
                    No CURs loaded
                    VTX form pages displayed to date: 0
                    Total number of requests made:    0
                    ----------------------------------------------------
                    Sessions       Current active:      0
                                   Current stopping:    0
                                   Total connects:      0
                    ----------------------------------------------------

                        * * * * *   S U C C E S S   * * * * *

                       VAX VTX V4.1 IVP completed successfully

                        * * * * *   S U C C E S S   * * * * *

                     Installation of VTX V4.1 completed at 10:16

                     VMSINSTAL procedure done at 10:17




















                                                      Sample Installation  A-13

 

















                                                                     Appendix B


                           VTX Files and Logical Names Installed on Your System
               ________________________________________________________________


                  The VAX VTX installation procedure installs various files on
                  your system and defines several logical names. Section B.1
                  lists the files the procedure installs. Section B.2 lists
                  the logical names that are added to the system logical name
                  table.

               ____________________________________________________________

               B.1  File Names

                  The following subsections contain the names of all files the
                  VAX VTX installation procedure installs on your system. These
                  lists contain files left by the full VTX installation. If you
                  choose to install a different option, only a subset of these
                  files will remain.

                                               NOTE

                      The figures given in the Blocks columns of the tables
                      are approximate values and may differ from the size of
                      the files installed on your system.

               ____________________________________________________________

               B.1.1  SYS$COMMON:[ELKLIB]

                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VTXELKDEF.BAS                     28


                      VTX Files and Logical Names Installed on Your System  B-1

 










                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VTXELKDEF.COB                     28

                  VTXELKDEF.FOR                     26

                  VTXELKDEF.H                       21

                  VTXELKDEF.PAS                     27

                  VTXELKDEF.REQ                     23

                  VTXELKLIB.OPT______________________3_________________________

                  Total of 7 files and 156 blocks

               ____________________________________________________________

               B.1.2  SYS$COMMON:[RUSLLIB]


                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  RUSLDEF.BAS                       41

                  RUSLDEF.COB                       41

                  RUSLDEF.FOR                       27

                  RUSLDEF.H                         41

                  RUSLDEF.PAS                       56

                  RUSLDEF.R32                       28

                  RUSLOPT.OPT________________________3_________________________

                  Total of 7 files and 237 blocks






               B-2  VTX Files and Logical Names Installed on Your System

 










               ____________________________________________________________

               B.1.3  SYS$COMMON:[SYS$STARTUP]


                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VTXWPS_STARTUP.COM_________________8_________________________

                  Total of 1 file and 8 blocks

               ____________________________________________________________

               B.1.4  SYS$COMMON:[SYSEXE]

                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VAS.EXE                          167

                  VASSNA.EXE                        22

                  VTX$PAGER.EXE                     32

                  VTX$WBCLU.EXE                    181

                  VTX$WBGI.EXE                     428

                  VTX$WBSRV.EXE                    240

                  VTXACU.EXE                       103

                  VTXAPMS.EXE                      123

                  VTXCON.EXE                       875

                  VTXCTL.EXE                       275

                  VTXIAF_V4_CONVERT.EXE             12

                  VTXIVU.EXE                        62

                  VTXPAD.EXE                       954


                      VTX Files and Logical Names Installed on Your System  B-3

 










                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VTXPFC_V4.EXE                     27

                  VTXSRV.EXE                       140

                  VTXUPD.EXE                       543

                  VTXUPDSRV.EXE                     96

                  VTXVLC_V4.EXE                     31

                  VTXWPSSMB.EXE____________________107_________________________

                  Total of 19 files and 4418 blocks

               ____________________________________________________________

               B.1.5  SYS$COMMON:[SYSHLP]


                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VASCTLHLP.HLB                     90

                  VTX$TCP_DW.HLB                   145

                  VTX041.RELEASE_NOTES             101

                  VTXACUHLP.HLB                    106

                  VTXAPMS.HLB                       58

                  VTXCTLCON.HLB                     65

                  VTXCTLCTL.HLB                    151

                  VTXCTLSRV.HLB                     73

                  VTXCTLUPD.HLB                     40




               B-4  VTX Files and Logical Names Installed on Your System

 










                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VTXCTLWBSRV.HLB                   44

                  VTXDCLHLP.HLP                     54

                  VTXIVUHLP.HLB                     22

                  VTXUPDHLP.HLB                    209

                  VTXUPDMNUHLP.HLB__________________37_________________________

                  Total of 14 files and 1195 blocks

               ____________________________________________________________

               B.1.6  SYS$COMMON:[SYSLIB]


                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  ELKSHR.EXE                        37

                  RUSLSHR.EXE                       78

                  VTPDCL.CLD                        38

                  VTX$DSLSHR.EXE                   112

                  VTX$PANESHR.EXE                   44

                  VTX$TCP_DW.UID                   152

                  VTX$WSSVNSHR.EXE_________________202_________________________

                  Total of 7 files and 663 blocks








                      VTX Files and Logical Names Installed on Your System  B-5

 










               ____________________________________________________________

               B.1.7  SYS$COMMON:[SYSMSG]


                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  TCPMSG.EXE                       388

                  VASMSGSHR.EXE                     44

                  VTX$MSGSHR.EXE___________________388_________________________

                  Total of 3 files and 820 blocks

               ____________________________________________________________

               B.1.8  SYS$COMMON:[SYSTEST.VTX]

                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VTX$IVPTDS.TDS                     2

                  VTX$IVPVTD.VTD                    21

                  VTX$IVPVTU.VTU                     1

                  VTX$IVPWORKBENCH.VTD              21

                  VTX$IVP_BACKEND.COM               10

                  VTX$IVP_IPTOOL.COM                10

                  VTX$IVP_SERVER.COM________________16_________________________

                  Total of 7 files and 81 blocks








               B-6  VTX Files and Logical Names Installed on Your System

 










               ____________________________________________________________

               B.1.9  SYS$COMMON:[SYSTEST]


                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VTX$IVP.COM________________________7_________________________

                  Total of 1 file and 7 blocks

               ____________________________________________________________

               B.1.10  SYS$COMMON:[TCPLIB]

                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  A1_LOCAL_COMMAND.OBJ               2

                  A2VTPDEC.B32                     544

                  A2VTPLOCAL.CLD                     3

                  ADVTPDEC.B32                     544

                  CALLPADLNK.COM                    43

                  CONCMD.CLD                        32

                  CONCMD.OBJ                        27

                  CTL.OLB                          896

                  CTLCMD.CLD                        12

                  CTLCMD.OBJ                        13

                  CTLDEF.L32                        28

                  CTLMSG.MSG                        49

                  CTLMSG.OBJ                        49


                      VTX Files and Logical Names Installed on Your System  B-7

 










                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  DSLDEF.L32                        24

                  LINKCON.COM                        4

                  LINKCON_3270.COM                   4

                  LINKCTL.COM                        4

                  LINKPAD.COM                        4

                  LINKPAD_NODECW.COM                 4

                  LINKTCPMSG.COM                     3

                  LOCAL_COMMAND.OBJ                  2

                  MINILOCAL.CLD                      4

                  MINITEL_LOCAL_COMMAND.OBJ          2

                  PAD.OLB                         2208

                  PADXFER.OLB                      122

                  SRVCMD.CLD                        17

                  SRVCMD.OBJ                        12

                  SRVMSG.MSG                         6

                  TCPDEF.L32                       525

                  TCPHLPMSG.MSG                    382

                  TCPHLPMSG.OBJ                    579

                  TCPMSG.MSG                        50

                  TCPMSG.OBJ                        57




               B-8  VTX Files and Logical Names Installed on Your System

 










                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  UPDSRVCMD.CLD                     10

                  UPDSRVCMD.OBJ                      8

                  VAPDEF.L32                        74

                  VASMSG.MSG                       146

                  VASMSG.OBJ                        56

                  VISTASRV_CMD.CLD                  12

                  VISTASRV_CMD.OBJ                   9

                  VTCDECWINDOWS.OBJ                  2

                  VTPCEPT.B32                      202

                  VTPDCL.CLD                        38

                  VTPDEC.B32                       333

                  VTPDECWINDOWS.B32                537

                  VTPDECW_DEFS.L32                 339

                  VTPDECW_HELP.HLP                 137

                  VTPDECW_HELP.L32                  34

                  VTPDECW_UIL.UIL                    5

                  VTPDECW_UILDEF.UIL               138

                  VTPDECW_UILHELP.UIL                8

                  VTPDECW_UILMENU.UIL              159

                  VTPDECW_UILMISC.UIL               14




                      VTX Files and Logical Names Installed on Your System  B-9

 










                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VTPIBM.B32                       245

                  VTPINIT.B32                       58

                  VTPLOCAL.CLD                       4

                  VTPMINITEL.B32                   253

                  VTPNAPLPS.B32                    280

                  VTPNORPAK.B32                    241

                  VTPPN.B32                        223

                  VTPPSI.B32                       100

                  VTPRESTEL.B32                    236

                  VTPSNA3270DS.B32                 409

                  VTPTALK.B32                      185

                  VTPVTX20.B32                     494

                  VTPVWS.B32                       258

                  VTX$IDENT.OPT                      2

                  VTX$LMF.OBJ                        4

                  VTX$SNA3270DF.R32                 43

                  VTX$UISENTRY.R32                 181

                  VTX.MSG                          528

                  VTX.OBJ                          574

                  VTX20LOCAL.CLD                     4




               B-10  VTX Files and Logical Names Installed on Your System

 










                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VTX20_LOCAL_COMMAND.OBJ            2

                  VTXUTIL.OBJ________________________5_________________________

                  Total of 75 files and 12845 blocks

               ____________________________________________________________

               B.1.11  SYS$COMMON:[VASLIB]


                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VAS.COM                            4

                  VASSNA.COM_________________________3_________________________

                  Total of 2 files and 7 blocks
























                     VTX Files and Logical Names Installed on Your System  B-11

 










               ____________________________________________________________

               B.1.12  SYS$COMMON:[VTX$LIBRARY]


                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  SAMPLE_STYLE.VTX                   1

                  VTX$DOSTCP.EXE                   175

                  VTX$PCHLPAT.TXT                   19

                  VTX$PCHLPATAP.TXT                 19

                  VTX$PCHLPEP.TXT                   19

                  VTX$PCHLPEPAP.TXT                 19

                  VTX$PCHLPLK.TXT                   20

                  VTX$PCHLPLKAP.TXT                 20

                  VTX$PCHLPXT.TXT                   19

                  VTX$PCHLPXTAP.TXT                 19

                  VTX$WBSRV.COM                      6

                  VTX.PRA                            1

                  VTX.PRC                            7

                  VTXBASE.TXT                        2

                  VTXCON.COM                         5

                  VTXDOSIN.BAT                       4

                  VTXDOSQ.EXE                       32

                  VTXIAF_V4_CONVERT.CLD              3



               B-12  VTX Files and Logical Names Installed on Your System

 










                  _____________________________________________________________
                  File____________________________Blocks_______________________

                  VTXIAF_V4_CONVERT.COM              4

                  VTXIAF_V4_CONVERT.FDL              6

                  VTXMAIN.VTU                       67

                  VTXOPTIONS.OPT                     7

                  VTXPFC_V3_UNTUNED.FDL              4

                  VTXPFC_V4_CLD.CLD                  3

                  VTXPFC_V4_CONVERT.COM              5

                  VTXPFC_V4_FDL.FDL                  5

                  VTXSERVER.COM                      8

                  VTXUPDSRV.COM                      6

                  VTXVLC_V4.COM                      5

                  VTXVLC_V4_CLD.CLD                  3

                  VTXWPS_FILE_HEADERS.               3

                  VTX_INTERNALS.VTU_________________39_________________________


               ____________________________________________________________

               B.2  Logical Names

                  VAX VTX enters no logical names into the system logical
                  name table when you install VAX VTX. The VTXWPS_STARTUP.COM
                  file defines the following logical names. These names are
                  automatically entered into the system logical name table if
                  the system is rebooted or if the software is invoked.

                   o VTX$WB_FILES-Points to SYS$COMMON:[VTX$WB_FILES]

                   o VTX$VTU_FILES-Points to SYS$COMMON:[VTU_FILES]

                     VTX Files and Logical Names Installed on Your System  B-13

 











                  If you are installing the VALU components of VAX VTX, you
                  should define three system logicals at startup time. These
                  logicals are needed to compile ELK and RUSL applications.
                  You can include these DEFINE commands in the system startup
                  command file:

                    $ DEFINE/SYSTEM/EXECUTIVE ELK$LIB SYS$SYSROOT:[ELKLIB]
                    $ DEFINE/SYSTEM/EXECUTIVE RUSL$LIBRARY SYS$SYSROOT:[RUSLLIB]
                    $ DEFINE/SYSTEM/EXECUTIVE RUSL$LIB SYS$SYSROOT:[RUSLLIB]




































               B-14  VTX Files and Logical Names Installed on Your System

 




















                                                                      Index
               ________________________________________________________________


               A___________________________    After installing VAX VTX

               Aborting the installation,        Enhancing performance
                  2-2                              (Cont.)
               Accessing the online release         Installing VTX as a
                  notes, 2-1                          shared image, 3-13
               Account quotas, 3-6                  Tuning your system,
               After installing VAX VTX               3-13
                 Cluster considerations,         Establishing a print queue
                    3-5                            , 3-1
                 Configuring print tables,       Print queue and workbench
                    3-2                            output files, 3-17
                 Creating VTX Operator           Subscriber account
                    account, 3-10                  requirements and quotas,
                 DECnet, 3-8                       3-6
                    Establishing a DECnet           Privileges, 3-6
                       node, 3-8                 Using search lists, 3-12
                    Starting DECnet, 3-8       Audience, vii
                 Defining system logicals,     AUTOGEN command, 1-9
                    3-7
                 Deleting the .VTX$VISTA       B
                    subdirectory, 3-17         ____________________________
                 Editing the system startup    Books in the documentation
                    file, 3-2                     set, viii

                 Enhancing performance,        C
                    3-12                       ____________________________
                                               Changes

                                                                        Index-1

 






          Changes (Cont.)                 Deleting (Cont.)
            To the workbench server         VTX$VISTA subdirectory,
               command procedure, 3-18        3-17
            To VAS command procedure,     Determining and reporting
               3-18                          problems, 3-18
          Changing system parameters      Disk space needed to install
             with AUTOGEN, 1-9               VAX VTX, 1-5
          Checking
            System parameter values,      E___________________________

               1-8                        Editing the system startup
          Choosing                           file, 3-2
            To continue the installa-     Enhancing VTX performance,
               tion, 2-7                     3-12
            To purge files, 2-14            Installing VTX as a shared
            To run the Installation           image, 3-13
               Verification Procedure       Tuning your system, 3-13
               (IVP), 2-17                Error recovery, 2-23
          Cluster considerations, 3-5     Establishing
          Compatible Digital software,      DECnet node, 3-8
             1-2                            Print queue, 3-1
          Completing the installation     Example VAX VTX installation
             procedure, 2-18                 , A-1
          Configuring print tables for
             VTX$QUEUE, 3-2               F___________________________
          Conventions used in this        Files added to
             manual, ix                     SYS$COMMON:[ELKLIB], B-1
          Converting old VTX files,         SYS$COMMON:[RUSLLIB], B-2
             1-14                           SYS$COMMON:[SYS$STARTUP],
          Creating a VTX Operator             B-3
             account, 3-10                  SYS$COMMON:[SYSEXE], B-3
                                            SYS$COMMON:[SYSHLP], B-4
          D___________________________      SYS$COMMON:[SYSLIB], B-5
          DECnet                            SYS$COMMON:[SYSMSG], B-6
            Establishing a node, 3-8        SYS$COMMON:[SYSTEST.VTX],
            Starting, 3-8                     B-6
          Defining system logicals,         SYS$COMMON:[SYSTEST], B-7
             3-7                            SYS$COMMON:[TCPLIB], B-7
          Deleting                          SYS$COMMON:[VASLIB], B-11
            Obsolete files, 2-14            SYS$COMMON:[VTX$LIBRARY],
                                              B-12

          Index-2

 






          Files and logical names         Installing VAX VTX
             installed on your system,      General information
             B-1                              (Cont.)
          Files made obsolete by the           Aborting the installa-
             installation procedure,             tion, 2-2
             2-14                              Accessing online

          G                                      release notes, 2-1
          ____________________________         Running the IVP, 2-2
          General information on            Invoking VMSINSTAL, 2-3
             installing VAX VTX, 2-1        Media used, 1-4
            Aborting the installation,      Preparations and
               2-2                            requirements, 1-1
            Accessing online release        The installation procedure
               notes, 2-1                     , 2-2
            Running the IVP, 2-2               Completing the
                                                 procedure, 2-18
          H___________________________         Informational messages,
          Hardware requirements, 1-2             2-17
                                               Questions, 2-4
          I                                    Running the IVP, 2-17
          ____________________________    Intended audience, vii
          Installation procedure
             requirements, 1-4            L___________________________
            Disk space needed, 1-5        Licensing, 1-3
            Media used, 1-4                 Management of, 1-3
            Privileges needed, 1-4        Logical names added to your
            System parameters, 1-6           system, B-13
            Time taken, 1-4
          Installation Verification       M
             Procedure                    ____________________________
            Requirements, 1-13            Managing your licenses, 1-3
            Running the IVP, 4-2          Managing your VTX licenses
            Running the optional part,      See Licensing
               4-3                        Media used for VAX VTX
          Installing the MS-DOS TCP on       installation, 1-4
             Your PC, 2-18                Messages, 2-17
          Installing VAX VTX              MODPARAMS.DAT file, 1-9
            As a shared image, 3-13       MS-DOS Terminal Control
            Error recovery, 2-23             Program (TCP)
            General information, 2-1        Installing on PCs, 2-18

                                                                   Index-3

 






          N___________________________    Purging files during

          Names of files installed on        installation, 2-14
             your system, B-1             Purpose of this manual, vii

          ____________________________    Q___________________________

          Obsolete files, deleting,       Questions asked during
             2-14                            installation, 2-4
          Operating system                Quotas
            Components required, 1-1        For subscriber accounts,
            Information, vii                  3-6
          Operator account, 3-10            Page file, 1-10
          Optional software, 1-2            Process account, 1-10
          Output files directory for        Subscriber accounts, 3-6
             Workbench, 3-17              R

          P                               ____________________________
          ____________________________    Recovering from errors, 2-23
          Page file quotas, 1-10          Related documentation, viii
          Performance enhancements,       Reporting problems, 3-18
             3-12                         Required
            Installing VTX as a shared      Operating system
               image, 3-13                    components, 1-1
            Tuning your system, 3-13        System parameter values,
          Performing the optional part        3-13
             of the IVP, 4-3              Requirements
          Preparing to install VAX          For the IVP, 1-13
             VTX, 1-1                       For VAX VTX VISTA Utility,
          Prerequisite                        1-14
            Hardware, 1-2                   For VMSINSTAL, 1-12
            Software, 1-2                   Installation procedure,
          Print                               1-4
            Queues                             Disk space needed, 1-5
               Establishing, 3-1               Media, 1-4
               Workbench output files,         Privileges needed, 1-4
                  3-17                         System parameters, 1-6
            Tables, 3-2                        Time taken, 1-4
          Privileges                        Page file quota, 1-10
            Io install VAX VTX, 1-4         Process account quotas,
            Subscriber accounts, 3-6          1-10
          Problems, determining and         VAX VTX, 1-13

             reporting, 3-18
          Process account quotas, 1-10

          Index-4

 






          Running the Installation        SYS$COMMON:[VTX$LIBRARY]
             Verification Procedure         Files added, B-12
             (IVP), 2-2, 2-17, 4-2        System
                                            Generation Utility, 1-8
          S___________________________      Logicals, 3-7
          Search lists, 3-12                Parameters, 1-6
          Selecting VAX VTX components      Startup file, 3-2
                                          SYSUAF.DAT file, 3-6
             to install, 2-7
          Software                        T___________________________
            Optional, 1-2                 Tables
            Prerequisite, 1-2               Disk space requirements,
          Starting DECnet, 3-8                1-5
          Structure of this manual,         Process account quotas,
             viii                             1-10
          Subscriber account              The installation procedure,
            Privileges, 3-6
            Quotas, 3-6                      2-2
          Subscriber account                Choosing
             requirements and quotas,          To continue, 2-7
             3-6                               To purge files, 2-14
          SYS$COMMON:, B-1                     To run the IVP, 2-17
            See Files added to              Completing the installa-
          SYS$COMMON:[RUSLLIB]                tion procedure, 2-18
            Files added, B-2                Deleting obsolete files,
          SYS$COMMON:[SYS$STARTUP]            2-14
            Files added, B-3                Informational messages,
          SYS$COMMON:[SYSEXE]                 2-17
            Files added, B-3                Invoking VMSINSTAL, 2-3
          SYS$COMMON:[SYSHLP]               Questions, 2-4
            Files added, B-4                Running the IVP, 2-17
          SYS$COMMON:[SYSLIB]               Selecting VAX VTX
            Files added, B-5                  components, 2-7
          SYS$COMMON:[SYSMSG]             Time taken to install VAX
            Files added, B-6                 VTX, 1-4
          SYS$COMMON:[SYSTEST.VTX]        Tuning your system, 3-13
            Files added, B-6              Types of licenses for VAX
          SYS$COMMON:[SYSTEST]               VTX, 1-3
            Files added, B-7                See Licenses
          SYS$COMMON:[TCPLIB]
            Files added, B-7              U
          SYS$COMMON:[VASLIB]             ____________________________
            Files added, B-11

                                                                   Index-5

 






          Using AUTOGEN to change           Licensing, 1-3
             system parameter values,       Requirements, 1-13
             1-9                            VISTA Utility requirements
          Using search lists, 3-12            , 1-14
                                          VMS Authorize Utility, 3-6
          V___________________________    VMSINSTAL
          VAS command procedure             Invoking, 2-3
                                            Requirements, 1-12
             changes, 3-18                VMS tailoring classes, 1-1
          VAX VTX                         VTX$QUEUE, 3-2
            Components                    VTX$VISTA subdirectory,
               Selecting which ones to       deleting, 3-17
                  install, 2-7
            Converting old files, 1-14    W___________________________
            General information about     Workbench
               installing, 2-1              Output files directory,
               Aborting the installa-         3-17
                  tion, 2-2                 Server command procedure
               Accessing online               changes, 3-18
                  release notes, 2-1
               Running IVP, 2-2


















          Index-6

