 






          System
          Support
          Addendum

          ________________________________________________________________

          PRODUCT NAME:  WPS-PLUS/FRANÇAIS for VMS, Version 4.0         
	  SSA 27.91.03-A

          HARDWARE REQUIREMENTS

          Processors Supported

          VAX:      VAXft 3000-310,
                    VAX 4000 Model 300,
                    VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series,
                    VAX 6000 Model 500 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840

                    VAX 9000-210, VAX 9000-410

                    VAX-11/730, VAX-11/750, VAX-11/780,
                    VAX-11/785

          MicroVAX: MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,
                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900




                                       DIGITAL                  July 1991

                                                               AE-PGY8A-TE

 


          WPS-PLUS/FRANÇAIS for VMS, Version 4.0             SSA 27.91.03-A




          VAXstation: VAXstation II, VAXstation 2000,
                      VAXstation 3100 Series, VAXstation 3200,
                      VAXstation 3500, VAXstation 3520,
                      VAXstation 3540

          VAXserver:  VAXserver 3100, VAXserver 3300,
                      VAXserver 3400, VAXserver 3500,
                      VAXserver 3600, VAXserver 3602,
                      VAXserver 3800, VAXserver 3900,
                      VAXserver 4000 Model 300

                      VAXserver 6000-210, VAXserver 6000-220,
                      VAXserver 6000-310, VAXserver 6000-320,
                      VAXserver 6000-410, VAXserver 6000-420,
                      VAXserver 6000-510, VAXserver 6000-520

          Processors Not Supported

          MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXstation
          8000

          Processor Restrictions

          MicroVAX II and VAXstation II support requires either an RD53 or
          RD52 with at least one other hard disk configuration.

          Memory Requirements

          WPS-PLUS for VMS             6 Mbytes

          First 2 users                1 Mbyte

                                       --

          Minimum Configuration        7 Mbytes
          Total

          Each additional user         .5 Mbytes
          requires

                                          2

 


          WPS-PLUS/FRANÇAIS for VMS, Version 4.0             SSA 27.91.03-A





          A device capable of reading a TK50 is required to install this
          product on MicroVAX 2000 and VAXstation 2000 systems.

          Terminals supported include (text only):

          o  A VT100W series video terminal with the Advanced Video Option
             (AVO)*

          o  VT100 (AVO)*

          o  VT200, VT300, VT400, VT1000 series

          o  VAXstation series

          *  WPS-PLUS supports only those terminals which have Advanced
             Video Option (AVO). It does not support the VT100 without
             AVO, VT131, DECmate I, or WS78.

          Disk Space Requirements (Block Cluster Size = 1:)

          Users can install WPS-PLUS for VMS software on the system disk
          or on an alternate disk. WPS-PLUS installation requires the
          following amounts of disk space before and after installation:

          o  WPS-PLUS for VMS software on the system disk:

                BEFORE installation: 28,000 free blocks must be available
                on the system disk.

                AFTER installation: WPS-PLUS for VMS software will use
                23,000 blocks on the system disk.

          o  WPS-PLUS for VMS software on an alternate disk:

                BEFORE installation: 28,000 free blocks must be available
                on the system disk and 20,500 free blocks on the alternate
                disk.

                                          3

 


          WPS-PLUS/FRANÇAIS for VMS, Version 4.0             SSA 27.91.03-A



                AFTER installation: WPS-PLUS for VMS software will use
                4,000 blocks on the system disk and 20,500 blocks on the
                alternate disk.


          o  If installed, the Encapsulated PostScript[R] graphics files
             require an additional 3,000 blocks on the disk on which WPS-
             PLUS for VMS software is installed.

          o  The linguistic components packaged with the WPS-PLUS software
             require an additional 1,500 blocks on the disk on which it is
             to be installed.

          Note:

          The sizes are approximations; actual sizes may vary depending
          on the user's system environment, configuration, and software
          options selected.

          OPTIONAL HARDWARE

          o  LQP02 with optional Sheet Feeder

          o  LQP03 with optional Sheet Feeder

          o  LQP45 with optional Sheet Feeder

          o  LA50

          o  LA75

          o  LA100

          o  LA210

          o  LA324 with optional Sheet Feeder

          o  LN03

          o  LN03R

          o  DEClaser Series

          o  PrintServer40 (LPS40)

          o  PrintServer20 (LPS20)

                                          4

 


          WPS-PLUS/FRANÇAIS for VMS, Version 4.0             SSA 27.91.03-A



          o  LP11

          o  LJ250

          o  LJ252

          o  QUME 1

          o  HP LaserJet Series II Printer

          o  HP LaserJet Series III Printer

          Note:

          1 The QUME Sprint 11/40-130 WT PLUS Wide Track Letter Quality

          Printer is available only from QUME, and supports a 256 column
          width.

          CLUSTER ENVIRONMENT

          This layered product is fully supported when installed on any
          valid and licensed VAXcluster* configuration without restric-
          tions. The HARDWARE REQUIREMENTS sections of this product's
          Software Product Description and System Support Addendum detail
          any special hardware required by this product.

          *  V5.x VAXcluster configurations are fully described in the
             VAXcluster Software Product Description (SPD 29.78.xx) and
             include CI, Ethernet and Mixed Interconnect configurations.

          SOFTWARE REQUIREMENTS

          o  VMS Operating System V5.2 - V5.4

          o  VAX FMS (Runtime Only System) V2.4

          VAX ScriptPrinter Software is required to print non-PostScript
          files to a ScriptPrinter.


                                          5

 


          WPS-PLUS/FRANÇAIS for VMS, Version 4.0             SSA 27.91.03-A

          Note:

          VAX FMS Runtime Only System is a prerequisite to run WPS-PLUS
          for VMS. Customers who have not purchased the complete FMS
          product kit, must purchase the FMS Runtime Only System software
          license as well as the FMS Runtime Only Media Kit.

          VMS Tailoring

          For VMS V5.x systems, the following VMS classes are required for
          full functionality of this layered product:

          o  VMS Required Saveset

          o  Network Support

          o  Programming Support

          o  Secure User's Environment

          o  Utilities

          For more information on VMS classes and tailoring, refer to
          the VMS Operating System Software Product Description (SPD
          25.01.xx).

          OPTIONAL SOFTWARE

          o  DECpage V3.1

          o  VAX Grammar Checker V1.0

          o  DECprint Utility for PostScript to Sixel Printing for VMS
             V1.0

          o  CDA Converter Library for VMS V1.1

          GROWTH CONSIDERATIONS

          The minimum hardware/software requirements for any future ver-
          sion of this product may be different from the requirements for
          the current version.


                                          6

 


          WPS-PLUS/FRANÇAIS for VMS, Version 4.0             SSA 27.91.03-A


          DISTRIBUTION MEDIA

          Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

          This product is also available as part of VMS Consolidated
          Software Distribution on CDROM.

          ORDERING INFORMATION

          Software Licenses: QL-AAMP*-**
          Software Media: QA-AAMP*-**
          Software Documentation: QA-AAMPA-GZ
          Software Product Services: QT-AAMP*-**

          *  Denotes variant fields. For additional information on avail-
             able licenses, services and media, refer to the appropriate
             price book.

          The above information is valid at time of release. Please con-
          tact your local Digital office for the most up-to-date informa-
          tion.

          [R]  PostScript is a registered trademark of Adobe Systems, Inc.

          [R]  HP is a registered trademark of Hewlett-Packard Company.

          [TM] The DIGITAL Logo, WPS-PLUS, CDA, CI, DECmate, DDIF, DX,
               FMS, LQP02, LA50, LA324, PrintServer, MicroVAX, VAX,
               VAXserver, VAXstation, VMS and VT are trademarks of Digital
               Equipment Corporation.













                                          7
