 






          System
          Support
          Addendum

          ________________________________________________________________

          PRODUCT NAME:  VAX Xway, Version 1.2              SSA 27.36.03-A

          HARDWARE REQUIREMENTS

          Processors Supported:

          VAX:      VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840, VAX 8842,
                    VAX 8974, VAX 8978

                    VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

          MicroVAX: MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,
                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900

          VAXstationVAXstation II, VAXstation 2000,
                    VAXstation 3100 Series, VAXstation 3200,
                    VAXstation 3500, VAXstation 3520,
                    VAXstation 3540





                                       DIGITAL                   July 1990

                                                               AE-LT74C-TE

 


          VAX Xway, Version 1.2                             SSA 27.36.03-A




          VAXserver:VAXserver 3100, VAXserver 3300,
                    VAXserver 3400, VAXserver 3500,
                    VAXserver 3600, VAXserver 3602,
                    VAXserver 3800, VAXserver 3900

                    VAXserver 6000-210, VAXserver 6000-310,
                    VAXserver 6000-410, VAXserver 6000-420

          Processors Not Supported:

          MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXstation
          8000

          Block Space Requirements (Block Cluster Size = 1):

          Disk space required for      2,200 blocks
          installation:
                                       (1,100K bytes)

          Disk space required for      1,800 blocks
          use (permanent):
                                       (900K bytes)

          These counts refer to the disk space required on the system
          disk. The sizes are approximate; actual sizes may vary depending
          on the user's system environment, configuration, and software
          options.

          OPTIONAL HARDWARE

          None

          CLUSTER ENVIRONMENT

          This layered product is fully supported when installed on any
          valid and licensed VAXcluster* configuration without restric-
          tions. The HARDWARE REQUIREMENTS sections of this product's
          Software Product Description and System Support Addendum detail
          any special hardware required by this product.

                                          2

 


          VAX Xway, Version 1.2                             SSA 27.36.03-A



          *  V5.x VAXcluster configurations are fully described in the
             VAXcluster Software Product Description (29.78.xx) and in-
             clude CI, Ethernet and Mixed Interconnect configurations.

          SOFTWARE REQUIREMENTS

          VMS Operating System V5.0 - V5.3

          VMS Tailoring

          For VMS V5.x systems, the following VMS classes are required for
          full functionality of this layered product:

          o  VMS Required Saveset

          For more information on VMS classes and tailoring, refer to
          the VMS Operating System Software Product Description (SPD
          25.01.xx).





















                                          3

 


          VAX Xway, Version 1.2                             SSA 27.36.03-A



          OPTIONAL SOFTWARE

          VAX DECalc V3.1

          VAX DECalc-PLUS V3.1

          Any language which runs under VMS and supports the VMS calling
          standards.

          Certain versions of these products depend on a specific version
          of the operating system. Please refer to the System Support
          Addendum (SSA) of the products in question to determine which
          version is necessary.

          GROWTH CONSIDERATIONS

          The minimum hardware/software requirements for any future ver-
          sion of this product may be different from the requirements for
          the current version.

          DISTRIBUTION MEDIA

          Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

          This product is also available as part of the VMS Consolidated
          Software Distribution on CDROM.

          ORDERING INFORMATION

          Software Licenses: QL-729A*-**
          Software Media: QA-729A*-**
          Software Documentation: QA-729AA-GZ
          Software Product Services: QT-729A*-**

          *  Denotes variant fields. For additional information on avail-
             able licenses, services and media, refer to the appropriate
             price book.


                                          4

 


          VAX Xway, Version 1.2                             SSA 27.36.03-A



          The above information is valid at time of release. Please con-
          tact your local Digital office for the most up-to-date informa-
          tion.


          [R]  C-CALC is a registered trademark of DSD Corporation.

          [R]  LOTUS 1-2-3 and DIF are a registered trademark of Lotus
               Development Corporation.

          [TM] dBASE III is a trademark of Ashton-Tate Corporation.

          [TM] Multiplan is a trademark of Microsoft Corporation.

          [TM] Symphony, VisiCalc, WKS, WK1, and WRK are trademarks of
               Lotus Development Corporation.

          [TM] SuperCalc is a trademark of Computer Associates Interna-
               tional, Inc.

          [TM] Supercomp-Twenty and 20/20 are trademarks of Access Tech-
               nology, Inc.

          [TM] The DIGITAL Logo, VAX DECalc, VAX DECalc-PLUS, MicroVAX,
               VAX, VAXstation and VAXserver are trademarks of Digital
               Equipment Corporation.













                                          5
