dtApril, 1990VAX P.S.I. V4.3 Cover Letter

This cover letter includes information not found elsewhere in the VAX P.S.I. V4.3 documentation. Please read this cover letter before you install or use the VAX P.S.I. software.KMV1A, KMS1P and KMS11 Synchronous Devices VAX P.S.I. supports many different synchronous communications options, some of which overlap in functionality. The synchronous device drivers are being restructured to use common driver source code. Some older options are incompatible with the new driver structure. Consequently, within 9�15 months time, VAX P.S.I. will withdraw support for the KMV1A, KMS1P and KMS11 synchronous devices as part of a program to rationalise the range of synchronous communications options supported.Customers using KMV1A devices should consider moving to DSV11 devices, while customers with KMS1P and KMS11 devices should consider moving to DMF32 devices. To help customers move to these replacement devices, trade-in programs may be available. Please contact your local Digital sales of�ce for more information.Public Network Information Manual The Public Network Information (AD-KL20A-TK) manual includes information about all the public networks supported by VAX P.S.I. V4.3. Please note that this manual includes two updates:

� Addendum 1 (AD-KL20A-T1) contains information about PSDNs supported since the

original manual was published. It also contains new front and back covers.

� Addendum 2 (AD-KL20A-T2) contains information about PSDNs supported since Addendum 1 was published.Please add and replace the appropriate pages of the Public Network Information manual using Addendum 1 before adding and replacing the pages using Addendum 2. This will ensure that your Public Network Information manual contains the latest information about supported PSDNs in the correct order. A larger binder is included in your documentation kit to contain the complete Public Network Information manual.AV-PC6HA-TECopyright ' 1990 by Digital Equipment Corporation1