F F

Software

Product

Description

FPRODUCT NAME:

FVAX

REAL-TIME

ACCELERATOR

SOFTWARE,

SPD29.43.02

Version 2.0A

FDESCRIPTION HARDWARE REQUIREMENTS

FVAX REAL-TIME ACCELERATOR SOFTWARE (VAX

VAX configuration as specified in the System Support

RTA) is a VMS layered product that integrates the

Addendum (SSA 29.43.02-x).

VAXELN message passing capability with VMS

FSOFTWARE REQUIREMENTS*

FOperating System software.

FOperating System

FWith VAX RTA and the VAXELN Toolkit, users develop

realtime applications that can be distributed between the

VMS Operating System

VMS host processor and the VAXELN-based KA800

FLayered Products

Fprocessors.

VAX RTA enables the VMS host processor to control the

VAXELN Toolkit

VAXELN realtime processors using either program con-

A VAXELN Toolkit is required to develop a VAX RTA trol or through a command language interface. VAXELNapplication.

based KA800 processors communicate with the VMS host and each other at DMA speeds over the the VAXBI

*Refer to the System Support Addendum (SSA bus. Communication between processors occurs via

29.43.02-x) for availability and the required version of standard VAXELN message passing services and the prerequisite/optional software.

VAX RTA runtime library procedures.

FORDERING INFORMATION

FVAX RTA runs on the VMS Operating System and sup-

Software Licenses: QL-VJNA*-** ports the KA800 realtime processor running VAXELN.

Software Media: QA-VJNA*-**

FFeatures

FSoftware Documentation: QA-VJNAA-GZ

Software Product Services: QT-VJNA*-**

VAX RTA improves overall system performance by putting the computing power closer to the realtime event that

*Denotes variant fields. For additional information on is being controlled or monitored. This can reduce interavailable licenses, services and media, refer to the rupt overhead and increase the predictability of time critiappropriate price book.

cal operations.

FSOFTWARE LICENSING

FThe impact of an intensive operation on the VMS host

system can be reduced and even eliminated by distribut-

A VAXELN Runtime License is included with each KA800 ing realtime data handling to dedicated VAXELN VAX

VAX RTA processor.

RTA processors.

This software is furnished under the licensing provisions

Communication between processors occurs using high of Digital Equipment Corporation’s Standard Terms and speed DMA transfers. VAX RTA communication services

Conditions. For more information about Digital’s licensing are the same for both VMS and VAXELN applications.

terms and policies, contact your local Digital office.

VAXELN ports, messages, and the local name service

FLICENSE MANAGEMENT FACILITY

Fare implemented under VAX RTA.

This product supports the VMS License Management

Each realtime processor has its own local memory for the

Facility (LMF). License units for this this product are alloapplication program, increasing available memory for the cated on a CPU-capacity basis.

VMS system and increasing the performance of the realtime processor.

For more information on the License Management

Realtime applications are developed and debugged using

Facility, refer to the VMS Operating System Software the standard VAXELN Toolkit. VAXELN applications, in-

Product Description (SPD 25.01.xx) or the License cluding device drivers, can be developed entirely in a

Management Facility Manual of the VMS Operating high level language.

System documentation set.

FFebruary

1990

AE-LS83C-TE

FVAX REAL-TIME

ACCELERATOR

SOFTWARE,

SPD29.43.02

Version 2.0A

FFor more information about Digital’s licensing terms and

FSOFTWARE WARRANTY

Fpolicies, contact your local Digital office.

Warranty for this software product is provided by Digital

FSOFTWARE PRODUCT SERVICES

Fwith the purchase of a license for the product as defined

in the Software Warranty Addendum of this SPD.

A variety of service options are available from Digital. For more information contact your local Digital office.

F__________________

F� The DIGITAL Logo is a registered trademark of Digital Equipment Corporation.

F� VAX C, VAX FORTRAN, MicroVAX, VAX, and VAXstation are trademarks of Digital Equipment Corporation. F2