 



             DECimage Storage Manager
             Installation Guide

             Order Number: AA-LE63A-TE



             August 1989

             This guide contains instructions for installing DECimage
             Storage Manager (ISM) on the VAX/VMS operating system. It
             also explains how to read the online release notes before or
             after installing the product. This guide applies to DECimage
             Storage Manager Version T1.0-4.






                             DIGITAL EQUIPMENT CORPORATION

                                      PROPRIETARY
                                      INFORMATION

                         Furnished for Field Test Purposes Only

                      The information contained herein is furnished in
                      confidence
                      and is subject to the terms and conditions of the
                      Field Test
                      Agreement.


             Revision/Update Information:  This is a new guide.

             Operating System and Version: VMS Version 5.2
             Software Version:             DECimage Storage Manager
                                           Version T1.0-4
             digital equipment corporation
             maynard, massachusetts

 

             _______________________________________________________
             August 1989
             The information in this document is subject to change without
             notice and should not be construed as a commitment by Digital
             Equipment Corporation. Digital Equipment Corporation assumes
             no responsibility for any errors that may appear in this
             document.
             The software described in this document is furnished under a
             license and may be used or copied only in accordance with the
             terms of such license.
             No responsibility is assumed for the use or reliability
             of software on equipment that is not supplied by Digital
             Equipment Corporation or its affiliated companies.

             Restricted Rights: Use, duplication, or disclosure by the
             U.S. Government is subject to restrictions as set forth in
             subparagraph (c)(1)(ii) of the Rights in Technical Data and
             Computer Software clause at DFARS 252.227-7013.
             © Digital Equipment Corporation 1989.

             All Rights Reserved.
             Printed in U.S.A.

             The postpaid Reader's Comments forms at the end of this docu-
             ment request your critical evaluation to assist in preparing
             future documentation.
             The following are trademarks of Digital Equipment Corporation:
             CDA              MASSBUS          VAX RMS
             DDIF             MD300            VAXstation
             DEC              PrintServer 40   VMS
             DECimage         Q-bus            VT
             DECnet           ReGIS            XUI
             DECUS            ULTRIX
             DECwindows       UNIBUS
             LA               VAX
             LN03             VAXcluster       DIGITAL
             The following are third-party trademarks:

             BASIC is a trademark of Dartmouth College.
             EyeStar is a trademark of Microtek Labs, Inc.
             Microtek is a registered trademark of Microtek Labs, Inc.
             PostScript is a registered trademark of Adobe Systems, Inc.
             X Window System is a trademark of Massachusetts Institute of
             Technology.

 















                                                                  Contents
          ________________________________________________________________


          Preface .........................................................      v

               1    Preparing to Install DECimage Storage
                     Manager .............................................      1
                     1.1    Prerequisite Software.....................      1
                     1.2    Accessing the On Line Release Notes.....      1
                     1.3    Installation Procedure Requirements.....      2
                     1.4    User Account Quotas and Privileges......      2
                     1.5    Special Requirements ......................      3
                     1.6    Using VMSINSTAL............................      3

               2    Installing DECimage Storage Manager.............      5

               3    After the Installation............................      9

               4    Error Conditions...................................      9

               5    Maintenance Updates ...............................     10

               6    Improving Product Performance....................     11

               7    Determining and Reporting Problems..............     11

               8    Example Installation ..............................     12



                                                                       iii

 






          ________________________________________________________________
          Appendix A Files Created or Modified by ISM Installation
                     Procedure

               A.1  Files Created During Installation...............    A-1

          ________________________________________________________________
          Tables
               A-1  [ISM]................................................    A-1

               A-2  [ISM.PERM]..........................................    A-1
               A-3  [ISM.IMAGE].........................................    A-1
               A-4  [SYS0.SYSCOMMON.SYSEXE]...........................    A-1
               A-5  [SYSHLP.EXAMPLES.ISM](client only)..............    A-2
               A-6  [SYS0.SYSCOMMON.SYSHLP]...........................    A-2
               A-7  [SYS0.SYSCOMMON.SYSLIB] (client installations
                     only)................................................    A-2

               A-8  [SYS0.SYSCOMMON.SYSMGR]...........................    A-3
               A-9  [SYS0.SYSCOMMON.SYSTEST]..........................    A-3
               A-10 [VMS$COMMON.SYSEXE] ...............................    A-3
               A-11 [VMS$COMMON.SYSHLP] ...............................    A-3
               A-12 [VMS$COMMON.SYSLIB](client installations
                     only)................................................    A-4
               A-13 [VMS$COMMON.SYSMGR] ...............................    A-4

               A-14 [VMS$COMMON.SYSTEST] ..............................    A-4












          iv

 














                                                                   Preface
          ________________________________________________________________



             This guide describes how to install DECimage Storage Manager
             on the VAX/VMS operating system. It is intended for system
             managers. This guide applies to Version T1.0-4.
             Before continuing with this guide, please note the following:

              o  Keep this guide with your distribution kit. You will need
                to refer to it again should you need to reinstall DECimage
                Storage Manager for any reason.
              o  This guide describes the installation procedure step
                by step. The procedure, for the most part, is self-
                explanatory. The system prompts you to answer questions
                and change volumes, and waits for you to tell it to con-
                tinue.

              o  All user-entered commands are shown in bold letters.
              o  For information on reporting problems with DECimage
                Storage Manager, see the section Determining and Reporting
                Problems later in this guide.

              o  This document does not contain release notes information;
                instead, release notes are provided on line. You can
                read the release notes before you install the DECimage
                Storage Manager product and at any time after the product
                is installed.


                                                                         v

 






                                            NOTE

                    To gain access to the release notes before you in-
                    stall the DECimage Storage Manager product, follow
                    the installation procedure up to step 4, in which
                    you can choose to read or print the release notes
                    and discontinue the installation procedure.
                    Although the release notes file installed by
                    VMSINSTAL has a unique name from maintenance up-
                    date to maintenance update, take care not to delete
                    previous versions of that file.

                To read the release notes after the installation, display
                or print the file SYS$HELP:ISM010.RELEASE_NOTES.
                The HELP file also directs you to the release notes file.
                After the installation, enter the following:

                  $ HELP ISM010 RELEASE_NOTES

                For more information on installing the DECimage Storage
                Manager product on VAX/VMS systems, see the Guide to
                VAX/VMS Software Installation and the VAX/VMS System
                Manager's Reference Manual.
















          vi

 





          _________________________________________________________________
          1  Preparing to Install DECimage Storage Manager

             Your Bill of Materials specifies the number and contents
             of your media. Be sure to check the contents of your kit
             against the list in the Bill of Materials. If your kit is
             damaged or parts of it are missing, please call your DIGITAL
             representative.

          _________________________________________________________________

          1.1  Prerequisite Software
             The DECimage Storage Manager Version T1.0-4 product requires
             VAX/VMS Version 5.2. The DECimage Storage Manager product
             also requires the following VAX/VMS layered products:

              o  DECnet VAX Version 4.0
              o  Rdb/VMS Version 3.0B

              o  MMG Version 1.0 if an RV64 Optical Library Jukebox System
                is present

          _________________________________________________________________
          1.2  Accessing the On Line Release Notes

             The DECimage Storage Manager product provides on line release
             notes that you can choose to display or print during the
             installation procedure.
             The prompt to display or print the release notes appears in
             the installation procedure, as noted in the description of
             step 4, only when you invoke VMSINSTAL with the OPTIONS N
             parameter.

             To gain access to the release notes before you install
             DECimage Storage Manager, follow the installation proce-
             dure up to step 4, in which you can choose to read or print
             the release notes and discontinue the installation procedure.

 






             To read the release notes after the installation, display or
             print the file SYS$HELP:ISM010.RELEASE_NOTES.

             The HELP file also directs you to the release notes file.
             After the installation, type the following:
               $ HELP ISM010 RELEASE_NOTES

          _________________________________________________________________
          1.3  Installation Procedure Requirements

             Before you can install the DECimage Storage Manager product,
             you must have the following privileges and resources:

              o  SETPRV privileges, or CMKRNL, WORLD, and SYSPRV privileges
              o  At least 2500 blocks of free disk space during installa-
                tion, and ???? blocks of disk space after installation

              o  9 Mbytes of physical memory (minimum configuration)
              o  Approximately 20 to 40 minutes, depending on your type of
                media and your system configuration

          _________________________________________________________________
          1.4  User Account Quotas and Privileges

             To use the DECimage Storage Manager product, each account
             must meet the following requirements:

              o  TMPMBX and PRMMBX privileges
              o  AST limit (ASTLM): 24 (minimum)

              o  Buffered I/O quota (BIOLM): 18 (minimum)
              o  Buffered I/O byte count quota (BYTLM): 4096 (minimum)

              o  Direct I/O quota (DIOLM): 18 (minimum)
              o  Enqueue quota (ENQLM): 30 (minimum)

              o  Open file quota (FILLM): 50 (minimum)

 






              o  Paging file quota (PGFLQUO): 10,000 pages (minimum)

              o  Working set size (WSDEF): 300 pages (minimum); 512-1024
                pages (application dependent)
          _________________________________________________________________

          1.5  Special Requirements
             The ISM system manager needs CMKRNL and SYSNAM privileges to
             run ISM$SERVER_START.COM and ISM$SERVER_STOP.COM.

             This procedure creates identifier entries in the RIGHTSLIST.DAT
             file.
             This procedure prompts for the location of the server direc-
             tories and files. As the ISM software requires a large amount
             of disk space, select this device carefully.

             This procedure prompts for the type of installation: server,
             client, or both. A server installation installs the ISM
             server software on this node. A client installation installs
             the ISM client software on this node (provides access to the
             ISM language independent call interface). Both installs both
             the client and server software on this node.
             The installation verification procedure (IVP) attempts to do
             a loopback test when you install both the server and client.
             First, it attempts to connect to the server through proxy
             access (using the installing account). When this fails, it
             prompts you for your password and retries.

          _________________________________________________________________

          1.6  Using VMSINSTAL
             VMSINSTAL is a command procedure that installs this product.
             In step 2 of the installation procedure, described in the
             next section, you must invoke VMSINSTAL.

             The VMSINSTAL command line has the following format:
                     $@SYS$UPDATE:VMSINSTAL ISM010 ddn: OPTIONS N

 






             ISM010
             Refer to the label on the DECimage Storage Manager distribu-
             tion kit.

             ddn:
             Represents a device name for the DECimage Storage Manager
             installation media, where dd is the device code and n is the
             unit number. You do not need to use the console drive. CSA1:
             is the device name used in examples in this document.

             OPTIONS N
             Represents the qualifier you should provide if you want
             VMSINSTAL to prompt you to display or print the release
             notes.

             If you do not supply these parameters, VMSINSTAL prompts
             you for the product and device names. However, if you do not
             include the OPTIONS N parameter, VMSINSTAL does not prompt
             you to display or print the release notes.
             When you invoke VMSINSTAL, it checks the following:

              o  Whether you logged in to the system manager's account - It
                is recommended that you install layered software from the
                system manager's account.
              o  Whether you have adequate quotas for installing layered
                products - VMSINSTAL checks for the following quota val-
                ues:
                 _  ASTLM = 24

                 _  BIOLM = 18
                 _  BYTLM = 18000

                 _  DIOLM = 18
                 _  ENQLM = 30

                 _  FILLM = 20

 






             VMSINSTAL then checks to see if either of the following
             conditions exist. If so, you should discontinue them before
             resuming the installation procedure. The conditions are:

              o  Whether DECnet is up and running
              o  Whether there are any users logged in to the system

             If VMSINSTAL detects either of these conditions, it gives you
             the opportunity to stop the installation procedure by prompt-
             ing you to continue. If you want to stop the installation,
             press the RETURN key.
          _________________________________________________________________
          2  Installing DECimage Storage Manager


             This section contains excerpts from the installation proce-
             dure and provides explanatory text.
             If you need to abort the installation procedure, press
             CTRL/Y. When you press CTRL/Y, the installation procedure
             deletes all files it has created up to that point and ex-
             its. If you want to retry the installation procedure after
             pressing CTRL/Y, you must proceed from step 2.

             Note that enhancements to VMSINSTAL in future releases of
             the VAX/VMS operating system may result in additional prompts
             appearing during the course of the installation. Although
             such prompts may not be documented in this installation
             guide, the installation should proceed normally.
             Step 1: Log in to the system manager's account.

          <RET>
               Username: SYSTEM
               Password:         <RET>

 






             Step 2: Invoke VMSINSTAL.

               $ @SYS$UPDATE:VMSINSTAL ISM010 CSA1: OPTIONS N <RET>
                  VAX/VMS Software Product Installation Procedure

               It is 4-AUG-1989 at 16:20.
               Enter a question mark (?) at any time for help.

               * Are you satisfied with the backup of your system disk [YES]? <RET>
             Step 3: Insert the first installation kit volume.

               Please mount the first volume of the set on CSA1:.
               * Are you ready? Y <RET>
               %MOUNT-I-MOUNTED, ISM Mounted on _SYSTEM$MUA0:
               The following products will be installed:

                 ISM010 T1.0-4

               Beginning installation of ISM010 T1.0-4 at 16:20
               %VMSINSTAL-I-RESTORE, Restoring product saveset A...

             Step 4: Select a release notes option.
             This step applies only if you specified OPTIONS N in step 2.

               Release Notes Options:
                   1. Display release notes
                   2. Print release notes
                   3. Both 1 and 2
                   4. Copy release notes to SYS$HELP
                   5. Do not display, print or copy release notes

               * Select option [2]: 4

             If you select option 1, VMSINSTAL displays the release notes
             immediately on your screen. If you select option 2, VMSINSTAL
             prompts you for a queue name.
               * Queue name [SYS$PRINT]:

 






             You can type a queue name (or press the RETURN key to indi-
             cate the default output print device, SYS$PRINT).

             If you select option 4, VMSINSTAL copies the release notes to
             SYS$HELP.
             Next, VMSINSTAL displays the following prompt:

               Do you want to continue the installation [NO]?: Y <RET>
             If you type NO or press the RETURN key, VMSINSTAL discontin-
             ues the installation.

               %VMSINSTAL-I-RELMOVED, The product's release notes have been successfully
               moved to SYS$HELP.

             Step 5: Select installation options.

               * Do you want to run the IVP after installation [YES]? <RET>
               * Do you want to purge files replaced by this installation [YES]? <RET>
             The Installation Verification Procedure (IVP) runs tests to
             check that the installation procedure was successful. Press
             the RETURN key to run the IVP after the installation. If
             you do not want to run the IVP, type NO in response to the
             prompt.

             The files in SYS$SYSTEM and SYS$LIBRARY containing previous
             releases of DECimage Storage Manager are replaced during the
             installation with the new release. However, the old files
             are not automatically purged. Purging is recommended. In
             response to the purging prompt, press the RETURN key to purge
             the files, or type NO to keep them. The system HELP files are
             updated in either case.
             Step 6: Read Informational messages.

               %VMSINSTAL-I-MOVEFILES, files will now be moved to their
               target directories...
             The installation procedure displays a number of information
             messages. Be sure to read these messages.

 






             If the installation procedure is successful, the files will
             be moved to their target directory.

             In addition, the SYS$HELP:HELPLIB.HLB is updated to include
             the new version of the DECimage Storage Manager HELP text
             and the command-name command line definition, respectively;
             and the DECimage Storage Manager release notes are copied to
             SYS$HELP:ISM010.RELEASE_NOTES.
             The installation procedure creates or modifies a number of
             files. For a complete list of files created or modified, see
             Appendix A, Files Created or Modified by ISM Installation
             Procedure.

             Step 7: The Installation Verification Procedure.
             The installation procedure now calls the Installation
             Verification Procedure (IVP) to verify that DECimage Storage
             Manager was successfully installed. If this option was
             chosen, the installation procedure calls the Installation
             Verification Procedure (IVP) to verify that DECimage Storage
             Manager was successfully installed.

             Step 8: End the installation procedure.

                       VMSINSTAL procedure done at 17:10

               $ LOGOUT
               SYSTEM     logged out at 4-AUG-1989 17:15:14.05
             Note that VMSINSTAL deletes or changes entries in the process
             symbol tables during the installation. Therefore, if you are
             going to continue using the system manager's account, and
             want to restore those symbols, you should log out and log in
             again.

 





          _________________________________________________________________
          3  After the Installation

             The DECimage Storage Manager product is now installed.

          _________________________________________________________________
          4  Error Conditions

             If the installation procedure fails for any reason, the
             following message is displayed:

               DECimage Storage Manager T1.0-4 Installation failed.

               Please consult the DECimage Storage Manager Installation
                Guide for further information.
             One or more of the following conditions can cause an error
             during the installation:

              o  Insufficient disk space to complete the installation
              o  Insufficient system virtual page count parameter

              o  Insufficient AST quota
              o  Insufficient buffered I/O byte count

              o  Insufficient subprocess quota
              o  Insufficient open file quota

              o  Insufficient process paging file quota
              o  Insufficient process working set quota

              o  Insufficient system maximum working set
              o  Incorrect version of VAX/VMS

              o  Rdb/VMS not installed

             For descriptions of the error messages generated by these
             conditions, see the VAX/VMS System Messages and Recovery
             Procedures Reference Manual and the Guide to VAX/VMS Software
             Installation.

 






             If you are notified that any of these conditions exist,
             you should take the appropriate action, as described in
             the message. You may need to change a system parameter or
             increase an authorized quota value. If the installation
             fails, you must restart the installation procedure from step
             2.

             If the Installation Verification Procedure fails for any
             reason, the following message is displayed:
               DECimage Storage Manager T1.0-4 Installation Verification
               Procedure failed.
               Please consult the DECimage Storage Manager Installation
               Guide for further information.

             If you receive this message, contact your DIGITAL field
             service representative.
          _________________________________________________________________
          5  Maintenance Updates


             DIGITAL may periodically issue maintenance updates of
             DECimage Storage Manager. Each update will consist of an
             installation kit. You should install this kit as described in
             this document or in any documentation that may accompany the
             maintenance update.
             Each time DIGITAL releases a maintenance update, the prod-
             uct's version number changes. For example, if the current
             version is 1.0, the version number of the first maintenance
             update will be 1.1. In addition, the maintenance update will
             usually include changes to the release notes. The release
             notes describe the changes that have been made to DECimage
             Storage Manager since the previous release.

             The update release notes are provided on line. You can read
             the release notes before you install DECimage Storage Manager
             and at any time after you install the product. For in-
             formation on reading the release notes before installing

 






             the DECimage Storage Manager product, follow the instal-
             lation procedure up to step 4. To read the release notes
             after installing the product, display or print the file
             SYS$HELP:ISM010.RELEASE_NOTES.
          _________________________________________________________________

          6  Improving Product Performance

             To improve the DECimage Storage Manager product's perfor-
             mance:
              o  Install DSL$SHR.EXE.

              o  Vary the RUN command qualifiers in ISM$SERVER_STARTUP to
                allow greater system resource utilization.

          _________________________________________________________________
          7  Determining and Reporting Problems

             If an error occurs while you are using DECimage Storage
             Manager product, and you believe that the error is caused
             by a problem with the DECimage Storage Manager product, you
             should take one of the following actions:
              o  If you have a BASIC or DECsupport Software Agreement,
                you should call your Customer Support Center. (With these
                services, you receive telephone support that provides
                high-level advisory and remedial assistance. For more
                information, contact your local DIGITAL representative.)

              o  If you have a Self-Maintenance Software Agreement, you may
                submit a Software Performance Report (SPR).
              o  If you purchased DECimage Storage Manager within the last
                90 days and this is a nonconformance problem, you can
                submit a Software Performance Report (SPR).

 






             If you find an error in the DECimage Storage Manager documen-
             tation, you should fill out and submit the Reader's Comments
             form at the back of the guide in which the error was found.
             If you report a documentation error, specify the title of
             the guide or manual and the section and page number where the
             error was found.
          _________________________________________________________________

          8  Example Installation

             This section contains a sample installation of the DECimage
             Storage Manager product. Please note that this is only a
             sample.

               Username: SYSTEM
               Password:

               $ @sys$update:vmsinstal ISM010 extra$:[savesets.ISM010] options s,n
                VAX/VMS Software Product Installation Procedure B5.0-3PA

               It is 4-AUG-1989 at 16:29.
               Enter a question mark (?) at any time for help.
               %VMSINSTAL-W-DECNET, Your DECnet network is up and running.
               %VMSINSTAL-W-ACTIVE, The following processes are still active:
                MAIL
               * Do you want to continue anyway [NO]? yes
               * Are you satisfied with the backup of your system disk [YES]?
               The following products will be processed:
                 ISM V1.0
                Beginning installation of ISM V1.0 at 16:30

               %VMSINSTAL-I-RESTORE, Restoring product saveset  A...
                   Release Notes Options:

 






                1.  Display release notes
                2.  Print release notes
                3.  Both 1 and 2
                4.  Copy release notes to SYS$HELP
                5.  Do not display, print or copy release notes

               * Select option [2]: 4
               * Do you want to continue the installation? yes
               %VMSINSTAL-I-RELMOVED , The product's release notes have been successfully
               moved to SYS$HELP.

                Installation procedure for: ISM "T1.0"

                  *********************************************************************
                   Be sure you have read the section entitled:
                    "Preparing Your System and the Installing Account"
                   in the installation guide before continuing with the installation.
                  *********************************************************************
                   Checking system requirements ...

                  Installation Options:

                1. ISM server and client
                2. Server only
                3. Client only
               * Select option  [1]:
               * Do you want to run the IVP after the installation [YES]?
               * Do you want to purge files replaced by this installation [YES]?

                  *********************************************************************
                ISM requires a disk device for the server files.
                This installation will create a directory structure to contain them.
                If you are unsure of where to place these, you may exit this procedure
                now and review the pertinent documentation.

                  *********************************************************************
               * Do you know where you want to put your server directory  [NO]? yes
               * What is the name of the server disk: over40$dua1:

 






                 *************************************************************
                  Your input may be required during the IVP phase of this installation.

                 ***Please be aware ***
                  Important additional text will follow.
                 *************************************************************

               %VMSINSTAL-I-RESTORE, Restoring product saveset  B...
               %VMSINSTAL-I-RESTORE, Restoring product saveset  C...
               %VMSINSTAL-I-RESTORE, Restoring product saveset  D...
                   *************************************************************

                    This installation adds the following ACL identifiers
                    to the SYSUAF.DAT file:
                          ISM$CREATE_STORAGE_SET
                          ISM$SERVER_SHUTDOWN
                          ISM$ADMINSTRATOR
                    The identifier ISM$CREATE_STORAGE_SET is granted to this
                    account in order to run the ISM IVP...

                    Please review the documentation regarding their dispensation
                    to ISM server user accounts.
                   Please ignore any duplicate name or identifier errors.

                   *************************************************************

 






               %UAF-I-RDBADDMSG, identifier ISM$CREATE_STORAGE_SET value:
               %X80010001 added to RIGHTSLIST.DAT
               %UAF-I-RDBADDMSG, identifier ISM$SERVER_SHUTDOWN value:
               %X80010002 added to RIGHTSLIST.DAT
               %UAF-I-RDBADDMSG, identifier ISM$ADMINISTRATOR value:
               %X80010003 added to RIGHTSLIST.DAT
               %UAF-I-GRANTMSG, identifier ISM$CREATE_STORAGE_SET granted to SYSTEM
               %UAF-I-NOMODS, no modifications made to system authorization file
               %UAF-I-RDBDONEMSG, rights database modified
               %VMSINSTAL-I-SYSDIR, This product creates system disk directory
               OVER40$DUA1:[ISM].
               %VMSINSTAL-I-SYSDIR, This product creates system disk directory
               OVER40$DUA1:[ISM.SS].
               %VMSINSTAL-I-SYSDIR, This product creates system disk directory
               OVER40$DUA1:[ISM.PERM].
               %VMSINSTAL-I-SYSDIR, This product creates system disk directory
               OVER40$DUA1:[ISM.IMAGE].

                 ISM Server installation added the following files to your system:
                SYS$SYSTEM:ISM$SERVER_MAIN.EXE      [new]
                SYS$SYSTEM:ISM$SERVER_SHUTDOWN.EXE     [new]
                SYS$MANAGER:ISM$SERVER_STOP.COM      [new]
                SYS$MANAGER:ISM$SERVER_STARTUP.COM          [new]
                SYS$LIBRARY:ISM$SERVER.RDB      [new]
                ISM$SERVER_PERM:ISM$SERVER.SNP              [new]

                  Providing ISM client support for VAX-C
                  Providing ISM client support for FORTRAN
                  Providing ISM client support for BASIC
                 ISM Client installation added the following files to your system:

 






                       SYS$LIBRARY:DSL$SHR.EXE                [new]
                       SYS$LIBRARY:ISM$CLIENT_SHR.EXE         [new]
                       SYS$LIBRARY:ISM$MSG.BAS                [new]
                       SYS$LIBRARY:ISM$MSG.FOR                [new]
                       SYS$LIBRARY:ISM$MSG.H                  [new]
                       SYS$LIBRARY:ISM$MSG.OBJ                [new]
                       SYS$LIBRARY:ISM$USER_DEF.BAS           [new]
                       SYS$LIBRARY:ISM$USER_DEF.FOR           [new]
                       SYS$LIBRARY:ISM$USER_DEF.H             [new]
                SYS$HELP:ISM$HELP.HLP                [new]

                 *************************************************************
                 SYSTEM MANAGER:

                 Only one ISM Server can execute per system or cluster.  Please
                 add the following command line to the SYS$SPECIFIC: startup command
                 file of the designated ISM Server node on this system or cluster.
                    $ @SYS$MANAGER:ISM$SERVER_STARTUP

                 Add the following command line to the SYS$SPECIFIC: shutdown command
                 file of the designated ISM Server node on this system or cluster.
                    $ @SYS$MANAGER:ISM$SERVER_STOP
                 *************************************************************

               %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...
                 Beginning the ISM X1.0-00 Installation Verification
                      Please stand by.  Your input may be required!

                 Depending upon system loading, this procedure may take
                 from 1 to 3 minutes to complete.

                  Verifying ISM Server installation
                     ...starting Server
               %PURGE-W-SEARCHFAIL, error searching for SYS$COMMON:[SYSMGR]ISM$SERVER_ERROR.LOG;*
               -RMS-E-FNF, file not found
               %RUN-S-PROC_ID, identification of created process is 00000114
               ISM server started
                     ...Server running

 




                       Verifying ISM Client installation
                         ISM support for VAX C available.
                          ...linking VAX C version of ISM$IVP_TEST
                      Please ignore any informational messages.
                          ...running ISM$IVP_TEST

                      Initiating ISM session on using PROXY access.
                     Invalid ISM user account.
                     Failed to connect to server by proxy.
                       Need your password to initiate an ISM Session.
                       Your password will not be displayed.
                       Please enter your password now...
                    Initiating ISM session  using password.
                     Connected to server.
                      Storage Set Information for current user:
                      End of List
                     Creating storage set IVP_SS.
                     Creating image object.

                       The ISM Installation Verification procedure has succeeded.
                    %VMSINSTAL-S-SUCCESS, The IVP for ISM V1.0 has succeeded.
                     VMSINSTAL procedure done at 16:56
                    $ lo
                      SYSTEM       logged out at 21-MAR-1988 16:57:11.32

 










                                                                     Appendix A


                        Files Created or Modified by ISM Installation Procedure
               ________________________________________________________________


                  This appendix lists the files created or modified during the
                  installation of the DECimage Storage Manager (ISM) product.

               _________________________________________________________________
               A.1  Files Created During Installation

                  The tables in this section list the files created during the
                  installation procedure. The table name is the directory in
                  which the files are located.


                  Table A-1: [ISM]
                  _____________________________________________________________
                  IMAGE.DIR
                  PERM.DIR
                  _____________________________________________________________

                  Table A-2: [ISM.PERM]
                  _____________________________________________________________
                  ISM$SERVER.RDB

                  ISM$SERVER.SNP
                  _____________________________________________________________

                  Table A-3: [ISM.IMAGE]
                  _____________________________________________________________

                  _____________________________________________________________

                  Table A-4: [SYS0.SYSCOMMON.SYSEXE]
                  _____________________________________________________________
                  ISM$SERVER_MAIN.EXE

                  ISM$SERVER_SHUTDOWN.EXE

                  ISM$UTILITY.EXE
                  _____________________________________________________________








                   Files Created or Modified by ISM Installation Procedure  A-1

 




                  Table A-5: [SYSHLP.EXAMPLES.ISM](client only)
                  _____________________________________________________________
                  ISM$UTILITY_MAIN.C

                  ISM$DECW_GENERAL.C

                  ISM$DECW_WORK_WINDOW.C

                  ISM$DECW_SESSIONS.C

                  ISM$DECW_STORAGE_SETS.C

                  ISM$DECW_IMAGES.C

                  ISM$DECW_DATABASE.C

                  ISM$ISM_INTERFACE.C

                  ISM$DATABASE_INTERFACE.C

                  ISM$U_WIDGETS.H

                  ISM$U_STRUCT.H

                  ISM$UD_STRUCT.H

                  ISM$UTILITY_MSG.H

                  ISM$UTILITY_MSG.MSG

                  ISM$UTILITY.HLP

                  ISM$UTILITY.UIL

                  ISM$BUILD_UTILITY.COM
                  _____________________________________________________________

                  Table A-6: [SYS0.SYSCOMMON.SYSHLP]
                  _____________________________________________________________
                  ISM010.RELEASE_NOTES

                  ISM$HELP.HLP
                  _____________________________________________________________

                  Table A-7: [SYS0.SYSCOMMON.SYSLIB] (client installations
                              only)
                  _____________________________________________________________
                  DSL$SHR.EXE

                  ISM$CLIENT_SHR.EXE

                  ISM$MSG.BAS
                  _____________________________________________________________
                                                       (continued on next page)




               A-2  Files Created or Modified by ISM Installation Procedure

 




                  Table A-7 (Cont.): [SYS0.SYSCOMMON.SYSLIB] (client installa-
                                      tions only)
                  _____________________________________________________________

                  ISM$MSG.FOR

                  ISM$MSG.H

                  ISM$MSG.OBJ

                  ISM$USER_DEF.BAS

                  ISM$USER_DEF.FOR

                  ISM$USER_DEF.H
                  _____________________________________________________________

                  Table A-8: [SYS0.SYSCOMMON.SYSMGR]
                  _____________________________________________________________
                  ISM$SERVER_STARTUP.COM

                  ISM$SERVER_STOP.COM

                  ISM$CLIENT_STARTUP.COM
                  _____________________________________________________________

                  Table A-9: [SYS0.SYSCOMMON.SYSTEST]
                  _____________________________________________________________
                  ISM$IVP.COM

                  ISM$IVP_TEST.C

                  ISM$IVP_TEST.FOR

                  ISM$IVP_TEST.BAS

                  ISM$IVP_TEST.EXE

                  ISM$IVP_TEST_C.OBJ
                  _____________________________________________________________

                  Table A-10: [VMS$COMMON.SYSEXE]
                  _____________________________________________________________
                  ISM$SERVER_MAIN.EXE

                  ISM$SERVER_SHUTDOWN.EXE

                  ISM$UTILITY.EXE
                  _____________________________________________________________

                  Table A-11: [VMS$COMMON.SYSHLP]
                  _____________________________________________________________
                  ISM010.RELEASE_NOTES
                  _____________________________________________________________
                                                       (continued on next page)



                   Files Created or Modified by ISM Installation Procedure  A-3

 




                  Table A-11 (Cont.): [VMS$COMMON.SYSHLP]
                  _____________________________________________________________

                  ISM$HELP.HLP
                  _____________________________________________________________

                  Table A-12: [VMS$COMMON.SYSLIB](client installations only)
                  _____________________________________________________________
                  DSL$SHR.EXE

                  ISM$CLIENT_SHR.EXE

                  ISM$MSG.BAS

                  ISM$MSG.FOR

                  ISM$MSG.H

                  ISM$MSG.OBJ

                  ISM$USER_DEF.BAS

                  ISM$USER_DEF.FOR

                  ISM$USER_DEF.H
                  _____________________________________________________________

                  Table A-13: [VMS$COMMON.SYSMGR]
                  _____________________________________________________________
                  ISM$SERVER_STARTUP.COM

                  ISM$SERVER_STOP.COM

                  ISM$CLIENT_STARTUP.COM
                  _____________________________________________________________

                  Table A-14: [VMS$COMMON.SYSTEST]
                  _____________________________________________________________
                  ISM$IVP.COM

                  ISM$IVP_TEST.C

                  ISM$IVP_TEST.FOR

                  ISM$IVP_TEST.BAS

                  ISM$IVP_TEST.EXE

                  ISM$IVP_TEST_C.OBJ
                  _____________________________________________________________








               A-4  Files Created or Modified by ISM Installation Procedure
