 















             VAX LISP/VMS Installation Guide

             Order Number: AA-Y922F-TE





             This document contains instructions for installing VAX LISP
             on the VMS operating system. It also explains how to read the
             online release notes before or after installing the product.
             This document applies to VAX LISP Version 3.1.




             Revision/Update Information:  This is a revised manual.

             Operating System and Version: VMS Version 5.2 or 5.3

             Software Version:             VAX LISP Version 3.1






             digital equipment corporation
             maynard, massachusetts

 


             First Printing,  June 1984
             Revised, December 1984
             Revised, May 1986
             Revised, July 1987
             Revised, July 1989
             Revised, March 1990

             The information in this document is subject to change without
             notice and should not be construed as a commitment by Digital
             Equipment Corporation. Digital Equipment Corporation assumes
             no responsibility for any errors that may appear in this
             document.

             The software described in this document is furnished under a
             license and may be used or copied only in accordance with the
             terms of such license.

             No responsibility is assumed for the use or reliability
             of software on equipment that is not supplied by Digital
             Equipment Corporation or its affiliated companies.

             Restricted Rights: Use, duplication, or disclosure by the
             U.S. Government is subject to restrictions as set forth in
             subparagraph (c)(1)(ii) of the Rights in Technical Data and
             Computer Software Clause at DFARS 252.227-7013.

             © Digital Equipment Corporation 1984, 1986, 1987, 1989, 1990.

             All rights reserved.
             Printed in U.S.A.

             The postpaid Reader's Comments form at the end of this docu-
             ment requests your critical evaluation to assist in preparing
             future documentation.

             The following are trademarks of Digital Equipment Corporation:

             AI VAXstation  MicroVMS       VAX LISP
             DEC            PDP            VAX LISP/VMS
             DECnet         ULTRIX         VAX LISP/ULTRIX
             DECUS          ULTRIX-11      VAXstation                
             DECwindows     ULTRIX-32      VAXstation II
             MicroVAX       UNIBUS         VMS
	     MicroVAX II    VAX		   DIGITAL












								     S1368



             This document was prepared with VAX DOCUMENT, Version 1.2.

 















                                                                  Contents
          ________________________________________________________________

          Preface ......................................................vii


          ________________________________________________________________
          Chapter 1  Preparing to Install VAX LISP

               1.1   Prerequisite Software............................. 1-1

               1.2   Accessing the Online Release Notes...............  1-2

               1.3   Installation Procedure Requirements..............  1-2
                     1.3.1 Calculating the Values for WSMAX,
                           PQL_DWSDEFAULT, and PROSECTCNT............   1-3
                     1.3.2 Changing System Parameter Values with
                           AUTOGEN .................................... 1-3

               1.4   User Account Quotas and Privileges...............  1-4

               1.5   VMS Tailoring Classes............................. 1-4

               1.6   DECwindows Tailoring Classes...................... 1-5

               1.7   VMS License Management Facility .................. 1-5

               1.8   Using VMSINSTAL................................... 1-6



                                                                       iii

 






          ________________________________________________________________
          Chapter 2  Installing VAX LISP

               2.1   Installation Procedure............................ 2-1

               2.2   Installing VAX LISP on a VAXcluster..............  2-9


          ________________________________________________________________
          Chapter 3  Completing the Installation

               3.1   Modifying the System Startup File................  3-1

               3.2   Modifying the VAX LISP Startup File..............  3-2

               3.3   Defining the LISP System Logical Names ..........  3-3

          ________________________________________________________________
          Chapter 4  Using Previous Versions of VAX LISP


          ________________________________________________________________
          Chapter 5  Running the Installation Verification
                     Procedure Separately

          ________________________________________________________________
          Chapter 6  Error Conditions


          ________________________________________________________________
          Chapter 7  Installing VAX LISP as a Shared Image








          iv

 






          ________________________________________________________________
          Chapter 8  Maintenance Updates


          ________________________________________________________________
          Chapter 9  Tuning the VAXstation

               9.1   Recommended System Parameters..................... 9-1

               9.2   Recommended Authorization Quotas ................. 9-4

          ________________________________________________________________
          Chapter 10 Determining and Reporting Problems


          ________________________________________________________________
          Chapter 11 Sample Installation

          ________________________________________________________________
          Appendix A Files Added to the System

               A.1   LISP$SYSTEM: Directory............................ A-1

               A.2   LISP$EXAMPLES: Directory.......................... A-1

               A.3   LISP$GKS: Directory .............................. A-4

               A.4   LISP$LIBRARY: Directory........................... A-5

               A.5   LISP$PCL: Directory .............................. A-5

               A.6   LISP$STARLET: Directory........................... A-7

               A.7   LISP$VAXFLAVORS: Directory ...................... A-10

               A.8   RDBLISP$EXAMPLES: Directory...................... A-11

               A.9   FOXGLOVE$SYSTEM: Directory ...................... A-12

                                                                         v

 







               A.10  SYS$STARTUP: Directory........................... A-13

          ________________________________________________________________
          Tables

               3-1   .COM File Names for the System Startup File ....   3-2
































          vi

 














                                                                   Preface
          ________________________________________________________________



             This document is intended for system managers. It describes
             how to install VAX LISP on the VMS operating system. This
             document applies to VAX LISP Version 3.1. The major version
             number is represented by the digit to the left of the decimal
             point, and the maintenance update version number is indicated
             by the digit to the right of the decimal point.

             Keep this document with your distribution kit. You will need
             it to install maintenance updates or to reinstall VAX LISP
             for any other reason.

             At the back of this document is a Reader's Comments form. If
             you have any comments about this document, fill out the form
             and mail it; your comments will be considered for the next
             revision of the installation guide.

             For more information about installing VAX LISP on VMS sys-
             tems, see your processor-specific installation/operations
             guide.

             The installation procedure is described step-by-step and is,
             for the most part, self-explanatory. The system prompts you
             to answer questions and to change volumes, and waits for you
             to tell it to continue.

             Defaults appear in brackets ([])  throughout the installation
             procedure. Text you type is indicated in red.

                                                                       vii

 










                                                                      Chapter 1


                                                  Preparing to Install VAX LISP
               ________________________________________________________________


                  Your bill of materials (BOM) and indented bills report (BIL)
                  specify the number and contents of your media. Be sure to
                  check the contents of your kit against this information.
                  If your kit is damaged or if you find that parts of it are
                  missing, call your Digital representative.

                  Distribution media must be mounted in numerical order. The
                  installation procedure prompts you to mount the volumes. For
                  more information on how to mount distribution media, see your
                  processor-specific installation/operations guide, which also
                  details several options to the installation procedure.

               _________________________________________________________________

               1.1  Prerequisite Software

                  VAX LISP Version 3.1 requires VMS Version 5.2 or 5.3 or
                  higher.

               _________________________________________________________________

               1.2  Accessing the Online Release Notes

                  VAX LISP provides online release notes. The prompt to dis-
                  play or print the release notes during the installation
                  appears in step 3 of the installation procedure when you
                  invoke VMSINSTAL with the OPTIONS N parameter (the OPTIONS N
                  parameter is available only with VMS Version 4.4 or higher).

                  To obtain the release notes after the installation, type or
                  print the file SYS$HELP:LISP031.RELEASE_NOTES.

                  Online help also directs you to the release notes file. After
                  the installation, type the following command:

                    $ HELP LISP RELEASE_NOTES <Return>

               _________________________________________________________________

               1.3  Installation Procedure Requirements

                  The installation takes approximately two hours and forty-five
                  minutes to three hours depending on the type of media and


                                             Preparing to Install VAX LISP  1-1








                  your system configuration. Before installing VAX LISP, you
                  must have the following privileges and resources:

                   o CMKRNL, WORLD, and SYSNAM privileges.

                   o The following minimum blocks of free disk space during and
                     after installation based on which parts of the LISP kit
                     you install:

               ________________________________________________________________
                                     Blocks of Disk Space  Blocks of Disk Space
               Installation Option   During Installation   After Installation

               Only the VAX LISP     19,226                18,804
               /VMS image includ-
               ing support for
               DECwindows

               Only the VAX LISP     13,746                13,296
               /VMS image including
               support for VWS

               The entire VAX LISP   93,627                92,985
               /VMS kit includ-
               ing support for
               DECwindows
	       ________________________________________________________________

                      _ Saveset A occupies 350 blocks.

                      _ Saveset B occupies 20,000 blocks.

                      _ Saveset C occupies 14,300 blocks.

                      _ Saveset D occupies 22,500 blocks.

                      _ Saveset E occupies 4,400 blocks.

                      _ Saveset F occupies 4,400 blocks.

                      _ Saveset G occupies 2,100 blocks.

                      _ Saveset H occupies 26,400 blocks.

                      _ Saveset I occupies 4,400 blocks.

                      _ Saveset J occupies 2,000 blocks.

                      _ Saveset K occupies 16,000 blocks.

                   o Eight megabytes of address space.

                   o A minimum of 16,000 virtual pages (VIRTUALPAGECNT) at
                     installation.


               1-2  Preparing to Install VAX LISP








                   o Eight megabytes of memory to run in a standalone terminal
                     or VWS environment.

                   o Fourteen megabytes of memory to run in a standalone
                     DECwindows environment with both the client and server
                     executing on the same system.

                  Using VAX LISP in conjunction with increased memory capabil-
                  ity improves performance. The memory size for most typical
                  configurations is at least 16 megabytes.

                                               NOTE

                      You must ensure that your system has the necessary
                      global page and global section system parameters for
                      the installation. Failure to do so could cause the DCL
                      tables to be corrupted in some situations.

               _________________________________________________________________

               1.3.1  Calculating the Values for WSMAX, PQL_DWSDEFAULT, and
                      PROSECTCNT

                  To run VAX LISP, you must have appropriate values for the
                  WSMAX, PQL_DWSDEFAULT, and PROSECTCNT system parameters.
                  Inappropriate values result in the user's getting SECTBLFUL
                  (Section table is full) error messages when trying to ac-
                  tivate a LISP image. There is no hard and fast rule for
                  appropriate values for these system parameters, but large
                  images or processes that activate many images require more
                  PSTE space.

                  You can find further information about these SYSGEN pa-
                  rameters in VAX/VMS Internals and Data Structures and
                  Introduction to VMS System Services.

                  Section 1.3.2 describes the procedures for increasing these
                  values.

               _________________________________________________________________

               1.3.2  Changing System Parameter Values with AUTOGEN

                  You use the AUTOGEN command procedure to change system param-
                  eters. AUTOGEN automatically adjusts values for parameters
                  that are associated with the ones you reset manually. To
                  change system parameters with AUTOGEN, you must edit the
                  following file:

                    SYS$SYSTEM:MODPARAMS.DAT






                                             Preparing to Install VAX LISP  1-3








                  For example, to change the setting for the WSMAX system
                  parameter, add this line to the file:

                    WSMAX = 1024

                  Or for incremental system parameters:

                    ADD_GBLPAGES = 2000

                  (Digital recommends using the ADD_x form of system parameter
                  modifier. Avoid entering absolute values.)

                  Now, run the AUTOGEN procedure to recalculate your system
                  parameters. Enter the following command at the DCL prompt:

                    $ @SYS$UPDATE:AUTOGEN GETDATA REBOOT

                  AUTOGEN performs an automatic system shutdown and reboots
                  when it has finished. Rebooting your system makes the new
                  parameter values active. The /[NO]FEEDBACK qualifier on the
                  AUTOGEN command line could be appropriate for your system.
                  See the Guide to Setting Up a VMS System for more informa-
                  tion.

               _________________________________________________________________

               1.4  User Account Quotas and Privileges

                  To use VAX LISP, each account must have TMPMBX and NETMBX
                  privileges and the following requirements:

                   o Paging file quota (PGFLQUOTA) 10,500 pages (minimum)

                   o Working set size (WSDEF) 200 pages (minimum)

                  Use the VMS Authorize Utility (AUTHORIZE) to compare the
                  current values of these quotas with the requirements for VAX
                  LISP. For example, the account used in the following example
                  is the SYSTEM account:

                    $ SET DEFAULT SYS$SYSTEM <Return>
                    $ RUN AUTHORIZE <Return>
                    UAF> SHOW SYSTEM <Return>

                  To change the values of these quotas, use the VMS Authorize
                  Utility's MODIFY command. For more information, see the VMS
                  Authorize Utility Manual.









               1-4  Preparing to Install VAX LISP








               _________________________________________________________________

               1.5  VMS Tailoring Classes

                  For Version 5.0 or later systems, the following VMS classes
                  are required for full functionality for VAX LISP:

                   o Programming Support

                   o Utilities

                  For more information on VMS classes and tailoring, see the
                  VAX/VMS Operating System Software Product Description (SPD
                  25.01.xx).

               _________________________________________________________________

               1.6  DECwindows Tailoring Classes

                  You can run VAX LISP with a DECwindows interface. DECwindows
                  must be installed separately from VAX LISP and from the VMS
                  operating system. VAX LISP can use DECwindows in two modes:

                   o Standalone execution, running the X11 display server and
                     the client application on the same machine

                   o Remote execution, running the X11 display server and the
                     client application on different machines

                  To run VAX LISP with DECwindows in the standalone execution
                  mode, the following DECwindows components must be installed:

                   o VMS DECwindows Compute Server

                   o VMS DECwindows Device Support

                   o VMS DECwindows Programming Support

                  To run VAX LISP with DECwindows in the remote execution mode,
                  the following DECwindows components must be installed:

                   o On the server machine:

                      _ VMS DECwindows Device Support

                   o On the client machine:

                      _ VMS DECwindows Compute Server

                      _ VMS DECwindows Programming Support






                                             Preparing to Install VAX LISP  1-5








               _________________________________________________________________

               1.7  VMS License Management Facility

                  The VMS License Management Facility (LMF) became available
                  with Version 5.0 of the VMS operating system. If you are in-
                  stalling VAX LISP on a VMS Version 5.1 or later system, you
                  must register your VAX LISP software license. Normally, you
                  register your VAX LISP license before beginning the installa-
                  tion. This permits you to run the Installation Verification
                  Procedure (IVP) during the installation, and to use the soft-
                  ware immediately afterwards.

                  The license registration information you need is contained
                  in the Product Authorization Key (PAK) that is shipped with
                  VAX LISP. The PAK is a paper certificate that contains in-
                  formation about your license to run a particular piece of
                  software.

                  During the installation, you are asked if you have registered
                  the VAX LISP license and loaded the appropriate authorization
                  key. You must register and load your license for VAX LISP
                  before you start the installation in order to run the IVP and
                  use the software.

                  To register a license under VMS Version 5.0, first log in to
                  the system manager's account, SYSTEM. Choose only one of the
                  following two ways to perform the registration:

                   1. Set default to SYS$UPDATE and invoke the VMSLICENSE.COM
                      procedure.

                       $ SET DEFAULT SYS$UPDATE <Return>
                       $ @VMSLICENSE <Return>

                     When the procedure prompts you for information, respond
                     with data from your PAK. When the procedure asks if you
                     want to load the license, respond YES. When the procedure
                     completes successfully, you see the following message:

                       DEC VAX LISP has been registered.

                   2. Issue the LICENSE REGISTER command at the DCL level with
                      the appropriate qualifiers that correspond to information
                      on the PAK. (See the VMS License Management Utility Manual
                      for instructions.) Then activate the license with the
                      LICENSE LOAD command.

                  For complete information on using LMF, see the VMS License
                  Management Utility Manual.






               1-6  Preparing to Install VAX LISP








               _________________________________________________________________

               1.8  Using VMSINSTAL

                  After you log in to a privileged account to install VAX LISP,
                  invoke VMSINSTAL, the command procedure that installs this
                  product. An example of this procedure is shown in steps 1 and
                  2 of Chapter 2.

                  The VMSINSTAL command procedure has the following syntax:

                    $ @SYS$UPDATE:VMSINSTAL LISP ddcu: [OPTIONS N]

                  You can also type an asterisk (*) in place of LISP. If you
                  are installing from magnetic tape, you can use the asterisk
                  to save installation time; the asterisk causes VAX LISP to
                  be installed with a minimum of tape passes. For example, the
                  first parameter to VMSINSTAL for VAX LISP Version 3.1 could
                  be either LISP or *.

                  ddcu:
                  The symbol :ddcu represents the name of the device on which
                  the distribution volumes will be mounted for the VAX LISP
                  installation media, where dd is the device code, c is the
                  controller code, and u is the unit number. It is not nec-
                  essary to use the console drive to install VAX LISP. If you
                  do use the console drive, you should replace any media you
                  removed from the drive. MUA0: is the device name used in
                  examples in this document.

                  OPTIONS N
                  OPTIONS N is an optional parameter you should provide if you
                  want to be prompted to display or print the release notes.
                  If you do not include the OPTIONS N parameter, VMSINSTAL
                  does not prompt you to display or print the release notes.
                  VMSINSTAL permits the use of several other options. For more
                  information on the other options, see your processor-specific
                  installation/operations guide.

                  If you do not supply the first two parameters, VMSINSTAL
                  prompts you for the product and device names. If you wish to
                  be prompted for the product and device names and to display
                  or print the release notes, type the following:

                    $ @SYS$UPDATE:VMSINSTAL <Return>

                  When you invoke VMSINSTAL, it checks the following:

                   o Whether you logged in to a privileged account. Digital
                     recommends that you install software from the system
                     manager's account with your default device and directory
                     set to SYS$UPDATE.




                                             Preparing to Install VAX LISP  1-7








                   o Whether you have adequate quotas for installation.
                     VMSINSTAL checks for the following quota values:

                      _ ASTLM = 24

                      _ BIOLM = 18

                      _ BYTLM = 18000

                      _ DIOLM = 18

                      _ ENQLM = 30

                      _ FILLM = 20

                  VMSINSTAL then checks whether the following conditions ex-
                  ist. If so, discontinue the conditions before resuming the
                  installation procedure.

                   o Whether DECnet is up and running

                   o Whether any users are logged in to the system

                  If VMSINSTAL detects either of these conditions, you will
                  be asked whether you want to continue the installation.
                  If you want to continue, type YES. If you want to stop the
                  installation, press Return.





























                                             Preparing to Install VAX LISP  1-8












                                                                      Chapter 2


                                                            Installing VAX LISP
               ________________________________________________________________


                  This chapter explains how to use the VMSINSTAL procedure
                  to install VAX LISP and to verify the installation. The
                  chapter contains excerpts from the installation procedure and
                  explains each step. Defaults appear in brackets throughout
                  the installation procedure.

                  To abort the installation procedure at any time, press Ctrl
                  /Y. When you press Ctrl/Y, the installation procedure deletes
                  all files it has created up to that point and then returns
                  you to the DCL level. If you want to retry the installation
                  procedure after pressing Ctrl/Y, you must proceed from step
                  2.

               _________________________________________________________________

               2.1  Installation Procedure

                  Step 1: Log in to a privileged account and set your default
                  device and directory to SYS$UPDATE.

                    Username: SYSTEM  <Return>
                    Password:         <Return>
                    $ SET DEFAULT SYS$UPDATE <Return>

                  Step 2: Invoke VMSINSTAL.

                                             REMINDER

                      If you have not yet registered and loaded a license
                      for VAX LISP, be sure to read Section 1.7 before you
                      start the installation.

                    $ @VMSINSTAL LISP MUA0: OPTIONS N <Return>

                          VAX/VMS Software Product Installation Procedure V5.3

                    It is 07-FEB-1990 at 18:02.
                    Enter a question mark (?) at any time for help.

                    * Are you satisfied with the backup of your system disk
		      [YES]? <Return>




                                                       Installing VAX LISP  2-1

 






                  If you are satisfied with the backup of your system disk,
                  press Return. Otherwise, type NO and press Return to discon-
                  tinue the installation.

                  VMSINSTAL begins installing the kit.

                    The following products will be processed:
                    VAX LISP V3.1

                         Beginning installation of VAX LISP V3.1 at 18:13

                    %VMSINSTAL-I-RESTORE, Restoring product saveset A ...

                  Step 3: Select a release notes option.

                  This step applies only if you specified OPTIONS N in step 2.

                    Release Notes Options:

                        1. Display release notes
                        2. Print release notes
                        3. Both 1 and 2
                        4. Copy release notes to SYS$HELP
                        5. Do not display, print or copy release notes

                    * Select option [3]: <Return>

                  If you select option 1, VMSINSTAL displays the release notes
                  on line immediately. You can terminate the display at any
                  time by pressing Ctrl/C.

                  If you select option 2, VMSINSTAL prompts you for a queue
                  name. Either type a queue name or press Return to send the
                  file to the default output print device.

                    * Queue name [SYS$PRINT]: <Return>

                  If you select option 3, VMSINSTAL displays the release notes
                  on line immediately. You can terminate the display at any
                  time by pressing Ctrl/C. VMSINSTAL then prompts you for a
                  queue name. Either type a queue name or press Return to send
                  the file to the default output print device. The VAX LISP
                  release notes are then copied to SYS$HELP:LISP031.RELEASE_
                  NOTES.

                  If you select option 4, VMSINSTAL copies the release notes to
                  SYS$HELP immediately.

                  If you select option 5, VMSINSTAL does not display, print, or
                  copy the release notes; typically, this option is selected
                  when the user wants to terminate the installation.





               2-2  Installing VAX LISP








                                               NOTE

                      This version of the release notes file installed by
                      VMSINSTAL is labeled with the current product name and
                      version number. Take care not to delete release notes
                      for previous versions of VAX LISP.


                  Next, VMSINSTAL displays the following prompt:

                    * Do you want to continue the installation [N]?: Y <Return>
                    %VMSINSTAL-I-RELMOVED, The product release notes have been
	            successfully moved to SYS$HELP.

                  If you want to continue the installation, type YES and press
                  Return. If you type NO or press Return, VMSINSTAL discon-
                  tinues the installation. In either case, VMSINSTAL moves the
                  release notes to SYS$HELP.

                  Step 4: Respond to purging previous versions of VAX LISP
                  check.

                    * Do you want to purge files replaced by this installation
		      [YES]? <Return>

                  The directories SYS$HELP, SYS$MANAGER, and SYS$SYSROOT may
                  contain previous versions of VAX LISP files. These files are
                  replaced during the installation with new files, but the old
                  files are not automatically purged. Purging is recommended,
                  unless it is necessary to save a LISP "suspended system"
                  built with a previous version of VAX LISP. In response to the
                  purging prompt, press Return to purge the files or type NO to
                  keep them.

                  Step 5: Respond to license registration queries.

                  VAX LISP supports the VMS License Management Facility (LMF).
                  The installation procedure displays license information about
                  your product and then asks if you have registered and loaded
                  your authorization key for VAX LISP. The following is an
                  example of such information:

                    Product:       LISP
                    Producer:      DEC
                    Version:       3.1
                    Release Date:  23-MAR-1990

                    * Does this product have an authorization key registered
		      and loaded?







                                                    Installing VAX LISP  2-3








                  If you have not registered and loaded your authorization key,
                  you must answer NO to this question. You have to register and
                  load your product authorization key (PAK) to successfully
                  complete the installation. If you have not done so, you
                  should stop the installation, register and load your PAK,
                  and then restart the installation.

                  Step 6: Install the VAX LISP product files.

                    Do you wish to install the VAX LISP product files
		    (20000 blocks) [YES]? <Return>

                  The procedure now asks whether you want to install the prod-
                  uct files saveset on the tape, and displays the size of the
                  saveset. The product files contain everything you need to
                  run VAX LISP: the LISP executable image, online documenta-
                  tion library, the CLD file, and Installation Verification
                  Procedure (IVP). Press the Return key if you want to install
                  the saveset. Type NO if you do not.

                  Step 7: Respond to DECwindows check.

                    Do you want the DECwindows version of VAX LISP
		    [YES]?<Return>

                  The procedure now asks whether you want to install the
                  DECwindows version of VAX LISP. Press the Return key to
                  install the DECwindows version. If you do not want the
                  DECwindows version, type NO in response to the prompt. Typing
                  NO gives you the UIS version of VAX LISP. When you press the
                  Return key, the procedure asks you for the directory where
                  the VAX LISP product files are to be installed:

                    In which directory are the VAX LISP product files to be
		    installed [SYS$COMMON:[VAXLISP]]? <Return>

                  You must now tell VMSINSTAL the desired location of the
                  saveset you selected to install. Press the Return key if
                  you are satisfied with the default directory, or enter a
                  different location. If the directory you specify does not
                  already exist, the procedure asks:

                    Directory SYS$COMMON:[VAXLISP] does not exist.  Should it
		    be created [YES]?<Return>

                  Step 8: Install the VAX LISP system-building library files.

                    Do you wish to install the VAX LISP system-building library
		    files (22500 blocks) [NO]? <Return>







               2-4  Installing VAX LISP








                  The VAX LISP System-Building Utility enables you to create
                  a LISP system that is a single executable image. This user-
                  built system can serve as a customized VAX LISP development
                  environment that can be shared efficiently by multiple users
                  at the same time or as a delivery vehicle for applications
                  based on VAX LISP. The system-building library files are not
                  required to run VAX LISP.

                  Type YES to install the system-building library files at this
                  time. Type NO or press the Return key to skip installing the
                  files. If you choose to install the system-building library
                  files, the procedure asks you for a directory.

                  Step 9: Install the VAX LISP example files.

                    Do you wish to install the VAX LISP examples (4400 blocks)
		    [NO]?<Return>

                  The procedure now asks whether you want to install the VAX
                  LISP example files. The VAX LISP example files contain some
                  useful VAX LISP utilities that serve as examples of LISP pro-
                  gramming style. The VAX LISP example files are not required
                  in order to run VAX LISP.

                  Type YES to install the VAX LISP example files at this time.
                  Type NO or press the Return key to skip installing the exam-
                  ple files. If you choose to install the example files, the
                  procedure asks you for the name of the directory where the
                  files are to be installed.

                  Step 10: Install the Portable Common Loops (PCL) example
                  files.

                    Do you wish to install the PCL examples (4400 blocks) 
		    [NO]<Return>

                  The procedure now asks whether you want to install the PCL
                  example files. The kit contains the 05/23/89 (Victoria Day)
                  version of Portable Common Loops, the publicly available
                  version of the Common LISP Object System (CLOS). The PCL
                  example files are not required to run VAX LISP.

                  Type YES to install the PCL files at this time. Type NO or
                  press the Return key to skip installing the files. If you
                  choose to install the PCL files, the procedure asks you for a
                  directory. PCL is normally installed in its own subdirectory.

                  Step 11: Install the RdbLISP example files.

                    Do you wish to install the RdbLISP examples (2100 blocks)
                    [NO]? <Return>





                                                       Installing VAX LISP  2-5








                  The procedure now asks whether you want to install the
                  RdbLISP example files. The RdbLISP software provides an in-
                  terface layer between Digital's relational database (Rdb) and
                  VAX LISP. The RdbLISP example files are not required to run
                  VAX LISP.

                  Type YES to install the RdbLISP files at this time. Type NO
                  or press the Return key to skip installing the files. If you
                  choose to install the RdbLISP files, the procedure asks you
                  for a directory.

                  Step 12: Install the Foxglove example files.

                    Do you wish to install the Foxglove examples (26400 blocks)
                    [NO]? <Return>

                  The procedure now asks whether you want to install the
                  Foxglove example files. Foxglove is a rapid-prototyping lan-
                  guage for developing rule-based application systems. The
                  Foxglove example files are not required to run VAX LISP.

                  Type YES to install the Foxglove files at this time. Type NO
                  or press the Return key to skip installing the files. If you
                  choose to install the Foxglove files, the procedure asks you
                  for a directory.

                  Step 13: Install the GKS and GKS3D LISP bindings.

                    Do you wish to install the GKS and GKS3D bindings
                    (4400 blocks) [NO]? <Return>

                  The procedure now asks whether you want to install the
                  LISP bindings for GKS and GKS3D. GKS is the Graphics Kernel
                  System; GKS3D is its three-dimensional version. The GKS and
                  GKS3D bindings are not required to run VAX LISP.

                  Type YES to install the GKS and GKS3D bindings at this time.
                  Type NO or press the Return key to skip installing the files.
                  If you choose to install the GKS and GKS3D files, the proce-
                  dure asks you for a directory.

                  Step 14: Install the VAXFlavors example files.

                    Do you wish to install the VAXFlavors examples (2000 blocks)
                    [NO]? <Return>

                  The procedure now asks whether you want to install the
                  VAXFlavors example files. VAXFlavors is an implementation
                  of Flavors under VAX LISP. It implements an object-oriented
                  programming system under Common LISP. The VAXFlavors example
                  files are not required to run VAX LISP.





               2-6  Installing VAX LISP








                  Type YES to install the VAXFlavors example files at this
                  time. Type NO or press the Return key to skip installing the
                  files. If you choose to install the VAXFlavors files, the
                  procedure asks you for a directory.

                  Step 15: Install the VMS Starlet example files.

                    Do you wish to install the Starlet examples (16000 blocks)
                    [NO]? <Return>

                  The procedure now asks whether you want to install the VMS
                  Starlet example files. Starlet is an interface to VMS system
                  services routines. The Starlet example files are not required
                  to run VAX LISP.

                  Type YES to install the Starlet example files at this time.
                  Type NO or press the Return key to skip installing the files.
                  If you choose to install the Starlet files, the procedure
                  asks you for a directory.

                  Step 16: Respond to previous version save check.

                    Do you want to save the previous version of VAX LISP
		    (95380 blocks) [NO]?<Return>

                  This question does not appear unless a previous version of
                  VAX LISP is already installed in the default directory.

                  VAX LISP users can create "suspended systems" that contain
                  LISP programs and data. A suspended system depends on the
                  version of VAX LISP used to create it. Since the installation
                  procedure overwrites any previous version of VAX LISP in the
                  default directory, installing the new version makes user-
                  created suspended systems unusable. You may want to save your
                  previous versions of VAX LISP so that users can resume their
                  suspended systems.

                  To save the previous version of VAX LISP, you can allow the
                  procedure to move it to another directory before you install
                  the new version in SYS$COMMON:[VAXLISP].

                  If you do not want to save your previous version, type NO
                  or press the Return key. If you want to save it, type YES.
                  The procedure now asks for a new location for the previous
                  version of VAX LISP:

                    In which directory should the previous version be saved
                    [SYS$COMMON:[VAXLISP.V030]]? <Return>

                  Press the Return key if you are satisfied with the default
                  directory, or enter a different location. (The default di-
                  rectory automatically includes the correct version number.)
                  Again, if the directory you specify does not already exist,
                  the procedure asks you if it should be created.


                                                       Installing VAX LISP  2-7








                  See Chapter 4 of this manual for directions on using the
                  old version of VAX LISP after you have moved it out of
                  SYS$COMMON:[VAXLISP].

                  Step 17: Respond to IVP check.

                    * Do you want to run the IVP after the installation
		      [YES]? <Return>

                  The IVP runs tests to check whether the installation proce-
                  dure was successful. Press Return to run the IVP after the
                  installation only if you have properly configured your sys-
                  tem. Because VAX LISP will not run until you have properly
                  configured your system, you cannot run the IVP if you have
                  not already configured your system. If you do not want to run
                  the IVP, type NO in response to the prompt.

                  Step 18: Read informational messages.

                  The VAX LISP installation procedure produces a number of
                  informational messages that report on the progress of the
                  installation.

                  The success of the installation is indicated by the following
                  messages:

                    %LISP-I-QUESDONE, There are no more installation questions
		    to be answered

                    %VMSINSTAL-I-RESTORE, Restoring product saveset B ...

                    %VMSINSTAL-I-MOVEFILES, files will now be moved to their
		    target directories...
                    Executing VAX LISP startup procedure...

                  If the installation procedure is successful, the new or
                  modified files are moved to their target directories.

                  The SYS$HELP:HELPLIB.HLB file is updated to include the new
                  version of the VAX LISP HELP text.

                  See Appendix A for a complete list of the files added to the
                  system.

                  If you typed YES in response to the prompt that requests a
                  file purge at step 4, previous versions of the VAX LISP files
                  are now purged.

                                 NOTICE TO 9-TRACK TAPE CUSTOMERS

                      For 9-Track Tape installations only, if you are in-
                      stalling one or more of the examples files, there
                      is an additional step in the middle of Step 18. The
                      installation procedure asks you to mount the next
                      distribution volume.

               2-8  Installing VAX LISP








                        Please mount the next distribution volume on
		        HSC001$MUA16:.
                        (If no more volumes, answer NO.)
                        Are you ready? yes
                        %MOUNT-I-MOUNTED, LSP031 mounted on _HSC001$MUA16:.
                        %VMSISNTAL-I-RESTORE, Restoring product saveset F ...

                  Step 19: Observe the Installation Verification Procedure.

                  If you chose to run the IVP in step 17, VMSINSTAL now calls
                  the IVP to verify that VAX LISP was installed successfully.

                    VAX LISP Installation Verification Procedure (IVP)
                    Starting compilation of file
                      VMI$ROOT:[SYSUPD.LISP031]LISPIVP.LSP;1

                    FIBONACCI compiled.
                    PRINT-FIBONACCI-TABLE compiled.
                       .
                       .
                       .
                    Finished compilation of file
                     VMI$ROOT:[SYSUPD.LISP031]LISPIVP.LSP;1
                    0 Errors, 0 Warnings

                    VAX LISP [TM]
                    V3.1

                    © Digital Equipment Corporation. 1989, 1990.

                    All Rights Reserved.

                    A table of the first 20 Fibonacci numbers
                       .
                       .
                       .
                    VAX LISP V3.1 IVP Completed Successfully

                  Step 20: End the installation procedure.

                       Installation of VAX LISP V3.1 completed at 18:51

                       VMSINSTAL procedure done at 18:54

                    $ LOGOUT <Return>
                    SYSTEM     logged out at 07-FEB-1990 18:56:42.19

                  When the product installation procedure is complete, you
                  can choose to install more products or to log out (as shown
                  here). If you removed any media from the console drive before
                  beginning the installation, you should replace it now.





                                                       Installing VAX LISP  2-9








                  VMSINSTAL deletes or changes entries in the process symbol
                  tables during the installation. Therefore, if you are going
                  to continue using the system manager's account and you want
                  to restore these symbols, you should log out and log in
                  again.


               _________________________________________________________________

               2.2  Installing VAX LISP on a VAXcluster

                  If you want to run VAX LISP on multiple nodes of a VAXcluster,
                  first check to see that you have the appropriate software
                  license. Then, follow these steps after installing VAX LISP:

                   1. Issue the LICENSE LOAD command to activate the license
                      on each node in the VAXcluster on which VAX LISP is to
                      be executed as described in the VMS License Management
                      Utility Manual.

                   2. Run SYS$MANAGER:LISPSTART.COM on each node of the cluster
                      that has a software license.

                   3. To use the product on other nodes in the VAXcluster,
                      you must replace the version of the DCL tables that is
                      installed on the other VAXcluster nodes. To do this,
                      perform the following steps:

                      a. Log in to a node on the cluster.

                      b. Run INSTALL and enter the following command at the
                         INSTALL> prompt:

                          INSTALL> REPLACE SYS$LIBRARY:DCLTABLES.EXE <Return>

                      c. Repeat steps a and b for each node of the cluster.




















               2-10  Installing VAX LISP










 

                                                                      Chapter 3


                                                    Completing the Installation
               ________________________________________________________________


                  To complete a new installation of VAX LISP, you must modify
                  the site-specific system startup file,
		  SYS$MANAGER:SYS$STARTUP_V5.COM. You should also modify the
		  default site-specific startup file for VAX LISP,
		  SYS$STARTUP:LISP$SITE.COM. If you are installing VAX LISP on
		  an AI VAXstation, read Chapter 9 on recommended system
		  parameters and authorization quotas.  Chapter 4 explains how
		  to use a previous version of VAX LISP	that has been moved out
		  of the main directory.

               _________________________________________________________________

               3.1  Modifying the System Startup File

                  After the installation procedure is concluded, add the
                  following line to your site-specific system startup file,
                  SYS$MANAGER:SYS$STARTUP_V5.COM:

                    $ @SYS$COMMON:[SYS$STARTUP]LISP$STARTUP.COM

                  This command line invokes the VAX LISP system startup proce-
                  dure every time you boot your system. The startup procedure
                  defines:

                   o The system logical name LISP$SYSTEM to mean the VAX LISP
                     product directory

                   o The logical name LISP$LIBRARY to mean the library files
                     directory

                  You must add the following line to the site-specific system
                  startup file if you are installing the UIS version of VAX
                  LISP.

                    $ @SYS$COMMON:[SYS$STARTUP]LISP$UIS_STARTUP.COM

                  You must also add a line to the site-specific system startup
                  file for each of the example files that you have installed.
                  For example, to invoke the PCL example files, you must add
                  the following line in the system startup file:

                    $ @SYS$COMMON:[SYS$STARTUP]LISP$PCL_STARTUP.COM



                                               Completing the Installation  3-1








                  Each command line defines a logical that points to the direc-
                  tory containing the example files. Table 3-1 gives the name
                  of the .COM file to add to the system startup file for each
                  of the example files.


                  Table 3-1:  .COM File Names for the System Startup File
                  ____________________________________________________________
                  File                .COM File
		  ____________________________________________________________

                  LISP Example        LISP$EXAMPLE_STARTUP.COM

                  PCL Example         LISP$PCL_STARTUP.COM

                  RdbLISP Example     LISP$RDBLISP_STARTUP.COM

                  Foxglove Example    LISP$FOXGLOVE_STARTUP.COM

                  GKS/GKS3D Bindings  LISP$GKS_STARTUP.COM

                  VAXFlavors Example  LISP$VAXFLAVORS_STARTUP.COM

                  Starlet Example     LISP$STARLET_STARTUP.COM

                  UIS                 LISP$UIS_STARTUP.COM
		  ____________________________________________________________
               _______________________________________________________________

               3.2  Modifying the VAX LISP Startup File

                  The file SYS$MANAGER:SYS$STARTUP_V5.COM invokes the LISP
                  command file LISP$STARTUP.COM when you boot your VMS system.
                  This, in turn, invokes the file SYS$STARTUP:LISP$SITE.COM.
                  This last command file is a default site-specific startup
                  procedure for VAX LISP.

                  This file includes default LISP system logical names and
                  default commands for installing shareable sections. You
                  should modify the logical name definitions to make them
                  appropriate for your site.

                  If your VAX LISP system has only one user or if enough global
                  pages are not available, you may not want to install LISP
                  shareable. The benefit of installing shareable sections is
                  that multiple users running VAX LISP use only one copy of
                  the LISP system rather than a separate copy for each user,
                  thereby saving valuable system resources.

                  This skeleton LISPSITE.COM file will be installed in
                  SYS$STARTUP, provided such a file is not already there:





               3-2  Completing the Installation


 





       $!      VAX LISP site-specific startup procedure.
       $!      This procedure is invoked by the lispstart procedure.
       $!      Remove comments and alter this file to suit your site.
       $
       $       DEFINE/SYSTEM/EXECUTIVE LISP$TIME_ZONE 0
       $       DEFINE/SYSTEM/EXECUTIVE LISP$DAYLIGHT_SAVING_TIME_P NO
       $!      DEFINE/SYSTEM/EXECUTIVE LISP$SHORT_SITE_NAME "?"
       $!      DEFINE/SYSTEM/EXECUTIVE LISP$LONG_SITE_NAME "?"
       $!      DEFINE/SYSTEM/EXECUTIVE LISP$MACHINE_INSTANCE "?"
       $
       $       SET NOON
       $!      INSTALL :=$SYS$SYSTEM:INSTALL/COMMAND_MODE
       $!      INSTALL CREATE LISP$SYSTEM:LISP/OPEN/HEADER_RESIDENT/SHARED
       $       SET ON
       $       EXIT

                  You can add to this file any other site-specific commands for
                  starting VAX LISP.

                  To install your system shareable, delete the comment charac-
                  ter (!) from the beginning of each command between SET NOON
                  and SET ON in the default LISPSITE.COM file.

               _________________________________________________________________

               3.3  Defining the LISP System Logical Names

                  The following list describes the LISP system logical names
                  and shows how to define them.

                   o LISP$TIME_ZONE

                     Define LISP$TIME_ZONE to indicate your local time zone
                     relative to Greenwich Mean Time (GMT). The value can
                     be an integer or a floating-point number in the range
                     0 (inclusive) to 24 (exclusive). Floating-point numbers
                     are used when an area is not in a full hour time zone and
                     are specified by format "hour.fraction". To determine your
                     local time zone, consult an atlas.

                     Examples:

                       $DEFINE/SYSTEM LISP$TIME_ZONE 4.5   !Newfoundland
                       $DEFINE/SYSTEM LISP$TIME_ZONE 5     !Boston
                       $DEFINE/SYSTEM LISP$TIME_ZONE 8     !San Francisco
                       $DEFINE/SYSTEM LISP$TIME_ZONE 12.75 !Chatham Island
                       $DEFINE/SYSTEM LISP$TIME_ZONE 23    !Munich

                                                 NOTE

                         This logical name is required.

                   o LISP$DAYLIGHT_SAVING_TIME_P



                                               Completing the Installation  3-3








                     Define LISP$DAYLIGHT_SAVING_TIME_P to specify whether you
                     are on daylight saving time. The values T, TRUE, YES, and
                     1 mean YES; the values F, FALSE, NO and 0 mean NO. You
                     should update this logical name each time daylight saving
                     time changes.

                     In the following example, the NO after the logical name
                     means it is not daylight saving time.

                     Example:

                       $ DEFINE/SYSTEM-
                                 LISP$DAYLIGHT_SAVING_TIME_P NO


                   o LISP$SHORT_SITE_NAME

                     Define LISP_SHORT_SITE_NAME to specify a short string that
                     describes your site. This string is returned by the LISP
                     SHORT-SITE-NAME function. An example is "Widget Group".

                     Example:

                       $ DEFINE/SYSTEM/-
                                 LISP$SHORT_SITE_NAME "Widget Group"

                   o LISP$LONG_SITE_NAME

                     Define LISP$LONG_SITE_NAME to specify a long string that
                     describes your site. This string is returned by the LISP
                     LONG-SITE-NAME function. An example is "Super Widget
                     Development Group, Widget Corp".

                     Example:

                       $ DEFINE/SYSTEM LISP$LONG_SITE_NAME-
                                 "Super Widget Development Group, Widget Corp"

                     If you would like the long site name to occupy several
                     lines, you can create a text file for it. Then, refer
                     to the text file with the logical name. Suppose, for
                     example, that the file SYS$MANAGER:LISPSITE.TXT contained
                     the following text:

                            Super Widget Development Group
                            Intelligent Widget Corporation
                            One First Street
                            Any Town, Massachusetts 01001

                     You can define LISP$LONG_SITE_NAME by placing an at sign
                     (@) in front of the name of the text file you created.





               3-4  Completing the Installation








                     Example:

                       $ DEFINE/SYSTEM LISP$LONG_SITE_NAME-
                                 "@SYS$STARTUP:LISPSITE.TXT"

                   o LISP$MACHINE_INSTANCE

                     Define LISP$MACHINE_INSTANCE as a string that identifies
                     the specific computer on which VAX LISP is running. This
                     string is returned by the LISP-MACHINE-INSTANCE function.
                     An example is "Super Widget VAX-6240".

                     Example:

                       $ DEFINE/SYSTEM LISP$MACHINE_INSTANCE-
                                "Super Widget VAX-6240"

                     If this logical name is not defined and you are running
                     DECnet, your computer's node name is used as the machine
                     instance.

                  In the preceding list of system logical names, the two log-
                  ical names LISP$TIME_ZONE and LISP$DAYLIGHT_SAVING_TIME_P
                  are used by the LISP function GET-DECODED-TIME, which is de-
                  scribed in Common LISP: The Language. The VAX LISP functions
                  SHORT-SITE-NAME, LONG-SITE-NAME, and MACHINE-INSTANCE are
                  described in the VAX LISP/VMS Object Reference Manual.





























                                               Completing the Installation  3-5

 










                                                                      Chapter 4


                                            Using Previous Versions of VAX LISP
               ________________________________________________________________


                  By default, the files comprising a saved version of VAX LISP
                  are put in a subdirectory under the main VAX LISP directory
                  (referred to by the logical name LISP$SYSTEM). The subdi-
                  rectory name uses the VAX LISP version number in the format
                  Vvvu, with vv representing the 2-digit version and u repre-
                  senting the 1-digit update. For example, Version 3.0 would be
                  saved in the subdirectory V030.

                  To run a saved version of VAX LISP, you must define the logi-
                  cal name LISP$SYSTEM to refer to the subdirectory containing
                  the files of that saved version. Then you use the standard
                  LISP command to invoke the old version of the LISP system.

































                                       Using Previous Versions of VAX LISP  4-1

 










                                                                      Chapter 5


                     Running the Installation Verification Procedure Separately
               ________________________________________________________________


                  The Installation Verification Procedure (IVP) is usually run
                  at installation. If you want to run the IVP separately to
                  ensure the integrity of installed files if system problems
                  occur, execute the following command procedure:

                   $ @SYS$TEST:LISP$IVP

                  If the IVP fails for any reason, the following messages are
                  displayed:

                   The VAX LISP V3.1 Installation Verification Procedure failed.

                   %VMSINSTAL-E-IVPFAIL, The IVP for VAX LISP V3.1 has failed.
































                Running the Installation Verification Procedure Separately  5-1

 










                                                                      Chapter 6


                                                               Error Conditions
               ________________________________________________________________


                  If the installation procedure fails for any reason, a message
                  such as the one following is displayed:

                    %VMSINSTAL-E-INSFAIL, The installation of VAX LISP V3.1
		    has failed.

                  An error during the installation can occur if one or more of
                  the following conditions exist:

                   o Operating system version is incorrect.

                   o Quotas necessary for successful installation are insuffi-
                     cient (see Section 1.3).

                   o Process quotas required by VMSINSTAL are incorrect (see
                     Section 1.8).

                   o The VMS HELP library is currently in use.

                   o The product was registered incorrectly or not registered.

                  For descriptions of the error messages generated by these
                  conditions, see the VMS System Messages and Recovery
                  Procedures Reference Volume, your processor-specific in-
                  stallation/operations guide, or the VMS License Management
                  Utility Manual.

                  If you are notified that any of these conditions exist, you
                  should take the appropriate action as described in the mes-
                  sage. You may need to change a system parameter or increase
                  an authorized quota value.

                  If the installation fails, you must restart the installation
                  procedure from step 2. If the installation fails due to an
                  IVP failure, contact a Digital field service representative.










                                                          Error Conditions  6-1

 










                                                                      Chapter 7


                                          Installing VAX LISP as a Shared Image
               ________________________________________________________________


                  If VAX LISP will be used extensively on your system, you
                  can reduce the system overhead and memory requirements by
                  installing it as a shared image. To perform the installation
                  on a system that is currently running, use the VMS Install
                  Utility while you are logged in to a privileged account. If
                  errors occur, see VMS System Messages and Recovery Procedures
                  Reference Volume.

                  First, determine the number of available global pages and
                  global sections on your system. See Section 1.3 for informa-
                  tion on how to do this. Installing VAX LISP as a shared image
                  requires:

                   o A minimum of 11,000 free global pages plus the
		     size (in number of disk blocks) of the file
		     SYS$LIBRARY:DCLTABLES.EXE at installation.

                   o A minimum of 4 free global sections at installation. Three
                     global sections are used after installation.

                  Then, invoke the VMS Install Utility and install VAX LISP as
                  a shared image by typing the following commands:

      $ INSTALL:= $SYS$SYSTEM:INSTALL/COMMAND_MODE <Return>

      INSTALL> CREATE LISP$SYSTEM:LISP.EXE/OPEN/SHARED/HEADER_RESIDENT <Return>
      INSTALL> EXIT <Return>

                  Finally, update the system startup file to install VAX LISP.
                  Modify SYS$STARTUP:LISPSITE.COM by removing the commented
                  lines (see Section 3.2).














                                     Installing VAX LISP as a Shared Image  7-1

 










                                                                      Chapter 8


                                                            Maintenance Updates
               ________________________________________________________________


                  Digital may periodically issue maintenance updates of VAX
                  LISP. Each update consists of an installation kit. You should
                  install this kit as described in this document or in any
                  documentation accompanying the maintenance update.

                  Each time a maintenance update is released, the version
                  number changes. For example, if the current version is 3.0,
                  the version number of the first maintenance update will
                  be 3.1. In addition, each maintenance update includes new
                  release notes. The release notes describe the changes that
                  have been made to VAX LISP since the previous release.

                  The update release notes are provided on line. You should
                  read the release notes when you first install VAX LISP;
                  they are also accessible at any time after the product is
                  installed. For information on reading the release notes
                  at the time that you install VAX LISP, follow the instal-
                  lation procedure through step 5. To locate the release
                  notes after VAX LISP is installed, display or print the
                  file SYS$HELP:LISP031.RELEASE_NOTES, or type the following
                  command:

                    $ HELP LISP RELEASE_NOTES <Return>






















                                                       Maintenance Updates  8-1

 










                                                                      Chapter 9


                                                          Tuning the VAXstation
               ________________________________________________________________


                  You can tune your VAXstation in one of two ways:

                   o By adjusting parameter values in your system parameters
                     file

                   o By adjusting authorization quotas in your user accounts


               _________________________________________________________________

               9.1  Recommended System Parameters

                  The following sample MODPARAMS.DAT file is for a typical
                  monochrome VAXstation. The values of these AUTOGEN parameters
                  are recommended for optimal performance of VAX LISP on a
                  VAXstation with 9 megabytes of memory.


                               SAMPLE SYS$SYSTEM:MODPARAMS.DAT FILE


         !Site specific AUTOGEN data file.  In a VAXcluster where a
         !common system disk is being used, this file should reside
         !in SYS$SPECIFIC:[SYSEXE], not a common system directory.
         !
         !Add modifications that you wish to make to AUTOGEN's hardware
         !configuration data, system parameter calculations, and page,
         !swap, and dump file sizes to the bottom of this file.
         !
         CHANNELCNT=2048       !Number of allowed channels
         CTLPAGES=500          !Used with workstation windows
         SPTREQ=2000           !Required number of system page table
			       !  entries
         MPW_HILIMIT=2500      !Modified page-list size at which writing
         		       !  to free-list page occurs
         MPW_WAITLIMIT=2500    !Wait-limit number of pages on the
         		       !  modified page list; this number must
			       !  be greater than or equal to the
			       !  MPW_HILIMIT number or a system
			       !  deadlock will occur
         MPW_LOLIMIT=500       !Writing of the modified page list stops
                               !  when it is less than or equal to the
			       !  MPW_LOLIMIT number


                                                     Tuning the VAXstation  9-1

 




         NPAGEDYN=330000       !Size of the non-paged dynamic pool in
    			       !  bytes
	 PAGFILCNT=1           !1 page file; the maximum number of
			       !  page files that can be installed
	 PAGEFILE=30000        !Size of a page file in bytes
	 PAGEDYN=4000000       !Size of the paged dynamic pool in bytes
	 PHYSICALPAGES=18432   !9 megabytes of physical memory
	 SWPFILCNT=1           !1 swap file; the maximum number of
                               !  swapping that can be installed
	 SWAPFILE=8000         !Size of a swap file in pages
         WSMAX=12000           !Maximum working set size
         WSINC=350             !Amount by which the working set of a
			       !  process is increased by AWSA
                               !  (Automatic Working Set Adjustment)
	 WSDEC=0               !Amount by which the working set of a
                               !  process is decreased by AWSA
	 VIRTUALPAGECNT=30000  !Maximum amount of virtual pages
         		       !  a process can map

                  The following three values are recommended for a VAXstation
                  II/GPX:

	 CTLPAGES=850          !Used with workstation windows
         SPTREQ=2300           !Required number of system page table
    			       !  entries
	 NPAGEDYN=450000       !Size of the non-paged dynamic pool in
                               !  bytes

                                               NOTE

                      These values are recommended only for a 9-megabyte
                      system and should not be used on systems with less
                      than 9 megabytes of memory. Using these values on
                      systems with less than 9 megabytes could prevent your
                      workstation from booting.

                      The values are valid only for a system that can be
                      characterized as a single-use system running primarily
                      VAX LISP. Although running only VAX LISP is not a
                      requirement, these values tune the system to run VAX
                      LISP efficiently and may have an adverse effect on
                      systems that heavily use other products concurrently
                      with VAX LISP.

                      Therefore, you should review the requirements of other
                      products and evaluate these recommended values in that
                      context.

                  To adjust your system's parameter values:

                   1. Add the preceding values to the file
		      SYS$SYSTEM:MODPARAMS.DAT






               9-2  Tuning the VAXstation








                   2. Reconfigure your system, using the AUTOGEN Utility by
                      executing the command:

                       @SYS$UPDATE:AUTOGEN SAVPARAMS REBOOT

                  For details on using the AUTOGEN Utility, see your processor-
                  specific installation/operations guide.

                  Since these parameters are not dynamic, your system will need
                  to be rebooted. AUTOGEN will perform an automatic shutdown
                  and reboot when it has finished.

               _________________________________________________________________

               9.2  Recommended Authorization Quotas

                  The following are recommended authorization quotas for VAX
                  LISP accounts on a VAXstation:

	 	    WSDEFAULT:       1024      ! Default working set size
                    WSQUOTA:         8000      ! Limit for the amount of
                                               !   physical memory a user
                                               !   process may lock into its
					       !   working set
                    WSEXTENT:       18000      ! Absolute limit on physical
                                               !   memory the system allows the
                                               !   process
                    PGFLQUOTA:      30000      ! Maximum number of pages a
                                               !   user's process can use in
                                               !   the system paging file

                  To adjust these quotas, invoke the Authorize Utility, as
                  shown in Section 1.4.























                                                     Tuning the VAXstation  9-3

 










                                                                     Chapter 10


                                             Determining and Reporting Problems
               ________________________________________________________________


                  If an error occurs while you are using VAX LISP and you
                  believe that the error is caused by a problem with VAX LISP,
                  take one of the following actions:

                   o If you purchased VAX LISP within the past 90 days and you
                     think the problem is caused by a software error, you can
                     submit a Software Performance Report (SPR).

                   o If you have a Basic or DECsupport Software Agreement,
                     you should call your Customer Support Center. With these
                     services, you receive telephone support that provides
                     high-level advisory and remedial assistance. For more
                     information, contact your local Digital representative.

                   o If you have a Self-Maintenance Software Agreement, you can
                     submit an SPR.

                  If you find an error in the VAX LISP documentation, you
                  should fill out and submit a Reader's Comments form from the
                  back of the document in which the error was found. Include
                  the section and page number where the error was found.
























                                       Determining and Reporting Problems  10-1

 










                                                                     Chapter 11


                                                            Sample Installation
               ________________________________________________________________


                  This section contains a sample installation of VAX LISP.
                  Note that this is only a sample. Sometimes the installation
                  procedure is modified in maintenance updates of this prod-
                  uct. Because this installation guide is not usually revised
                  for maintenance updates, be sure to read the Read Before
                  Installing or Using VAX LISP letter before you install this
                  product. This letter notes any significant changes in the
                  installation that vary from this sample.

           Welcome to VAX/VMS V5.3

          Username: SYSTEM
          Password:
           Welcome to VAX/VMS version V5.3 on node HBA
              Last interactive login on Wednesday, 07-FEB-1990 17:59
              Last non-interactive login on Wednesday, 07-FEB-1990 17:59
          SYSTEM> @SYS$UPDATE:VMSINSTAL LISP MUA0
           VAX/VMS Software Product Installation Procedure V5.3
           It is 07-FEB-1990 at 18:02.
          Enter a question mark (?) at any time for help.
          * Are you satisfied with the backup of your system disk [YES]?

          The following products will be processed:
            LISP V3.1
           Beginning installation of LISP V3.1 at 18:13

          %VMSINSTAL-I-RESTORE, Restoring product saveset A ...
          %VMSINSTAL-I-RELMOVED , The product's release notes have been
          successfully moved to SYS$HELP.
          * Do you want to purge files replaced by this installation [YES]? no
                  Product:      LISP
                  Producer:     DEC
                  Version:      3.1
                  Release Date: 23-MAR-1990
          * Does this product have an authorization key registered and loaded?
           yes

          The LISP installation kit contains the VAX LISP product files
          (i.e., the files which are needed to run VAX LISP), some example
          files, and some special library files for building customized





                                                      Sample Installation  11-1








          LISP systems.  It is possible to install just VAX LISP, and
          nothing else.  It is also possible to install just the examples,
          or just the library files, or any combination of these.

          Enter YES to this question if you wish to install VAX LISP at
          this time.  Enter NO to this question if you only wish to install
          the examples and/or library files at this time.

          * Do you wish to install the VAX LISP product files (20000 blocks)
          [YES]?

          VAX LISP can be installed with built-in code either for
          DECwindows or for the UIS windowing system.  (The choice of
          windowing system for the installed VAX LISP product does not
          limit the choice of windowing system for custom-built VAX LISP
          systems.)  You should select the windowing system which is
          preferred at your site.

          Answer YES to this question to select DECwindows as your
          windowing system.  Answer NO to this question to select UIS as
          your windowing system.

          * Do you want the DECwindows version of VAX LISP [YES]?
          * In which directory are the VAX LISP product files to be installed
          [SYS$COMMON:[VAXLISP]]:) mua0:[vaxlisp]

          * Do you wish to install the VAX LISP system-building library files
          (22500 blocks) [NO]?  yes
          * In which directory are the VAX LISP system-building library files
          to be installed [MUA0:[VAXLISP.LIBRARY]]:
          * Directory MUA0:[VAXLISP.LIBRARY] does not exist.  Should it be
          created [YES]?

          The installation kit contains some unsupported example Lisp
          files, which contain some useful VAX LISP utilities, and which
          additionally serve as examples of LISP programming style.  They
          are not required in order to run VAX LISP.

          Additional unsupported utilities and examples are included in separate
          savesets.  These include PCL, RdbLISP, Foxglove, GKS, and GKS3D
          bindings, VAXFlavors, and Starlet routines.

          You can install all the examples or just some of them.  You will be
          asked separately which ones you wish to install.  Enter YES to the
          questions for those examples you wish to install and NO for those you
          wish to skip at this time.
          * Do you wish to install the VAX LISP examples (4400 blocks)
          [NO]? yes
          In which directory are the VAX LISP examples to be installed
          [MUA0:[VAXLISP.EXAMPLE]]:
          * Directory MUA0:[VAXLISP.EXAMPLES] does not exist.  Should it be
          created [YES]?




               11-2  Sample Installation

 






          Included in the examples are the 05/23/89 (Victoria Day) version of
          Portable Common Loops (PCL), the publicly-available implementation of
          the Common Lisp Object System (CLOS).  PCL is normally installed in
          its own sub-directory.

          Do you wish to install the PCL examples (4400 blocks) [NO]? yes
          * In which directory are the PCL examples to be installed
          [MUA0:[VAXLISP.EXAMPLES.PCL]]:
          * Directory MUA0:[VAXLISP.EXAMPLES.PCL] does not exist. Should it be
          created [YES]?


          * The RdbLISP software provides an interface layer between Digital's
          relational database (Rdb) and VAX LISP/VMS.

          * Do you wish to install the RdbLISP examples (2100 blocks) [NO]?
          yes
          In which directory are the RdbLISP examples to be installed
          [MUA0:[VAXLISP.EXAMPLES.RDBLISP]]:
          * Directory MUA0:[VAXLISP.EXAMPLES.RDBLISP] does not exist.  Should
          it be created [YES]?

          Foxglove is a rapid-prototyping language for developing rule-based
          expert system applications.

          * Do you wish to install the Foxglove examples (26400 blocks) [NO]?
          yes
          In which directory are the Foxglove examples to be installed
          [MUA0:[VAXLISP.EXAMPLES.FOXGLOVE]]:
          * Directory [MUA0:[VAXLISP.EXAMPLES.FOXGLOVE] does not exist. Should
          it be created [YES]?

          Both GKS and GKS3D LISP bindings are included in this saveset.
          * Do you wish to install the GKS and GKS3D bindings (4400 blocks)
          [NO]? yes
          In which directory are the GKS and GKS3D bindings to be installed
          [MUA0:VAXLISP.EXAMPLES.GKS]]:
          * Directory MUA0:[VAXLISP.EXAMPLES.GKS] does not exist.  Should it be
          created [YES]?

          VAXFlavors is an implementation of Flavors under VAX LISP.  It
          implements an object-oriented programming system under Common LISP.
          * Do you wish to install the VAXFlavors examples (2000 blocks) [NO]?
           yes
          *In which directory are the VAXFlavors examples to be installed
          [MUA0:[VAXLISP.EXAMPLES.VAXFLAVORS]]:
          * Directory MUA0:[VAXLISP.EXAMPLES.VAXFLAVORS] does not exist.  Should
          it be created [YES]?

          The VAX LISP interface to VMS Starlet routines are included in this
          saveset.
          * Do you wish to install the Starlet examples (16000 blocks) [NO]?
          yes
          In which directory are the Starlet examples to be installed
          [MUA0:[VAXLISP.EXAMPLES.STARLET]]:

                                                      Sample Installation  11-3

 






      * Directory MUA0:[VAXLISP.EXAMPLES.STARLET] does not exist.  Should it be
      created [YES]?
      HBA::_RTA1: 00:15:52   (DCL) CPU=00:02:23.53 PF=7892 IO=1542 MEM=312
      * Do you want to run the IVP after the installation [YES]?
      %LISP-I-QUESDONE, There are no more installation questions to be answered
      %VMSINSTAL-I-RESTORE, Restoring product saveset B ...
      %VMSINSTAL-I-RESTORE, Restoring product saveset D ...
      %VMSINSTAL-I-RESTORE, Restoring product saveset E ...
      HBA::_RTA1: 00:41:59   (DCL) CPU=00:09:29.81 PF=48883 IO=13819 MEM=337
      %VMSINSTAL-I-RESTORE, Restoring product saveset F ...
      %VMSINSTAL-I-RESTORE, Restoring product saveset G ...
      HBA::_RTA1: 01:26:02   (DCL) CUP=00:34:26.96 PF=263302 IO=39961 MEM=303
      %VMSINSTAL-I-RESTORE, Restoring product saveset H ...
      %VMSINSTAL-I-RESTORE, Restoring product saveset I ...
      %VMSINSTAL-I-RESTORE, Restoring product saveset J ...
      %VMSINSTAL-I-RESTORE, Restoring product saveset K ...
      Executing VAX LISP startup procedure...

              VAX LISP Installation Verification Procedure (IVP)

      Starting compilation of file
      MUA0:[SYS0.SYSUPD.LISP031]LISPIVP.LSP;1

      FIBONACCI compiled.
      PRINT-FIBONACCI-TABLE  compiled.
      Finished compilation of file MUA0:[SYS0.SYSUPD.LISP031]LISPIVP.LSP;1

      0 Errors, 0 Warnings

      VAX LISP [TM], version V3.1

      © Digital Equipment Corporation. 1989, 1990.
      All Rights Reserved.























               11-4  Sample Installation

 




          A table of the first 20 Fibonacci numbers:

          n   Fibonacci(n)

          --   ------------

          0        0
          1        1
          2        1
          3        2
          4        3
          5        5
          6        8
          7        13
          8        21
          9        34
          10       55
          11       89
          12       144
          13       233
          14       377
          15       610
          16       987
          17       1,597
          18       2,584
          19       4,181

                  VAX LISP V3.1 IVP Completed Successfully

           Installation of LISP V3.1 completed at 18:51

           VMSINSTAL procedure done at 15:54
          SYSTEM> dir sys$startup:lispstart.com

          Directory SYS$STARTUP:[SYSMGR]

          LISPSTART.COM;2

          Total of 1 file.
          SYSTEM> lo
            SYSTEM       logged out at 07-FEB-1990 18:56:42.19
 
















                                                      Sample Installation  11-5

 










                                                                     Appendix A


                                                      Files Added to the System
               ________________________________________________________________


                  As a result of the installation procedure, several files are
                  added to your system.

               _________________________________________________________________

               A.1  LISP$SYSTEM: Directory

                   o EXAMPLES.DIR
                   o LIBRARY.DIR
                   o LISP$DECWINDOWS-V1.UID
                   o LISP$DECWINDOWS-V2.UID
                   o LISP$DECWINDOWS.HLB
                   o LISP$DECWINDOWS.UID
                   o LISP.CLD
                   o LISP.EXE
                   o LISPDOC.TLB
                   o SYS$TEST:LISP$IVP.COM

               _________________________________________________________________

               A.2  LISP$EXAMPLES: Directory

                   o ANIMATE.FAS
                   o ANIMATE.LSP
                   o BLACKBOARD.FAS
                   o BLACKBOARD.LSP
                   o CHAOS.FAS
                   o CHAOS.LSP
                   o CLX-COLORMAP-EXAMPLE.FAS
                   o CLX-COLORMAP-EXAMPLE.LSP
                   o CLX-EXAMPLES.FAS
                   o CLX-EXAMPLES.LSP
                   o CLX-HELLOJUNK.FAS
                   o CLX-HELLOJUNK.LSP
                   o CLX-HELLOWORLD.FAS
                   o CLX-HELLOWORLD.LSP
                   o CLX-PUBLIC.FAS
                   o CLX-PUBLIC.LSP
                   o COLOR-IMAGE-ARRAYS.FAS
                   o COLOR-IMAGE-ARRAYS.LSP





                                                 Files Added to the System  A-1

 






                   o COLOR-SYMBOLS.FAS
                   o COLOR-SYMBOLS.LSP
                   o CURSORFONT.FAS
                   o CURSORFONT.LSP
                   o CURSORS.FAS
                   o CURSORS.LSP
                   o DECBURGER.FAS
                   o DECBURGER.LSP
                   o DECW$CURSOR.FAS
                   o DECW$CURSOR.LSP
                   o DECW-CALLBACK-STRUCTURES.FAS
                   o DECW-CALLBACK-STRUCTURES.LSP
                   o DECW-PUBLIC.FAS
                   o DECW-PUBLIC.LSP
                   o DECW-README.TXT
                   o DISPLAY-BITMAP.FAS
                   o DISPLAY-BITMAP.LSP
                   o DRAGON.FAS
                   o DRAGON.LSP
                   o DWTAPPL.FAS
                   o DWTAPPL.LSP
                   o EDINIT.FAS
                   o EDINIT.LSP
                   o FAS-HEADER.COM
                   o FOXGLOVE.DIR
                   o GKS.DIR
                   o GRAPH.FAS
                   o GRAPH.LSP
                   o HELLOWORLD.COM
                   o HELLOWORLD.FAS
                   o HELLOWORLD.LSP
                   o HELLOWORLD.UID
                   o HELLOWORLD.UIL
                   o ISAM-DEMO.FAS
                   o ISAM-DEMO.LSP
                   o ISAM-RMSBLOCKS.FAS
                   o ISAM-RMSBLOCKS.LSP
                   o ISAM-RMSUTIL.FAS
                   o ISAM-RMSUTIL.LSP
                   o ISAM-RUN-DEMO.COM
                   o ISAM-STARLET.FAS
                   o ISAM-STARLET.LSP
                   o ISAM-TEST.FDL
                   o ISAM.FAS
                   o ISAM.LSP
                   o LK201.FAS
                   o LK201.LSP
                   o MENU.FAS
                   o MENU.LSP
                   o PARSE-DISPLAY.FAS
                   o PARSE-DISPLAY.LSP
                   o PROFILE.FAS
                   o PROFILE.LSP



               A-2  Files Added to the System

 






                   o PSEUDOSCHEME.FAS
                   o PSEUDOSCHEME.LSP
                   o RADAR.FAS
                   o RADAR.LSP
                   o REBOUND.FAS
                   o REBOUND.LSP
                   o RECIPE.COM
                   o RECIPE.FAS
                   o RECIPE.LSP
                   o RECIPE_RUN.LSP
                   o RECIPE.UID
                   o RECIPE.UIL
                   o SET-BACKGROUND.FAS
                   o SET-BACKGROUND.LSP
                   o SIEVE.FAS
                   o SIEVE.LSP
                   o STARLET.DIR
                   o VAXFLAVORS.DIR
                   o WATCH.FAS
                   o WATCH.LSP
                   o XREF.FAS
                   o XREF.LSP
                   o XREFANALYZERS.FAS
                   o XREFANALYZERS.LSP
                   o XREFBUILD.FAS
                   o XREFBUILD.LSP
                   o XREFCATALOG.FAS
                   o XREFCATALOG.LSP
                   o XREFCROSSREF.FAS
                   o XREFCROSSREF.LSP
                   o XREFDUMPER.FAS
                   o XREFDUMPER.LSP
                   o XREFEXAMPLE.FAS
                   o XREFEXAMPLE.LSP
                   o XREFGRAPH.FAS
                   o XREFGRAPH.LSP
                   o XREFQUERY.FAS
                   o XREFQUERY.LSP
                   o XREFRELATIONS.FAS
                   o XREFRELATIONS.LSP
                   o XREFREPORT.FAS
                   o XREFREPORT.LSP
                   o XREFSYSTEM.FAS
                   o XREFSYSTEM.LSP
                   o XREFTOOLS.FAS
                   o XREFTOOLS.LSP
                   o XREFUSERGUIDE.MEM
                   o XREF_READ_ME_1ST.TXT
                   o XREF_READ_ME_VU_1ST.TXT







                                                 Files Added to the System  A-3

 






               _________________________________________________________________

               A.3  LISP$GKS: Directory

                   o GKS3D.FAS
                   o GKS3D.LSP
                   o GKSDEFS.FAS
                   o GKSDEFS.LSP

               _________________________________________________________________

               A.4  LISP$LIBRARY: Directory

                   o LISP$FASLIB.TLB
                   o LISP$OBJLIB.OLB
                   o LISP$BUILD-VAXLISP.CLD
                   o LISP$BUILD-VAXLISP.EXE

               _________________________________________________________________

               A.5  LISP$PCL: Directory

                   o 3-17-88-NOTES.TXT
                   o 3-19-87-NOTES.TXT
                   o 4-21-87-NOTES.TXT
                   o 4-29-87-NOTES.TXT
                   o 5-22-87-NOTES.TXT
                   o 8-28-88-NOTES.TXT
                   o BOOT.FAS
                   o BOOT.LSP
                   o BRAID1.FAS
                   o BRAID1.LSP
                   o COMBIN-TEST.LSP
                   o COMBIN.FAS
                   o COMBIN.LSP
                   o COMPAT.FAS
                   o COMPAT.LSP
                   o COMPILE-PCL.LOG
                   o CONSTRUCT.FAS
                   o CONSTRUCT.LSP
                   o DCODE-PRE1.FAS
                   o DCODE-PRE1.LSP
                   o DCODE-PRE2.FAS
                   o DCODE-PRE2.LSP
                   o DCODE-PRE3.FAS
                   o DCODE-PRE3.LSP
                   o DCODE-PRE4.FAS
                   o DCODE-PRE4.LSP
                   o DCODE.FAS
                   o DCODE.LSP
                   o DEFCLASS.FAS
                   o DEFCLASS.LSP




               A-4  Files Added to the System








                   o DEFS.FAS
                   o DEFS.LSP
                   o DEFSYS.LSP
                   o ENV.FAS
                   o ENV.LSP
                   o FIN-V2.LSP
                   o FIN.FAS
                   o FIN.LSP
                   o FIXUP.FAS
                   o FIXUP.LSP
                   o FSC.FAS
                   o FSC.LSP
                   o GET-PCL.TXT
                   o HIGH.FAS
                   o HIGH.LSP
                   o INIT.FAS
                   o INIT.LSP
                   o ITERATE.FAS
                   o ITERATE.LSP
                   o LAP.LSP
                   o LOW.FAS
                   o LOW.LSP
                   o MACROS.FAS
                   o MACROS.LSP
                   o METHODS.FAS
                   o METHODS.LSP
                   o MKI.FAS
                   o MKI.LSP
                   o NOTES.TXT
                   o PCL-ENV.LSP
                   o PKG.FAS
                   o PKG.LSP
                   o POINTS.FAS
                   o POINTS.LSP
                   o PRECOM1.FAS
                   o PRECOM1.LSP
                   o PRECOM2.FAS
                   o PRECOM2.LSP
                   o PRECOM3.FAS
                   o PRECOM3.LSP
                   o PRECOM4.LSP
                   o PRECOM4.FAS
                   o README.TXT
                   o REL-7-2-PATCHES.LSP
                   o SLOTS.FAS
                   o SLOTS.LSP
                   o STD-CLASS.FAS
                   o STD-CLASS.LSP
                   o TEST.FAS
                   o TEST.LSP
                   o VAXL-LOW-V2.LSP
                   o VAXL-LOW.FAS
                   o VAXL-LOW.LSP



                                                 Files Added to the System  A-5

 






                   o VECTOR.FAS
                   o VECTOR.LSP
                   o WALK-V2.LSP
                   o WALK.FAS
                   o WALK.LSP

               _________________________________________________________________

               A.6  LISP$STARLET: Directory

                   o BASMSG.FAS
                   o BASMSG.LSP
                   o COBMSG.FAS
                   o COBMSG.LSP
                   o CRF.FAS
                   o CRF.LSP
                   o CRFERRMSG.FAS
                   o CRFERRMSG.LSP
                   o DSTDEF.FAS
                   o DSTDEF.LSP
                   o DTK$ROUTINES.FAS
                   o DTK$ROUTINES.LSP
                   o DTKDEF.FAS
                   o DTKDEF.LSP
                   o DTKMSG.FAS
                   o DTKMSG.LSP
                   o FORMSG.FAS
                   o FORMSG.LSP
                   o JBCMSG.FAS
                   o JBCMSG.LSP
                   o LATMSG.FAS
                   o LATMSG.LSP
                   o LBRUSR.FAS
                   o LBRUSR.LSP
                   o LIB$ROUTINES.FAS
                   o LIB$ROUTINES.LSP
                   o LIBCLIDEF.FAS
                   o LIBCLIDEF.LSP
                   o LIBCQDEF.FAS
                   o LIBCQDEF.LSP
                   o LIBDCFDEF.FAS
                   o LIBDCFDEF.LSP
                   o LIBDTDEF.FAS
                   o LIBDTDEF.LSP
                   o LIBMSG.FAS
                   o LIBMSG.LSP
                   o LIBVMDEF.FAS
                   o LIBVMDEF.LSP
                   o MTH$ROUTINES.FAS
                   o MTH$ROUTINES.LSP
                   o MTHMSG.FAS
                   o MTHMSG.LSP




               A-6  Files Added to the System

 






                   o NCS$ROUTINES.FAS
                   o NCS$ROUTINES.LSP
                   o NCSMSG.FAS
                   o NCSMSG.LSP
                   o OBJFMT.FAS
                   o OBJFMT.LSP
                   o OPCDEF.FAS
                   o OPCDEF.LSP
                   o OPCMSG.FAS
                   o OPCMSG.LSP
                   o OPDEF.FAS
                   o OPDEF.LSP
                   o OTS$ROUTINES.FAS
                   o OTS$ROUTINES.LSP
                   o OTSMSG.FAS
                   o OTSMSG.LSP
                   o PPL$DEF.FAS
                   o PPL$DEF.LSP
                   o PPL$ROUTINES.FAS
                   o PPL$ROUTINES.LSP
                   o PPLMSG.FAS
                   o PPLMSG.LSP
                   o PSMMSG.FAS
                   o PSMMSG.LSP
                   o RMSDEF.FAS
                   o RMSDEF.LSP
                   o RMSFALMSG.FAS
                   o RMSFALMSG.LSP
                   o RMSUSR.LSP
                   o SCRDEF.FAS
                   o SCRDEF.LSP
                   o SHRMSG.FAS
                   o SHRMSG.LSP
                   o SMBMSG.FAS
                   o SMBMSG.LSP
                   o SMG$ROUTINES.FAS
                   o SMG$ROUTINES.LSP
                   o SMGDEF.FAS
                   o SMGDEF.LSP
                   o SMGMSG.FAS
                   o SMGMSG.LSP
                   o SMGTRMPTR.FAS
                   o SMGTRMPTR.LSP
                   o SOR$ROUTINES.FAS
                   o SOR$ROUTINES.LSP
                   o SORMSG.FAS
                   o SORMSG.LSP
                   o SRMDEF.FAS
                   o SRMDEF.LSP
                   o SSMSG.FAS
                   o SSMSG.LSP
                   o STARDEFAE.FAS
                   o STARDEFAE.LSP



                                                 Files Added to the System  A-7

 






                   o STARDEFFL.FAS
                   o STARDEFFL.LSP
                   o STARDEFMP.FAS
                   o STARDEFMP.LSP
                   o STARDEFQZ.FAS
                   o STARDEFQZ.LSP
                   o STARLET.FAS
                   o STARLET.LSP
                   o STR$ROUTINES.FAS
                   o STR$ROUTINES.LSP
                   o STRMSG.FAS
                   o STRMSG.LSP

               _________________________________________________________________

               A.7  LISP$VAXFLAVORS: Directory

                   o FLAVORS.FAS
                   o FLAVORS.LSP
                   o FLVBUILD.FAS
                   o FLVBUILD.LSP
                   o FLVCOMPILE.FAS
                   o FLVCOMPILE.LSP
                   o FLVDEFFLAVOR.FAS
                   o FLVDEFFLAVOR.LSP
                   o FLVDEFMETHOD.FAS
                   o FLVDEFMETHOD.LSP
                   o FLVDESCRIBE.FAS
                   o FLVDESCRIBE.LSP
                   o FLVINIT.FAS
                   o FLVINIT.LSP
                   o FLVMAKE.FAS
                   o FLVMAKE.LSP
                   o FLVSEND.FAS
                   o FLVSEND.LSP
                   o FLVTRACE.FAS
                   o FLVTRACE.LSP
                   o FLVVANILLA.FAS
                   o FLVVANILLA.LSP
                   o VAXFLAVORS_UG.LN3

               _________________________________________________________________

               A.8  RDBLISP$EXAMPLES: Directory

                   o BUILD-RDBLISP.COM
                   o DB-HANDLE.LSP
                   o DEMO-DATE.LSP
                   o DEMO-RDBKEY.LSP
                   o DEMO-RESUME.TXT
                   o DEMO-SEGMENTED-STRING.LSP
                   o DEMO.LSP
                   o DSRI.FAS



               A-8  Files Added to the System

 






                   o RDBBLR.FAS
                   o RDBBLR.LSP
                   o RDBCONSTANTS.FAS
                   o RDBCONSTANTS.LSP
                   o RDBDDL.FAS
                   o RDBDDL.LSP
                   o RDBDML.FAS
                   o RDBDML.LSP
                   o RDBERRORS.FAS
                   o RDBERRORS.LSP
                   o RDBLISP-COMPILE.COM
                   o RDBLISP-LOAD.LSP
                   o RDBLISP-V11-RN.DVI
                   o RDBLISP-V11-RN.MEM
                   o RDBLISP-V11-RN.TEX
                   o RDBLISP-V11.DVI
                   o RDBLISP-V11.MEM
                   o RDBLISP-V11.TEX
                   o RDBLISP.MMS
                   o RDBLISP_EXAMPLES.LSP
                   o RDBLOAD.LSP
                   o RDBMETA.FAS
                   o RDBMETA.LSP
                   o RDBSUBS.FAS
                   o RDBSUBS.LSP
                   o RDBUTILITIES.FAS
                   o RDBUTILITIES.LSP
                   o RDBVARIABLES.FAS
                   o RDBVARIABLES.LSP

               _________________________________________________________________

               A.9  FOXGLOVE$SYSTEM: Directory

                   o APPLICATION.UID
                   o APPLICATION_V2.UID
                   o CAR.FOX
                   o FACTORIAL.FOX
                   o FOXGLOVE.CLD
                   o FOXGLOVE.EXE
                   o FOXGLOVE.FAS
                   o FOXGLOVE.UID
                   o FOXGLOVE_V2.UID
                   o FOXGLOVE.HLP
                   o 1READ.ME
                   o REFERENCE_MANUAL.LN03
                   o REFERENCE_MANUAL.POST
                   o REFERENCE_MANUAL.TXT
                   o TUTORIAL_LESSON_3.FOX
                   o TUTORIAL_LESSION_4.FOX
                   o USERS_GUIDE.LN03
                   o USERS_GUIDE.POST
                   o USERS_GUIDE.TXT
                   o WINES.FOX


                                                 Files Added to the System  A-9

 






               _________________________________________________________________

               A.10  SYS$STARTUP: Directory

                   o LISP$EXAMPLES_STARTUP.COM
                   o LISP$FOXGLOVE_STARTUP.COM
                   o LISP$GKS_STARTUP.COM
                   o LISP$LIBRARY_STARTUP.COM
                   o LISP$PCL_STARTUP.COM
                   o LISP$RDBLISP_STARTUP.COM
                   o LISP$SITE.COM
                   o LISP$STARLET_STARTUP.COM
                   o LISP$STARTUP.COM
                   o LISP$UIS_STARTUP.COM
                   o LISP$VAXFLAVORS_STARTUP.COM









































               A-10  Files Added to the System
