 






           System
           Support
           Addendum

           _________________________________________________________
           _________________________________________________________

           PRODUCT NAME:  VAX Rdb/VMS, Version 4.0    SSA 25.59.12-A
                          Relational Database Manage-
                          ment System

           HARDWARE REQUIREMENTS

           Processors Supported

           VAX:     VAX 9000 Model 400 Series
                    VAX 9000 Model 210
                    VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series,
                    VAX 4000 Model 300 Series,
                    VAXft 3000 Model 310

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840, VAX 8842,
                    VAX 8974, VAX 8978

                    VAX-11/730, VAX-11/750, VAX-11/780,
                    VAX-11/785

           MicroVAX:MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,
                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900



                                    DIGITAL                June 1991

                                                         AE-LT08H-TE

 



           VAX Rdb/VMS, Version 4.0                  SSA 25.59.12-A
           Relational Database Management System


           VAXstatioVAXstation II, VAXstation 2000,
                    VAXstation 3100, VAXstation 3200,
                    VAXstation 3500, VAXstation 3520,
                    VAXstation 3540

           VAXserverVAXserver 3100, VAXserver 3300,
                    VAXserver 3400, VAXserver 3500,
                    VAXserver 3600, VAXserver 3602,
                    VAXserver 3800, VAXserver 3900

                    VAXserver 6000-210, VAXserver 6000-310,
                    VAXserver 6000-410, VAXserver 6000-420

           Processors Not Supported

           VAX-11/725, VAX-11/782, MicroVAX I, VAXstation I, VAXsta-
           tion 8000

           Processor Restrictions

           o  All processors require mass storage units to backup and
              restore established databases.

           o  All processors require a specified minimum memory (Re-
              fer to Chart I).

           o  All processors require a device for installation of the
              software (see chart below). (Magnetic tape = One 9-track
              1600 BPI magnetic tape)

           o  Certain processors have other requirements (Refer to Chart
              I).

           Block Space Requirements (Block Cluster Size = 1):

           Disk space required for installation of VAX Rdb/VMS:




                                       2

 



           VAX Rdb/VMS, Version 4.0                  SSA 25.59.12-A
           Relational Database Management System


           Development Option:         45,000 blocks
                                       (22M bytes)

           Interactive Option:         28,000 blocks
                                       (14M bytes)

           Run-Time Only Option:       25,000 blocks
                                       (12M bytes)

           Disk space required for use (permanent):


           Development Option:         40,000 blocks
                                       (20M bytes)

           Interactive Option:         24,000 blocks
                                       (12M bytes)

           Run-Time Only Option:       20,000 blocks
                                       (10M bytes)

           These counts refer to the disk space required on the sys-
           tem disk. The sizes are approximate; actual sizes may vary
           depending on the user's system environment, configuration,
           and software options.















                                       3

 



           VAX Rdb/VMS, Version 4.0                  SSA 25.59.12-A
           Relational Database Management System

           OPTIONAL HARDWARE

           For SQL/Services MS-DOS® or OS/2[TM] platform:

           o  Personal Computer XT®, Personal Computer AT® or equiv-
              alent

           For SQL/Services Macintosh[TM] platform:

           o  Macintosh Plus, Macintosh SE and SE/30, Macintosh II, IIx,
              IIcx, IIci, and IIfx, Macintosh portable

           CLUSTER ENVIRONMENT

           This layered product is fully supported when installed on
           any valid and licensed VAXcluster* configuration without re-
           strictions. The HARDWARE REQUIREMENTS sections of this prod-
           uct's Software Product Description and System Support Ad-
           dendum detail any special hardware required by this prod-
           uct.

           *  V5.x VAXcluster configurations are fully described in the
              VAXcluster Software Product Description (29.78.xx) and
              include CI, Ethernet and Mixed Interconnect configura-
              tions.

           SOFTWARE REQUIREMENTS

           VMS Operating System V5.3 - V5.4

           Note: VMS Operating System V5.4 with DECdtm component in-
           stalled (required for Two Phase Commit support)

           VMS Workstation Software V4.2 (Workstations Only)

           For all SQL/Services platforms:

           DECnet-VAX V5.3 - V5.4

           For SQL/Services ULTRIX platform:

           ULTRIX Operating System V2.2 - V4.0

                                       4

 



           VAX Rdb/VMS, Version 4.0                  SSA 25.59.12-A
           Relational Database Management System

           DECnet-ULTRIX V2.2 - V4.0

           For SQL/Services MS-DOS platform:

           MS-DOS
           Operating System V3.1 - V3.3

           DECnet PCSA Client for DOS V3.0

           C Run-Time Library compatible with Microsoft C V5.0

           For SQL/Services OS/2 platform:

           OS/2 Operating System V1.0

           PCSA for OS/2 V1.0

           C Run-Time Library compatible with Microsoft C V5.0

           For SQL/Services Macintosh platform:

           o  Macintosh Operating System 6.0.5

           o  AppleShare Workstation Software for System 6.0.5

           o  Apple's ADSP driver Version 1.0.2

           o  MPW 3.1 and the MPW 3.1 C compiler

           o  Apple's Communication Toolbox 1.0

           o  Digital's Macintosh Integration Product

           VMS Tailoring

           For VMS V5.x, the following VMS classes are required for full
           functionality of this layered product:

           o  VMS Required Saveset

           o  Network Support

           o  Programming Support

           o  Secure User's Environment

                                       5

 



           VAX Rdb/VMS, Version 4.0                  SSA 25.59.12-A
           Relational Database Management System

           o  Utilities

           For more information on VMS classes and tailoring, refer to
           the VMS Operating System Software Product Description (SPD
           25.01.xx).

           OPTIONAL SOFTWARE

           Certain versions of these products depend upon a specific
           version of the Operating System. Please see the System Soft-
           ware Addendum of the product in question to determine which
           version you need.

           VAX ACMS V3.1
           VAX Ada V2.1
           VAX BASIC V3.4
           VAX BLISS-32 Implementation Language V4.6
           VAX C V3.1
           VAX COBOL V4.3
           VAX COBOL Generator V1.3
           VAX CDD/Plus V4.2
           VAX Data Distributor V2.2
           VAX DATATRIEVE V5.0
           VAX DIBOL V4.1
           VAX FORTRAN V5.5
           VAX PASCAL V4.1
           VAX PL/I V3.3
           VAX RALLY V2.1
           VAX RPG II V2.1
           VAX TEAMDATA V1.4
           VIDA with DB2[TM] V1.0










                                       6

 



           VAX Rdb/VMS, Version 4.0                  SSA 25.59.12-A
           Relational Database Management System

           GROWTH CONSIDERATIONS


           The minimum hardware/software requirements for any future
           version of this product may be different from the require-
           ments for the current version.

           DISTRIBUTION MEDIA

           Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

           This product is also available as part of the VMS Consol-
           idated Software Distribution on CDROM.

           ORDERING INFORMATION

           VAX Rdb/VMS Full Development Option (VD2)

           Software Licenses: QL-VD2A*-**
           Software Media: QA-VD2A*-**
           Software Documentation: QA-VD2AA-GZ
           Software Product Services: QT-VD2A*-**

           VAX Rdb/VMS Interactive Option (VCL)

           Software Licenses: QL-VCLA*-**
           Software Media: QA-VCLA*-**
           Software Documentation: QA-VCLAA-GZ
           Software Product Services: QT-VCLA*-**

           VAX Rdb/VMS Run-Time Option

           Note: The license for the Run-Time option is included with
           VMS).

           Software Media: QA-358A*-**
           Software Documentation: QA-358AA-GZ
           Software Product Services: QT-358A*-**



                                       7

 



           VAX Rdb/VMS, Version 4.0                  SSA 25.59.12-A
           Relational Database Management System

           *  Denotes variant fields. For additional information on li-
              censes, services and media, refer to the appropriate price
              book.

           The above information is valid at time of release. Please
           contact your local Digital office for the most up-to-date
           information.


                                                  Chart I
           _________________________________________________________
                                          Minimum         Installation         Other Require-
           _______________________________(megabytes)_____Device____           ments


           For VAX-11/730 Systems:        3               Magnetic Tape        -

           For VAX-11/750 Systems:        4               Magnetic Tape        ECO level 3 or
                                                                               later

           For VAX-11/780 or VAX-11       4               Magnetic Tape        ECO level 4 or
           /785:                                                               later (VAX-11
                                                                               /780) WCS mi-
                                                                               crocode version
                                                                               123 or later

           For VAX 82xx Systems:          4               Magnetic Tape        -

           For VAX 83xx Systems:          4               Magnetic Tape        -

           For VAX 8974 and VAX 8978      4 (per pro-     Magnetic Tape        -
           Systems:                       cessor)

           All other supported VAX        4               Magnetic Tape or     -
           Systems:_______________________________________TK50_tape_drive

           ®    MS-DOS and Microsoft are registered trademarks of
                Microsoft Corporation.

           [TM] OS/2 and DB2 are trademarks of International Busi-
                ness Machines Corporation.

                                       8

 



           VAX Rdb/VMS, Version 4.0                  SSA 25.59.12-A
           Relational Database Management System


           ®    XT and AT are registered trademarks of International
                Business Machines Corporation.

           [TM] Macintosh, MPW, Apple and Appleshare are trademarks
                of Apple Computer, Inc.

           [TM] The DIGITAL Logo, VAX, VMS, MicroVAX, VAXserver
                VAXstation, Rdb/VMS, ULTRIX, DECnet, VAX ACMS,
                VAX FORTRAN, VAX DATATRIEVE, VAX DIBOL, VAX RALLY,
                VAX TEAMDATA, DEC, CDD/Plus, VAX Ada, VAX BASIC,
                VAX COBOL, VAX C and VAX Pascal are trademarks of
                Digital Equipment Corporation.




























                                       9
